IFC building model
Schema: "IFC4"
Description: "ViewDefinition [DesignTransferView_V1.0]"
File name: "2018_01"
Time stamp: "2020-09-04T17:37:24"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20190108_1515(x64) - Exporter 19.3.0.0 - Alternative Benutzeroberfläche 19.3.0.0"
Application: "Autodesk Revit 2019 (DEU)" version "2019" identifier "Revit" by Organization "Autodesk Revit 2019 (DEU)"

People and organizations
  Person "lubocholt" of Organization (no name given)
  Owner history of Person "lubocholt" of Organization (no name given) | application "Autodesk Revit 2019 (DEU)" version "2019" identifier "Revit" by Organization "Autodesk Revit 2019 (DEU)" | change NOCHANGE | created 1582881606 (2020-02-28T09:20:06Z)

Units
  LENGTHUNIT: METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  CURRENCY: €
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived

Spatial structure
IFCPROJECT "2018_01" | phase "Projekt Status"
  IFCSITE "Default" | latitude 48° 8′ 15.359802″ | longitude 11° 34′ 47.783432″ | elevation above sea level 519.
    IFCBUILDING
      IFCBUILDINGSTOREY "B01_OKRD" | long name "B01_OKRD" | object type "Ebene:Ebene" | elevation -3.37
        contains 65 elements
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Oberfläche:2437498" | names: "Oberfläche:2437498"
          4 x IFCWALL | type IFCWALLTYPE "Basiswand:STB 300" | object type "Basiswand:STB 300" | names: "Basiswand:STB 300:2397830", "Basiswand:STB 300:2397918", "Basiswand:STB 300:2397985" (+1 more) | material: layers "Basiswand:STB 300" ("Ortbeton - bewehrt Verputzt" 0.3) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCSLAB | type IFCSLABTYPE "Bodenplatte:STB 300" | object type "Bodenplatte:STB 300" | BASESLAB | names: "Bodenplatte:STB 300:2398103" | material: layers "Bodenplatte:STB 300" ("Ortbeton - bewehrt" 0.3) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSTAIR | type IFCSTAIRTYPE "Fertigbetontreppe:Fertigbetontreppe - 2 Stockwerkstrennlinien" | object type "Fertigbetontreppe:Fertigbetontreppe - 2 Stockwerkstrennlinien" | HALF_TURN_STAIR | names: "Fertigbetontreppe:Treppe:2421041" | parts: 2 IFCSTAIRFLIGHT, 1 IFCRAILING, 1 IFCSLAB | property sets: Pset_EnvironmentalImpactIndicators, Pset_StairCommon, Pset_StairFlightCommon
          15 x IFCWALL | type IFCWALLTYPE "Basiswand:STB 200" | object type "Basiswand:STB 200" | names: "Basiswand:STB 200:2421082", "Basiswand:STB 200:2421085", "Basiswand:STB 200:2421086" (+12 more) | material: layers "Basiswand:STB 200" ("Ortbeton - bewehrt" 0.2) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          7 x IFCWALL | type IFCWALLTYPE "Basiswand:STB 250" | object type "Basiswand:STB 250" | names: "Basiswand:STB 250:2421084", "Basiswand:STB 250:2423926", "Basiswand:STB 250:2433081" (+4 more) | material: layers "Basiswand:STB 250" ("Ortbeton - bewehrt" 0.25) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCSTAIR | type IFCSTAIRTYPE "Fertigbetontreppe:Fertigbetontreppe - 2 Stockwerkstrennlinien" | object type "Fertigbetontreppe:Fertigbetontreppe - 2 Stockwerkstrennlinien" | HALF_TURN_STAIR | names: "Fertigbetontreppe:Treppe:2423887" | parts: 2 IFCSTAIRFLIGHT, 1 IFCRAILING, 1 IFCSLAB | property sets: Pset_EnvironmentalImpactIndicators, Pset_StairCommon, Pset_StairFlightCommon
          5 x IFCDOOR | type IFCDOORTYPE "TU DF 1 - Rahmenstock flächenbündig:DL - 1000 x 2000" | object type "TU DF 1 - Rahmenstock flächenbündig:DL - 1000 x 2000" | DOOR | SINGLE_SWING_LEFT | names: "TU DF 1 - Rahmenstock flächenbündig:DL - 1000 x 2000:2432934", "TU DF 1 - Rahmenstock flächenbündig:DL - 1000 x 2000:2433295", "TU DF 1 - Rahmenstock flächenbündig:DL - 1000 x 2000:2434521" (+2 more) | material: constituents "MaterialConstituentSet" ("Holz - generisch 140-100-70": "Holz - generisch 140-100-70", "Metall - Edelstahl gebürstet": "Metall - Edelstahl gebürstet", "Lack - grau 80-80-80": "Lack - grau 80-80-80") | property sets: Pset_DoorCommon, Pset_DoorWindowGlazingType, Pset_EnvironmentalImpactIndicators
          1 x IFCDOOR | type IFCDOORTYPE "TU Durchgang:DL - 1200 x 2100" | object type "TU Durchgang:DL - 1200 x 2100" | DOOR | names: "TU Durchgang:DL - 1200 x 2100:2432935" | property sets: Pset_DoorCommon, Pset_EnvironmentalImpactIndicators
          8 x IFCDOOR | type IFCDOORTYPE "TU DF 1 - Rahmenstock flächenbündig:DL - 1000 x 2000" | object type "TU DF 1 - Rahmenstock flächenbündig:DL - 1000 x 2000" | DOOR | SINGLE_SWING_RIGHT | names: "TU DF 1 - Rahmenstock flächenbündig:DL - 1000 x 2000:2432938", "TU DF 1 - Rahmenstock flächenbündig:DL - 1000 x 2000:2432971", "TU DF 1 - Rahmenstock flächenbündig:DL - 1000 x 2000:2434145" (+5 more) | material: constituents "MaterialConstituentSet" ("Holz - generisch 140-100-70": "Holz - generisch 140-100-70", "Metall - Edelstahl gebürstet": "Metall - Edelstahl gebürstet", "Lack - grau 80-80-80": "Lack - grau 80-80-80") | property sets: Pset_DoorCommon, Pset_DoorWindowGlazingType, Pset_EnvironmentalImpactIndicators
          1 x IFCDOOR | type IFCDOORTYPE "TU Durchgang:DL - 1200 x 2100" | object type "TU Durchgang:DL - 1200 x 2100" | DOOR | names: "TU Durchgang:DL - 1200 x 2100:2432939" | property sets: Pset_DoorCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Plattenkante:Rechteckig_300x250" | object type "Plattenkante:Rechteckig_300x250" | names: "Plattenkante:Rechteckig_300x250:2436806" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCSLAB | type IFCSLABTYPE "Sohle:Sohle 1 mm" | object type "Sohle:Sohle 1 mm" | FLOOR | names: "Sohle:Sohle 1 mm:2437499" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Oberfläche:2437789" | names: "Oberfläche:2437789"
          1 x IFCSLAB | type IFCSLABTYPE "Sohle:Sohle 1 mm" | object type "Sohle:Sohle 1 mm" | FLOOR | names: "Sohle:Sohle 1 mm:2437790" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Geschossdecke:FB 100 leer" | object type "Geschossdecke:FB 100 leer" | FLOOR | names: "Geschossdecke:FB 100 leer:2438670" | material: layers "Geschossdecke:FB 100 leer" ("Fußbodenaufbau" 0.1) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          12 x IFCWALL | type IFCWALLTYPE "Basiswand:WD hart 200" | object type "Basiswand:WD hart 200" | names: "Basiswand:WD hart 200:2720250", "Basiswand:WD hart 200:2720354", "Basiswand:WD hart 200:2720413" (+9 more) | material: layers "Basiswand:WD hart 200" ("Dämmung - hart" 0.2) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCSLAB | type IFCSLABTYPE "Geschossdecke:WD 200 hart" | object type "Geschossdecke:WD 200 hart" | FLOOR | names: "Geschossdecke:WD 200 hart:2720852" | material: layers "Geschossdecke:WD 200 hart" ("Dämmung - hart" 0.2) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Geschossdecke:WD 200 hart" | object type "Geschossdecke:WD 200 hart" | FLOOR | names: "Geschossdecke:WD 200 hart:2721280" | material: layers "Geschossdecke:WD 200 hart" ("Dämmung - hart" 0.2) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Geschossdecke:STB 200 + WD 200" | object type "Geschossdecke:STB 200 + WD 200" | FLOOR | names: "Geschossdecke:STB 200 + WD 200:2751473" | material: layers "Geschossdecke:STB 200 + WD 200" ("Ortbeton - bewehrt" 0.2, "Dämmung - hart" 0.2) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
        IFCSPACE "0-1" | long name "Flur - UG" | SPACE
        IFCSPACE "0-2" | long name "Putzmittel" | SPACE
        IFCSPACE "0-3" | long name "Hausanschluss" | SPACE
        IFCSPACE "0-4" | long name "Wasser-/Gasverteilung" | SPACE
        IFCSPACE "0-5" | long name "Heizzentrale" | SPACE
        IFCSPACE "0-6" | long name "NSHV" | SPACE
        IFCSPACE "0-7" | long name "Lager 1" | SPACE
        IFCSPACE "0-8" | long name "Lager2" | SPACE
        IFCSPACE "0-9" | long name "BMZ" | SPACE
        IFCSPACE "0-10" | long name "RLT-Raum" | SPACE
        IFCSPACE "0-11" | long name "Treppenhaus Ost - UG" | SPACE
        IFCSPACE "0-12" | long name "Treppenhaus West - UG" | SPACE
      IFCBUILDINGSTOREY "E00_OKRD" | long name "E00_OKRD" | object type "Ebene:Ebene" | elevation -0.15
        contains 316 elements
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 400" | object type "STB Stütze - rechteckig:STB 250 x 400" | COLUMN | names: "STB Stütze - rechteckig:STB 250 x 400:2395272" | material: profiles "STB 250 x 400" ("STB 250 x 400": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 400" | object type "STB Stütze - rechteckig:STB 250 x 400" | COLUMN | names: "STB Stütze - rechteckig:STB 250 x 400:2395469" | material: profiles "STB 250 x 400" ("STB 250 x 400": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 400" | object type "STB Stütze - rechteckig:STB 250 x 400" | COLUMN | names: "STB Stütze - rechteckig:STB 250 x 400:2395484" | material: profiles "STB 250 x 400" ("STB 250 x 400": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 400" | object type "STB Stütze - rechteckig:STB 250 x 400" | COLUMN | names: "STB Stütze - rechteckig:STB 250 x 400:2395499" | material: profiles "STB 250 x 400" ("STB 250 x 400": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 400" | object type "STB Stütze - rechteckig:STB 250 x 400" | COLUMN | names: "STB Stütze - rechteckig:STB 250 x 400:2395514" | material: profiles "STB 250 x 400" ("STB 250 x 400": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 400" | object type "STB Stütze - rechteckig:STB 250 x 400" | COLUMN | names: "STB Stütze - rechteckig:STB 250 x 400:2395527" | material: profiles "STB 250 x 400" ("STB 250 x 400": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 400" | object type "STB Stütze - rechteckig:STB 250 x 400" | COLUMN | names: "STB Stütze - rechteckig:STB 250 x 400:2395565" | material: profiles "STB 250 x 400" ("STB 250 x 400": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 400" | object type "STB Stütze - rechteckig:STB 250 x 400" | COLUMN | names: "STB Stütze - rechteckig:STB 250 x 400:2395567" | material: profiles "STB 250 x 400" ("STB 250 x 400": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 400" | object type "STB Stütze - rechteckig:STB 250 x 400" | COLUMN | names: "STB Stütze - rechteckig:STB 250 x 400:2395569" | material: profiles "STB 250 x 400" ("STB 250 x 400": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 400" | object type "STB Stütze - rechteckig:STB 250 x 400" | COLUMN | names: "STB Stütze - rechteckig:STB 250 x 400:2395571" | material: profiles "STB 250 x 400" ("STB 250 x 400": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 400" | object type "STB Stütze - rechteckig:STB 250 x 400" | COLUMN | names: "STB Stütze - rechteckig:STB 250 x 400:2395573" | material: profiles "STB 250 x 400" ("STB 250 x 400": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 400" | object type "STB Stütze - rechteckig:STB 250 x 400" | COLUMN | names: "STB Stütze - rechteckig:STB 250 x 400:2395575" | material: profiles "STB 250 x 400" ("STB 250 x 400": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          2 x IFCCOLUMN | type IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 250" | object type "STB Stütze - rechteckig:STB 250 x 250" | COLUMN | names: "STB Stütze - rechteckig:STB 250 x 250:2395932", "STB Stütze - rechteckig:STB 250 x 250:2396022" | material: profiles "STB 250 x 250" ("STB 250 x 250": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 250" | object type "STB Stütze - rechteckig:STB 250 x 250" | COLUMN | names: "STB Stütze - rechteckig:STB 250 x 250:2396101" | material: profiles "STB 250 x 250" ("STB 250 x 250": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 250" | object type "STB Stütze - rechteckig:STB 250 x 250" | COLUMN | names: "STB Stütze - rechteckig:STB 250 x 250:2396170" | material: profiles "STB 250 x 250" ("STB 250 x 250": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 250" | object type "STB Stütze - rechteckig:STB 250 x 250" | COLUMN | names: "STB Stütze - rechteckig:STB 250 x 250:2396259" | material: profiles "STB 250 x 250" ("STB 250 x 250": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 250" | object type "STB Stütze - rechteckig:STB 250 x 250" | COLUMN | names: "STB Stütze - rechteckig:STB 250 x 250:2396380" | material: profiles "STB 250 x 250" ("STB 250 x 250": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 250" | object type "STB Stütze - rechteckig:STB 250 x 250" | COLUMN | names: "STB Stütze - rechteckig:STB 250 x 250:2396427" | material: profiles "STB 250 x 250" ("STB 250 x 250": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 250" | object type "STB Stütze - rechteckig:STB 250 x 250" | COLUMN | names: "STB Stütze - rechteckig:STB 250 x 250:2396482" | material: profiles "STB 250 x 250" ("STB 250 x 250": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          1 x IFCSLAB | type IFCSLABTYPE "Geschossdecke:STB 220" | object type "Geschossdecke:STB 220" | FLOOR | names: "Geschossdecke:STB 220:2397091" | material: layers "Geschossdecke:STB 220" ("Ortbeton - bewehrt" 0.22) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCBEAM | type IFCBEAMTYPE "STB Träger - rechteckig:STB 250 x 500" | object type "STB Träger - rechteckig:STB 250 x 500" | BEAM | names: "STB Träger - rechteckig:STB 250 x 500:2401047" | material: profiles "STB 250 x 500" ("STB 250 x 500": "Ortbeton - bewehrt") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "STB Träger - rechteckig:STB 250 x 500" | object type "STB Träger - rechteckig:STB 250 x 500" | BEAM | names: "STB Träger - rechteckig:STB 250 x 500:2401049" | material: profiles "STB 250 x 500" ("STB 250 x 500": "Ortbeton - bewehrt") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "STB Träger - rechteckig:STB 250 x 500" | object type "STB Träger - rechteckig:STB 250 x 500" | BEAM | names: "STB Träger - rechteckig:STB 250 x 500:2401051" | material: profiles "STB 250 x 500" ("STB 250 x 500": "Ortbeton - bewehrt") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "STB Träger - rechteckig:STB 250 x 500" | object type "STB Träger - rechteckig:STB 250 x 500" | BEAM | names: "STB Träger - rechteckig:STB 250 x 500:2418716" | material: profiles "STB 250 x 500" ("STB 250 x 500": "Ortbeton - bewehrt") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "STB Träger - rechteckig:STB 250 x 500" | object type "STB Träger - rechteckig:STB 250 x 500" | BEAM | names: "STB Träger - rechteckig:STB 250 x 500:2418767" | material: profiles "STB 250 x 500" ("STB 250 x 500": "Ortbeton - bewehrt") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "STB Träger - rechteckig:STB 250 x 500" | object type "STB Träger - rechteckig:STB 250 x 500" | BEAM | names: "STB Träger - rechteckig:STB 250 x 500:2418820" | material: profiles "STB 250 x 500" ("STB 250 x 500": "Ortbeton - bewehrt") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 400" | object type "STB Stütze - rechteckig:STB 250 x 400" | COLUMN | names: "STB Stütze - rechteckig:STB 250 x 400:2419951" | material: profiles "STB 250 x 400" ("STB 250 x 400": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 400" | object type "STB Stütze - rechteckig:STB 250 x 400" | COLUMN | names: "STB Stütze - rechteckig:STB 250 x 400:2419953" | material: profiles "STB 250 x 400" ("STB 250 x 400": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 400" | object type "STB Stütze - rechteckig:STB 250 x 400" | COLUMN | names: "STB Stütze - rechteckig:STB 250 x 400:2420031" | material: profiles "STB 250 x 400" ("STB 250 x 400": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 400" | object type "STB Stütze - rechteckig:STB 250 x 400" | COLUMN | names: "STB Stütze - rechteckig:STB 250 x 400:2420033" | material: profiles "STB 250 x 400" ("STB 250 x 400": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          10 x IFCWALL | type IFCWALLTYPE "Basiswand:STB 250" | object type "Basiswand:STB 250" | names: "Basiswand:STB 250:2421031", "Basiswand:STB 250:2421032", "Basiswand:STB 250:2421033" (+7 more) | material: layers "Basiswand:STB 250" ("Ortbeton - bewehrt" 0.25) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          10 x IFCWALL | type IFCWALLTYPE "Basiswand:STB 200" | object type "Basiswand:STB 200" | names: "Basiswand:STB 200:2421057", "Basiswand:STB 200:2421058", "Basiswand:STB 200:2421075" (+7 more) | material: layers "Basiswand:STB 200" ("Ortbeton - bewehrt" 0.2) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCSTAIR | type IFCSTAIRTYPE "Fertigbetontreppe:Fertigbetontreppe - 2 Stockwerkstrennlinien" | object type "Fertigbetontreppe:Fertigbetontreppe - 2 Stockwerkstrennlinien" | HALF_TURN_STAIR | names: "Fertigbetontreppe:Treppe:2421059" | parts: 2 IFCSTAIRFLIGHT, 1 IFCRAILING, 1 IFCSLAB | property sets: Pset_EnvironmentalImpactIndicators, Pset_StairCommon, Pset_StairFlightCommon
          2 x IFCDOOR | type IFCDOORTYPE "TU DF 1 - Fluchttüre Endausgang:EN 179 - ML - 1010 x 2250" | object type "TU DF 1 - Fluchttüre Endausgang:EN 179 - ML - 1010 x 2250" | DOOR | SINGLE_SWING_LEFT | names: "TU DF 1 - Fluchttüre Endausgang:EN 179 - ML - 1010 x 2250:2421088", "TU DF 1 - Fluchttüre Endausgang:EN 179 - ML - 1010 x 2250:2423931" | material: constituents "MaterialConstituentSet" ("Metall - Edelstahl gebürstet": "Metall - Edelstahl gebürstet", "Kunststoff - weiß 250-250-250": "Kunststoff - weiß 250-250-250", "Metall - Edelstahl satiniert": "Metall - Edelstahl satiniert", "Lack - grau 80-80-80": "Lack - grau 80-80-80", "Dämmung - hart": "Dämmung - hart") | property sets: Pset_DoorCommon, Pset_DoorWindowGlazingType, Pset_EnvironmentalImpactIndicators
          2 x IFCDOOR | type IFCDOORTYPE "TU DF 1 - Fluchttüre Endausgang:EN 179 - ML - 1010 x 2250" | object type "TU DF 1 - Fluchttüre Endausgang:EN 179 - ML - 1010 x 2250" | DOOR | SINGLE_SWING_RIGHT | names: "TU DF 1 - Fluchttüre Endausgang:EN 179 - ML - 1010 x 2250:2421089", "TU DF 1 - Fluchttüre Endausgang:EN 179 - ML - 1010 x 2250:2423930" | material: constituents "MaterialConstituentSet" ("Metall - Edelstahl gebürstet": "Metall - Edelstahl gebürstet", "Kunststoff - weiß 250-250-250": "Kunststoff - weiß 250-250-250", "Metall - Edelstahl satiniert": "Metall - Edelstahl satiniert", "Lack - grau 80-80-80": "Lack - grau 80-80-80", "Dämmung - hart": "Dämmung - hart") | property sets: Pset_DoorCommon, Pset_DoorWindowGlazingType, Pset_EnvironmentalImpactIndicators
          1 x IFCDOOR | type IFCDOORTYPE "TU Durchgang:DL - 1200 x 2100" | object type "TU Durchgang:DL - 1200 x 2100" | DOOR | names: "TU Durchgang:DL - 1200 x 2100:2421090" | property sets: Pset_DoorCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCDOOR | type IFCDOORTYPE "TU DF 1 - Fluchttüre Endausgang:EN 179 - ML - 1010 x 2250" | object type "TU DF 1 - Fluchttüre Endausgang:EN 179 - ML - 1010 x 2250" | DOOR | SINGLE_SWING_RIGHT | names: "TU DF 1 - Fluchttüre Endausgang:EN 179 - ML - 1010 x 2250:2421363" | material: constituents "MaterialConstituentSet" ("Metall - Edelstahl gebürstet": "Metall - Edelstahl gebürstet", "Kunststoff - weiß 250-250-250": "Kunststoff - weiß 250-250-250", "Metall - Edelstahl satiniert": "Metall - Edelstahl satiniert", "Lack - grau 80-80-80": "Lack - grau 80-80-80", "Dämmung - hart": "Dämmung - hart") | property sets: Pset_DoorCommon, Pset_DoorWindowGlazingType, Pset_EnvironmentalImpactIndicators
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 250" | object type "STB Stütze - rechteckig:STB 250 x 250" | COLUMN | names: "STB Stütze - rechteckig:STB 250 x 250:2421639" | material: profiles "STB 250 x 250" ("STB 250 x 250": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 250" | object type "STB Stütze - rechteckig:STB 250 x 250" | COLUMN | names: "STB Stütze - rechteckig:STB 250 x 250:2421693" | material: profiles "STB 250 x 250" ("STB 250 x 250": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 250" | object type "STB Stütze - rechteckig:STB 250 x 250" | COLUMN | names: "STB Stütze - rechteckig:STB 250 x 250:2421772" | material: profiles "STB 250 x 250" ("STB 250 x 250": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 250" | object type "STB Stütze - rechteckig:STB 250 x 250" | COLUMN | names: "STB Stütze - rechteckig:STB 250 x 250:2421823" | material: profiles "STB 250 x 250" ("STB 250 x 250": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          1 x IFCSTAIR | type IFCSTAIRTYPE "Fertigbetontreppe:Fertigbetontreppe - 2 Stockwerkstrennlinien" | object type "Fertigbetontreppe:Fertigbetontreppe - 2 Stockwerkstrennlinien" | HALF_TURN_STAIR | names: "Fertigbetontreppe:Treppe:2423903" | parts: 2 IFCSTAIRFLIGHT, 1 IFCRAILING, 1 IFCSLAB | property sets: Pset_EnvironmentalImpactIndicators, Pset_StairCommon, Pset_StairFlightCommon
          1 x IFCDOOR | type IFCDOORTYPE "TU Durchgang:DL - 1200 x 2100" | object type "TU Durchgang:DL - 1200 x 2100" | DOOR | names: "TU Durchgang:DL - 1200 x 2100:2423932" | property sets: Pset_DoorCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCDOOR | type IFCDOORTYPE "TU DF 1 - Fluchttüre Endausgang:EN 179 - ML - 1010 x 2250" | object type "TU DF 1 - Fluchttüre Endausgang:EN 179 - ML - 1010 x 2250" | DOOR | SINGLE_SWING_LEFT | names: "TU DF 1 - Fluchttüre Endausgang:EN 179 - ML - 1010 x 2250:2423939" | material: constituents "MaterialConstituentSet" ("Metall - Edelstahl gebürstet": "Metall - Edelstahl gebürstet", "Kunststoff - weiß 250-250-250": "Kunststoff - weiß 250-250-250", "Metall - Edelstahl satiniert": "Metall - Edelstahl satiniert", "Lack - grau 80-80-80": "Lack - grau 80-80-80", "Dämmung - hart": "Dämmung - hart") | property sets: Pset_DoorCommon, Pset_DoorWindowGlazingType, Pset_EnvironmentalImpactIndicators
          1 x IFCSTAIR | type IFCSTAIRTYPE "Zusammengebaute Treppe:Wangen Stahl - Stufen Stahl - 2 Stockwerkstrennlinien" | object type "Zusammengebaute Treppe:Wangen Stahl - Stufen Stahl - 2 Stockwerkstrennlinien" | HALF_TURN_STAIR | names: "Zusammengebaute Treppe:Treppe:2424673" | parts: 8 IFCMEMBER, 2 IFCRAILING, 2 IFCSTAIRFLIGHT, 1 IFCSLAB | property sets: Pset_EnvironmentalImpactIndicators, Pset_StairCommon, Pset_StairFlightCommon
          1 x IFCSLAB | type IFCSLABTYPE "Geschossdecke:FB 150 leer" | object type "Geschossdecke:FB 150 leer" | FLOOR | names: "Geschossdecke:FB 150 leer:2428424" | material: layers "Geschossdecke:FB 150 leer" ("Fußbodenaufbau" 0.15) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Geschossdecke:FB 150 leer" | object type "Geschossdecke:FB 150 leer" | FLOOR | names: "Geschossdecke:FB 150 leer:2431108" | material: layers "Geschossdecke:FB 150 leer" ("Fußbodenaufbau" 0.15) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Geschossdecke:FB 150 leer" | object type "Geschossdecke:FB 150 leer" | FLOOR | names: "Geschossdecke:FB 150 leer:2431503" | material: layers "Geschossdecke:FB 150 leer" ("Fußbodenaufbau" 0.15) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 250" | object type "STB Stütze - rechteckig:STB 250 x 250" | COLUMN | names: "STB Stütze - rechteckig:STB 250 x 250:2434069" | material: profiles "STB 250 x 250" ("STB 250 x 250": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 250" | object type "STB Stütze - rechteckig:STB 250 x 250" | COLUMN | names: "STB Stütze - rechteckig:STB 250 x 250:2434111" | material: profiles "STB 250 x 250" ("STB 250 x 250": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          1 x IFCSLAB | type IFCSLABTYPE "Geschossdecke:STB 220" | object type "Geschossdecke:STB 220" | FLOOR | names: "Geschossdecke:STB 220:2437032" | material: layers "Geschossdecke:STB 220" ("Ortbeton - bewehrt" 0.22) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Unterregion:2439145" | names: "Unterregion:2439145"
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Oberfläche:2439928" | names: "Oberfläche:2439928"
          1 x IFCSLAB | type IFCSLABTYPE "Sohle:Sohle 1 mm" | object type "Sohle:Sohle 1 mm" | FLOOR | names: "Sohle:Sohle 1 mm:2439929" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Oberfläche:2440033" | names: "Oberfläche:2440033"
          13 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Parkplatz - 01 90:2500 x 5000" | object type "Parkplatz - 01 90:2500 x 5000" | names: "Parkplatz - 01 90:2500 x 5000:2440801", "Parkplatz - 01 90:2500 x 5000:2440915", "Parkplatz - 01 90:2500 x 5000:2440923" (+10 more) | material: "Farbe - Straßenmarkierung weiß" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators, Pset_ProvisionForVoid
          13 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Parkplatz - 01 90:2500 x 5000" | object type "Parkplatz - 01 90:2500 x 5000" | names: "Parkplatz - 01 90:2500 x 5000:2441054", "Parkplatz - 01 90:2500 x 5000:2441055", "Parkplatz - 01 90:2500 x 5000:2441056" (+10 more) | material: "Farbe - Straßenmarkierung weiß" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators, Pset_ProvisionForVoid
          45 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Markierung:B 120" | object type "Markierung:B 120" | names: "Markierung:B 120:2442929", "Markierung:B 120:2442993", "Markierung:B 120:2443013" (+42 more) | material: "Farbe - Straßenmarkierung" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators, Pset_ProvisionForVoid
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Richtungspfeil - Abzweigung und geradeaus:Typ1" | object type "Richtungspfeil - Abzweigung und geradeaus:Typ1" | names: "Richtungspfeil - Abzweigung und geradeaus:Typ1:2444438" | material: "Farbe - Straßenmarkierung" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators, Pset_ProvisionForVoid
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Richtungspfeil - Abzweigung und geradeaus:Typ1" | object type "Richtungspfeil - Abzweigung und geradeaus:Typ1" | names: "Richtungspfeil - Abzweigung und geradeaus:Typ1:2444764" | material: "Farbe - Straßenmarkierung" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators, Pset_ProvisionForVoid
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "PKW Verkehrsinsel Schranken Ein-Ausfahrt:Typ1" | object type "PKW Verkehrsinsel Schranken Ein-Ausfahrt:Typ1" | names: "PKW Verkehrsinsel Schranken Ein-Ausfahrt:Typ1:2448711" | material: constituents "MaterialConstituentSet" ("Dachdeckung - Kies": "Dachdeckung - Kies", "Naturstein - Granit grau": "Naturstein - Granit grau", "Kunststoff - weiß 250-250-250": "Kunststoff - weiß 250-250-250", "Kunststoff - grau 50-50-50": "Kunststoff - grau 50-50-50", "Lack - rot 255-51-0": "Lack - rot 255-51-0", "Metall - Zink": "Metall - Zink", "Metall - Edelstahl satiniert": "Metall - Edelstahl satiniert") | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          13 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "E-Ladestation - 03:Typ1" | object type "E-Ladestation - 03:Typ1" | names: "E-Ladestation - 03:Typ1:2450207", "E-Ladestation - 03:Typ1:2451006", "E-Ladestation - 03:Typ1:2451015" (+10 more) | material: constituents "MaterialConstituentSet" ("Kunststoff - grau 50-50-50": "Kunststoff - grau 50-50-50", "Metall - Edelstahl satiniert": "Metall - Edelstahl satiniert", "Kunststoff - blau 51-79-234": "Kunststoff - blau 51-79-234", "Kunststoff - weiß 250-250-250": "Kunststoff - weiß 250-250-250") | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          26 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Anfahrschutz Rohr:1000 x 700" | object type "Anfahrschutz Rohr:1000 x 700" | names: "Anfahrschutz Rohr:1000 x 700:2450788", "Anfahrschutz Rohr:1000 x 700:2450815", "Anfahrschutz Rohr:1000 x 700:2450822" (+23 more) | material: "Metall - Zink" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          5 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Radständer - 04:3000, 5 Räder" | object type "Radständer - 04:3000, 5 Räder" | names: "Radständer - 04:3000, 5 Räder:2452406", "Radständer - 04:3000, 5 Räder:2452480", "Radständer - 04:3000, 5 Räder:2452739" (+2 more) | material: "Metall - Edelstahl satiniert" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators, Pset_ProvisionForVoid
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Fahrrad - Rennrad:Typ1" | object type "Fahrrad - Rennrad:Typ1" | names: "Fahrrad - Rennrad:Typ1:2454038", "Fahrrad - Rennrad:Typ1:2454141" | material: constituents "MaterialConstituentSet" ("Metall - Edelstahl satiniert": "Metall - Edelstahl satiniert", "Kunststoff - grau 50-50-50": "Kunststoff - grau 50-50-50", "Autodesk Sky Blue 6-150-215": "Autodesk Sky Blue 6-150-215", "Kunststoff - grau 70-70-70": "Kunststoff - grau 70-70-70") | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Unterregion:2454499" | names: "Unterregion:2454499"
          17 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Baum RPC - Laubbaum:Rotesche - 7,6 Meter" | object type "Baum RPC - Laubbaum:Rotesche - 7,6 Meter" | names: "Baum RPC - Laubbaum:Rotesche - 7,6 Meter:2455374", "Baum RPC - Laubbaum:Rotesche - 7,6 Meter:2455382", "Baum RPC - Laubbaum:Rotesche - 7,6 Meter:2455390" (+14 more) | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Unterregion:2460265" | names: "Unterregion:2460265"
          6 x IFCWALL | type IFCWALLTYPE "Basiswand:Leichtbetonmauerwerk 250" | object type "Basiswand:Leichtbetonmauerwerk 250" | names: "Basiswand:Leichtbetonmauerwerk 250:2516516", "Basiswand:Leichtbetonmauerwerk 250:2516624", "Basiswand:Leichtbetonmauerwerk 250:2516752" (+3 more) | material: layers "Basiswand:Leichtbetonmauerwerk 250" ("Leichtbeton - Mauerwerk" 0.25) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          4 x IFCWALL | type IFCWALLTYPE "Basiswand:WD 200 + Luft 40 + Bekleidung 12" | object type "Basiswand:WD 200 + Luft 40 + Bekleidung 12" | names: "Basiswand:WD 200 + Luft 40 + Bekleidung 12:2518046", "Basiswand:WD 200 + Luft 40 + Bekleidung 12:2518180", "Basiswand:WD 200 + Luft 40 + Bekleidung 12:2518308" (+1 more) | material: layers "Basiswand:WD 200 + Luft 40 + Bekleidung 12" ("Faserzementplatte (Equitone - natura)" 0.012, "Luftschicht" 0.04, "Steinwolle (Rockwool Fixrock033 VS)" 0.2) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Fassade:Standard" | object type "Fassade:Standard" | names: "Fassade:Standard:2542860" | parts: 18 IFCMEMBER, 5 IFCPLATE, 2 IFCDOOR | property sets: Pset_CurtainWallCommon, Pset_EnvironmentalImpactIndicators
          16 x IFCWINDOW | type IFCWINDOWTYPE "FE 3 tlg - DK-Fix im Rahmen-DK-2:6000 x 1500" | object type "FE 3 tlg - DK-Fix im Rahmen-DK-2:6000 x 1500" | WINDOW | names: "FE 3 tlg - DK-Fix im Rahmen-DK-2:6000 x 1500:2543664", "FE 3 tlg - DK-Fix im Rahmen-DK-2:6000 x 1500:2543665", "FE 3 tlg - DK-Fix im Rahmen-DK-2:6000 x 1500:2543666" (+13 more) | material: constituents "MaterialConstituentSet" ("Metall - Edelstahl gebürstet": "Metall - Edelstahl gebürstet", "Kunststoff - grau 70-70-70": "Kunststoff - grau 70-70-70", "Glas - Isolierverglasung klar": "Glas - Isolierverglasung klar", "Holz - generisch 140-100-70": "Holz - generisch 140-100-70") | property sets: Pset_EnvironmentalImpactIndicators, Pset_OpeningElementCommon
          1 x IFCWINDOW | type IFCWINDOWTYPE "FE 3 tlg - DK-Fix im Rahmen-DK-2:6000 x 1500" | object type "FE 3 tlg - DK-Fix im Rahmen-DK-2:6000 x 1500" | WINDOW | names: "FE 3 tlg - DK-Fix im Rahmen-DK-2:6000 x 1500:2545646" | material: constituents "MaterialConstituentSet" ("Metall - Edelstahl gebürstet": "Metall - Edelstahl gebürstet", "Kunststoff - grau 70-70-70": "Kunststoff - grau 70-70-70", "Glas - Isolierverglasung klar": "Glas - Isolierverglasung klar", "Holz - generisch 140-100-70": "Holz - generisch 140-100-70") | property sets: Pset_EnvironmentalImpactIndicators, Pset_OpeningElementCommon
          19 x IFCWALL | type IFCWALLTYPE "Basiswand:Metall-Einfachständerwand 2-lagig beplankt (MW12BF)" | object type "Basiswand:Metall-Einfachständerwand 2-lagig beplankt (MW12BF)" | names: "Basiswand:Metall-Einfachständerwand 2-lagig beplankt (MW12BF):2546401", "Basiswand:Metall-Einfachständerwand 2-lagig beplankt (MW12BF):2546889", "Basiswand:Metall-Einfachständerwand 2-lagig beplankt (MW12BF):2547526" (+16 more) | material: layers "Basiswand:Metall-Einfachständerwand 2-lagig beplankt (MW12BF)" ("Trockenbau - Rigips Die Blaue RFI" 0.025, "Dämmung - Isover Akustik TF" 0.08, "Luftschicht" 0.02, "Trockenbau - Rigips Die Blaue RFI" 0.025) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          6 x IFCDOOR | type IFCDOORTYPE "TU DF 1 - Rahmenstock flächenbündig:DL - 1000 x 2000" | object type "TU DF 1 - Rahmenstock flächenbündig:DL - 1000 x 2000" | DOOR | SINGLE_SWING_RIGHT | names: "TU DF 1 - Rahmenstock flächenbündig:DL - 1000 x 2000:2549490", "TU DF 1 - Rahmenstock flächenbündig:DL - 1000 x 2000:2549587", "TU DF 1 - Rahmenstock flächenbündig:DL - 1000 x 2000:2549876" (+3 more) | material: constituents "MaterialConstituentSet" ("Holz - generisch 140-100-70": "Holz - generisch 140-100-70", "Metall - Edelstahl gebürstet": "Metall - Edelstahl gebürstet", "Lack - grau 80-80-80": "Lack - grau 80-80-80") | property sets: Pset_DoorCommon, Pset_DoorWindowGlazingType, Pset_EnvironmentalImpactIndicators
          6 x IFCDOOR | type IFCDOORTYPE "TU DF 1 - Rahmenstock flächenbündig:DL - 1000 x 2000" | object type "TU DF 1 - Rahmenstock flächenbündig:DL - 1000 x 2000" | DOOR | SINGLE_SWING_LEFT | names: "TU DF 1 - Rahmenstock flächenbündig:DL - 1000 x 2000:2549557", "TU DF 1 - Rahmenstock flächenbündig:DL - 1000 x 2000:2549631", "TU DF 1 - Rahmenstock flächenbündig:DL - 1000 x 2000:2550105" (+3 more) | material: constituents "MaterialConstituentSet" ("Holz - generisch 140-100-70": "Holz - generisch 140-100-70", "Metall - Edelstahl gebürstet": "Metall - Edelstahl gebürstet", "Lack - grau 80-80-80": "Lack - grau 80-80-80") | property sets: Pset_DoorCommon, Pset_DoorWindowGlazingType, Pset_EnvironmentalImpactIndicators, Pset_OpeningElementCommon
          1 x IFCDOOR | type IFCDOORTYPE "TU DF 2 - Rahmenstock flächenbündig:ML - 1635 x 2135" | object type "TU DF 2 - Rahmenstock flächenbündig:ML - 1635 x 2135" | DOOR | DOUBLE_DOOR_SINGLE_SWING | names: "TU DF 2 - Rahmenstock flächenbündig:ML - 1635 x 2135:2550600" | material: constituents "MaterialConstituentSet" ("Holz - generisch 140-100-70": "Holz - generisch 140-100-70", "Metall - Edelstahl gebürstet": "Metall - Edelstahl gebürstet", "Lack - grau 80-80-80": "Lack - grau 80-80-80") | property sets: Pset_DoorCommon, Pset_DoorWindowGlazingType, Pset_EnvironmentalImpactIndicators
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | object type "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | CEILING | names: "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25:2554837" | material: layers "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" ("Trockenbau - Rigips Die Dicke RFI" 0.025) | property sets: Pset_CoveringCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | object type "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | CEILING | names: "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25:2554917" | material: layers "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" ("Trockenbau - Rigips Die Dicke RFI" 0.025) | property sets: Pset_CoveringCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | object type "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | CEILING | names: "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25:2554958" | material: layers "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" ("Trockenbau - Rigips Die Dicke RFI" 0.025) | property sets: Pset_CoveringCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | object type "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | CEILING | names: "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25:2555175" | material: layers "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" ("Trockenbau - Rigips Die Dicke RFI" 0.025) | property sets: Pset_CoveringCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | object type "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | CEILING | names: "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25:2555207" | material: layers "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" ("Trockenbau - Rigips Die Dicke RFI" 0.025) | property sets: Pset_CoveringCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | object type "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | CEILING | names: "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25:2555722" | material: layers "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" ("Trockenbau - Rigips Die Dicke RFI" 0.025) | property sets: Pset_CoveringCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | object type "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | CEILING | names: "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25:2555774" | material: layers "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" ("Trockenbau - Rigips Die Dicke RFI" 0.025) | property sets: Pset_CoveringCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | object type "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | CEILING | names: "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25:2555831" | material: layers "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" ("Trockenbau - Rigips Die Dicke RFI" 0.025) | property sets: Pset_CoveringCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | object type "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | CEILING | names: "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25:2555870" | material: layers "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" ("Trockenbau - Rigips Die Dicke RFI" 0.025) | property sets: Pset_CoveringCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | object type "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | CEILING | names: "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25:2555920" | material: layers "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" ("Trockenbau - Rigips Die Dicke RFI" 0.025) | property sets: Pset_CoveringCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | object type "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | CEILING | names: "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25:2556004" | material: layers "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" ("Trockenbau - Rigips Die Dicke RFI" 0.025) | property sets: Pset_CoveringCommon, Pset_EnvironmentalImpactIndicators
          2 x IFCWINDOW | type IFCWINDOWTYPE "FE 2 tlg - DK Fix mit Pfosten - 2:4000 x 1500" | object type "FE 2 tlg - DK Fix mit Pfosten - 2:4000 x 1500" | WINDOW | names: "FE 2 tlg - DK Fix mit Pfosten - 2:4000 x 1500:2679447", "FE 2 tlg - DK Fix mit Pfosten - 2:4000 x 1500:2679448" | material: constituents "MaterialConstituentSet" ("Metall - Edelstahl gebürstet": "Metall - Edelstahl gebürstet", "Kunststoff - grau 70-70-70": "Kunststoff - grau 70-70-70", "Glas - Isolierverglasung klar": "Glas - Isolierverglasung klar", "Holz - generisch 140-100-70": "Holz - generisch 140-100-70") | property sets: Pset_EnvironmentalImpactIndicators, Pset_OpeningElementCommon
          2 x IFCWINDOW | type IFCWINDOWTYPE "FE 2 tlg - DK Fix mit Pfosten - 2:4000 x 1500" | object type "FE 2 tlg - DK Fix mit Pfosten - 2:4000 x 1500" | WINDOW | names: "FE 2 tlg - DK Fix mit Pfosten - 2:4000 x 1500:2679449", "FE 2 tlg - DK Fix mit Pfosten - 2:4000 x 1500:2679450" | material: constituents "MaterialConstituentSet" ("Metall - Edelstahl gebürstet": "Metall - Edelstahl gebürstet", "Kunststoff - grau 70-70-70": "Kunststoff - grau 70-70-70", "Glas - Isolierverglasung klar": "Glas - Isolierverglasung klar", "Holz - generisch 140-100-70": "Holz - generisch 140-100-70") | property sets: Pset_EnvironmentalImpactIndicators, Pset_OpeningElementCommon
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | object type "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | CEILING | names: "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25:2695208" | material: layers "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" ("Trockenbau - Rigips Die Dicke RFI" 0.025) | property sets: Pset_CoveringCommon, Pset_EnvironmentalImpactIndicators
          2 x IFCWALL | type IFCWALLTYPE "Basiswand:Metall-Einfachständerwand 2-lagig beplankt - Sanitär" | object type "Basiswand:Metall-Einfachständerwand 2-lagig beplankt - Sanitär" | names: "Basiswand:Metall-Einfachständerwand 2-lagig beplankt - Sanitär:2699455", "Basiswand:Metall-Einfachständerwand 2-lagig beplankt - Sanitär:2699813" | material: layers "Basiswand:Metall-Einfachständerwand 2-lagig beplankt - Sanitär" ("Trockenbau - Rigips Die Blaue RFI" 0.025, "Steinwolle (Rockwool Fixrock033 VS)" 0.08, "Luftschicht" 0.19, "Steinwolle (Rockwool Fixrock033 VS)" 0.08, "Trockenbau - Rigips Die Blaue RFI" 0.025) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          2 x IFCDOOR | type IFCDOORTYPE "TU DF 1 - Stahl-Eckzarge Falztüre:DL - 800 x 2000" | object type "TU DF 1 - Stahl-Eckzarge Falztüre:DL - 800 x 2000" | DOOR | SINGLE_SWING_RIGHT | names: "TU DF 1 - Stahl-Eckzarge Falztüre:DL - 800 x 2000:2699597", "TU DF 1 - Stahl-Eckzarge Falztüre:DL - 800 x 2000:2699876" | material: constituents "MaterialConstituentSet" ("Holz - generisch 140-100-70": "Holz - generisch 140-100-70", "Metall - Edelstahl gebürstet": "Metall - Edelstahl gebürstet", "Metall - Edelstahl satiniert": "Metall - Edelstahl satiniert", "Lack - grau 80-80-80": "Lack - grau 80-80-80") | property sets: Pset_DoorCommon, Pset_DoorWindowGlazingType, Pset_EnvironmentalImpactIndicators
          2 x IFCDOOR | type IFCDOORTYPE "TU DF 1 - Stahl-Eckzarge Falztüre:DL - 800 x 2000" | object type "TU DF 1 - Stahl-Eckzarge Falztüre:DL - 800 x 2000" | DOOR | SINGLE_SWING_LEFT | names: "TU DF 1 - Stahl-Eckzarge Falztüre:DL - 800 x 2000:2699634", "TU DF 1 - Stahl-Eckzarge Falztüre:DL - 800 x 2000:2699940" | material: constituents "MaterialConstituentSet" ("Holz - generisch 140-100-70": "Holz - generisch 140-100-70", "Metall - Edelstahl gebürstet": "Metall - Edelstahl gebürstet", "Metall - Edelstahl satiniert": "Metall - Edelstahl satiniert", "Lack - grau 80-80-80": "Lack - grau 80-80-80") | property sets: Pset_DoorCommon, Pset_DoorWindowGlazingType, Pset_EnvironmentalImpactIndicators
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | object type "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | CEILING | names: "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25:2700290" | material: layers "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" ("Trockenbau - Rigips Die Dicke RFI" 0.025) | property sets: Pset_CoveringCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | object type "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | CEILING | names: "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25:2700332" | material: layers "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" ("Trockenbau - Rigips Die Dicke RFI" 0.025) | property sets: Pset_CoveringCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | object type "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | CEILING | names: "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25:2700368" | material: layers "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" ("Trockenbau - Rigips Die Dicke RFI" 0.025) | property sets: Pset_CoveringCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | object type "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | CEILING | names: "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25:2700405" | material: layers "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" ("Trockenbau - Rigips Die Dicke RFI" 0.025) | property sets: Pset_CoveringCommon, Pset_EnvironmentalImpactIndicators
          2 x IFCWALL | type IFCWALLTYPE "Basiswand:GK VS - Sanitär" | object type "Basiswand:GK VS - Sanitär" | names: "Basiswand:GK VS - Sanitär:2723848", "Basiswand:GK VS - Sanitär:2726102" | material: layers "Basiswand:GK VS - Sanitär" ("Trockenbau - Gipsplatte" 0.025, "Dämmung - weich" 0.04) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          4 x IFCWALL | type IFCWALLTYPE "Basiswand:GK 100 - Doppelbeplankt" | object type "Basiswand:GK 100 - Doppelbeplankt" | names: "Basiswand:GK 100 - Doppelbeplankt:2724228", "Basiswand:GK 100 - Doppelbeplankt:2724298", "Basiswand:GK 100 - Doppelbeplankt:2725316" (+1 more) | material: layers "Basiswand:GK 100 - Doppelbeplankt" ("Trockenbau - Gipsplatte" 0.025, "Dämmung - weich" 0.05, "Trockenbau - Gipsplatte" 0.025) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          8 x IFCWALL | type IFCWALLTYPE "Basiswand:GK 75 - Toilettentrennwand" | object type "Basiswand:GK 75 - Toilettentrennwand" | names: "Basiswand:GK 75 - Toilettentrennwand:2742447", "Basiswand:GK 75 - Toilettentrennwand:2742530", "Basiswand:GK 75 - Toilettentrennwand:2742676" (+5 more) | material: layers "Basiswand:GK 75 - Toilettentrennwand" ("Trockenbau - Gipsplatte" 0.0125, "Dämmung - weich" 0.05, "Trockenbau - Gipsplatte" 0.0125) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCDOOR | type IFCDOORTYPE "TU DF 2 - Rahmenstock flächenbündig:ML - 1635 x 2135" | object type "TU DF 2 - Rahmenstock flächenbündig:ML - 1635 x 2135" | DOOR | DOUBLE_DOOR_SINGLE_SWING | names: "TU DF 2 - Rahmenstock flächenbündig:ML - 1635 x 2135:2749010" | material: constituents "MaterialConstituentSet" ("Holz - generisch 140-100-70": "Holz - generisch 140-100-70", "Metall - Edelstahl gebürstet": "Metall - Edelstahl gebürstet", "Lack - grau 80-80-80": "Lack - grau 80-80-80") | property sets: Pset_DoorCommon, Pset_DoorWindowGlazingType, Pset_EnvironmentalImpactIndicators
        IFCSPACE "1-1" | long name "Eingangsbereich / Flur" | SPACE
        IFCSPACE "1-2" | long name "Cafeteria" | SPACE
        IFCSPACE "1-3" | long name "Küche" | SPACE
        IFCSPACE "1-4" | long name "Gruppenbüro 1" | SPACE
        IFCSPACE "1-5" | long name "Gruppenbüro 2" | SPACE
        IFCSPACE "1-6" | long name "Gruppenbüro 3" | SPACE
        IFCSPACE "1-7" | long name "Open Workspace EG" | SPACE
        IFCSPACE "1-8" | long name "Gruppenbüro 4" | SPACE
        IFCSPACE "1-9" | long name "Gruppenbüro 5" | SPACE
        IFCSPACE "1-10" | long name "Gruppenbüro 6" | SPACE
        IFCSPACE "1-11" | long name "VR/AR LAB" | SPACE
        IFCSPACE "1-12" | long name "Veranstaltungsraum" | SPACE
        IFCSPACE "1-15" | long name "WC Damen West - EG" | SPACE
        IFCSPACE "1-16" | long name "WC Herren West - EG" | SPACE
        IFCSPACE "1-17" | long name "Treppenhaus Ost - EG" | SPACE
        IFCSPACE "1-18" | long name "Fluchtflur Ost" | SPACE
        IFCSPACE "1-19" | long name "Treppenhaus West - EG" | SPACE
        IFCSPACE "1-20" | long name "Fluchtflur West" | SPACE
        IFCSPACE "13" | long name "WC Damen Ost - EG" | SPACE
        IFCSPACE "14" | long name "WC Herren Ost - EG" | SPACE
        IFCSPACE "300" | long name "Aufzug West" | SPACE
        IFCSPACE "301" | long name "Schacht West 1" | SPACE
        IFCSPACE "302" | long name "Schacht West 2" | SPACE
        IFCSPACE "400" | long name "Aufzug Ost" | SPACE
        IFCSPACE "401" | long name "Schacht Ost 1" | SPACE
        IFCSPACE "402" | long name "Schacht Ost 2" | SPACE
      IFCBUILDINGSTOREY "E01_OKRD" | long name "E01_OKRD" | object type "Ebene:Ebene" | elevation 3.75
        contains 210 elements
          1 x IFCSLAB | type IFCSLABTYPE "Geschossdecke:STB 250" | object type "Geschossdecke:STB 250" | FLOOR | names: "Geschossdecke:STB 250:2396591" | material: layers "Geschossdecke:STB 250" ("Ortbeton - bewehrt" 0.25) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Geschossdecke:STB 250" | object type "Geschossdecke:STB 250" | FLOOR | names: "Geschossdecke:STB 250:2396819" | material: layers "Geschossdecke:STB 250" ("Ortbeton - bewehrt" 0.25) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 400" | object type "STB Stütze - rechteckig:STB 250 x 400" | COLUMN | names: "STB Stütze - rechteckig:STB 250 x 400:2396916" | material: profiles "STB 250 x 400" ("STB 250 x 400": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 400" | object type "STB Stütze - rechteckig:STB 250 x 400" | COLUMN | names: "STB Stütze - rechteckig:STB 250 x 400:2396918" | material: profiles "STB 250 x 400" ("STB 250 x 400": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 400" | object type "STB Stütze - rechteckig:STB 250 x 400" | COLUMN | names: "STB Stütze - rechteckig:STB 250 x 400:2396920" | material: profiles "STB 250 x 400" ("STB 250 x 400": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 400" | object type "STB Stütze - rechteckig:STB 250 x 400" | COLUMN | names: "STB Stütze - rechteckig:STB 250 x 400:2396922" | material: profiles "STB 250 x 400" ("STB 250 x 400": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 400" | object type "STB Stütze - rechteckig:STB 250 x 400" | COLUMN | names: "STB Stütze - rechteckig:STB 250 x 400:2396924" | material: profiles "STB 250 x 400" ("STB 250 x 400": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 400" | object type "STB Stütze - rechteckig:STB 250 x 400" | COLUMN | names: "STB Stütze - rechteckig:STB 250 x 400:2396926" | material: profiles "STB 250 x 400" ("STB 250 x 400": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 400" | object type "STB Stütze - rechteckig:STB 250 x 400" | COLUMN | names: "STB Stütze - rechteckig:STB 250 x 400:2396928" | material: profiles "STB 250 x 400" ("STB 250 x 400": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 400" | object type "STB Stütze - rechteckig:STB 250 x 400" | COLUMN | names: "STB Stütze - rechteckig:STB 250 x 400:2396930" | material: profiles "STB 250 x 400" ("STB 250 x 400": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 400" | object type "STB Stütze - rechteckig:STB 250 x 400" | COLUMN | names: "STB Stütze - rechteckig:STB 250 x 400:2396932" | material: profiles "STB 250 x 400" ("STB 250 x 400": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 400" | object type "STB Stütze - rechteckig:STB 250 x 400" | COLUMN | names: "STB Stütze - rechteckig:STB 250 x 400:2396934" | material: profiles "STB 250 x 400" ("STB 250 x 400": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 400" | object type "STB Stütze - rechteckig:STB 250 x 400" | COLUMN | names: "STB Stütze - rechteckig:STB 250 x 400:2396936" | material: profiles "STB 250 x 400" ("STB 250 x 400": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 400" | object type "STB Stütze - rechteckig:STB 250 x 400" | COLUMN | names: "STB Stütze - rechteckig:STB 250 x 400:2396938" | material: profiles "STB 250 x 400" ("STB 250 x 400": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 250" | object type "STB Stütze - rechteckig:STB 250 x 250" | COLUMN | names: "STB Stütze - rechteckig:STB 250 x 250:2396948" | material: profiles "STB 250 x 250" ("STB 250 x 250": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 250" | object type "STB Stütze - rechteckig:STB 250 x 250" | COLUMN | names: "STB Stütze - rechteckig:STB 250 x 250:2396950" | material: profiles "STB 250 x 250" ("STB 250 x 250": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 250" | object type "STB Stütze - rechteckig:STB 250 x 250" | COLUMN | names: "STB Stütze - rechteckig:STB 250 x 250:2396952" | material: profiles "STB 250 x 250" ("STB 250 x 250": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 250" | object type "STB Stütze - rechteckig:STB 250 x 250" | COLUMN | names: "STB Stütze - rechteckig:STB 250 x 250:2396954" | material: profiles "STB 250 x 250" ("STB 250 x 250": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 250" | object type "STB Stütze - rechteckig:STB 250 x 250" | COLUMN | names: "STB Stütze - rechteckig:STB 250 x 250:2396956" | material: profiles "STB 250 x 250" ("STB 250 x 250": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 250" | object type "STB Stütze - rechteckig:STB 250 x 250" | COLUMN | names: "STB Stütze - rechteckig:STB 250 x 250:2396958" | material: profiles "STB 250 x 250" ("STB 250 x 250": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 250" | object type "STB Stütze - rechteckig:STB 250 x 250" | COLUMN | names: "STB Stütze - rechteckig:STB 250 x 250:2396960" | material: profiles "STB 250 x 250" ("STB 250 x 250": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 250" | object type "STB Stütze - rechteckig:STB 250 x 250" | COLUMN | names: "STB Stütze - rechteckig:STB 250 x 250:2396962" | material: profiles "STB 250 x 250" ("STB 250 x 250": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          20 x IFCWALL | type IFCWALLTYPE "Basiswand:STB 200" | object type "Basiswand:STB 200" | names: "Basiswand:STB 200:2399773", "Basiswand:STB 200:2399940", "Basiswand:STB 200:2400045" (+17 more) | material: layers "Basiswand:STB 200" ("Ortbeton - bewehrt" 0.2) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCBEAM | type IFCBEAMTYPE "STB Träger - rechteckig:STB 250 x 500" | object type "STB Träger - rechteckig:STB 250 x 500" | BEAM | names: "STB Träger - rechteckig:STB 250 x 500:2400804" | material: profiles "STB 250 x 500" ("STB 250 x 500": "Ortbeton - bewehrt") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "STB Träger - rechteckig:STB 250 x 500" | object type "STB Träger - rechteckig:STB 250 x 500" | BEAM | names: "STB Träger - rechteckig:STB 250 x 500:2400830" | material: profiles "STB 250 x 500" ("STB 250 x 500": "Ortbeton - bewehrt") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "STB Träger - rechteckig:STB 250 x 500" | object type "STB Träger - rechteckig:STB 250 x 500" | BEAM | names: "STB Träger - rechteckig:STB 250 x 500:2400850" | material: profiles "STB 250 x 500" ("STB 250 x 500": "Ortbeton - bewehrt") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "STB Träger - rechteckig:STB 250 x 500" | object type "STB Träger - rechteckig:STB 250 x 500" | BEAM | names: "STB Träger - rechteckig:STB 250 x 500:2400867" | material: profiles "STB 250 x 500" ("STB 250 x 500": "Ortbeton - bewehrt") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "STB Träger - rechteckig:STB 250 x 500" | object type "STB Träger - rechteckig:STB 250 x 500" | BEAM | names: "STB Träger - rechteckig:STB 250 x 500:2400964" | material: profiles "STB 250 x 500" ("STB 250 x 500": "Ortbeton - bewehrt") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "STB Träger - rechteckig:STB 250 x 500" | object type "STB Träger - rechteckig:STB 250 x 500" | BEAM | names: "STB Träger - rechteckig:STB 250 x 500:2400966" | material: profiles "STB 250 x 500" ("STB 250 x 500": "Ortbeton - bewehrt") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "STB Träger - rechteckig:STB 250 x 500" | object type "STB Träger - rechteckig:STB 250 x 500" | BEAM | names: "STB Träger - rechteckig:STB 250 x 500:2400968" | material: profiles "STB 250 x 500" ("STB 250 x 500": "Ortbeton - bewehrt") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "STB Träger - rechteckig:STB 250 x 500" | object type "STB Träger - rechteckig:STB 250 x 500" | BEAM | names: "STB Träger - rechteckig:STB 250 x 500:2400970" | material: profiles "STB 250 x 500" ("STB 250 x 500": "Ortbeton - bewehrt") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          8 x IFCWALL | type IFCWALLTYPE "Basiswand:STB 250" | object type "Basiswand:STB 250" | names: "Basiswand:STB 250:2421035", "Basiswand:STB 250:2421036", "Basiswand:STB 250:2421037" (+5 more) | material: layers "Basiswand:STB 250" ("Ortbeton - bewehrt" 0.25) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 400" | object type "STB Stütze - rechteckig:STB 250 x 400" | COLUMN | names: "STB Stütze - rechteckig:STB 250 x 400:2422235" | material: profiles "STB 250 x 400" ("STB 250 x 400": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 400" | object type "STB Stütze - rechteckig:STB 250 x 400" | COLUMN | names: "STB Stütze - rechteckig:STB 250 x 400:2422237" | material: profiles "STB 250 x 400" ("STB 250 x 400": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 250" | object type "STB Stütze - rechteckig:STB 250 x 250" | COLUMN | names: "STB Stütze - rechteckig:STB 250 x 250:2422254" | material: profiles "STB 250 x 250" ("STB 250 x 250": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 250" | object type "STB Stütze - rechteckig:STB 250 x 250" | COLUMN | names: "STB Stütze - rechteckig:STB 250 x 250:2422256" | material: profiles "STB 250 x 250" ("STB 250 x 250": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 400" | object type "STB Stütze - rechteckig:STB 250 x 400" | COLUMN | names: "STB Stütze - rechteckig:STB 250 x 400:2422275" | material: profiles "STB 250 x 400" ("STB 250 x 400": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 400" | object type "STB Stütze - rechteckig:STB 250 x 400" | COLUMN | names: "STB Stütze - rechteckig:STB 250 x 400:2422277" | material: profiles "STB 250 x 400" ("STB 250 x 400": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 250" | object type "STB Stütze - rechteckig:STB 250 x 250" | COLUMN | names: "STB Stütze - rechteckig:STB 250 x 250:2422296" | material: profiles "STB 250 x 250" ("STB 250 x 250": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 250" | object type "STB Stütze - rechteckig:STB 250 x 250" | COLUMN | names: "STB Stütze - rechteckig:STB 250 x 250:2422298" | material: profiles "STB 250 x 250" ("STB 250 x 250": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 250" | object type "STB Stütze - rechteckig:STB 250 x 250" | COLUMN | names: "STB Stütze - rechteckig:STB 250 x 250:2423552" | material: profiles "STB 250 x 250" ("STB 250 x 250": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 250" | object type "STB Stütze - rechteckig:STB 250 x 250" | COLUMN | names: "STB Stütze - rechteckig:STB 250 x 250:2423567" | material: profiles "STB 250 x 250" ("STB 250 x 250": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 250" | object type "STB Stütze - rechteckig:STB 250 x 250" | COLUMN | names: "STB Stütze - rechteckig:STB 250 x 250:2423612" | material: profiles "STB 250 x 250" ("STB 250 x 250": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 250" | object type "STB Stütze - rechteckig:STB 250 x 250" | COLUMN | names: "STB Stütze - rechteckig:STB 250 x 250:2423627" | material: profiles "STB 250 x 250" ("STB 250 x 250": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          1 x IFCDOOR | type IFCDOORTYPE "TU DF 1 - Fluchttüre Endausgang:EN 179 - ML - 1010 x 2250" | object type "TU DF 1 - Fluchttüre Endausgang:EN 179 - ML - 1010 x 2250" | DOOR | SINGLE_SWING_LEFT | names: "TU DF 1 - Fluchttüre Endausgang:EN 179 - ML - 1010 x 2250:2426178" | material: constituents "MaterialConstituentSet" ("Metall - Edelstahl gebürstet": "Metall - Edelstahl gebürstet", "Kunststoff - weiß 250-250-250": "Kunststoff - weiß 250-250-250", "Metall - Edelstahl satiniert": "Metall - Edelstahl satiniert", "Lack - grau 80-80-80": "Lack - grau 80-80-80", "Dämmung - hart": "Dämmung - hart") | property sets: Pset_DoorCommon, Pset_DoorWindowGlazingType, Pset_EnvironmentalImpactIndicators
          1 x IFCDOOR | type IFCDOORTYPE "TU DF 1 - Fluchttüre Endausgang:EN 179 - ML - 1010 x 2250" | object type "TU DF 1 - Fluchttüre Endausgang:EN 179 - ML - 1010 x 2250" | DOOR | SINGLE_SWING_RIGHT | names: "TU DF 1 - Fluchttüre Endausgang:EN 179 - ML - 1010 x 2250:2426180" | material: constituents "MaterialConstituentSet" ("Metall - Edelstahl gebürstet": "Metall - Edelstahl gebürstet", "Kunststoff - weiß 250-250-250": "Kunststoff - weiß 250-250-250", "Metall - Edelstahl satiniert": "Metall - Edelstahl satiniert", "Lack - grau 80-80-80": "Lack - grau 80-80-80", "Dämmung - hart": "Dämmung - hart") | property sets: Pset_DoorCommon, Pset_DoorWindowGlazingType, Pset_EnvironmentalImpactIndicators
          1 x IFCDOOR | type IFCDOORTYPE "TU Durchgang:DL - 1200 x 2100" | object type "TU Durchgang:DL - 1200 x 2100" | DOOR | names: "TU Durchgang:DL - 1200 x 2100:2426586" | property sets: Pset_DoorCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCDOOR | type IFCDOORTYPE "TU Durchgang:DL - 1200 x 2100" | object type "TU Durchgang:DL - 1200 x 2100" | DOOR | names: "TU Durchgang:DL - 1200 x 2100:2426588" | property sets: Pset_DoorCommon, Pset_EnvironmentalImpactIndicators
          2 x IFCROOF | type IFCCURTAINWALLTYPE "Dachverglasung:Dachverglasung" | object type "Dachverglasung:Dachverglasung" | names: "Dachverglasung:Dachverglasung:2427545", "Dachverglasung:Dachverglasung:2428025" | parts: 54 IFCMEMBER, 20 IFCPLATE | property sets: Pset_EnvironmentalImpactIndicators, Pset_RoofCommon
          1 x IFCSLAB | type IFCSLABTYPE "Geschossdecke:FB 150 leer" | object type "Geschossdecke:FB 150 leer" | FLOOR | names: "Geschossdecke:FB 150 leer:2428082" | material: layers "Geschossdecke:FB 150 leer" ("Fußbodenaufbau" 0.15) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Geschossdecke:FB 150 leer" | object type "Geschossdecke:FB 150 leer" | FLOOR | names: "Geschossdecke:FB 150 leer:2431572" | material: layers "Geschossdecke:FB 150 leer" ("Fußbodenaufbau" 0.15) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Geschossdecke:FB 150 leer" | object type "Geschossdecke:FB 150 leer" | FLOOR | names: "Geschossdecke:FB 150 leer:2431802" | material: layers "Geschossdecke:FB 150 leer" ("Fußbodenaufbau" 0.15) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          5 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Baum RPC - Laubbaum:Rotesche - 7,6 Meter" | object type "Baum RPC - Laubbaum:Rotesche - 7,6 Meter" | names: "Baum RPC - Laubbaum:Rotesche - 7,6 Meter:2454919", "Baum RPC - Laubbaum:Rotesche - 7,6 Meter:2454976", "Baum RPC - Laubbaum:Rotesche - 7,6 Meter:2455021" (+2 more) | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          4 x IFCWALL | type IFCWALLTYPE "Basiswand:Leichtbetonmauerwerk 250" | object type "Basiswand:Leichtbetonmauerwerk 250" | names: "Basiswand:Leichtbetonmauerwerk 250:2517374", "Basiswand:Leichtbetonmauerwerk 250:2517481", "Basiswand:Leichtbetonmauerwerk 250:2517600" (+1 more) | material: layers "Basiswand:Leichtbetonmauerwerk 250" ("Leichtbeton - Mauerwerk" 0.25) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          18 x IFCWINDOW | type IFCWINDOWTYPE "FE 3 tlg - DK-Fix im Rahmen-DK-2:6000 x 1500" | object type "FE 3 tlg - DK-Fix im Rahmen-DK-2:6000 x 1500" | WINDOW | names: "FE 3 tlg - DK-Fix im Rahmen-DK-2:6000 x 1500:2529359", "FE 3 tlg - DK-Fix im Rahmen-DK-2:6000 x 1500:2529899", "FE 3 tlg - DK-Fix im Rahmen-DK-2:6000 x 1500:2530077" (+15 more) | material: constituents "MaterialConstituentSet" ("Metall - Edelstahl gebürstet": "Metall - Edelstahl gebürstet", "Kunststoff - grau 70-70-70": "Kunststoff - grau 70-70-70", "Glas - Isolierverglasung klar": "Glas - Isolierverglasung klar", "Holz - generisch 140-100-70": "Holz - generisch 140-100-70") | property sets: Pset_EnvironmentalImpactIndicators, Pset_OpeningElementCommon
          2 x IFCWINDOW | type IFCWINDOWTYPE "FE 2 tlg - DK Fix mit Pfosten - 2:4000 x 1500" | object type "FE 2 tlg - DK Fix mit Pfosten - 2:4000 x 1500" | WINDOW | names: "FE 2 tlg - DK Fix mit Pfosten - 2:4000 x 1500:2536377", "FE 2 tlg - DK Fix mit Pfosten - 2:4000 x 1500:2544252" | material: constituents "MaterialConstituentSet" ("Metall - Edelstahl gebürstet": "Metall - Edelstahl gebürstet", "Kunststoff - grau 70-70-70": "Kunststoff - grau 70-70-70", "Glas - Isolierverglasung klar": "Glas - Isolierverglasung klar", "Holz - generisch 140-100-70": "Holz - generisch 140-100-70") | property sets: Pset_EnvironmentalImpactIndicators, Pset_OpeningElementCommon
          2 x IFCWINDOW | type IFCWINDOWTYPE "FE 2 tlg - DK Fix mit Pfosten - 2:4000 x 1500" | object type "FE 2 tlg - DK Fix mit Pfosten - 2:4000 x 1500" | WINDOW | names: "FE 2 tlg - DK Fix mit Pfosten - 2:4000 x 1500:2544255", "FE 2 tlg - DK Fix mit Pfosten - 2:4000 x 1500:2608692" | material: constituents "MaterialConstituentSet" ("Metall - Edelstahl gebürstet": "Metall - Edelstahl gebürstet", "Kunststoff - grau 70-70-70": "Kunststoff - grau 70-70-70", "Glas - Isolierverglasung klar": "Glas - Isolierverglasung klar", "Holz - generisch 140-100-70": "Holz - generisch 140-100-70") | property sets: Pset_EnvironmentalImpactIndicators, Pset_OpeningElementCommon
          27 x IFCWALL | type IFCWALLTYPE "Basiswand:Metall-Einfachständerwand 2-lagig beplankt (MW12BF)" | object type "Basiswand:Metall-Einfachständerwand 2-lagig beplankt (MW12BF)" | names: "Basiswand:Metall-Einfachständerwand 2-lagig beplankt (MW12BF):2551026", "Basiswand:Metall-Einfachständerwand 2-lagig beplankt (MW12BF):2551123", "Basiswand:Metall-Einfachständerwand 2-lagig beplankt (MW12BF):2551287" (+24 more) | material: layers "Basiswand:Metall-Einfachständerwand 2-lagig beplankt (MW12BF)" ("Trockenbau - Rigips Die Blaue RFI" 0.025, "Dämmung - Isover Akustik TF" 0.08, "Luftschicht" 0.02, "Trockenbau - Rigips Die Blaue RFI" 0.025) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          9 x IFCDOOR | type IFCDOORTYPE "TU DF 1 - Rahmenstock flächenbündig:DL - 1000 x 2000" | object type "TU DF 1 - Rahmenstock flächenbündig:DL - 1000 x 2000" | DOOR | SINGLE_SWING_RIGHT | names: "TU DF 1 - Rahmenstock flächenbündig:DL - 1000 x 2000:2553177", "TU DF 1 - Rahmenstock flächenbündig:DL - 1000 x 2000:2553337", "TU DF 1 - Rahmenstock flächenbündig:DL - 1000 x 2000:2553405" (+6 more) | material: constituents "MaterialConstituentSet" ("Holz - generisch 140-100-70": "Holz - generisch 140-100-70", "Metall - Edelstahl gebürstet": "Metall - Edelstahl gebürstet", "Lack - grau 80-80-80": "Lack - grau 80-80-80") | property sets: Pset_DoorCommon, Pset_DoorWindowGlazingType, Pset_EnvironmentalImpactIndicators
          10 x IFCDOOR | type IFCDOORTYPE "TU DF 1 - Rahmenstock flächenbündig:DL - 1000 x 2000" | object type "TU DF 1 - Rahmenstock flächenbündig:DL - 1000 x 2000" | DOOR | SINGLE_SWING_LEFT | names: "TU DF 1 - Rahmenstock flächenbündig:DL - 1000 x 2000:2553215", "TU DF 1 - Rahmenstock flächenbündig:DL - 1000 x 2000:2553265", "TU DF 1 - Rahmenstock flächenbündig:DL - 1000 x 2000:2553451" (+7 more) | material: constituents "MaterialConstituentSet" ("Holz - generisch 140-100-70": "Holz - generisch 140-100-70", "Metall - Edelstahl gebürstet": "Metall - Edelstahl gebürstet", "Lack - grau 80-80-80": "Lack - grau 80-80-80") | property sets: Pset_DoorCommon, Pset_DoorWindowGlazingType, Pset_EnvironmentalImpactIndicators
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | object type "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | CEILING | names: "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25:2557367" | material: layers "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" ("Trockenbau - Rigips Die Dicke RFI" 0.025) | property sets: Pset_CoveringCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | object type "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | CEILING | names: "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25:2557421" | material: layers "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" ("Trockenbau - Rigips Die Dicke RFI" 0.025) | property sets: Pset_CoveringCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | object type "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | CEILING | names: "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25:2557681" | material: layers "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" ("Trockenbau - Rigips Die Dicke RFI" 0.025) | property sets: Pset_CoveringCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | object type "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | CEILING | names: "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25:2557724" | material: layers "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" ("Trockenbau - Rigips Die Dicke RFI" 0.025) | property sets: Pset_CoveringCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | object type "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | CEILING | names: "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25:2557762" | material: layers "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" ("Trockenbau - Rigips Die Dicke RFI" 0.025) | property sets: Pset_CoveringCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | object type "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | CEILING | names: "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25:2557797" | material: layers "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" ("Trockenbau - Rigips Die Dicke RFI" 0.025) | property sets: Pset_CoveringCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | object type "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | CEILING | names: "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25:2557842" | material: layers "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" ("Trockenbau - Rigips Die Dicke RFI" 0.025) | property sets: Pset_CoveringCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | object type "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | CEILING | names: "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25:2557893" | material: layers "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" ("Trockenbau - Rigips Die Dicke RFI" 0.025) | property sets: Pset_CoveringCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | object type "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | CEILING | names: "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25:2557931" | material: layers "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" ("Trockenbau - Rigips Die Dicke RFI" 0.025) | property sets: Pset_CoveringCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | object type "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | CEILING | names: "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25:2557970" | material: layers "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" ("Trockenbau - Rigips Die Dicke RFI" 0.025) | property sets: Pset_CoveringCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | object type "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | CEILING | names: "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25:2558008" | material: layers "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" ("Trockenbau - Rigips Die Dicke RFI" 0.025) | property sets: Pset_CoveringCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | object type "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | CEILING | names: "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25:2558046" | material: layers "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" ("Trockenbau - Rigips Die Dicke RFI" 0.025) | property sets: Pset_CoveringCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | object type "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | CEILING | names: "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25:2558084" | material: layers "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" ("Trockenbau - Rigips Die Dicke RFI" 0.025) | property sets: Pset_CoveringCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | object type "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | CEILING | names: "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25:2558119" | material: layers "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" ("Trockenbau - Rigips Die Dicke RFI" 0.025) | property sets: Pset_CoveringCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | object type "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | CEILING | names: "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25:2558156" | material: layers "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" ("Trockenbau - Rigips Die Dicke RFI" 0.025) | property sets: Pset_CoveringCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | object type "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | CEILING | names: "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25:2558194" | material: layers "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" ("Trockenbau - Rigips Die Dicke RFI" 0.025) | property sets: Pset_CoveringCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | object type "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | CEILING | names: "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25:2558232" | material: layers "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" ("Trockenbau - Rigips Die Dicke RFI" 0.025) | property sets: Pset_CoveringCommon, Pset_EnvironmentalImpactIndicators
          2 x IFCWINDOW | type IFCWINDOWTYPE "FE 1 tlg - DrehKipp:2000 x 1500" | object type "FE 1 tlg - DrehKipp:2000 x 1500" | WINDOW | names: "FE 1 tlg - DrehKipp:2000 x 1500:2653437", "FE 1 tlg - DrehKipp:2000 x 1500:2660775" | material: constituents "MaterialConstituentSet" ("Metall - Edelstahl gebürstet": "Metall - Edelstahl gebürstet", "Kunststoff - grau 70-70-70": "Kunststoff - grau 70-70-70", "Glas - Isolierverglasung klar": "Glas - Isolierverglasung klar", "Holz - generisch 140-100-70": "Holz - generisch 140-100-70") | property sets: Pset_EnvironmentalImpactIndicators, Pset_OpeningElementCommon
          2 x IFCWINDOW | type IFCWINDOWTYPE "FE 1 tlg - DrehKipp:2000 x 1500" | object type "FE 1 tlg - DrehKipp:2000 x 1500" | WINDOW | names: "FE 1 tlg - DrehKipp:2000 x 1500:2660375", "FE 1 tlg - DrehKipp:2000 x 1500:2660776" | material: constituents "MaterialConstituentSet" ("Metall - Edelstahl gebürstet": "Metall - Edelstahl gebürstet", "Kunststoff - grau 70-70-70": "Kunststoff - grau 70-70-70", "Glas - Isolierverglasung klar": "Glas - Isolierverglasung klar", "Holz - generisch 140-100-70": "Holz - generisch 140-100-70") | property sets: Pset_EnvironmentalImpactIndicators, Pset_OpeningElementCommon
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | object type "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | CEILING | names: "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25:2698514" | material: layers "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" ("Trockenbau - Rigips Die Dicke RFI" 0.025) | property sets: Pset_CoveringCommon, Pset_EnvironmentalImpactIndicators
          2 x IFCWALL | type IFCWALLTYPE "Basiswand:Metall-Einfachständerwand 2-lagig beplankt - Sanitär" | object type "Basiswand:Metall-Einfachständerwand 2-lagig beplankt - Sanitär" | names: "Basiswand:Metall-Einfachständerwand 2-lagig beplankt - Sanitär:2700772", "Basiswand:Metall-Einfachständerwand 2-lagig beplankt - Sanitär:2701263" | material: layers "Basiswand:Metall-Einfachständerwand 2-lagig beplankt - Sanitär" ("Trockenbau - Rigips Die Blaue RFI" 0.025, "Steinwolle (Rockwool Fixrock033 VS)" 0.08, "Luftschicht" 0.19, "Steinwolle (Rockwool Fixrock033 VS)" 0.08, "Trockenbau - Rigips Die Blaue RFI" 0.025) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          2 x IFCDOOR | type IFCDOORTYPE "TU DF 1 - Stahl-Eckzarge Falztüre:DL - 800 x 2000" | object type "TU DF 1 - Stahl-Eckzarge Falztüre:DL - 800 x 2000" | DOOR | SINGLE_SWING_RIGHT | names: "TU DF 1 - Stahl-Eckzarge Falztüre:DL - 800 x 2000:2700827", "TU DF 1 - Stahl-Eckzarge Falztüre:DL - 800 x 2000:2701363" | material: constituents "MaterialConstituentSet" ("Holz - generisch 140-100-70": "Holz - generisch 140-100-70", "Metall - Edelstahl gebürstet": "Metall - Edelstahl gebürstet", "Metall - Edelstahl satiniert": "Metall - Edelstahl satiniert", "Lack - grau 80-80-80": "Lack - grau 80-80-80") | property sets: Pset_DoorCommon, Pset_DoorWindowGlazingType, Pset_EnvironmentalImpactIndicators
          2 x IFCDOOR | type IFCDOORTYPE "TU DF 1 - Stahl-Eckzarge Falztüre:DL - 800 x 2000" | object type "TU DF 1 - Stahl-Eckzarge Falztüre:DL - 800 x 2000" | DOOR | SINGLE_SWING_LEFT | names: "TU DF 1 - Stahl-Eckzarge Falztüre:DL - 800 x 2000:2700881", "TU DF 1 - Stahl-Eckzarge Falztüre:DL - 800 x 2000:2701309" | material: constituents "MaterialConstituentSet" ("Holz - generisch 140-100-70": "Holz - generisch 140-100-70", "Metall - Edelstahl gebürstet": "Metall - Edelstahl gebürstet", "Metall - Edelstahl satiniert": "Metall - Edelstahl satiniert", "Lack - grau 80-80-80": "Lack - grau 80-80-80") | property sets: Pset_DoorCommon, Pset_DoorWindowGlazingType, Pset_EnvironmentalImpactIndicators
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | object type "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | CEILING | names: "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25:2701103" | material: layers "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" ("Trockenbau - Rigips Die Dicke RFI" 0.025) | property sets: Pset_CoveringCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | object type "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | CEILING | names: "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25:2701143" | material: layers "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" ("Trockenbau - Rigips Die Dicke RFI" 0.025) | property sets: Pset_CoveringCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | object type "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | CEILING | names: "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25:2701475" | material: layers "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" ("Trockenbau - Rigips Die Dicke RFI" 0.025) | property sets: Pset_CoveringCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | object type "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | CEILING | names: "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25:2701512" | material: layers "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" ("Trockenbau - Rigips Die Dicke RFI" 0.025) | property sets: Pset_CoveringCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCROOF | type IFCROOFTYPE "Basisdach:Flachdachaufbau begrünt 320" | object type "Basisdach:Flachdachaufbau begrünt 320" | names: "Basisdach:Flachdachaufbau begrünt 320:2719837" | parts: 1 IFCSLAB | property sets: Pset_EnvironmentalImpactIndicators, Pset_RoofCommon
          2 x IFCWALL | type IFCWALLTYPE "Basiswand:GK VS - Sanitär" | object type "Basiswand:GK VS - Sanitär" | names: "Basiswand:GK VS - Sanitär:2745104", "Basiswand:GK VS - Sanitär:2747323" | material: layers "Basiswand:GK VS - Sanitär" ("Trockenbau - Gipsplatte" 0.025, "Dämmung - weich" 0.04) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          8 x IFCWALL | type IFCWALLTYPE "Basiswand:GK 75 - Toilettentrennwand" | object type "Basiswand:GK 75 - Toilettentrennwand" | names: "Basiswand:GK 75 - Toilettentrennwand:2745851", "Basiswand:GK 75 - Toilettentrennwand:2745908", "Basiswand:GK 75 - Toilettentrennwand:2746121" (+5 more) | material: layers "Basiswand:GK 75 - Toilettentrennwand" ("Trockenbau - Gipsplatte" 0.0125, "Dämmung - weich" 0.05, "Trockenbau - Gipsplatte" 0.0125) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          4 x IFCWALL | type IFCWALLTYPE "Basiswand:GK 100 - Doppelbeplankt" | object type "Basiswand:GK 100 - Doppelbeplankt" | names: "Basiswand:GK 100 - Doppelbeplankt:2746759", "Basiswand:GK 100 - Doppelbeplankt:2746832", "Basiswand:GK 100 - Doppelbeplankt:2747962" (+1 more) | material: layers "Basiswand:GK 100 - Doppelbeplankt" ("Trockenbau - Gipsplatte" 0.025, "Dämmung - weich" 0.05, "Trockenbau - Gipsplatte" 0.025) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          7 x IFCRAILING | object type "Geländer:Vertikale Stäbe mit Handlauf" | names: "Geländer:Vertikale Stäbe mit Handlauf:2418060", "Geländer:Vertikale Stäbe mit Handlauf:2418173", "Geländer:Vertikale Stäbe mit Handlauf:2424801" (+4 more) | material: "Kunststoff - grau 70-70-70" | property sets: Pset_EnvironmentalImpactIndicators, Pset_RailingCommon
        IFCSPACE "2-1" | long name "Flur - OG" | SPACE
        IFCSPACE "2-2" | long name "Konferenzraum 2" | SPACE
        IFCSPACE "2-3" | long name "Konferenzraum 1" | SPACE
        IFCSPACE "2-4" | long name "Gruppenbüro 7" | SPACE
        IFCSPACE "2-5" | long name "Gruppenbüro 8" | SPACE
        IFCSPACE "2-6" | long name "Offene Lounge 1" | SPACE
        IFCSPACE "2-7" | long name "Open Workspace 2" | SPACE
        IFCSPACE "2-8" | long name "Gruppenbüro 9" | SPACE
        IFCSPACE "2-9" | long name "Gruppenbüro 10" | SPACE
        IFCSPACE "2-10" | long name "Gruppenbüro 11" | SPACE
        IFCSPACE "2-11" | long name "Konferenzraum 3" | SPACE
        IFCSPACE "2-12" | long name "Konferenzraum 4" | SPACE
        IFCSPACE "2-13" | long name "Gruppenbüro 12" | SPACE
        IFCSPACE "2-14" | long name "Gruppenbüro 13" | SPACE
        IFCSPACE "2-15" | long name "Offene Lounge 2" | SPACE
        IFCSPACE "2-16" | long name "Seminarraum" | SPACE
        IFCSPACE "2-17" | long name "Seminarraum Groß - teilbar" | SPACE
        IFCSPACE "2-18" | long name "Gruppenbüro 14" | SPACE
        IFCSPACE "2-19" | long name "Gruppenbüro 15" | SPACE
        IFCSPACE "2-20" | long name "Gruppenbüro 16" | SPACE
        IFCSPACE "2-21" | long name "WC Damen West - OG" | SPACE
        IFCSPACE "2-22" | long name "WC Herren West OG" | SPACE
        IFCSPACE "2-23" | long name "WC Damen Ost - OG" | SPACE
        IFCSPACE "2-24" | long name "WC Herren Ost - OG" | SPACE
        IFCSPACE "2-25" | long name "Treppenhaus West - OG" | SPACE
        IFCSPACE "2-26" | long name "Treppenhaus Ost - OG" | SPACE

Types
  IFCBUILDINGELEMENTPROXYTYPE "Oberfläche:2437498" | 1 occurrence
  IFCWALLTYPE "Basiswand:STB 300" | 4 occurrences | material: layers "Basiswand:STB 300" ("Ortbeton - bewehrt Verputzt" 0.3) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCSLABTYPE "Bodenplatte:STB 300" | BASESLAB | 1 occurrence | material: layers "Bodenplatte:STB 300" ("Ortbeton - bewehrt" 0.3) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSTAIRTYPE "Fertigbetontreppe:Fertigbetontreppe - 2 Stockwerkstrennlinien" | HALF_TURN_STAIR | 1 occurrence | property sets: Pset_EnvironmentalImpactIndicators, Pset_StairCommon, Pset_StairFlightCommon
  IFCWALLTYPE "Basiswand:STB 200" | 45 occurrences | material: layers "Basiswand:STB 200" ("Ortbeton - bewehrt" 0.2) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Basiswand:STB 250" | 25 occurrences | material: layers "Basiswand:STB 250" ("Ortbeton - bewehrt" 0.25) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCSTAIRTYPE "Fertigbetontreppe:Fertigbetontreppe - 2 Stockwerkstrennlinien" | HALF_TURN_STAIR | 1 occurrence | property sets: Pset_EnvironmentalImpactIndicators, Pset_StairCommon, Pset_StairFlightCommon
  IFCDOORTYPE "TU DF 1 - Rahmenstock flächenbündig:DL - 1000 x 2000" | DOOR | SINGLE_SWING_LEFT | 5 occurrences | material: materials ("<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "Holz - generisch 140-100-70") | property sets: TU DF 1 - Rahmenstock flächenbündig:DL - 1000 x 2000:2432934, Pset_DoorCommon, Pset_DoorWindowGlazingType, Pset_EnvironmentalImpactIndicators
  IFCDOORTYPE "TU Durchgang:DL - 1200 x 2100" | DOOR | 2 occurrences | property sets: TU Durchgang:DL - 1200 x 2100:2426586, Pset_DoorCommon, Pset_EnvironmentalImpactIndicators
  IFCDOORTYPE "TU DF 1 - Rahmenstock flächenbündig:DL - 1000 x 2000" | DOOR | SINGLE_SWING_RIGHT | 8 occurrences | material: materials ("<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "Holz - generisch 140-100-70") | property sets: TU DF 1 - Rahmenstock flächenbündig:DL - 1000 x 2000:2432938, Pset_DoorCommon, Pset_DoorWindowGlazingType, Pset_EnvironmentalImpactIndicators
  IFCDOORTYPE "TU Durchgang:DL - 1200 x 2100" | DOOR | 2 occurrences | property sets: TU Durchgang:DL - 1200 x 2100:2426588, Pset_DoorCommon, Pset_EnvironmentalImpactIndicators
  IFCBUILDINGELEMENTPROXYTYPE "Plattenkante:Rechteckig_300x250" | 1 occurrence | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
  IFCSLABTYPE "Sohle:Sohle 1 mm" | FLOOR | 1 occurrence | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCBUILDINGELEMENTPROXYTYPE "Oberfläche:2437789" | 1 occurrence
  IFCSLABTYPE "Sohle:Sohle 1 mm" | FLOOR | 1 occurrence | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Geschossdecke:FB 100 leer" | FLOOR | 1 occurrence | material: layers "Geschossdecke:FB 100 leer" ("Fußbodenaufbau" 0.1) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCWALLTYPE "Basiswand:WD hart 200" | 12 occurrences | material: layers "Basiswand:WD hart 200" ("Dämmung - hart" 0.2) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCSLABTYPE "Geschossdecke:WD 200 hart" | FLOOR | 1 occurrence | material: layers "Geschossdecke:WD 200 hart" ("Dämmung - hart" 0.2) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Geschossdecke:WD 200 hart" | FLOOR | 1 occurrence | material: layers "Geschossdecke:WD 200 hart" ("Dämmung - hart" 0.2) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Geschossdecke:STB 200 + WD 200" | FLOOR | 1 occurrence | material: layers "Geschossdecke:STB 200 + WD 200" ("Ortbeton - bewehrt" 0.2, "Dämmung - hart" 0.2) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 400" | COLUMN | 1 occurrence | material: profiles "STB 250 x 400" ("STB 250 x 400": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 400" | COLUMN | 1 occurrence | material: profiles "STB 250 x 400" ("STB 250 x 400": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 400" | COLUMN | 1 occurrence | material: profiles "STB 250 x 400" ("STB 250 x 400": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 400" | COLUMN | 1 occurrence | material: profiles "STB 250 x 400" ("STB 250 x 400": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 400" | COLUMN | 1 occurrence | material: profiles "STB 250 x 400" ("STB 250 x 400": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 400" | COLUMN | 1 occurrence | material: profiles "STB 250 x 400" ("STB 250 x 400": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 400" | COLUMN | 1 occurrence | material: profiles "STB 250 x 400" ("STB 250 x 400": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 400" | COLUMN | 1 occurrence | material: profiles "STB 250 x 400" ("STB 250 x 400": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 400" | COLUMN | 1 occurrence | material: profiles "STB 250 x 400" ("STB 250 x 400": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 400" | COLUMN | 1 occurrence | material: profiles "STB 250 x 400" ("STB 250 x 400": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 400" | COLUMN | 1 occurrence | material: profiles "STB 250 x 400" ("STB 250 x 400": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 400" | COLUMN | 1 occurrence | material: profiles "STB 250 x 400" ("STB 250 x 400": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 250" | COLUMN | 2 occurrences | material: profiles "STB 250 x 250" ("STB 250 x 250": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 250" | COLUMN | 1 occurrence | material: profiles "STB 250 x 250" ("STB 250 x 250": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 250" | COLUMN | 1 occurrence | material: profiles "STB 250 x 250" ("STB 250 x 250": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 250" | COLUMN | 1 occurrence | material: profiles "STB 250 x 250" ("STB 250 x 250": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 250" | COLUMN | 1 occurrence | material: profiles "STB 250 x 250" ("STB 250 x 250": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 250" | COLUMN | 1 occurrence | material: profiles "STB 250 x 250" ("STB 250 x 250": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 250" | COLUMN | 1 occurrence | material: profiles "STB 250 x 250" ("STB 250 x 250": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
  IFCSLABTYPE "Geschossdecke:STB 220" | FLOOR | 1 occurrence | material: layers "Geschossdecke:STB 220" ("Ortbeton - bewehrt" 0.22) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCBEAMTYPE "STB Träger - rechteckig:STB 250 x 500" | BEAM | 1 occurrence | material: profiles "STB 250 x 500" ("STB 250 x 500": "Ortbeton - bewehrt") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
  IFCBEAMTYPE "STB Träger - rechteckig:STB 250 x 500" | BEAM | 1 occurrence | material: profiles "STB 250 x 500" ("STB 250 x 500": "Ortbeton - bewehrt") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
  IFCBEAMTYPE "STB Träger - rechteckig:STB 250 x 500" | BEAM | 1 occurrence | material: profiles "STB 250 x 500" ("STB 250 x 500": "Ortbeton - bewehrt") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
  IFCBEAMTYPE "STB Träger - rechteckig:STB 250 x 500" | BEAM | 1 occurrence | material: profiles "STB 250 x 500" ("STB 250 x 500": "Ortbeton - bewehrt") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
  IFCBEAMTYPE "STB Träger - rechteckig:STB 250 x 500" | BEAM | 1 occurrence | material: profiles "STB 250 x 500" ("STB 250 x 500": "Ortbeton - bewehrt") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
  IFCBEAMTYPE "STB Träger - rechteckig:STB 250 x 500" | BEAM | 1 occurrence | material: profiles "STB 250 x 500" ("STB 250 x 500": "Ortbeton - bewehrt") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
  IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 400" | COLUMN | 1 occurrence | material: profiles "STB 250 x 400" ("STB 250 x 400": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 400" | COLUMN | 1 occurrence | material: profiles "STB 250 x 400" ("STB 250 x 400": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 400" | COLUMN | 1 occurrence | material: profiles "STB 250 x 400" ("STB 250 x 400": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 400" | COLUMN | 1 occurrence | material: profiles "STB 250 x 400" ("STB 250 x 400": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
  IFCSTAIRTYPE "Fertigbetontreppe:Fertigbetontreppe - 2 Stockwerkstrennlinien" | HALF_TURN_STAIR | 1 occurrence | property sets: Pset_EnvironmentalImpactIndicators, Pset_StairCommon, Pset_StairFlightCommon
  IFCDOORTYPE "TU DF 1 - Fluchttüre Endausgang:EN 179 - ML - 1010 x 2250" | DOOR | SINGLE_SWING_LEFT | 3 occurrences | material: materials ("<Unnamed>", "Glas - klar", "Metall - Edelstahl satiniert", "Dämmung - hart", "Kunststoff - weiß 250-250-250", "Metall - Edelstahl satiniert", "Metall - Edelstahl gebürstet") | property sets: TU DF 1 - Fluchttüre Endausgang:EN 179 - ML - 1010 x 2250:2421088, Pset_DoorCommon, Pset_DoorWindowGlazingType, Pset_EnvironmentalImpactIndicators
  IFCDOORTYPE "TU DF 1 - Fluchttüre Endausgang:EN 179 - ML - 1010 x 2250" | DOOR | SINGLE_SWING_RIGHT | 3 occurrences | material: materials ("Metall - Edelstahl satiniert", "Dämmung - hart", "Kunststoff - weiß 250-250-250", "Glas - klar", "Metall - Edelstahl satiniert", "<Unnamed>", "Metall - Edelstahl gebürstet") | property sets: TU DF 1 - Fluchttüre Endausgang:EN 179 - ML - 1010 x 2250:2421089, Pset_DoorCommon, Pset_DoorWindowGlazingType, Pset_EnvironmentalImpactIndicators
  IFCDOORTYPE "TU Durchgang:DL - 1200 x 2100" | DOOR | 1 occurrence | property sets: TU Durchgang:DL - 1200 x 2100:2421090, Pset_DoorCommon, Pset_EnvironmentalImpactIndicators
  IFCDOORTYPE "TU DF 1 - Fluchttüre Endausgang:EN 179 - ML - 1010 x 2250" | DOOR | SINGLE_SWING_RIGHT | 1 occurrence | material: materials ("Metall - Edelstahl satiniert", "Kunststoff - weiß 250-250-250", "<Unnamed>", "Glas - klar", "Metall - Edelstahl satiniert", "Dämmung - hart", "Metall - Edelstahl gebürstet") | property sets: TU DF 1 - Fluchttüre Endausgang:EN 179 - ML - 1010 x 2250:2421363, Pset_DoorCommon, Pset_DoorWindowGlazingType, Pset_EnvironmentalImpactIndicators
  IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 250" | COLUMN | 1 occurrence | material: profiles "STB 250 x 250" ("STB 250 x 250": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 250" | COLUMN | 1 occurrence | material: profiles "STB 250 x 250" ("STB 250 x 250": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 250" | COLUMN | 1 occurrence | material: profiles "STB 250 x 250" ("STB 250 x 250": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 250" | COLUMN | 1 occurrence | material: profiles "STB 250 x 250" ("STB 250 x 250": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
  IFCSTAIRTYPE "Fertigbetontreppe:Fertigbetontreppe - 2 Stockwerkstrennlinien" | HALF_TURN_STAIR | 1 occurrence | property sets: Pset_EnvironmentalImpactIndicators, Pset_StairCommon, Pset_StairFlightCommon
  IFCDOORTYPE "TU Durchgang:DL - 1200 x 2100" | DOOR | 1 occurrence | property sets: TU Durchgang:DL - 1200 x 2100:2423932, Pset_DoorCommon, Pset_EnvironmentalImpactIndicators
  IFCDOORTYPE "TU DF 1 - Fluchttüre Endausgang:EN 179 - ML - 1010 x 2250" | DOOR | SINGLE_SWING_LEFT | 1 occurrence | material: materials ("Kunststoff - weiß 250-250-250", "<Unnamed>", "Dämmung - hart", "Glas - klar", "Metall - Edelstahl satiniert", "Metall - Edelstahl satiniert", "Metall - Edelstahl gebürstet") | property sets: TU DF 1 - Fluchttüre Endausgang:EN 179 - ML - 1010 x 2250:2423939, Pset_DoorCommon, Pset_DoorWindowGlazingType, Pset_EnvironmentalImpactIndicators
  IFCSTAIRTYPE "Zusammengebaute Treppe:Wangen Stahl - Stufen Stahl - 2 Stockwerkstrennlinien" | HALF_TURN_STAIR | 1 occurrence | property sets: Pset_EnvironmentalImpactIndicators, Pset_StairCommon, Pset_StairFlightCommon
  IFCSLABTYPE "Geschossdecke:FB 150 leer" | FLOOR | 1 occurrence | material: layers "Geschossdecke:FB 150 leer" ("Fußbodenaufbau" 0.15) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Geschossdecke:FB 150 leer" | FLOOR | 1 occurrence | material: layers "Geschossdecke:FB 150 leer" ("Fußbodenaufbau" 0.15) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Geschossdecke:FB 150 leer" | FLOOR | 1 occurrence | material: layers "Geschossdecke:FB 150 leer" ("Fußbodenaufbau" 0.15) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 250" | COLUMN | 1 occurrence | material: profiles "STB 250 x 250" ("STB 250 x 250": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 250" | COLUMN | 1 occurrence | material: profiles "STB 250 x 250" ("STB 250 x 250": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
  IFCSLABTYPE "Geschossdecke:STB 220" | FLOOR | 1 occurrence | material: layers "Geschossdecke:STB 220" ("Ortbeton - bewehrt" 0.22) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCBUILDINGELEMENTPROXYTYPE "Unterregion:2439145" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "Oberfläche:2439928" | 1 occurrence
  IFCSLABTYPE "Sohle:Sohle 1 mm" | FLOOR | 1 occurrence | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCBUILDINGELEMENTPROXYTYPE "Oberfläche:2440033" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "Parkplatz - 01 90:2500 x 5000" | 13 occurrences | material: "Farbe - Straßenmarkierung weiß" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
  IFCBUILDINGELEMENTPROXYTYPE "Parkplatz - 01 90:2500 x 5000" | 13 occurrences | material: "Farbe - Straßenmarkierung weiß" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
  IFCBUILDINGELEMENTPROXYTYPE "Markierung:B 120" | 45 occurrences | material: "Farbe - Straßenmarkierung" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
  IFCBUILDINGELEMENTPROXYTYPE "Richtungspfeil - Abzweigung und geradeaus:Typ1" | 1 occurrence | material: "Farbe - Straßenmarkierung" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
  IFCBUILDINGELEMENTPROXYTYPE "Richtungspfeil - Abzweigung und geradeaus:Typ1" | 1 occurrence | material: "Farbe - Straßenmarkierung" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
  IFCBUILDINGELEMENTPROXYTYPE "PKW Verkehrsinsel Schranken Ein-Ausfahrt:Typ1" | 1 occurrence | material: materials ("Metall - Zink", "Metall - Zink", "Metall - Edelstahl gebürstet", "Lack - rot 255-51-0", "Metall - Zink", "Dachdeckung - Kies", "Kunststoff - grau 50-50-50", "Naturstein - Granit grau", "Kunststoff - grau 50-50-50") | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
  IFCBUILDINGELEMENTPROXYTYPE "E-Ladestation - 03:Typ1" | 13 occurrences | material: materials ("Metall - Edelstahl satiniert", "Kunststoff - grau 50-50-50", "Kunststoff - blau 51-79-234", "Kunststoff - weiß 250-250-250") | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
  IFCBUILDINGELEMENTPROXYTYPE "Anfahrschutz Rohr:1000 x 700" | 26 occurrences | material: "Metall - Zink" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
  IFCBUILDINGELEMENTPROXYTYPE "Radständer - 04:3000, 5 Räder" | 5 occurrences | material: "Metall - Edelstahl satiniert" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
  IFCBUILDINGELEMENTPROXYTYPE "Fahrrad - Rennrad:Typ1" | 2 occurrences | material: materials ("Metall - Edelstahl satiniert", "Metall - Edelstahl satiniert", "Autodesk Sky Blue 6-150-215", "Kunststoff - grau 70-70-70", "Kunststoff - grau 50-50-50") | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
  IFCBUILDINGELEMENTPROXYTYPE "Unterregion:2454499" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "Baum RPC - Laubbaum:Rotesche - 7,6 Meter" | 22 occurrences | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
  IFCBUILDINGELEMENTPROXYTYPE "Unterregion:2460265" | 1 occurrence
  IFCWALLTYPE "Basiswand:Leichtbetonmauerwerk 250" | 10 occurrences | material: layers "Basiswand:Leichtbetonmauerwerk 250" ("Leichtbeton - Mauerwerk" 0.25) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Basiswand:WD 200 + Luft 40 + Bekleidung 12" | 4 occurrences | material: layers "Basiswand:WD 200 + Luft 40 + Bekleidung 12" ("Faserzementplatte (Equitone - natura)" 0.012, "Luftschicht" 0.04, "Steinwolle (Rockwool Fixrock033 VS)" 0.2) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCCURTAINWALLTYPE "Fassade:Standard" | 1 occurrence | property sets: Pset_CurtainWallCommon, Pset_EnvironmentalImpactIndicators
  IFCWINDOWTYPE "FE 3 tlg - DK-Fix im Rahmen-DK-2:6000 x 1500" | WINDOW | 34 occurrences | material: materials ("<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "Metall - Edelstahl gebürstet") | property sets: FE 3 tlg - DK-Fix im Rahmen-DK-2:6000 x 1500:2529359, Pset_DoorWindowGlazingType, Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
  IFCWINDOWTYPE "FE 3 tlg - DK-Fix im Rahmen-DK-2:6000 x 1500" | WINDOW | 1 occurrence | material: materials ("<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "Metall - Edelstahl gebürstet") | property sets: FE 3 tlg - DK-Fix im Rahmen-DK-2:6000 x 1500:2545646, Pset_DoorWindowGlazingType, Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
  IFCWALLTYPE "Basiswand:Metall-Einfachständerwand 2-lagig beplankt (MW12BF)" | 46 occurrences | material: layers "Basiswand:Metall-Einfachständerwand 2-lagig beplankt (MW12BF)" ("Trockenbau - Rigips Die Blaue RFI" 0.025, "Dämmung - Isover Akustik TF" 0.08, "Luftschicht" 0.02, "Trockenbau - Rigips Die Blaue RFI" 0.025) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCDOORTYPE "TU DF 1 - Rahmenstock flächenbündig:DL - 1000 x 2000" | DOOR | SINGLE_SWING_RIGHT | 15 occurrences | material: materials ("<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "Holz - generisch 140-100-70") | property sets: TU DF 1 - Rahmenstock flächenbündig:DL - 1000 x 2000:2549490, Pset_DoorCommon, Pset_DoorWindowGlazingType, Pset_EnvironmentalImpactIndicators
  IFCDOORTYPE "TU DF 1 - Rahmenstock flächenbündig:DL - 1000 x 2000" | DOOR | SINGLE_SWING_LEFT | 16 occurrences | material: materials ("<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "Holz - generisch 140-100-70") | property sets: TU DF 1 - Rahmenstock flächenbündig:DL - 1000 x 2000:2549557, Pset_DoorCommon, Pset_DoorWindowGlazingType, Pset_EnvironmentalImpactIndicators
  IFCDOORTYPE "TU DF 2 - Rahmenstock flächenbündig:ML - 1635 x 2135" | DOOR | DOUBLE_DOOR_SINGLE_SWING | 1 occurrence | material: materials ("<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "Holz - generisch 140-100-70") | property sets: TU DF 2 - Rahmenstock flächenbündig:ML - 1635 x 2135:2550600, Pset_DoorCommon, Pset_DoorWindowGlazingType, Pset_EnvironmentalImpactIndicators
  IFCCOVERINGTYPE "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_EnvironmentalImpactIndicators
  IFCCOVERINGTYPE "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_EnvironmentalImpactIndicators
  IFCCOVERINGTYPE "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_EnvironmentalImpactIndicators
  IFCCOVERINGTYPE "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_EnvironmentalImpactIndicators
  IFCCOVERINGTYPE "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_EnvironmentalImpactIndicators
  IFCCOVERINGTYPE "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_EnvironmentalImpactIndicators
  IFCCOVERINGTYPE "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_EnvironmentalImpactIndicators
  IFCCOVERINGTYPE "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_EnvironmentalImpactIndicators
  IFCCOVERINGTYPE "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_EnvironmentalImpactIndicators
  IFCCOVERINGTYPE "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_EnvironmentalImpactIndicators
  IFCCOVERINGTYPE "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_EnvironmentalImpactIndicators
  IFCWINDOWTYPE "FE 2 tlg - DK Fix mit Pfosten - 2:4000 x 1500" | WINDOW | 4 occurrences | material: materials ("<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "Metall - Edelstahl gebürstet") | property sets: FE 2 tlg - DK Fix mit Pfosten - 2:4000 x 1500:2536377, Pset_DoorWindowGlazingType, Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
  IFCWINDOWTYPE "FE 2 tlg - DK Fix mit Pfosten - 2:4000 x 1500" | WINDOW | 4 occurrences | material: materials ("<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "Metall - Edelstahl gebürstet") | property sets: FE 2 tlg - DK Fix mit Pfosten - 2:4000 x 1500:2544255, Pset_DoorWindowGlazingType, Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
  IFCCOVERINGTYPE "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_EnvironmentalImpactIndicators
  IFCWALLTYPE "Basiswand:Metall-Einfachständerwand 2-lagig beplankt - Sanitär" | 4 occurrences | material: layers "Basiswand:Metall-Einfachständerwand 2-lagig beplankt - Sanitär" ("Trockenbau - Rigips Die Blaue RFI" 0.025, "Steinwolle (Rockwool Fixrock033 VS)" 0.08, "Luftschicht" 0.19, "Steinwolle (Rockwool Fixrock033 VS)" 0.08, "Trockenbau - Rigips Die Blaue RFI" 0.025) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCDOORTYPE "TU DF 1 - Stahl-Eckzarge Falztüre:DL - 800 x 2000" | DOOR | SINGLE_SWING_RIGHT | 4 occurrences | material: materials ("<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "Holz - generisch 140-100-70") | property sets: TU DF 1 - Stahl-Eckzarge Falztüre:DL - 800 x 2000:2699597, Pset_DoorCommon, Pset_DoorWindowGlazingType, Pset_EnvironmentalImpactIndicators
  IFCDOORTYPE "TU DF 1 - Stahl-Eckzarge Falztüre:DL - 800 x 2000" | DOOR | SINGLE_SWING_LEFT | 4 occurrences | material: materials ("<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "Holz - generisch 140-100-70") | property sets: TU DF 1 - Stahl-Eckzarge Falztüre:DL - 800 x 2000:2699634, Pset_DoorCommon, Pset_DoorWindowGlazingType, Pset_EnvironmentalImpactIndicators
  IFCCOVERINGTYPE "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_EnvironmentalImpactIndicators
  IFCCOVERINGTYPE "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_EnvironmentalImpactIndicators
  IFCCOVERINGTYPE "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_EnvironmentalImpactIndicators
  IFCCOVERINGTYPE "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_EnvironmentalImpactIndicators
  IFCWALLTYPE "Basiswand:GK VS - Sanitär" | 4 occurrences | material: layers "Basiswand:GK VS - Sanitär" ("Trockenbau - Gipsplatte" 0.025, "Dämmung - weich" 0.04) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Basiswand:GK 100 - Doppelbeplankt" | 8 occurrences | material: layers "Basiswand:GK 100 - Doppelbeplankt" ("Trockenbau - Gipsplatte" 0.025, "Dämmung - weich" 0.05, "Trockenbau - Gipsplatte" 0.025) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Basiswand:GK 75 - Toilettentrennwand" | 16 occurrences | material: layers "Basiswand:GK 75 - Toilettentrennwand" ("Trockenbau - Gipsplatte" 0.0125, "Dämmung - weich" 0.05, "Trockenbau - Gipsplatte" 0.0125) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCDOORTYPE "TU DF 2 - Rahmenstock flächenbündig:ML - 1635 x 2135" | DOOR | DOUBLE_DOOR_SINGLE_SWING | 1 occurrence | material: materials ("<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "Holz - generisch 140-100-70") | property sets: TU DF 2 - Rahmenstock flächenbündig:ML - 1635 x 2135:2749010, Pset_DoorCommon, Pset_DoorWindowGlazingType, Pset_EnvironmentalImpactIndicators
  IFCSLABTYPE "Geschossdecke:STB 250" | FLOOR | 1 occurrence | material: layers "Geschossdecke:STB 250" ("Ortbeton - bewehrt" 0.25) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Geschossdecke:STB 250" | FLOOR | 1 occurrence | material: layers "Geschossdecke:STB 250" ("Ortbeton - bewehrt" 0.25) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 400" | COLUMN | 1 occurrence | material: profiles "STB 250 x 400" ("STB 250 x 400": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 400" | COLUMN | 1 occurrence | material: profiles "STB 250 x 400" ("STB 250 x 400": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 400" | COLUMN | 1 occurrence | material: profiles "STB 250 x 400" ("STB 250 x 400": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 400" | COLUMN | 1 occurrence | material: profiles "STB 250 x 400" ("STB 250 x 400": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 400" | COLUMN | 1 occurrence | material: profiles "STB 250 x 400" ("STB 250 x 400": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 400" | COLUMN | 1 occurrence | material: profiles "STB 250 x 400" ("STB 250 x 400": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 400" | COLUMN | 1 occurrence | material: profiles "STB 250 x 400" ("STB 250 x 400": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 400" | COLUMN | 1 occurrence | material: profiles "STB 250 x 400" ("STB 250 x 400": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 400" | COLUMN | 1 occurrence | material: profiles "STB 250 x 400" ("STB 250 x 400": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 400" | COLUMN | 1 occurrence | material: profiles "STB 250 x 400" ("STB 250 x 400": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 400" | COLUMN | 1 occurrence | material: profiles "STB 250 x 400" ("STB 250 x 400": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 400" | COLUMN | 1 occurrence | material: profiles "STB 250 x 400" ("STB 250 x 400": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 250" | COLUMN | 1 occurrence | material: profiles "STB 250 x 250" ("STB 250 x 250": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 250" | COLUMN | 1 occurrence | material: profiles "STB 250 x 250" ("STB 250 x 250": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 250" | COLUMN | 1 occurrence | material: profiles "STB 250 x 250" ("STB 250 x 250": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 250" | COLUMN | 1 occurrence | material: profiles "STB 250 x 250" ("STB 250 x 250": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 250" | COLUMN | 1 occurrence | material: profiles "STB 250 x 250" ("STB 250 x 250": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 250" | COLUMN | 1 occurrence | material: profiles "STB 250 x 250" ("STB 250 x 250": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 250" | COLUMN | 1 occurrence | material: profiles "STB 250 x 250" ("STB 250 x 250": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 250" | COLUMN | 1 occurrence | material: profiles "STB 250 x 250" ("STB 250 x 250": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
  IFCBEAMTYPE "STB Träger - rechteckig:STB 250 x 500" | BEAM | 1 occurrence | material: profiles "STB 250 x 500" ("STB 250 x 500": "Ortbeton - bewehrt") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
  IFCBEAMTYPE "STB Träger - rechteckig:STB 250 x 500" | BEAM | 1 occurrence | material: profiles "STB 250 x 500" ("STB 250 x 500": "Ortbeton - bewehrt") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
  IFCBEAMTYPE "STB Träger - rechteckig:STB 250 x 500" | BEAM | 1 occurrence | material: profiles "STB 250 x 500" ("STB 250 x 500": "Ortbeton - bewehrt") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
  IFCBEAMTYPE "STB Träger - rechteckig:STB 250 x 500" | BEAM | 1 occurrence | material: profiles "STB 250 x 500" ("STB 250 x 500": "Ortbeton - bewehrt") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
  IFCBEAMTYPE "STB Träger - rechteckig:STB 250 x 500" | BEAM | 1 occurrence | material: profiles "STB 250 x 500" ("STB 250 x 500": "Ortbeton - bewehrt") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
  IFCBEAMTYPE "STB Träger - rechteckig:STB 250 x 500" | BEAM | 1 occurrence | material: profiles "STB 250 x 500" ("STB 250 x 500": "Ortbeton - bewehrt") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
  IFCBEAMTYPE "STB Träger - rechteckig:STB 250 x 500" | BEAM | 1 occurrence | material: profiles "STB 250 x 500" ("STB 250 x 500": "Ortbeton - bewehrt") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
  IFCBEAMTYPE "STB Träger - rechteckig:STB 250 x 500" | BEAM | 1 occurrence | material: profiles "STB 250 x 500" ("STB 250 x 500": "Ortbeton - bewehrt") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
  IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 400" | COLUMN | 1 occurrence | material: profiles "STB 250 x 400" ("STB 250 x 400": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 400" | COLUMN | 1 occurrence | material: profiles "STB 250 x 400" ("STB 250 x 400": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 250" | COLUMN | 1 occurrence | material: profiles "STB 250 x 250" ("STB 250 x 250": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 250" | COLUMN | 1 occurrence | material: profiles "STB 250 x 250" ("STB 250 x 250": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 400" | COLUMN | 1 occurrence | material: profiles "STB 250 x 400" ("STB 250 x 400": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 400" | COLUMN | 1 occurrence | material: profiles "STB 250 x 400" ("STB 250 x 400": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 250" | COLUMN | 1 occurrence | material: profiles "STB 250 x 250" ("STB 250 x 250": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 250" | COLUMN | 1 occurrence | material: profiles "STB 250 x 250" ("STB 250 x 250": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 250" | COLUMN | 1 occurrence | material: profiles "STB 250 x 250" ("STB 250 x 250": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 250" | COLUMN | 1 occurrence | material: profiles "STB 250 x 250" ("STB 250 x 250": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 250" | COLUMN | 1 occurrence | material: profiles "STB 250 x 250" ("STB 250 x 250": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "STB Stütze - rechteckig:STB 250 x 250" | COLUMN | 1 occurrence | material: profiles "STB 250 x 250" ("STB 250 x 250": "Ortbeton - bewehrt") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
  IFCCURTAINWALLTYPE "Dachverglasung:Dachverglasung" | 2 occurrences | property sets: Pset_CurtainWallCommon, Pset_EnvironmentalImpactIndicators
  IFCSLABTYPE "Geschossdecke:FB 150 leer" | FLOOR | 1 occurrence | material: layers "Geschossdecke:FB 150 leer" ("Fußbodenaufbau" 0.15) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Geschossdecke:FB 150 leer" | FLOOR | 1 occurrence | material: layers "Geschossdecke:FB 150 leer" ("Fußbodenaufbau" 0.15) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Geschossdecke:FB 150 leer" | FLOOR | 1 occurrence | material: layers "Geschossdecke:FB 150 leer" ("Fußbodenaufbau" 0.15) | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCCOVERINGTYPE "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_EnvironmentalImpactIndicators
  IFCCOVERINGTYPE "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_EnvironmentalImpactIndicators
  IFCCOVERINGTYPE "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_EnvironmentalImpactIndicators
  IFCCOVERINGTYPE "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_EnvironmentalImpactIndicators
  IFCCOVERINGTYPE "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_EnvironmentalImpactIndicators
  IFCCOVERINGTYPE "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_EnvironmentalImpactIndicators
  IFCCOVERINGTYPE "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_EnvironmentalImpactIndicators
  IFCCOVERINGTYPE "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_EnvironmentalImpactIndicators
  IFCCOVERINGTYPE "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_EnvironmentalImpactIndicators
  IFCCOVERINGTYPE "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_EnvironmentalImpactIndicators
  IFCCOVERINGTYPE "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_EnvironmentalImpactIndicators
  IFCCOVERINGTYPE "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_EnvironmentalImpactIndicators
  IFCCOVERINGTYPE "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_EnvironmentalImpactIndicators
  IFCCOVERINGTYPE "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_EnvironmentalImpactIndicators
  IFCCOVERINGTYPE "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_EnvironmentalImpactIndicators
  IFCCOVERINGTYPE "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_EnvironmentalImpactIndicators
  IFCCOVERINGTYPE "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_EnvironmentalImpactIndicators
  IFCWINDOWTYPE "FE 1 tlg - DrehKipp:2000 x 1500" | WINDOW | 2 occurrences | material: materials ("<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "Metall - Edelstahl gebürstet") | property sets: FE 1 tlg - DrehKipp:2000 x 1500:2653437, Pset_DoorWindowGlazingType, Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
  IFCWINDOWTYPE "FE 1 tlg - DrehKipp:2000 x 1500" | WINDOW | 2 occurrences | material: materials ("<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "Metall - Edelstahl gebürstet") | property sets: FE 1 tlg - DrehKipp:2000 x 1500:2660375, Pset_DoorWindowGlazingType, Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
  IFCCOVERINGTYPE "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_EnvironmentalImpactIndicators
  IFCCOVERINGTYPE "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_EnvironmentalImpactIndicators
  IFCCOVERINGTYPE "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_EnvironmentalImpactIndicators
  IFCCOVERINGTYPE "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_EnvironmentalImpactIndicators
  IFCCOVERINGTYPE "Deckensystem:Abgehängte Decke - Rigips Die Dicke 25" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_EnvironmentalImpactIndicators
  IFCROOFTYPE "Basisdach:Flachdachaufbau begrünt 320" | 1 occurrence | property sets: Pset_EnvironmentalImpactIndicators, Pset_RoofCommon

Property sets
  Pset_SiteCommon | properties | on 1 object (1 IFCSITE)
    Reference = "Projektinformationen" (IFCIDENTIFIER)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCSPACE)
    Name = "Flur - UG" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCSPACE)
    Name = "Putzmittel" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCSPACE)
    Name = "Hausanschluss" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCSPACE)
    Name = "Wasser-/Gasverteilung" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCSPACE)
    Name = "Heizzentrale" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCSPACE)
    Name = "NSHV" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCSPACE)
    Name = "Lager 1" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCSPACE)
    Name = "Lager2" (IFCLABEL)
  Pset_AirSideSystemInformation: 56 more contents on 56 objects not shown
  Pset_SpaceCommon | properties | on 1 object (1 IFCSPACE)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Flur - UG 0-1" (IFCIDENTIFIER)
  Pset_SpaceCommon | properties | on 1 object (1 IFCSPACE)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Putzmittel 0-2" (IFCIDENTIFIER)
  Pset_SpaceCommon | properties | on 1 object (1 IFCSPACE)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Hausanschluss 0-3" (IFCIDENTIFIER)
  Pset_SpaceCommon | properties | on 1 object (1 IFCSPACE)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Wasser-/Gasverteilung 0-4" (IFCIDENTIFIER)
  Pset_SpaceCommon | properties | on 1 object (1 IFCSPACE)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Heizzentrale 0-5" (IFCIDENTIFIER)
  Pset_SpaceCommon | properties | on 1 object (1 IFCSPACE)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "NSHV 0-6" (IFCIDENTIFIER)
  Pset_SpaceCommon | properties | on 1 object (1 IFCSPACE)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Lager 1 0-7" (IFCIDENTIFIER)
  Pset_SpaceCommon | properties | on 1 object (1 IFCSPACE)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Lager2 0-8" (IFCIDENTIFIER)
  Pset_SpaceCommon: 56 more contents on 56 objects not shown
  Pset_SpaceHeaterTypeCommon | properties | on 1 object (1 IFCSPACE)
    Reference = "Flur - UG 0-1" (IFCIDENTIFIER)
  Pset_SpaceHeaterTypeCommon | properties | on 1 object (1 IFCSPACE)
    Reference = "Putzmittel 0-2" (IFCIDENTIFIER)
  Pset_SpaceHeaterTypeCommon | properties | on 1 object (1 IFCSPACE)
    Reference = "Hausanschluss 0-3" (IFCIDENTIFIER)
  Pset_SpaceHeaterTypeCommon | properties | on 1 object (1 IFCSPACE)
    Reference = "Wasser-/Gasverteilung 0-4" (IFCIDENTIFIER)
  Pset_SpaceHeaterTypeCommon | properties | on 1 object (1 IFCSPACE)
    Reference = "Heizzentrale 0-5" (IFCIDENTIFIER)
  Pset_SpaceHeaterTypeCommon | properties | on 1 object (1 IFCSPACE)
    Reference = "NSHV 0-6" (IFCIDENTIFIER)
  Pset_SpaceHeaterTypeCommon | properties | on 1 object (1 IFCSPACE)
    Reference = "Lager 1 0-7" (IFCIDENTIFIER)
  Pset_SpaceHeaterTypeCommon | properties | on 1 object (1 IFCSPACE)
    Reference = "Lager2 0-8" (IFCIDENTIFIER)
  Pset_SpaceHeaterTypeCommon: 56 more contents on 56 objects not shown
  Pset_SpaceOccupancyRequirements | properties | on 45 objects (45 IFCSPACE)
    MinimumHeadroom = 3. (IFCLENGTHMEASURE) [METRE]
  Pset_SpaceOccupancyRequirements | properties | on 10 objects (10 IFCSPACE)
    MinimumHeadroom = 2.4384 (IFCLENGTHMEASURE) [METRE]
  Pset_SpaceOccupancyRequirements | properties | on 4 objects (4 IFCSPACE)
    MinimumHeadroom = 7.77 (IFCLENGTHMEASURE) [METRE]
  Pset_SpaceOccupancyRequirements | properties | on 2 objects (2 IFCSPACE)
    MinimumHeadroom = 10.77 (IFCLENGTHMEASURE) [METRE]
  Pset_SpaceOccupancyRequirements | properties | on 1 object (1 IFCSPACE)
    MinimumHeadroom = 3.22 (IFCLENGTHMEASURE) [METRE]
  Pset_SpaceOccupancyRequirements | properties | on 1 object (1 IFCSPACE)
    MinimumHeadroom = 3.9 (IFCLENGTHMEASURE) [METRE]
  Pset_SpaceOccupancyRequirements | properties | on 1 object (1 IFCSPACE)
    MinimumHeadroom = 3.65 (IFCLENGTHMEASURE) [METRE]
  Pset_ColumnCommon | properties | on 32 objects (32 IFCCOLUMN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "STB 250 x 400" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_ColumnCommon | properties | on 30 objects (30 IFCCOLUMN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "STB 250 x 250" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_ColumnCommon | properties | on 32 type objects
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "STB 250 x 400" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 29 type objects
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "STB 250 x 250" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 70 objects (35 IFCOPENINGELEMENT, 35 IFCWINDOW) | on 2 type objects
    Reference = "6000 x 1500" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 54 objects (54 IFCMEMBER)
    Reference = "60 x 120" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 49 objects (39 IFCOPENINGELEMENT, 10 IFCWALL) | on 1 type object
    Reference = "Leichtbetonmauerwerk 250" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 46 objects (46 IFCWALL) | on 1 type object
    Reference = "Metall-Einfachständerwand 2-lagig beplankt (MW12BF)" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 45 objects (44 IFCDOOR, 1 IFCOPENINGELEMENT) | on 4 type objects
    Reference = "DL - 1000 x 2000" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 45 objects (45 IFCWALL) | on 1 type object
    Reference = "STB 200" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 45 objects (45 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "B 120" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 38 objects (38 IFCCOVERING) | on 38 type objects
    Reference = "Abgehängte Decke - Rigips Die Dicke 25" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators: 47 more contents on 454 objects not shown
  Pset_ReinforcementBarPitchOfColumn | properties | on 32 objects (32 IFCCOLUMN) | on 32 type objects
    Reference = "STB 250 x 400" (IFCLABEL)
  Pset_ReinforcementBarPitchOfColumn | properties | on 30 objects (30 IFCCOLUMN) | on 29 type objects
    Reference = "STB 250 x 250" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 6 objects (6 IFCSLAB) | on 6 type objects
    Reference = "FB 150 leer" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 4 objects (4 IFCSLAB)
    Reference = "Podest 180" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 3 objects (3 IFCSLAB) | on 3 type objects
    Reference = "Sohle 1 mm" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 2 objects (2 IFCSLAB) | on 2 type objects
    Reference = "STB 250" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 2 objects (2 IFCSLAB) | on 2 type objects
    Reference = "STB 220" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 2 objects (2 IFCSLAB) | on 2 type objects
    Reference = "WD 200 hart" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 1 object (1 IFCSLAB) | on 1 type object
    Reference = "STB 300" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 1 object (1 IFCSLAB) | on 1 type object
    Reference = "FB 100 leer" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab: 3 more contents on 3 objects not shown
  Pset_SlabCommon | properties | on 6 objects (6 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "FB 150 leer" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 4 objects (4 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Podest 180" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 3 objects (3 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Sohle 1 mm" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 2 objects (2 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "STB 250" (IFCIDENTIFIER)
    ThermalTransmittance = 1.628 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_SlabCommon | properties | on 2 objects (2 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "STB 220" (IFCIDENTIFIER)
    ThermalTransmittance = 1.85 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_SlabCommon | properties | on 2 objects (2 IFCSLAB)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "WD 200 hart" (IFCIDENTIFIER)
    ThermalTransmittance = 0.135 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "STB 300" (IFCIDENTIFIER)
    ThermalTransmittance = 1.35666666666667 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Podest (nicht massiv)" (IFCIDENTIFIER)
  Pset_SlabCommon: 11 more contents on 3 objects not shown
  Pset_OpeningElementCommon | properties | on 70 objects (35 IFCOPENINGELEMENT, 35 IFCWINDOW)
    Reference = "6000 x 1500" (IFCIDENTIFIER)
  Pset_OpeningElementCommon | properties | on 39 objects (39 IFCOPENINGELEMENT)
    Reference = "Leichtbetonmauerwerk 250" (IFCIDENTIFIER)
  Pset_OpeningElementCommon | properties | on 24 objects (16 IFCOPENINGELEMENT, 8 IFCWINDOW)
    Reference = "4000 x 1500" (IFCIDENTIFIER)
  Pset_OpeningElementCommon | properties | on 16 objects (16 IFCOPENINGELEMENT)
    Reference = "GK 75 - Toilettentrennwand" (IFCIDENTIFIER)
  Pset_OpeningElementCommon | properties | on 8 objects (4 IFCOPENINGELEMENT, 4 IFCWINDOW)
    Reference = "2000 x 1500" (IFCIDENTIFIER)
  Pset_OpeningElementCommon | properties | on 5 objects (5 IFCOPENINGELEMENT)
    Reference = "STB 250" (IFCIDENTIFIER)
  Pset_OpeningElementCommon | properties | on 3 objects (3 IFCOPENINGELEMENT)
    Reference = "FB 150 leer" (IFCIDENTIFIER)
  Pset_OpeningElementCommon | properties | on 3 objects (3 IFCOPENINGELEMENT)
    Reference = "WD hart 200" (IFCIDENTIFIER)
  Pset_OpeningElementCommon: 4 more contents on 7 objects not shown
  Pset_ReinforcementBarPitchOfWall | properties | on 46 objects (46 IFCWALL) | on 1 type object
    Reference = "Metall-Einfachständerwand 2-lagig beplankt (MW12BF)" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 45 objects (45 IFCWALL) | on 1 type object
    Reference = "STB 200" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 25 objects (25 IFCWALL) | on 1 type object
    Reference = "STB 250" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 16 objects (16 IFCWALL) | on 1 type object
    Reference = "GK 75 - Toilettentrennwand" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 12 objects (12 IFCWALL) | on 1 type object
    Reference = "WD hart 200" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 10 objects (10 IFCWALL) | on 1 type object
    Reference = "Leichtbetonmauerwerk 250" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 8 objects (8 IFCWALL) | on 1 type object
    Reference = "GK 100 - Doppelbeplankt" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 4 objects (4 IFCWALL) | on 1 type object
    Reference = "STB 300" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall: 3 more contents on 12 objects not shown
  Pset_WallCommon | properties | on 46 objects (46 IFCWALL)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Metall-Einfachständerwand 2-lagig beplankt (MW12BF)" (IFCIDENTIFIER)
    ThermalTransmittance = 0.333333333333333 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 45 objects (45 IFCWALL)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "STB 200" (IFCIDENTIFIER)
    ThermalTransmittance = 2.035 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 25 objects (25 IFCWALL)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "STB 250" (IFCIDENTIFIER)
    ThermalTransmittance = 1.628 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 16 objects (16 IFCWALL)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "GK 75 - Toilettentrennwand" (IFCIDENTIFIER)
    ThermalTransmittance = 0.740740740740741 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 12 objects (12 IFCWALL)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "WD hart 200" (IFCIDENTIFIER)
    ThermalTransmittance = 0.135 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 10 objects (10 IFCWALL)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Leichtbetonmauerwerk 250" (IFCIDENTIFIER)
    ThermalTransmittance = 4. (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 8 objects (8 IFCWALL)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "GK 100 - Doppelbeplankt" (IFCIDENTIFIER)
    ThermalTransmittance = 0.689655172413793 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 4 objects (4 IFCWALL)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "STB 300" (IFCIDENTIFIER)
    ThermalTransmittance = 1.35666666666667 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon: 14 more contents on 12 objects not shown
  Pset_BeamCommon | properties | on 8 objects (8 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "STB 250 x 500" (IFCIDENTIFIER)
    Roll = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 7. (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_BeamCommon | properties | on 6 objects (6 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "STB 250 x 500" (IFCIDENTIFIER)
    Roll = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 5.6 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_BeamCommon | properties | on 14 type objects
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "STB 250 x 500" (IFCIDENTIFIER)
  Pset_ReinforcementBarPitchOfBeam | properties | on 14 objects (14 IFCBEAM) | on 14 type objects
    Reference = "STB 250 x 500" (IFCLABEL)
  Pset_StairCommon | properties | on 2 objects (2 IFCSTAIR)
    IsExternal = FALSE (IFCBOOLEAN)
    NosingLength = 0. (IFCLENGTHMEASURE) [METRE]
    NumberOfRiser = 18. (IFCCOUNTMEASURE)
    NumberOfTreads = 18. (IFCCOUNTMEASURE)
    Reference = "Fertigbetontreppe - 2 Stockwerkstrennlinien" (IFCIDENTIFIER)
    RiserHeight = 0.178888888888889 (IFCPOSITIVELENGTHMEASURE) [METRE]
    TreadLength = 0.277222222222222 (IFCPOSITIVELENGTHMEASURE) [METRE]
    TreadLengthAtInnerSide = 0.277222222222222 (IFCPOSITIVELENGTHMEASURE) [METRE]
    TreadLengthAtOffset = 0.277222222222222 (IFCPOSITIVELENGTHMEASURE) [METRE]
    WalkingLineOffset = 2.13254593175853 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_StairCommon | properties | on 2 objects (2 IFCSTAIR)
    IsExternal = FALSE (IFCBOOLEAN)
    NosingLength = 0. (IFCLENGTHMEASURE) [METRE]
    NumberOfRiser = 22. (IFCCOUNTMEASURE)
    NumberOfTreads = 22. (IFCCOUNTMEASURE)
    Reference = "Fertigbetontreppe - 2 Stockwerkstrennlinien" (IFCIDENTIFIER)
    RiserHeight = 0.177272727272727 (IFCPOSITIVELENGTHMEASURE) [METRE]
    TreadLength = 0.27 (IFCPOSITIVELENGTHMEASURE) [METRE]
    TreadLengthAtInnerSide = 0.27 (IFCPOSITIVELENGTHMEASURE) [METRE]
    TreadLengthAtOffset = 0.27 (IFCPOSITIVELENGTHMEASURE) [METRE]
    WalkingLineOffset = 2.13254593175853 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_StairCommon | properties | on 1 object (1 IFCSTAIR)
    IsExternal = FALSE (IFCBOOLEAN)
    NosingLength = 0.03 (IFCLENGTHMEASURE) [METRE]
    NumberOfRiser = 22. (IFCCOUNTMEASURE)
    NumberOfTreads = 22. (IFCCOUNTMEASURE)
    Reference = "Wangen Stahl - Stufen Stahl - 2 Stockwerkstrennlinien" (IFCIDENTIFIER)
    RiserHeight = 0.177272727272727 (IFCPOSITIVELENGTHMEASURE) [METRE]
    TreadLength = 0.280454545454545 (IFCPOSITIVELENGTHMEASURE) [METRE]
    TreadLengthAtInnerSide = 0.280454545454545 (IFCPOSITIVELENGTHMEASURE) [METRE]
    TreadLengthAtOffset = 0.280454545454545 (IFCPOSITIVELENGTHMEASURE) [METRE]
    WalkingLineOffset = 2.13254593175853 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_StairCommon | properties | on 4 type objects
    IsExternal = FALSE (IFCBOOLEAN)
    NosingLength = 0. (IFCLENGTHMEASURE) [METRE]
    NumberOfRiser = 0. (IFCCOUNTMEASURE)
    NumberOfTreads = 0. (IFCCOUNTMEASURE)
    Reference = "Fertigbetontreppe - 2 Stockwerkstrennlinien" (IFCIDENTIFIER)
  Pset_StairCommon | properties | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    NosingLength = 0. (IFCLENGTHMEASURE) [METRE]
    NumberOfRiser = 0. (IFCCOUNTMEASURE)
    NumberOfTreads = 0. (IFCCOUNTMEASURE)
    Reference = "Wangen Stahl - Stufen Stahl - 2 Stockwerkstrennlinien" (IFCIDENTIFIER)
  Pset_StairFlightCommon | properties | on 4 objects (4 IFCSTAIRFLIGHT)
    NosingLength = 0. (IFCLENGTHMEASURE) [METRE]
    NumberOfRiser = 9. (IFCCOUNTMEASURE)
    NumberOfTreads = 9. (IFCCOUNTMEASURE)
    Reference = "Naturstein - Auftritt 40 / Trittüberstand 30" (IFCIDENTIFIER)
    RiserHeight = 0.3048 (IFCPOSITIVELENGTHMEASURE) [METRE]
    TreadLength = 0.3048 (IFCPOSITIVELENGTHMEASURE) [METRE]
    TreadLengthAtInnerSide = 0.277222222222222 (IFCPOSITIVELENGTHMEASURE) [METRE]
    TreadLengthAtOffset = 0.277222222222222 (IFCPOSITIVELENGTHMEASURE) [METRE]
    WalkingLineOffset = 2.13254593175853 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_StairFlightCommon | properties | on 4 objects (4 IFCSTAIRFLIGHT)
    NosingLength = 0. (IFCLENGTHMEASURE) [METRE]
    NumberOfRiser = 11. (IFCCOUNTMEASURE)
    NumberOfTreads = 11. (IFCCOUNTMEASURE)
    Reference = "Naturstein - Auftritt 40 / Trittüberstand 30" (IFCIDENTIFIER)
    RiserHeight = 0.3048 (IFCPOSITIVELENGTHMEASURE) [METRE]
    TreadLength = 0.3048 (IFCPOSITIVELENGTHMEASURE) [METRE]
    TreadLengthAtInnerSide = 0.27 (IFCPOSITIVELENGTHMEASURE) [METRE]
    TreadLengthAtOffset = 0.27 (IFCPOSITIVELENGTHMEASURE) [METRE]
    WalkingLineOffset = 2.13254593175853 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_StairFlightCommon | properties | on 2 objects (2 IFCSTAIR)
    NosingLength = 0. (IFCLENGTHMEASURE) [METRE]
    NumberOfRiser = 18. (IFCCOUNTMEASURE)
    NumberOfTreads = 18. (IFCCOUNTMEASURE)
    Reference = "Fertigbetontreppe - 2 Stockwerkstrennlinien" (IFCIDENTIFIER)
    RiserHeight = 0.178888888888889 (IFCPOSITIVELENGTHMEASURE) [METRE]
    TreadLength = 0.277222222222222 (IFCPOSITIVELENGTHMEASURE) [METRE]
    TreadLengthAtInnerSide = 0.277222222222222 (IFCPOSITIVELENGTHMEASURE) [METRE]
    TreadLengthAtOffset = 0.277222222222222 (IFCPOSITIVELENGTHMEASURE) [METRE]
    WalkingLineOffset = 2.13254593175853 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_StairFlightCommon | properties | on 2 objects (2 IFCSTAIR)
    NosingLength = 0. (IFCLENGTHMEASURE) [METRE]
    NumberOfRiser = 22. (IFCCOUNTMEASURE)
    NumberOfTreads = 22. (IFCCOUNTMEASURE)
    Reference = "Fertigbetontreppe - 2 Stockwerkstrennlinien" (IFCIDENTIFIER)
    RiserHeight = 0.177272727272727 (IFCPOSITIVELENGTHMEASURE) [METRE]
    TreadLength = 0.27 (IFCPOSITIVELENGTHMEASURE) [METRE]
    TreadLengthAtInnerSide = 0.27 (IFCPOSITIVELENGTHMEASURE) [METRE]
    TreadLengthAtOffset = 0.27 (IFCPOSITIVELENGTHMEASURE) [METRE]
    WalkingLineOffset = 2.13254593175853 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_StairFlightCommon | properties | on 2 objects (2 IFCSTAIRFLIGHT)
    NosingLength = 0.03 (IFCLENGTHMEASURE) [METRE]
    NumberOfRiser = 11. (IFCCOUNTMEASURE)
    NumberOfTreads = 11. (IFCCOUNTMEASURE)
    Reference = "Metall_20 mm Auftritt" (IFCIDENTIFIER)
    RiserHeight = 0.177272727272727 (IFCPOSITIVELENGTHMEASURE) [METRE]
    TreadLength = 0.3048 (IFCPOSITIVELENGTHMEASURE) [METRE]
    TreadLengthAtInnerSide = 0.280454545454545 (IFCPOSITIVELENGTHMEASURE) [METRE]
    TreadLengthAtOffset = 0.280454545454545 (IFCPOSITIVELENGTHMEASURE) [METRE]
    WalkingLineOffset = 2.13254593175853 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_StairFlightCommon | properties | on 1 object (1 IFCSTAIR)
    NosingLength = 0.03 (IFCLENGTHMEASURE) [METRE]
    NumberOfRiser = 22. (IFCCOUNTMEASURE)
    NumberOfTreads = 22. (IFCCOUNTMEASURE)
    Reference = "Wangen Stahl - Stufen Stahl - 2 Stockwerkstrennlinien" (IFCIDENTIFIER)
    RiserHeight = 0.177272727272727 (IFCPOSITIVELENGTHMEASURE) [METRE]
    TreadLength = 0.280454545454545 (IFCPOSITIVELENGTHMEASURE) [METRE]
    TreadLengthAtInnerSide = 0.280454545454545 (IFCPOSITIVELENGTHMEASURE) [METRE]
    TreadLengthAtOffset = 0.280454545454545 (IFCPOSITIVELENGTHMEASURE) [METRE]
    WalkingLineOffset = 2.13254593175853 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_StairFlightCommon | properties | on 4 type objects
    NosingLength = 0. (IFCLENGTHMEASURE) [METRE]
    NumberOfRiser = 0. (IFCCOUNTMEASURE)
    NumberOfTreads = 0. (IFCCOUNTMEASURE)
    Reference = "Fertigbetontreppe - 2 Stockwerkstrennlinien" (IFCIDENTIFIER)
  Pset_StairFlightCommon | properties | on 1 type object
    NosingLength = 0. (IFCLENGTHMEASURE) [METRE]
    NumberOfRiser = 0. (IFCCOUNTMEASURE)
    NumberOfTreads = 0. (IFCCOUNTMEASURE)
    Reference = "Wangen Stahl - Stufen Stahl - 2 Stockwerkstrennlinien" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 43 objects (43 IFCDOOR) | on 4 type objects
    FireRating (no value)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "DL - 1000 x 2000" (IFCIDENTIFIER)
    ThermalTransmittance = 1.8737 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_DoorCommon | properties | on 14 objects (8 IFCDOOR, 6 IFCOPENINGELEMENT)
    FireRating (no value)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "EN 179 - ML - 1010 x 2250" (IFCIDENTIFIER)
    ThermalTransmittance = 1.817 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_DoorCommon | properties | on 8 objects (8 IFCDOOR) | on 2 type objects
    FireRating (no value)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "DL - 800 x 2000" (IFCIDENTIFIER)
    ThermalTransmittance = 1.8737 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_DoorCommon | properties | on 6 objects (6 IFCDOOR) | on 4 type objects
    FireRating (no value)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "DL - 1200 x 2100" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 2 objects (2 IFCDOOR) | on 2 type objects
    FireRating (no value)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "ML - 1635 x 2135" (IFCIDENTIFIER)
    ThermalTransmittance = 1.8737 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_DoorCommon | properties | on 2 objects (2 IFCDOOR)
    FireRating (no value)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "GG - Türe 10 mm" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 4 type objects
    FireRating (no value)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "EN 179 - ML - 1010 x 2250" (IFCIDENTIFIER)
    ThermalTransmittance = 1.817 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_DoorWindowGlazingType | properties | on 67 objects (61 IFCDOOR, 6 IFCOPENINGELEMENT) | on 12 type objects
    SolarHeatGainTransmittance = 0. (IFCNORMALISEDRATIOMEASURE)
  Pset_DoorWindowGlazingType | properties | on 4 type objects
    SolarHeatGainTransmittance = 0.62 (IFCNORMALISEDRATIOMEASURE)
  Pset_DoorWindowGlazingType | properties | on 2 type objects
    SolarHeatGainTransmittance = 0.41 (IFCNORMALISEDRATIOMEASURE)
  Pset_MemberCommon | properties | on 18 objects (18 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "60 x 120" (IFCIDENTIFIER)
    Span = 1.388 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_MemberCommon | properties | on 16 objects (16 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "60 x 120" (IFCIDENTIFIER)
    Span = 2.70999999999999 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_MemberCommon | properties | on 8 objects (8 IFCMEMBER)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Metall 10 x 260" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_MemberCommon | properties | on 8 objects (8 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "60 x 120" (IFCIDENTIFIER)
    Span = 2.73999999999999 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_MemberCommon | properties | on 8 objects (8 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "60 x 120" (IFCIDENTIFIER)
    Span = 1.418 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_MemberCommon | properties | on 6 objects (6 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Standard 100-30-25" (IFCIDENTIFIER)
    Span = 1.9 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_MemberCommon | properties | on 4 objects (4 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "60 x 120" (IFCIDENTIFIER)
    Span = 1.358 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_MemberCommon | properties | on 2 objects (2 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Standard 100-30-25" (IFCIDENTIFIER)
    Span = 0.975000000000002 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_MemberCommon: 7 more contents on 10 objects not shown
  Pset_RoofCommon | properties | on 2 objects (2 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Dachverglasung" (IFCIDENTIFIER)
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF) | on 1 type object
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Flachdachaufbau begrünt 320" (IFCIDENTIFIER)
    ThermalTransmittance = 0.127876590044442 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_PlateCommon | properties | on 20 objects (20 IFCPLATE)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Glas 4/16/4" (IFCIDENTIFIER)
  Pset_PlateCommon | properties | on 5 objects (5 IFCPLATE)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Verglasung" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 45 objects (45 IFCBUILDINGELEMENTPROXY) | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "B 120" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 26 objects (26 IFCBUILDINGELEMENTPROXY) | on 2 type objects
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "2500 x 5000" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 26 objects (26 IFCBUILDINGELEMENTPROXY) | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "1000 x 700" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 22 objects (22 IFCBUILDINGELEMENTPROXY) | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Rotesche - 7,6 Meter" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 18 objects (18 IFCBUILDINGELEMENTPROXY) | on 5 type objects
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Typ1" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 5 objects (5 IFCBUILDINGELEMENTPROXY) | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "3000, 5 Räder" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Rechteckig_300x250" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDING)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Projektinformationen" (IFCIDENTIFIER)
  Pset_ProvisionForVoid | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    Depth = 0.005 (IFCPOSITIVELENGTHMEASURE) [METRE]
    Width = 0.005 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_ProvisionForVoid | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Depth = 0.001 (IFCPOSITIVELENGTHMEASURE) [METRE]
    Height = 4.99999999999999 (IFCPOSITIVELENGTHMEASURE) [METRE]
    Width = 0.001 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_ProvisionForVoid | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Depth = 0.001 (IFCPOSITIVELENGTHMEASURE) [METRE]
    Height = 0.1 (IFCPOSITIVELENGTHMEASURE) [METRE]
    Width = 0.001 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_ProvisionForVoid | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Depth = 0.00200000000000292 (IFCPOSITIVELENGTHMEASURE) [METRE]
    Height = 2. (IFCPOSITIVELENGTHMEASURE) [METRE]
    Width = 0.00200000000000292 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_ProvisionForVoid | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Depth = 0.05 (IFCPOSITIVELENGTHMEASURE) [METRE]
    Width = 0.05 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_CurtainWallCommon | properties | on 1 object (1 IFCCURTAINWALL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Standard" (IFCIDENTIFIER)
  Pset_CurtainWallCommon | properties | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Standard" (IFCIDENTIFIER)
  Pset_CurtainWallCommon | properties | on 1 type object
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Dachverglasung" (IFCIDENTIFIER)
  Pset_CoveringCommon | properties | on 38 objects (38 IFCCOVERING)
    Finish = "Trockenbau - Rigips Die Dicke RFI;" (IFCTEXT)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Abgehängte Decke - Rigips Die Dicke 25" (IFCIDENTIFIER)
    ThermalTransmittance = 10. (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_CoveringCommon | properties | on 38 type objects
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Abgehängte Decke - Rigips Die Dicke 25" (IFCIDENTIFIER)
    ThermalTransmittance = 10. (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_RailingCommon | properties | on 9 objects (9 IFCRAILING)
    Height = 1.2192 (IFCPOSITIVELENGTHMEASURE) [METRE]
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Vertikale Stäbe mit Handlauf" (IFCIDENTIFIER)
  Pset_RailingCommon | properties | on 4 objects (4 IFCRAILING)
    Height = 1.2192 (IFCPOSITIVELENGTHMEASURE) [METRE]
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Vertikale Stäbe" (IFCIDENTIFIER)
  Pset_BuildingStoreyCommon | properties | on 3 objects (3 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
    Reference = "Ebene" (IFCIDENTIFIER)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDING)
    AboveGround = UNKNOWN (IFCLOGICAL)
    Reference = "Projektinformationen" (IFCIDENTIFIER)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 3 (IFCINTEGER)
    Reference = "Projektinformationen" (IFCIDENTIFIER)
  Pset_BuildingSystemCommon | properties | on 1 object (1 IFCBUILDING)
    Reference = "Projektinformationen" (IFCIDENTIFIER)
  TU DF 1 - Rahmenstock flächenbündig:DL - 1000 x 2000:2432934 | predefined | on 2 type objects
  TU Durchgang:DL - 1200 x 2100:2426586 | predefined | on 2 type objects
  TU DF 1 - Rahmenstock flächenbündig:DL - 1000 x 2000:2432938 | predefined | on 2 type objects
  TU Durchgang:DL - 1200 x 2100:2426588 | predefined | on 2 type objects
  TU DF 1 - Fluchttüre Endausgang:EN 179 - ML - 1010 x 2250:2421088 | predefined | on 2 type objects
  TU DF 1 - Fluchttüre Endausgang:EN 179 - ML - 1010 x 2250:2421089 | predefined | on 2 type objects
  TU Durchgang:DL - 1200 x 2100:2421090 | predefined | on 2 type objects
  TU DF 1 - Fluchttüre Endausgang:EN 179 - ML - 1010 x 2250:2421363 | predefined | on 2 type objects
  TU Durchgang:DL - 1200 x 2100:2423932 | predefined | on 2 type objects
  TU DF 1 - Fluchttüre Endausgang:EN 179 - ML - 1010 x 2250:2423939 | predefined | on 2 type objects
  FE 3 tlg - DK-Fix im Rahmen-DK-2:6000 x 1500:2529359 | predefined | on 1 type object
  Pset_WindowCommon | properties | on 2 type objects
    FireRating (no value)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "6000 x 1500" (IFCIDENTIFIER)
    ThermalTransmittance = 0.8 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WindowCommon | properties | on 2 type objects
    FireRating (no value)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "4000 x 1500" (IFCIDENTIFIER)
    ThermalTransmittance = 1.4554 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WindowCommon | properties | on 2 type objects
    FireRating (no value)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "2000 x 1500" (IFCIDENTIFIER)
    ThermalTransmittance = 1.4554 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  FE 3 tlg - DK-Fix im Rahmen-DK-2:6000 x 1500:2545646 | predefined | on 1 type object
  TU DF 1 - Rahmenstock flächenbündig:DL - 1000 x 2000:2549490 | predefined | on 2 type objects
  TU DF 1 - Rahmenstock flächenbündig:DL - 1000 x 2000:2549557 | predefined | on 2 type objects
  TU DF 2 - Rahmenstock flächenbündig:ML - 1635 x 2135:2550600 | predefined | on 2 type objects
  FE 2 tlg - DK Fix mit Pfosten - 2:4000 x 1500:2536377 | predefined | on 1 type object
  FE 2 tlg - DK Fix mit Pfosten - 2:4000 x 1500:2544255 | predefined | on 1 type object
  TU DF 1 - Stahl-Eckzarge Falztüre:DL - 800 x 2000:2699597 | predefined | on 2 type objects
  TU DF 1 - Stahl-Eckzarge Falztüre:DL - 800 x 2000:2699634 | predefined | on 2 type objects
  TU DF 2 - Rahmenstock flächenbündig:ML - 1635 x 2135:2749010 | predefined | on 2 type objects
  FE 1 tlg - DrehKipp:2000 x 1500:2653437 | predefined | on 1 type object
  FE 1 tlg - DrehKipp:2000 x 1500:2660375 | predefined | on 1 type object

Other addresses and roles
  2 x postal address: "Projektadresse", "Platzl 9", "80331", "München", "Deutschland"