IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0, QuantityTakeOffAddOnView]"
File name: "170016"
Time stamp: "2021-01-12T15:32:57"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20190808_0900(x64) - Exporter 19.2.20.24 - Alternate UI 19.2.20.24"
Application: "Autodesk Revit 2019 (ENG)" version "2019" identifier "Revit" by Organization "Autodesk Revit 2019 (ENG)"

People and organizations
  Person "hkAAKU6" of Organization (no name given)
  Owner history of Person "hkAAKU6" of Organization (no name given) | application "Autodesk Revit 2019 (ENG)" version "2019" identifier "Revit" by Organization "Autodesk Revit 2019 (ENG)" | change NOCHANGE | created 1610460677 (2021-01-12T14:11:17Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "170016" | long name "Nittedal ungdomsskole" | phase "DETALJPROSJEKT"
  IFCSITE "Default" | latitude 59° 54′ 44.239196″ | longitude 10° 45′ 0″ | elevation above sea level 131200.
    IFCBUILDING | postal address: "Stasjonsveien 8-10", "Oslo", "Norway"
      IFCBUILDINGSTOREY "Plan 00U" | long name "Plan 00U" | elevation -4000.00000000053
        contains 32 elements
          5 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVL 5.1 100mm leca EI60" | object type "Basic Wall:IVL 5.1 100mm leca EI60:6657650" | names: "Basic Wall:IVL 5.1 100mm leca EI60:1769948", "Basic Wall:IVL 5.1 100mm leca EI60:2969152", "Basic Wall:IVL 5.1 100mm leca EI60:4089275" (+2 more) | material: layers "Basic Wall:IVL 5.1 100mm leca EI60" ("Mur" 100.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IV 100" | object type "Basic Wall:IV 100:1838506" | names: "Basic Wall:IV 100:1769965", "Basic Wall:IV 100:1770011", "Basic Wall:IV 100:1770095" (+1 more) | material: layers "Basic Wall:IV 100" ("hvit malt" 100.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCSLAB | object type "Floor:Betongdekke 250 + påstøp 70" | FLOOR | names: "Floor:Betongdekke 250 + påstøp 70:1851367" | material: layers "Floor:Betongdekke 250 + påstøp 70" ("Betong påstøp" 70., "Betong" 250.) | property sets: Pset_SlabCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Other
          2 x IFCSLAB | object type "Floor:Betongdekke 350" | FLOOR | names: "Floor:Betongdekke 350:1851385", "Floor:Betongdekke 350:3966644" | material: layers "Floor:Betongdekke 350" ("Betong" 350.) | property sets: Pset_SlabCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Other
          1 x IFCDOOR | type IFCDOORSTYLE "IDS 1.1 10x21 EI60S" | object type "IDS 1.1 10x21 EI60S" | names: "Dør Enkel:IDS 1.1 10x21 EI60S:2027286" | material: materials ("Light grey", "Lys grå", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDS 2.1 13x21M EI60S" | object type "IDS 2.1 13x21M EI60S" | names: "Dør Dobbel_Ulike_Dørblader:IDS 2.1 13x21M EI60S:2027581" | material: materials ("Lys grå", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCANNOTATION
          1 x IFCDOOR | type IFCDOORSTYLE "IDS 1.2 10x21M EI120CS" | object type "IDS 1.2 10x21M EI120CS" | names: "Dør Enkel:IDS 1.2 10x21M EI120CS:2294117" | material: materials ("Light grey", "Lys grå", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDS 2.1 13x21M EI60S" | object type "IDS 2.1 13x21M EI60S" | names: "Dør Dobbel_Ulike_Dørblader:IDS 2.1 13x21M EI60S:2294242" | material: materials ("Lys grå", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 3.3 145mm EI60 (RN-95-NR)" | object type "Basic Wall:IVA 3.3 145mm EI60 (RN-95-NR):2850935" | names: "Basic Wall:IVA 3.3 145mm EI60 (RN-95-NR):2775761", "Basic Wall:IVA 3.3 145mm EI60 (RN-95-NR):2775801" | material: layers "Basic Wall:IVA 3.3 145mm EI60 (RN-95-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          1 x IFCCOVERING | object type "Compound Ceiling:Himling System 600x600 hygiene" | CEILING | names: "Compound Ceiling:Himling System 600x600 hygiene:3054899" | material: layers "Compound Ceiling:Himling System 600x600 hygiene" ("Himling Metallprofil" 38., "Himling System 600x600" 12.) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:110mm Heisvegg" | object type "Basic Wall:110mm Heisvegg:3943637" | names: "Basic Wall:110mm Heisvegg:3943971" | material: layers "Basic Wall:110mm Heisvegg" ("hvit malt" 110.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCDOOR | type IFCDOORSTYLE "IDS 2.1 13x21M EI60S" | object type "IDS 2.1 13x21M EI60S" | names: "Dør Dobbel_Ulike_Dørblader:IDS 2.1 13x21M EI60S:4093959" | material: materials ("Lys grå", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDS 6.1 8x21M" | object type "IDS 6.1 8x21M" | names: "Dør Enkel:IDS 6.1 8x21M:4109271" | material: materials ("_White", "Lys grå", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCSTAIR | object type "Cast-In-Place Stair:Betongtrapp t=150 repo=200:306564" | names: "Cast-In-Place Stair:Stair:4428879" | parts: 2 IFCSLAB, 2 IFCSTAIRFLIGHT, 1 IFCRAILING | property sets: Pset_StairCommon, Pset_TFM, Constraints, Dimensions, Other, Phasing
          1 x IFCDOOR | type IFCDOORSTYLE "IDS 5.1 13x21M EI60CS" | object type "IDS 5.1 13x21M EI60CS" | names: "Dør Enkel:IDS 5.1 13x21M EI60CS:6509988" | material: materials ("Light grey", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDS 5.1 13x21M EI60CS" | object type "IDS 5.1 13x21M EI60CS" | names: "Dør Enkel:IDS 5.1 13x21M EI60CS:6510584" | material: materials ("Light grey", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          2 x IFCDOOR | type IFCDOORSTYLE "IDA 11 10x6" | object type "IDA 11 10x6" | names: "Luke600:IDA 11 10x6:6972200", "Luke600:IDA 11 10x6:6972584" | material: materials ("Light grey", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Innvendig screen" | object type "Innvendig screen" | names: "Screen_aula:Innvendig screen:7128359" | material: "hvit malt" | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Innvendig screen" | object type "Innvendig screen" | names: "Screen_aula:Innvendig screen:7128723" | material: "hvit malt" | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Innvendig screen" | object type "Innvendig screen" | names: "Screen_aula:Innvendig screen:7285495" | material: "hvit malt" | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 7.2 108mm Skjørt" | object type "Basic Wall:IVA 7.2 108mm Skjørt:5366897" | names: "Basic Wall:IVA 7.2 108mm Skjørt:7495318" | material: layers "Basic Wall:IVA 7.2 108mm Skjørt" ("Gips" 13., "stender/isolasjon" 95.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
        IFCSPACE "19" | long name "Area" | INTERNAL
        IFCSPACE "0U143" | long name "ventilasjon/varme" | INTERNAL
          contains 2 elements
            1 x IFCFLOWTERMINAL | object type "Utslagsvask" | names: "intra_gub1_bucket_sink_wall_mounted:Utslagsvask:3639507" | material: "f26d4e4b_a025_4dbf_b085_30ed485788cf" | property sets: Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data, Mechanical
            1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "Blandebatteri 3970" | object type "Blandebatteri 3970" | names: "Oras Saga:Blandebatteri 3970:7601868" | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
        IFCSPACE "0U146" | long name "tekn basseng/ventilasjon" | INTERNAL
          contains 3 elements
            1 x IFCFLOWTERMINAL | object type "Utslagsvask" | names: "intra_gub1_bucket_sink_wall_mounted:Utslagsvask:3639732" | material: "f26d4e4b_a025_4dbf_b085_30ed485788cf" | property sets: Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data, Mechanical
            1 x IFCFLOWTERMINAL | object type "Haws nøddusjsøyle 8320 Axion ECO" | names: "Dusj:Haws nøddusjsøyle 8320 Axion ECO:5272796" | material: "Aluminum" | property sets: Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data, Other
            1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "Blandebatteri 3970" | object type "Blandebatteri 3970" | names: "Oras Saga:Blandebatteri 3970:7602005" | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
        IFCSPACE "0U147" | long name "el-tavle" | INTERNAL
        IFCSPACE "0U142" | long name "rengj. sentral" | INTERNAL
          contains 19 elements
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Moppekjøleskap" | object type "Moppekjøleskap" | names: "NO_Kjøleskap:Moppekjøleskap:2209681" | material: materials ("Metal - Chrome", "Metal - Paint Finish - Ivory,Matte") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Skap, krogsæter 600 x 600 x 860mm" | object type "Skap, krogsæter 600 x 600 x 860mm" | names: "Base Cabinet Single Door:Skap, krogsæter 600 x 600 x 860mm:2211931" | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Other, Phasing
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Skap, krogsæter 600 x 600 x 860mm" | object type "Skap, krogsæter 600 x 600 x 860mm" | names: "Base Cabinet Single Door:Skap, krogsæter 600 x 600 x 860mm:2211932" | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
            1 x IFCFLOWTERMINAL | object type "Intra vaskekar, krogsæter" | names: "Utslagsvask:Intra vaskekar, krogsæter:4110444" | material: "Metal - Aluminium" | property sets: Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data, Other
            3 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Stålhylle, Krogsæter 900 x 500mm" | object type "Stålhylle, Krogsæter 900 x 500mm" | names: "M_Light Shelf Interior:Stålhylle, Krogsæter 900 x 500mm:6905551", "M_Light Shelf Interior:Stålhylle, Krogsæter 900 x 500mm:6906049", "M_Light Shelf Interior:Stålhylle, Krogsæter 900 x 500mm:6906073" | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
            3 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Stålhylle, Krogsæter 600 x 500mm" | object type "Stålhylle, Krogsæter 600 x 500mm" | names: "M_Light Shelf Interior:Stålhylle, Krogsæter 600 x 500mm:6905678", "M_Light Shelf Interior:Stålhylle, Krogsæter 600 x 500mm:6906050", "M_Light Shelf Interior:Stålhylle, Krogsæter 600 x 500mm:6906074" | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
            2 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Stålhylle, Krogsæter 900 x 300mm" | object type "Stålhylle, Krogsæter 900 x 300mm" | names: "M_Light Shelf Interior:Stålhylle, Krogsæter 900 x 300mm:6906101", "M_Light Shelf Interior:Stålhylle, Krogsæter 900 x 300mm:6906123" | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Other, Phasing
            2 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Stålhylle, Krogsæter 600 x 300mm" | object type "Stålhylle, Krogsæter 600 x 300mm" | names: "M_Light Shelf Interior:Stålhylle, Krogsæter 600 x 300mm:6906102", "M_Light Shelf Interior:Stålhylle, Krogsæter 600 x 300mm:6906124" | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Other, Phasing
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Benkeplate 625mm, krogsæter" | object type "Benkeplate 625mm, krogsæter" | names: "N_CounterTop:Benkeplate 625mm, krogsæter:6906665" | material: "hvit malt" | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Other, Phasing
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Miele moppevaskemaskin" | object type "Miele moppevaskemaskin" | names: "Spesialutstyr:Miele moppevaskemaskin:6907118" | material: "hvit malt" | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Miele vaskemaskin" | object type "Miele vaskemaskin" | names: "Spesialutstyr:Miele vaskemaskin:6907400" | material: "hvit malt" | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "gard skap 30cm 3" | object type "gard skap 30cm 3" | names: "Locker_Metal_Hadrian_Replacement-Front:gard skap 30cm 3:6908147" | material: materials ("Gul avdeling", "Steel - Hadrian - Black") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_TFM, Constraints, Construction, Dimensions
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "gard skap 30cm 3" | object type "gard skap 30cm 3" | names: "Locker_Metal_Hadrian_Replacement-Front:gard skap 30cm 3:6908372" | material: materials ("Gul avdeling", "Steel - Hadrian - Black") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_TFM, Constraints, Construction, Dimensions
        IFCSPACE "0U140" | long name "trapp" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | object type "Compound Ceiling:Himling System 600x600" | CEILING | names: "Compound Ceiling:Himling System 600x600:4433222" | material: layers "Compound Ceiling:Himling System 600x600" ("Himling Metallprofil" 38., "Himling System 600x600" 12.) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
        IFCSPACE "0U017" | long name "heis" | INTERNAL
        IFCSPACE "0U141" | long name "korridor" | INTERNAL
        IFCSPACE "0U144" | long name "krypkjeller" | INTERNAL
        IFCSPACE "0U145" | long name "sjakt" | INTERNAL
        IFCSPACE "0U148" | long name "varmesentral" | INTERNAL
        IFCSPACE "1" | long name "Area" | INTERNAL
        IFCSPACE "0U149" | long name "sluse" | INTERNAL
        IFCSPACE "0U151" | long name "Syrerom" | INTERNAL
        IFCSPACE "0U150" | long name "Klorrom" | INTERNAL
      IFCBUILDINGSTOREY "Plan 01" | long name "Plan 01" | elevation -5.28439159097616E-10
        contains 966 elements
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:YV 10.1 295mm Vindfang 2" | object type "Basic Wall:YV 10.1 295mm Vindfang 2:7424293" | names: "Basic Wall:YV 10.1 295mm Vindfang 2:1664553" | material: layers "Basic Wall:YV 10.1 295mm Vindfang 2" ("Cembrit Metro Copenhagen" 8., "Luftsjikt" 36., "Vindsperre" 9., "Stender isolert vegg" 198., "NO_Utlekting" 173., "<Unnamed>" 36., "Gips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Curtain Wall:Glassfasade 7" | object type "Curtain Wall:Glassfasade 7:4182498" | names: "Curtain Wall:Glassfasade 7:1665513" | parts: 59 IFCMEMBER, 22 IFCPLATE | property sets: Pset_CurtainWallCommon, Pset_TFM, Constraints, Dimensions, Horizontal Grid, Identity Data
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:YV 10.1 295mm Vindfang" | object type "Basic Wall:YV 10.1 295mm Vindfang:4779032" | names: "Basic Wall:YV 10.1 295mm Vindfang:1683692", "Basic Wall:YV 10.1 295mm Vindfang:1683732", "Basic Wall:YV 10.1 295mm Vindfang:6442880" | material: layers "Basic Wall:YV 10.1 295mm Vindfang" ("Cembrit Metro Copenhagen" 8., "Luftsjikt" 36., "Vindsperre" 9., "Stender isolert vegg" 198., "NO_Utlekting" 36., "Cembrit Metro Copenhagen" 8.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          6 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:YV 1.1 517mm" | object type "Basic Wall:YV 1.1 517mm:1735105" | names: "Basic Wall:YV 1.1 517mm:1737001", "Basic Wall:YV 1.1 517mm:1737009", "Basic Wall:YV 1.1 517mm:1737010" (+3 more) | material: layers "Basic Wall:YV 1.1 517mm" ("Trekledning" 19., "Luftsjikt" 48., "Luftsjikt" 36., "Luftsjikt" 48., "Vindsperre" 9., "Stender isolert vegg" 296., "NO_Utlekting" 48., "Robustgips" 12.5) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:YV 2.1 406M" | object type "Basic Wall:YV 2.1 406M:2979516" | names: "Basic Wall:YV 2.1 406M:1737746", "Basic Wall:YV 2.1 406M:2984329" | material: layers "Basic Wall:YV 2.1 406M" ("Trekledning" 19., "Luftsjikt" 48., "Luftsjikt" 36., "Luftsjikt" 48., "Vindsperre" 9., "Stender isolert vegg" 246.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          18 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 3.3 145mm EI60 (RN-95-NR)" | object type "Basic Wall:IVA 3.3 145mm EI60 (RN-95-NR):2850935" | names: "Basic Wall:IVA 3.3 145mm EI60 (RN-95-NR):1752869", "Basic Wall:IVA 3.3 145mm EI60 (RN-95-NR):1753274", "Basic Wall:IVA 3.3 145mm EI60 (RN-95-NR):1814431" (+15 more) | material: layers "Basic Wall:IVA 3.3 145mm EI60 (RN-95-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 6.1 272mm 60dB EI60 (HN-95-30-95-NH)" | object type "Basic Wall:IVA 6.1 272mm 60dB EI60 (HN-95-30-95-NH):2866155" | names: "Basic Wall:IVA 6.1 272mm 60dB EI60 (HN-95-30-95-NH):1752871", "Basic Wall:IVA 6.1 272mm 60dB EI60 (HN-95-30-95-NH):2133627" | material: layers "Basic Wall:IVA 6.1 272mm 60dB EI60 (HN-95-30-95-NH)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 95., "Luftsjikt" 30., "stender/isolasjon" 95., "Gips" 13., "Habito" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          16 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 3.3 145mm 48dB (RN-95-NR)" | object type "Basic Wall:IVA 3.3 145mm 48dB (RN-95-NR):2849733" | names: "Basic Wall:IVA 3.3 145mm 48dB (RN-95-NR):1752873", "Basic Wall:IVA 3.3 145mm 48dB (RN-95-NR):1752874", "Basic Wall:IVA 3.3 145mm 48dB (RN-95-NR):1752875" (+13 more) | material: layers "Basic Wall:IVA 3.3 145mm 48dB (RN-95-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 2.3 134mm 34dB (R-95-NR)" | object type "Basic Wall:IVA 2.3 134mm 34dB (R-95-NR):4809032" | names: "Basic Wall:IVA 2.3 134mm 34dB (R-95-NR):1752879", "Basic Wall:IVA 2.3 134mm 34dB (R-95-NR):2017474" | material: layers "Basic Wall:IVA 2.3 134mm 34dB (R-95-NR)" ("Robustgips" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          5 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 3.3 145mm 37dB EI60 (RN-95-NR)" | object type "Basic Wall:IVA 3.3 145mm 37dB EI60 (RN-95-NR):4823028" | names: "Basic Wall:IVA 3.3 145mm 37dB EI60 (RN-95-NR):1752880", "Basic Wall:IVA 3.3 145mm 37dB EI60 (RN-95-NR):1752884", "Basic Wall:IVA 3.3 145mm 37dB EI60 (RN-95-NR):1753279" (+2 more) | material: layers "Basic Wall:IVA 3.3 145mm 37dB EI60 (RN-95-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 3.3 145mm 44dB EI60 (RN-95-NR)" | object type "Basic Wall:IVA 3.3 145mm 44dB EI60 (RN-95-NR):5059915" | names: "Basic Wall:IVA 3.3 145mm 44dB EI60 (RN-95-NR):1752881" | material: layers "Basic Wall:IVA 3.3 145mm 44dB EI60 (RN-95-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 3.3 145mm 34dB E30 (RN-95-NR)" | object type "Basic Wall:IVA 3.3 145mm 34dB E30 (RN-95-NR):5067709" | names: "Basic Wall:IVA 3.3 145mm 34dB E30 (RN-95-NR):1752885" | material: layers "Basic Wall:IVA 3.3 145mm 34dB E30 (RN-95-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 3.1 145mm EI60 (HN-95-NH)" | object type "Basic Wall:IVA 3.1 145mm EI60 (HN-95-NH):6783876" | names: "Basic Wall:IVA 3.1 145mm EI60 (HN-95-NH):1752989" | material: layers "Basic Wall:IVA 3.1 145mm EI60 (HN-95-NH)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          10 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 3.2 145mm EI60 (HN-95-NR)" | object type "Basic Wall:IVA 3.2 145mm EI60 (HN-95-NR):4816814" | names: "Basic Wall:IVA 3.2 145mm EI60 (HN-95-NR):1752990", "Basic Wall:IVA 3.2 145mm EI60 (HN-95-NR):1785147", "Basic Wall:IVA 3.2 145mm EI60 (HN-95-NR):1814441" (+7 more) | material: layers "Basic Wall:IVA 3.2 145mm EI60 (HN-95-NR)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          5 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 3.2 145mm 48dB EI60 (HN-95-NR)" | object type "Basic Wall:IVA 3.2 145mm 48dB EI60 (HN-95-NR):4821417" | names: "Basic Wall:IVA 3.2 145mm 48dB EI60 (HN-95-NR):1753090", "Basic Wall:IVA 3.2 145mm 48dB EI60 (HN-95-NR):1753213", "Basic Wall:IVA 3.2 145mm 48dB EI60 (HN-95-NR):2112576" (+2 more) | material: layers "Basic Wall:IVA 3.2 145mm 48dB EI60 (HN-95-NR)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 2.6 10x21M 38dB" | object type "IDT 2.6 10x21M 38dB" | names: "Dør Enkel:IDT 2.6 10x21M 38dB:1753119" | material: materials ("Light grey", "Lys grå", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 6.2 272mm 60dB (HN-95-30-95-NR)" | object type "Basic Wall:IVA 6.2 272mm 60dB (HN-95-30-95-NR):4827698" | names: "Basic Wall:IVA 6.2 272mm 60dB (HN-95-30-95-NR):1753125" | material: layers "Basic Wall:IVA 6.2 272mm 60dB (HN-95-30-95-NR)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 95., "Luftsjikt" 30., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 6.2 352mm 60dB (HN-95-110-95-NR)" | object type "Basic Wall:IVA 6.2 352mm 60dB (HN-95-110-95-NR):3570267" | names: "Basic Wall:IVA 6.2 352mm 60dB (HN-95-110-95-NR):1753126" | material: layers "Basic Wall:IVA 6.2 352mm 60dB (HN-95-110-95-NR)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 95., "Luftsjikt" 110., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          6 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 3.3 145mm 34dB (RN-95-NR)" | object type "Basic Wall:IVA 3.3 145mm 34dB (RN-95-NR):2849806" | names: "Basic Wall:IVA 3.3 145mm 34dB (RN-95-NR):1753207", "Basic Wall:IVA 3.3 145mm 34dB (RN-95-NR):2235122", "Basic Wall:IVA 3.3 145mm 34dB (RN-95-NR):2863196" (+3 more) | material: layers "Basic Wall:IVA 3.3 145mm 34dB (RN-95-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 2.3 10x21M 33dB" | object type "IDT 2.3 10x21M 33dB" | names: "Dør Enkel:IDT 2.3 10x21M 33dB:1753211" | material: materials ("Terskel Tre", "Lys grå", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 5.1 212mm EI60 (HN-160-NR)" | object type "Basic Wall:IVA 5.1 212mm EI60 (HN-160-NR):3435826" | names: "Basic Wall:IVA 5.1 212mm EI60 (HN-160-NR):1753217" | material: layers "Basic Wall:IVA 5.1 212mm EI60 (HN-160-NR)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 160., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 4.1 172mm (HN-120-NH)" | object type "Basic Wall:IVA 4.1 172mm (HN-120-NH):4085290" | names: "Basic Wall:IVA 4.1 172mm (HN-120-NH):1753218", "Basic Wall:IVA 4.1 172mm (HN-120-NH):1753220" | material: layers "Basic Wall:IVA 4.1 172mm (HN-120-NH)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 120., "Gips" 13., "Habito" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          8 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 1.1 121mm (H-95-H)" | object type "Basic Wall:IVA 1.1 121mm (H-95-H):4814431" | names: "Basic Wall:IVA 1.1 121mm (H-95-H):1753221", "Basic Wall:IVA 1.1 121mm (H-95-H):1785180", "Basic Wall:IVA 1.1 121mm (H-95-H):2571144" (+5 more) | material: layers "Basic Wall:IVA 1.1 121mm (H-95-H)" ("Habito" 13., "stender/isolasjon" 95., "Habito" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 1.1 121mm 44dB (H-95-H)" | object type "Basic Wall:IVA 1.1 121mm 44dB (H-95-H):4807508" | names: "Basic Wall:IVA 1.1 121mm 44dB (H-95-H):1753222", "Basic Wall:IVA 1.1 121mm 44dB (H-95-H):1814430", "Basic Wall:IVA 1.1 121mm 44dB (H-95-H):2133998" | material: layers "Basic Wall:IVA 1.1 121mm 44dB (H-95-H)" ("Habito" 13., "stender/isolasjon" 95., "Habito" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 3.1 145mm 48dB (HN-95-NH)" | object type "Basic Wall:IVA 3.1 145mm 48dB (HN-95-NH):4820944" | names: "Basic Wall:IVA 3.1 145mm 48dB (HN-95-NH):1753225", "Basic Wall:IVA 3.1 145mm 48dB (HN-95-NH):1753237" | material: layers "Basic Wall:IVA 3.1 145mm 48dB (HN-95-NH)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Habito" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 2.1 10x21M" | object type "IDT 2.1 10x21M" | names: "Dør Enkel:IDT 2.1 10x21M:1753234" | material: materials ("_White", "NCS S 0500-N", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 2.1 10x21M" | object type "IDT 2.1 10x21M" | names: "Dør Enkel:IDT 2.1 10x21M:1753235" | material: materials ("_White", "NCS S 0500-N", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 3.3 145mm 34dB EI60 (RN-95-NR)" | object type "Basic Wall:IVA 3.3 145mm 34dB EI60 (RN-95-NR):2862672" | names: "Basic Wall:IVA 3.3 145mm 34dB EI60 (RN-95-NR):1753251", "Basic Wall:IVA 3.3 145mm 34dB EI60 (RN-95-NR):1753268", "Basic Wall:IVA 3.3 145mm 34dB EI60 (RN-95-NR):1851354" (+1 more) | material: layers "Basic Wall:IVA 3.3 145mm 34dB EI60 (RN-95-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          10 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 3.3 145mm 48dB EI60 (RN-95-NR)" | object type "Basic Wall:IVA 3.3 145mm 48dB EI60 (RN-95-NR):2860483" | names: "Basic Wall:IVA 3.3 145mm 48dB EI60 (RN-95-NR):1753252", "Basic Wall:IVA 3.3 145mm 48dB EI60 (RN-95-NR):1753253", "Basic Wall:IVA 3.3 145mm 48dB EI60 (RN-95-NR):1753256" (+7 more) | material: layers "Basic Wall:IVA 3.3 145mm 48dB EI60 (RN-95-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 3.3 145mm 44dB (RN-95-NR)" | object type "Basic Wall:IVA 3.3 145mm 44dB (RN-95-NR):4816971" | names: "Basic Wall:IVA 3.3 145mm 44dB (RN-95-NR):1753257" | material: layers "Basic Wall:IVA 3.3 145mm 44dB (RN-95-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 2.4 10x21M 38dB EI30S" | object type "IDT 2.4 10x21M 38dB EI30S" | names: "Dør Enkel:IDT 2.4 10x21M 38dB EI30S:1753266" | material: materials ("Terskel Tre", "Vindsperre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 3.4 10x21M 33dB E30CS" | object type "IDT 3.4 10x21M 33dB E30CS" | names: "Dør Enkel_ Glassfelt:IDT 3.4 10x21M 33dB E30CS:1753271" | material: materials ("Lys grå", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 3.2 10x21M 28dB EI30S" | object type "IDT 3.2 10x21M 28dB EI30S" | names: "Dør Enkel_ Glassfelt:IDT 3.2 10x21M 28dB EI30S:1753273" | material: materials ("Lys grå", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 2.1 10x21M" | object type "IDT 2.1 10x21M" | names: "Dør Enkel:IDT 2.1 10x21M:1753276" | material: materials ("_White", "NCS S 0500-N", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 3.8 10x21M 28dB E30CS" | object type "IDT 3.8 10x21M 28dB E30CS" | names: "Dør Enkel_ Glassfelt:IDT 3.8 10x21M 28dB E30CS:1753280" | material: materials ("Lys grå", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 3.2 145mm 37dB EI60 (HN-95-NR)" | object type "Basic Wall:IVA 3.2 145mm 37dB EI60 (HN-95-NR):2850426" | names: "Basic Wall:IVA 3.2 145mm 37dB EI60 (HN-95-NR):1753281", "Basic Wall:IVA 3.2 145mm 37dB EI60 (HN-95-NR):4822992" | material: layers "Basic Wall:IVA 3.2 145mm 37dB EI60 (HN-95-NR)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 2.3 10x21M 33dB" | object type "IDT 2.3 10x21M 33dB" | names: "Dør Enkel:IDT 2.3 10x21M 33dB:1753282" | material: materials ("Terskel Tre", "Lys grå", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          6 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVL 2.1 123mm (flis-leca) 34dB" | object type "Basic Wall:IVL 2.1 123mm (flis-leca) 34dB:3868920" | names: "Basic Wall:IVL 2.1 123mm (flis-leca) 34dB:1755286", "Basic Wall:IVL 2.1 123mm (flis-leca) 34dB:2107816", "Basic Wall:IVL 2.1 123mm (flis-leca) 34dB:2278872" (+3 more) | material: layers "Basic Wall:IVL 2.1 123mm (flis-leca) 34dB" ("Flis" 5., "Mur" 118.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCDOOR | type IFCDOORSTYLE "IDA 5.1 10x21M 33dB" | object type "IDA 5.1 10x21M 33dB" | names: "Dør Enkel_ Glassfelt:IDA 5.1 10x21M 33dB:1755293" | material: materials ("hvit", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          7 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVL 1.1 118mm leca" | object type "Basic Wall:IVL 1.1 118mm leca:4134165" | names: "Basic Wall:IVL 1.1 118mm leca:1755300", "Basic Wall:IVL 1.1 118mm leca:1812358", "Basic Wall:IVL 1.1 118mm leca:1813583" (+4 more) | material: layers "Basic Wall:IVL 1.1 118mm leca" ("Mur" 118.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:YV 7.1 410mm grå platekledning" | object type "Basic Wall:YV 7.1 410mm grå platekledning:3016199" | names: "Basic Wall:YV 7.1 410mm grå platekledning:1755319", "Basic Wall:YV 7.1 410mm grå platekledning:1882660", "Basic Wall:YV 7.1 410mm grå platekledning:3546343" (+1 more) | material: layers "Basic Wall:YV 7.1 410mm grå platekledning" ("Cembrit Metro London" 8., "Luftsjikt" 36., "Vindsperre" 9., "Stender isolert vegg" 296., "NO_Utlekting" 48., "Gips" 12.5) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          6 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:YV 6.1 299mm rød platekledning basseng" | object type "Basic Wall:YV 6.1 299mm rød platekledning basseng:2511119" | names: "Basic Wall:YV 6.1 299mm rød platekledning basseng:1755796", "Basic Wall:YV 6.1 299mm rød platekledning basseng:2215720", "Basic Wall:YV 6.1 299mm rød platekledning basseng:2215925" (+3 more) | material: layers "Basic Wall:YV 6.1 299mm rød platekledning basseng" ("Cembrit Metro Copenhagen" 8., "Luftsjikt" 36., "Vindsperre" 9., "Stender isolert vegg" 246.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 2.4 134mm (R-95-NH)" | object type "Basic Wall:IVA 2.4 134mm (R-95-NH):4818501" | names: "Basic Wall:IVA 2.4 134mm (R-95-NH):1785103", "Basic Wall:IVA 2.4 134mm (R-95-NH):2865575" | material: layers "Basic Wall:IVA 2.4 134mm (R-95-NH)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 95., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 3.1 145mm 34dB (HN-95-NH)" | object type "Basic Wall:IVA 3.1 145mm 34dB (HN-95-NH):4824008" | names: "Basic Wall:IVA 3.1 145mm 34dB (HN-95-NH):1785104", "Basic Wall:IVA 3.1 145mm 34dB (HN-95-NH):3071874" | material: layers "Basic Wall:IVA 3.1 145mm 34dB (HN-95-NH)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Habito" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 2.2 134mm 34dB (H-95-NR)" | object type "Basic Wall:IVA 2.2 134mm 34dB (H-95-NR):4823696" | names: "Basic Wall:IVA 2.2 134mm 34dB (H-95-NR):1785105", "Basic Wall:IVA 2.2 134mm 34dB (H-95-NR):2068495" | material: layers "Basic Wall:IVA 2.2 134mm 34dB (H-95-NR)" ("Habito" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 1.2T 121mm 34dB (R-95-H)" | object type "Basic Wall:IVA 1.2T 121mm 34dB (R-95-H):6703195" | names: "Basic Wall:IVA 1.2T 121mm 34dB (R-95-H):1785148", "Basic Wall:IVA 1.2T 121mm 34dB (R-95-H):2107118", "Basic Wall:IVA 1.2T 121mm 34dB (R-95-H):2107231" | material: layers "Basic Wall:IVA 1.2T 121mm 34dB (R-95-H)" ("Habito" 13., "stender/isolasjon" 95., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 3.3T 145mm EI60 (RN-95-NR)" | object type "Basic Wall:IVA 3.3T 145mm EI60 (RN-95-NR):6701511" | names: "Basic Wall:IVA 3.3T 145mm EI60 (RN-95-NR):1785149", "Basic Wall:IVA 3.3T 145mm EI60 (RN-95-NR):2107175" | material: layers "Basic Wall:IVA 3.3T 145mm EI60 (RN-95-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 4.2 172mm 52dB (HN-120-NR)" | object type "Basic Wall:IVA 4.2 172mm 52dB (HN-120-NR):2869906" | names: "Basic Wall:IVA 4.2 172mm 52dB (HN-120-NR):1785150" | material: layers "Basic Wall:IVA 4.2 172mm 52dB (HN-120-NR)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 120., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 3.3 145mm (RN-95-NR)" | object type "Basic Wall:IVA 3.3 145mm (RN-95-NR):4819687" | names: "Basic Wall:IVA 3.3 145mm (RN-95-NR):1785152", "Basic Wall:IVA 3.3 145mm (RN-95-NR):1785276" | material: layers "Basic Wall:IVA 3.3 145mm (RN-95-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 6.3T 332mm 34dB EI60 (RN-95-90-95-NR)" | object type "Basic Wall:IVA 6.3T 332mm 34dB EI60 (RN-95-90-95-NR):6703388" | names: "Basic Wall:IVA 6.3T 332mm 34dB EI60 (RN-95-90-95-NR):1785155" | material: layers "Basic Wall:IVA 6.3T 332mm 34dB EI60 (RN-95-90-95-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95., "Luftsjikt" 90., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          2 x IFCDOOR | type IFCDOORSTYLE "IDT 3.3 10x21M 33dB" | object type "IDT 3.3 10x21M 33dB" | names: "Dør Enkel_ Glassfelt:IDT 3.3 10x21M 33dB:1785179", "Dør Enkel_ Glassfelt:IDT 3.3 10x21M 33dB:1785181" | material: materials ("Lys grå", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 2.9 10x21M EI60S" | object type "IDT 2.9 10x21M EI60S" | names: "Dør Enkel:IDT 2.9 10x21M EI60S:1785182" | material: materials ("Light grey", "Lys grå", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 3.3T 145mm 48dB EI60 (RN-95-NR)" | object type "Basic Wall:IVA 3.3T 145mm 48dB EI60 (RN-95-NR):6691651" | names: "Basic Wall:IVA 3.3T 145mm 48dB EI60 (RN-95-NR):1785263" | material: layers "Basic Wall:IVA 3.3T 145mm 48dB EI60 (RN-95-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 3.6 10x21M 38dB" | object type "IDT 3.6 10x21M 38dB" | names: "Dør Enkel_ Glassfelt:IDT 3.6 10x21M 38dB:1785264" | material: materials ("NCS S 2500-N", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 2.1 134mm 48dB (H-95-NH)" | object type "Basic Wall:IVA 2.1 134mm 48dB (H-95-NH):4807019" | names: "Basic Wall:IVA 2.1 134mm 48dB (H-95-NH):1785267", "Basic Wall:IVA 2.1 134mm 48dB (H-95-NH):2866710" | material: layers "Basic Wall:IVA 2.1 134mm 48dB (H-95-NH)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 95., "Habito" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 2.6 10x21M 38dB" | object type "IDT 2.6 10x21M 38dB" | names: "Dør Enkel:IDT 2.6 10x21M 38dB:1785269" | material: materials ("Light grey", "Lys grå", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 3.2 145mm 48dB (HN-95-NR)" | object type "Basic Wall:IVA 3.2 145mm 48dB (HN-95-NR):4828215" | names: "Basic Wall:IVA 3.2 145mm 48dB (HN-95-NR):1785270", "Basic Wall:IVA 3.2 145mm 48dB (HN-95-NR):2017475", "Basic Wall:IVA 3.2 145mm 48dB (HN-95-NR):6821254" | material: layers "Basic Wall:IVA 3.2 145mm 48dB (HN-95-NR)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          2 x IFCDOOR | type IFCDOORSTYLE "IDT 3.3 10x21M 33dB" | object type "IDT 3.3 10x21M 33dB" | names: "Dør Enkel_ Glassfelt:IDT 3.3 10x21M 33dB:1785271", "Dør Enkel_ Glassfelt:IDT 3.3 10x21M 33dB:1785280" | material: materials ("Lys grå", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 4.1 172mm 52dB (HN-120-NH)" | object type "Basic Wall:IVA 4.1 172mm 52dB (HN-120-NH):4859170" | names: "Basic Wall:IVA 4.1 172mm 52dB (HN-120-NH):1785274", "Basic Wall:IVA 4.1 172mm 52dB (HN-120-NH):2068530" | material: layers "Basic Wall:IVA 4.1 172mm 52dB (HN-120-NH)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 120., "Gips" 13., "Habito" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 3.3 10x21M 33dB" | object type "IDT 3.3 10x21M 33dB" | names: "Dør Enkel_ Glassfelt:IDT 3.3 10x21M 33dB:1785275" | material: materials ("Lys grå", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 2.1 10x21M" | object type "IDT 2.1 10x21M" | names: "Dør Enkel:IDT 2.1 10x21M:1785281" | material: materials ("_White", "NCS S 0500-N", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 4.3 172mm 34dB (RN-120-NR)" | object type "Basic Wall:IVA 4.3 172mm 34dB (RN-120-NR):4859885" | names: "Basic Wall:IVA 4.3 172mm 34dB (RN-120-NR):1785282" | material: layers "Basic Wall:IVA 4.3 172mm 34dB (RN-120-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 120., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 1.2 121mm (R-95-H)" | object type "Basic Wall:IVA 1.2 121mm (R-95-H):6784406" | names: "Basic Wall:IVA 1.2 121mm (R-95-H):1785283", "Basic Wall:IVA 1.2 121mm (R-95-H):2222527" | material: layers "Basic Wall:IVA 1.2 121mm (R-95-H)" ("Habito" 13., "stender/isolasjon" 95., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 1.1 8x21M" | object type "IDT 1.1 8x21M" | names: "Dør Enkel:IDT 1.1 8x21M:1785284" | material: materials ("Terskel Tre", "Lys grå", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 2.2 134mm (H-95-NR)" | object type "Basic Wall:IVA 2.2 134mm (H-95-NR):4828766" | names: "Basic Wall:IVA 2.2 134mm (H-95-NR):1785290" | material: layers "Basic Wall:IVA 2.2 134mm (H-95-NR)" ("Habito" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 1.2 121mm 34dB (R-95-H)" | object type "Basic Wall:IVA 1.2 121mm 34dB (R-95-H):4824661" | names: "Basic Wall:IVA 1.2 121mm 34dB (R-95-H):1785297", "Basic Wall:IVA 1.2 121mm 34dB (R-95-H):2152155", "Basic Wall:IVA 1.2 121mm 34dB (R-95-H):3867136" | material: layers "Basic Wall:IVA 1.2 121mm 34dB (R-95-H)" ("Habito" 13., "stender/isolasjon" 95., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          7 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 1.3 121mm (R-95-R)" | object type "Basic Wall:IVA 1.3 121mm (R-95-R):4815917" | names: "Basic Wall:IVA 1.3 121mm (R-95-R):1788622", "Basic Wall:IVA 1.3 121mm (R-95-R):1824456", "Basic Wall:IVA 1.3 121mm (R-95-R):1988050" (+4 more) | material: layers "Basic Wall:IVA 1.3 121mm (R-95-R)" ("Robustgips" 13., "stender/isolasjon" 95., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 2.1 10x21M" | object type "IDT 2.1 10x21M" | names: "Dør Enkel:IDT 2.1 10x21M:1789941" | material: materials ("_White", "Light grey", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 5.1 15x21M" | object type "IDT 5.1 15x21M" | names: "Dør Dobbel:IDT 5.1 15x21M:1790017" | material: materials ("Lys grå", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          6 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVL 3.1 128mm (flis-leca-flis) 34dB" | object type "Basic Wall:IVL 3.1 128mm (flis-leca-flis) 34dB:3868780" | names: "Basic Wall:IVL 3.1 128mm (flis-leca-flis) 34dB:1792755", "Basic Wall:IVL 3.1 128mm (flis-leca-flis) 34dB:1813337", "Basic Wall:IVL 3.1 128mm (flis-leca-flis) 34dB:2110277" (+3 more) | material: layers "Basic Wall:IVL 3.1 128mm (flis-leca-flis) 34dB" ("Flis" 5., "Mur" 118., "Flis" 5.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          5 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVL 2.1 123mm (flis-leca)" | object type "Basic Wall:IVL 2.1 123mm (flis-leca):3395340" | names: "Basic Wall:IVL 2.1 123mm (flis-leca):1793231", "Basic Wall:IVL 2.1 123mm (flis-leca):2763548", "Basic Wall:IVL 2.1 123mm (flis-leca):2763602" (+2 more) | material: layers "Basic Wall:IVL 2.1 123mm (flis-leca)" ("Flis" 5., "Mur" 118.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCDOOR | type IFCDOORSTYLE "IDA 1.1 10x21M" | object type "IDA 1.1 10x21M" | names: "Dør Enkel_ Glassfelt:IDA 1.1 10x21M:1795541" | material: materials ("hvit", "Glassfiberfylling", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "YDA 1.2 16x21M EI 30S" | object type "YDA 1.2 16x21M EI 30S" | names: "_Dør Dobbel_Ulike_Dørblader_Glassfelt2:YDA 1.2 16x21M EI 30S:1796394" | material: materials ("Glass Klart", "Lys grå", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDA 7.1 15x21M EI60CS" | object type "IDA 7.1 15x21M EI60CS" | names: "Enfløyet_aludør:IDA 7.1 15x21M EI60CS:1796610" | material: materials ("Karm Malt", "Lys grå", "Terskel Tre") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          6 x IFCDOOR | type IFCDOORSTYLE "IDT 2.6 10x21M 38dB" | object type "IDT 2.6 10x21M 38dB" | names: "Dør Enkel:IDT 2.6 10x21M 38dB:1799472", "Dør Enkel:IDT 2.6 10x21M 38dB:1799534", "Dør Enkel:IDT 2.6 10x21M 38dB:1799577" (+3 more) | material: materials ("Terskel Tre", "Lys grå", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 2.6 10x21M 38dB" | object type "IDT 2.6 10x21M 38dB" | names: "Dør Enkel:IDT 2.6 10x21M 38dB:1799883" | material: materials ("Terskel Tre", "Lys grå", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 7.1 121mm (95-NR)" | object type "Basic Wall:IVA 7.1 121mm (95-NR):6248452" | names: "Basic Wall:IVA 7.1 121mm (95-NR):1811325", "Basic Wall:IVA 7.1 121mm (95-NR):2763576" | material: layers "Basic Wall:IVA 7.1 121mm (95-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVL 1.1 118mm leca EI60" | object type "Basic Wall:IVL 1.1 118mm leca EI60:4382750" | names: "Basic Wall:IVL 1.1 118mm leca EI60:1811883" | material: layers "Basic Wall:IVL 1.1 118mm leca EI60" ("Mur" 118.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVL 3.1 128mm (flis-leca-flis)" | object type "Basic Wall:IVL 3.1 128mm (flis-leca-flis):2882099" | names: "Basic Wall:IVL 3.1 128mm (flis-leca-flis):1813640", "Basic Wall:IVL 3.1 128mm (flis-leca-flis):1815466" | material: layers "Basic Wall:IVL 3.1 128mm (flis-leca-flis)" ("Flis" 5., "Mur" 118., "Flis" 5.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 3.5 10x21M 38dB EI30S" | object type "IDT 3.5 10x21M 38dB EI30S" | names: "Dør Enkel_ Glassfelt:IDT 3.5 10x21M 38dB EI30S:1814193" | material: materials ("Lys grå", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 6.1 272mm 60dB (HN-95-30-95-NH)" | object type "Basic Wall:IVA 6.1 272mm 60dB (HN-95-30-95-NH):4868230" | names: "Basic Wall:IVA 6.1 272mm 60dB (HN-95-30-95-NH):1814532" | material: layers "Basic Wall:IVA 6.1 272mm 60dB (HN-95-30-95-NH)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 95., "Luftsjikt" 30., "stender/isolasjon" 95., "Gips" 13., "Habito" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          2 x IFCDOOR | type IFCDOORSTYLE "IDT 3.3 10x21M 33dB" | object type "IDT 3.3 10x21M 33dB" | names: "Dør Enkel_ Glassfelt:IDT 3.3 10x21M 33dB:1814533", "Dør Enkel_ Glassfelt:IDT 3.3 10x21M 33dB:1814536" | material: materials ("Lys grå", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 7.1 121mm 37dB (95-NR)" | object type "Basic Wall:IVA 7.1 121mm 37dB (95-NR):6445986" | names: "Basic Wall:IVA 7.1 121mm 37dB (95-NR):1814537" | material: layers "Basic Wall:IVA 7.1 121mm 37dB (95-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 2.1 134mm 34dB (H-95-NH)" | object type "Basic Wall:IVA 2.1 134mm 34dB (H-95-NH):4843176" | names: "Basic Wall:IVA 2.1 134mm 34dB (H-95-NH):1814539", "Basic Wall:IVA 2.1 134mm 34dB (H-95-NH):4045775" | material: layers "Basic Wall:IVA 2.1 134mm 34dB (H-95-NH)" ("Habito" 13., "stender/isolasjon" 95., "Gips" 13., "Habito" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          5 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 2.4 134mm 34dB (R-95-NH)" | object type "Basic Wall:IVA 2.4 134mm 34dB (R-95-NH):4844120" | names: "Basic Wall:IVA 2.4 134mm 34dB (R-95-NH):1814543", "Basic Wall:IVA 2.4 134mm 34dB (R-95-NH):1814545", "Basic Wall:IVA 2.4 134mm 34dB (R-95-NH):2865342" (+2 more) | material: layers "Basic Wall:IVA 2.4 134mm 34dB (R-95-NH)" ("Robustgips" 13., "stender/isolasjon" 95., "Gips" 13., "Habito" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          1 x IFCDOOR | type IFCDOORSTYLE "IDA 1.1 10x21M" | object type "IDA 1.1 10x21M" | names: "Dør Enkel_ Glassfelt:IDA 1.1 10x21M:1816112" | material: materials ("hvit", "Glassfiberfylling", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVL 2.1 123mm (flis-leca) 34dB EI60" | object type "Basic Wall:IVL 2.1 123mm (flis-leca) 34dB EI60:4382819" | names: "Basic Wall:IVL 2.1 123mm (flis-leca) 34dB EI60:1817689", "Basic Wall:IVL 2.1 123mm (flis-leca) 34dB EI60:2078301", "Basic Wall:IVL 2.1 123mm (flis-leca) 34dB EI60:2868226" | material: layers "Basic Wall:IVL 2.1 123mm (flis-leca) 34dB EI60" ("Flis" 5., "Mur" 118.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 2.1 10x21M" | object type "IDT 2.1 10x21M" | names: "Dør Enkel:IDT 2.1 10x21M:1818637" | material: materials ("_White", "NCS S 0500-N", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 2.1 10x21M" | object type "IDT 2.1 10x21M" | names: "Dør Enkel:IDT 2.1 10x21M:1819618" | material: materials ("_White", "NCS S 0500-N", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 2.3 10x21M 33dB" | object type "IDT 2.3 10x21M 33dB" | names: "Dør Enkel:IDT 2.3 10x21M 33dB:1819877" | material: materials ("Terskel Tre", "Lys grå", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 3.3 10x21M 33dB" | object type "IDT 3.3 10x21M 33dB" | names: "Dør Enkel_ Glassfelt:IDT 3.3 10x21M 33dB:1824007" | material: materials ("Lys grå", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 1.3 121mm 34dB (R-95-R)" | object type "Basic Wall:IVA 1.3 121mm 34dB (R-95-R):4808382" | names: "Basic Wall:IVA 1.3 121mm 34dB (R-95-R):1824360", "Basic Wall:IVA 1.3 121mm 34dB (R-95-R):3867242" | material: layers "Basic Wall:IVA 1.3 121mm 34dB (R-95-R)" ("Robustgips" 13., "stender/isolasjon" 95., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 1.3 8x21M EI30S" | object type "IDT 1.3 8x21M EI30S" | names: "Dør Enkel:IDT 1.3 8x21M EI30S:1824685" | material: materials ("Terskel Tre", "Lys grå", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 1.1 8x21M" | object type "IDT 1.1 8x21M" | names: "Dør Enkel:IDT 1.1 8x21M:1824708" | material: materials ("Terskel Tre", "Lys grå", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 3.6 10x21M 38dB" | object type "IDT 3.6 10x21M 38dB" | names: "Dør Enkel_ Glassfelt:IDT 3.6 10x21M 38dB:1829818" | material: materials ("NCS S 2500-N", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 1.3 121mm 37dB (R-95-R)" | object type "Basic Wall:IVA 1.3 121mm 37dB (R-95-R):2851286" | names: "Basic Wall:IVA 1.3 121mm 37dB (R-95-R):1829859", "Basic Wall:IVA 1.3 121mm 37dB (R-95-R):2082152" | material: layers "Basic Wall:IVA 1.3 121mm 37dB (R-95-R)" ("Robustgips" 13., "stender/isolasjon" 95., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 3.2 10x21M 28dB EI30S" | object type "IDT 3.2 10x21M 28dB EI30S" | names: "Dør Enkel_ Glassfelt:IDT 3.2 10x21M 28dB EI30S:1830486" | material: materials ("Lys grå", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 3.6 10x21M 38dB" | object type "IDT 3.6 10x21M 38dB" | names: "Dør Enkel_ Glassfelt:IDT 3.6 10x21M 38dB:1830683" | material: materials ("NCS S 2500-N", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCROOF | object type "Basic Roof:Tak tre 223 - vindfang:5030382" | names: "Basic Roof:Tak tre 223 - vindfang:1836902" | material: "NO_Hard isolasjon" | property sets: Pset_RoofCommon, Pset_TFM, Constraints, Construction, Dimensions, Other
          1 x IFCDOOR | type IFCDOORSTYLE "IDA 3.3 18x21M 33dB EI60CS" | object type "IDA 3.3 18x21M 33dB EI60CS" | names: "_Dør Dobbel_Ulike_Dørblader_Glassfelt:IDA 3.3 18x21M 33dB EI60CS:1851355" | material: materials ("Glass Klart", "Lys grå", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDA 3.4 18x21M EI30CS" | object type "IDA 3.4 18x21M EI30CS" | names: "_Dør Dobbel_Ulike_Dørblader_Glassfelt:IDA 3.4 18x21M EI30CS:1851357" | material: materials ("Glass Klart", "Lys grå", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 3.3 10x21M 33dB" | object type "IDT 3.3 10x21M 33dB" | names: "Dør Enkel_ Glassfelt:IDT 3.3 10x21M 33dB:1851361" | material: materials ("Lys grå", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 3.3 10x21M 33dB" | object type "IDT 3.3 10x21M 33dB" | names: "Dør Enkel_ Glassfelt:IDT 3.3 10x21M 33dB:1851362" | material: materials ("Lys grå", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 3.3 10x21M 33dB" | object type "IDT 3.3 10x21M 33dB" | names: "Dør Enkel_ Glassfelt:IDT 3.3 10x21M 33dB:1851363" | material: materials ("Lys grå", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          3 x IFCWINDOW | type IFCWINDOWSTYLE "V13 12x16" | object type "V13 12x16" | names: "Vindu-Hengslet:V13 12x16:1852971", "Vindu-Hengslet:V13 12x16:1853366", "Vindu-Hengslet:V13 12x16:2427849" | material: materials ("Glass Klart", "NCS S 0502-Y", "Karm Malt") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 2.9 10x21M EI60S" | object type "IDT 2.9 10x21M EI60S" | names: "Dør Enkel:IDT 2.9 10x21M EI60S:1865778" | material: materials ("Light grey", "Lys grå", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDA 1.1 10x21M" | object type "IDA 1.1 10x21M" | names: "Dør Enkel_ Glassfelt:IDA 1.1 10x21M:1899884" | material: materials ("hvit", "Glassfiberfylling", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          2 x IFCDOOR | type IFCDOORSTYLE "IDT 5.2 15x21M EI60S" | object type "IDT 5.2 15x21M EI60S" | names: "Dør Dobbel:IDT 5.2 15x21M EI60S:1899943", "Dør Dobbel:IDT 5.2 15x21M EI60S:1904040" | material: materials ("NCS S 1000-N", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 2.2 10x21M 28dB EI30S" | object type "IDT 2.2 10x21M 28dB EI30S" | names: "Dør Enkel:IDT 2.2 10x21M 28dB EI30S:1924849" | material: materials ("Light grey", "Lys grå", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          2 x IFCDOOR | type IFCDOORSTYLE "IDT 5.2 15x21M EI60S" | object type "IDT 5.2 15x21M EI60S" | names: "Dør Dobbel:IDT 5.2 15x21M EI60S:1937615", "Dør Dobbel:IDT 5.2 15x21M EI60S:1937698" | material: materials ("NCS S 1000-N", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          3 x IFCDOOR | type IFCDOORSTYLE "IDT 1.2 8x21M 33dB" | object type "IDT 1.2 8x21M 33dB" | names: "Dør Enkel:IDT 1.2 8x21M 33dB:1963500", "Dør Enkel:IDT 1.2 8x21M 33dB:2152848", "Dør Enkel:IDT 1.2 8x21M 33dB:2152911" | material: materials ("Terskel Tre", "NCS S 0500-N", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 2.9 10x21M EI60S" | object type "IDT 2.9 10x21M EI60S" | names: "Dør Enkel:IDT 2.9 10x21M EI60S:1968215" | material: materials ("_White", "Lys grå", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 2.8 10x21M EI30S" | object type "IDT 2.8 10x21M EI30S" | names: "Dør Enkel:IDT 2.8 10x21M EI30S:2008423" | material: materials ("Terskel Tre", "Lys grå", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 3.6 10x21M 38dB" | object type "IDT 3.6 10x21M 38dB" | names: "Dør Enkel_ Glassfelt:IDT 3.6 10x21M 38dB:2017464" | material: materials ("NCS S 2500-N", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 6.3 272mm 60dB (RN-95-30-95-NR)" | object type "Basic Wall:IVA 6.3 272mm 60dB (RN-95-30-95-NR):2866583" | names: "Basic Wall:IVA 6.3 272mm 60dB (RN-95-30-95-NR):2017471", "Basic Wall:IVA 6.3 272mm 60dB (RN-95-30-95-NR):2017472", "Basic Wall:IVA 6.3 272mm 60dB (RN-95-30-95-NR):2130141" (+1 more) | material: layers "Basic Wall:IVA 6.3 272mm 60dB (RN-95-30-95-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95., "Luftsjikt" 30., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 2.6 10x21M 38dB" | object type "IDT 2.6 10x21M 38dB" | names: "Dør Enkel:IDT 2.6 10x21M 38dB:2017473" | material: materials ("Light grey", "Lys grå", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 2.6 10x21M 38dB" | object type "IDT 2.6 10x21M 38dB" | names: "Dør Enkel:IDT 2.6 10x21M 38dB:2017476" | material: materials ("Light grey", "Lys grå", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 2.3 10x21M 33dB" | object type "IDT 2.3 10x21M 33dB" | names: "Dør Enkel:IDT 2.3 10x21M 33dB:2017571" | material: materials ("_White", "Lys grå", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCSTAIR | object type "Stair:amfi:1485385" | names: "Stair:amfi:2067475" | parts: 1 IFCSTAIR | property sets: Pset_StairCommon, Pset_TFM, Constraints, Dimensions, Graphics, Other
          1 x IFCSTAIR | object type "Stair:Trapp amfi:3965809" | names: "Stair:Trapp amfi:2067496" | parts: 4 IFCRAILING, 1 IFCSTAIR | property sets: Pset_StairCommon, Pset_TFM, Constraints, Dimensions, Graphics, Identity Data
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 14.1 126mm (R-100-R)" | object type "Basic Wall:IVA 14.1 126mm (R-100-R):7316308" | names: "Basic Wall:IVA 14.1 126mm (R-100-R):2067524" | material: layers "Basic Wall:IVA 14.1 126mm (R-100-R)" ("Gips" 15., "Massivtre" 100., "Gips" 15.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          5 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 14.1 126mm EI60 (R-100-R)" | object type "Basic Wall:IVA 14.1 126mm EI60 (R-100-R):7315024" | names: "Basic Wall:IVA 14.1 126mm EI60 (R-100-R):2067529", "Basic Wall:IVA 14.1 126mm EI60 (R-100-R):3843703", "Basic Wall:IVA 14.1 126mm EI60 (R-100-R):7316869" (+2 more) | material: layers "Basic Wall:IVA 14.1 126mm EI60 (R-100-R)" ("Branngips" 15., "Massivtre" 100., "Branngips" 15.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 13.1 344mm EI60 (HN-95-110-100-N)" | object type "Basic Wall:IVA 13.1 344mm EI60 (HN-95-110-100-N):2860870" | names: "Basic Wall:IVA 13.1 344mm EI60 (HN-95-110-100-N):2067551" | material: layers "Basic Wall:IVA 13.1 344mm EI60 (HN-95-110-100-N)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 95., "Luftsjikt" 110., "Massivtre" 100., "Branngips" 15.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 2.11 10x21M 33dB EI30S" | object type "IDT 2.11 10x21M 33dB EI30S" | names: "Dør Enkel:IDT 2.11 10x21M 33dB EI30S:2067575" | material: materials ("Terskel Tre", "Lys grå", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 13.1 272mm EI60 (HN-95-100-95-NR) 2" | object type "Basic Wall:IVA 13.1 272mm EI60 (HN-95-100-95-NR) 2:7319444" | names: "Basic Wall:IVA 13.1 272mm EI60 (HN-95-100-95-NR) 2:2067581" | material: layers "Basic Wall:IVA 13.1 272mm EI60 (HN-95-100-95-NR) 2" ("Habito" 13., "Gips" 13., "stender/isolasjon" 95., "Luftsjikt" 144., "Massivtre" 100., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 2.3 10x21M 33dB" | object type "IDT 2.3 10x21M 33dB" | names: "Dør Enkel:IDT 2.3 10x21M 33dB:2072049" | material: materials ("_White", "Lys grå", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 1.2 8x21M 33dB" | object type "IDT 1.2 8x21M 33dB" | names: "Dør Enkel:IDT 1.2 8x21M 33dB:2072563" | material: materials ("Terskel Tre", "NCS S 0500-N", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 4.2T 172mm 34dB (HN-120-NR)" | object type "Basic Wall:IVA 4.2T 172mm 34dB (HN-120-NR):6703266" | names: "Basic Wall:IVA 4.2T 172mm 34dB (HN-120-NR):2072962" | material: layers "Basic Wall:IVA 4.2T 172mm 34dB (HN-120-NR)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 120., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 2.1 10x21M" | object type "IDT 2.1 10x21M" | names: "Dør Enkel:IDT 2.1 10x21M:2073002" | material: materials ("_White", "NCS S 0500-N", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 2.3 10x21M 33dB" | object type "IDT 2.3 10x21M 33dB" | names: "Dør Enkel:IDT 2.3 10x21M 33dB:2074784" | material: materials ("_White", "NCS S 0500-N", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 2.12 10x21M 24dB EI30S" | object type "IDT 2.12 10x21M 24dB EI30S" | names: "Dør Enkel:IDT 2.12 10x21M 24dB EI30S:2077177" | material: materials ("Terskel Tre", "Lys grå", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 1.1 121mm 34dB (H-95-H)" | object type "Basic Wall:IVA 1.1 121mm 34dB (H-95-H):4819050" | names: "Basic Wall:IVA 1.1 121mm 34dB (H-95-H):2077624", "Basic Wall:IVA 1.1 121mm 34dB (H-95-H):3866877" | material: layers "Basic Wall:IVA 1.1 121mm 34dB (H-95-H)" ("Habito" 13., "stender/isolasjon" 95., "Habito" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 1.4 121mm (B-95-B)" | object type "Basic Wall:IVA 1.4 121mm (B-95-B):4819950" | names: "Basic Wall:IVA 1.4 121mm (B-95-B):2079707" | material: layers "Basic Wall:IVA 1.4 121mm (B-95-B)" ("Baderomspanel" 13., "stender/isolasjon" 95., "Baderomspanel" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 3.4 10x21M 33dB E30CS" | object type "IDT 3.4 10x21M 33dB E30CS" | names: "Dør Enkel_ Glassfelt:IDT 3.4 10x21M 33dB E30CS:2080687" | material: materials ("Lys grå", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVL 1.1 118mm (leca) 34dB EI60" | object type "Basic Wall:IVL 1.1 118mm (leca) 34dB EI60:4398630" | names: "Basic Wall:IVL 1.1 118mm (leca) 34dB EI60:2106922", "Basic Wall:IVL 1.1 118mm (leca) 34dB EI60:3868889" | material: layers "Basic Wall:IVL 1.1 118mm (leca) 34dB EI60" ("Mur" 118.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          3 x IFCDOOR | type IFCDOORSTYLE "IDT 2.1 10x21M" | object type "IDT 2.1 10x21M" | names: "Dør Enkel:IDT 2.1 10x21M:2109495", "Dør Enkel:IDT 2.1 10x21M:2109711", "Dør Enkel:IDT 2.1 10x21M:2110892" | material: materials ("_White", "NCS S 0500-N", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDA 1.1 10x21M" | object type "IDA 1.1 10x21M" | names: "Dør Enkel_ Glassfelt:IDA 1.1 10x21M:2110693" | material: materials ("hvit", "Glassfiberfylling", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 2.3 10x21M 33dB" | object type "IDT 2.3 10x21M 33dB" | names: "Dør Enkel:IDT 2.3 10x21M 33dB:2111466" | material: materials ("Terskel Tre", "Lys grå", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 2.3 10x21M 33dB" | object type "IDT 2.3 10x21M 33dB" | names: "Dør Enkel:IDT 2.3 10x21M 33dB:2111527" | material: materials ("Terskel Tre", "Lys grå", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 1.1T 121mm (H-95-H)" | object type "Basic Wall:IVA 1.1T 121mm (H-95-H):6702424" | names: "Basic Wall:IVA 1.1T 121mm (H-95-H):2112241" | material: layers "Basic Wall:IVA 1.1T 121mm (H-95-H)" ("Habito" 13., "stender/isolasjon" 95., "Habito" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          3 x IFCDOOR | type IFCDOORSTYLE "IDT 1.2 8x21M 33dB" | object type "IDT 1.2 8x21M 33dB" | names: "Dør Enkel:IDT 1.2 8x21M 33dB:2112681", "Dør Enkel:IDT 1.2 8x21M 33dB:2112740", "Dør Enkel:IDT 1.2 8x21M 33dB:2112863" | material: materials ("Terskel Tre", "NCS S 0500-N", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDA 10.1 14x21M E30CS" | object type "IDA 10.1 14x21M E30CS" | names: "Dør Enkel:IDA 10.1 14x21M E30CS:2114687" | material: materials ("Light grey", "Karm Malt", "Lys grå") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 2.4 10x21M 38dB EI30S" | object type "IDT 2.4 10x21M 38dB EI30S" | names: "Dør Enkel:IDT 2.4 10x21M 38dB EI30S:2115769" | material: materials ("Terskel Tre", "Lys grå", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 3.1 10x21M EI 30S" | object type "IDT 3.1 10x21M EI 30S" | names: "Dør Enkel_ Glassfelt:IDT 3.1 10x21M EI 30S:2118010" | material: materials ("Lys grå", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IV 50 - skillevegg" | object type "Basic Wall:IV 50 - skillevegg:425527" | names: "Basic Wall:IV 50 - skillevegg:2118582", "Basic Wall:IV 50 - skillevegg:2119148", "Basic Wall:IV 50 - skillevegg:2123676" (+1 more) | material: layers "Basic Wall:IV 50 - skillevegg" ("<Unnamed>" 50.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 2.9 10x21M EI60S" | object type "IDT 2.9 10x21M EI60S" | names: "Dør Enkel:IDT 2.9 10x21M EI60S:2134991" | material: materials ("Light grey", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 2.10 10x21M 38dB EI60S" | object type "IDT 2.10 10x21M 38dB EI60S" | names: "Dør Enkel:IDT 2.10 10x21M 38dB EI60S:2135168" | material: materials ("Light grey", "Lys grå", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 3.6 10x21M 38dB" | object type "IDT 3.6 10x21M 38dB" | names: "Dør Enkel_ Glassfelt:IDT 3.6 10x21M 38dB:2135766" | material: materials ("NCS S 2500-N", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 4.2 13x21M EI 60S" | object type "IDT 4.2 13x21M EI 60S" | names: "Dør Dobbel_Ulike_Dørblader:IDT 4.2 13x21M EI 60S:2137996" | material: materials ("Trekledning", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 3.6 10x21M 38dB" | object type "IDT 3.6 10x21M 38dB" | names: "Dør Enkel_ Glassfelt:IDT 3.6 10x21M 38dB:2140876" | material: materials ("NCS S 2500-N", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 6.3 272mm 48dB (RN-95-30-95-NR)" | object type "Basic Wall:IVA 6.3 272mm 48dB (RN-95-30-95-NR):5057632" | names: "Basic Wall:IVA 6.3 272mm 48dB (RN-95-30-95-NR):2151525" | material: layers "Basic Wall:IVA 6.3 272mm 48dB (RN-95-30-95-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95., "Luftsjikt" 30., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 6.3 272mm 55dB EI60 (RN-95-30-95-NR)" | object type "Basic Wall:IVA 6.3 272mm 55dB EI60 (RN-95-30-95-NR):2851985" | names: "Basic Wall:IVA 6.3 272mm 55dB EI60 (RN-95-30-95-NR):2151742" | material: layers "Basic Wall:IVA 6.3 272mm 55dB EI60 (RN-95-30-95-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95., "Luftsjikt" 30., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 4.2 172mm 34dB (HN-120-NR)" | object type "Basic Wall:IVA 4.2 172mm 34dB (HN-120-NR):4862299" | names: "Basic Wall:IVA 4.2 172mm 34dB (HN-120-NR):2152400" | material: layers "Basic Wall:IVA 4.2 172mm 34dB (HN-120-NR)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 120., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 2.7 10x21M 38dB EI60S" | object type "IDT 2.7 10x21M 38dB EI60S" | names: "Dør Enkel:IDT 2.7 10x21M 38dB EI60S:2154214" | material: materials ("Light grey", "Lys grå", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDF 1.1 Foldevegg 6500x2800" | object type "IDF 1.1 Foldevegg 6500x2800" | names: "Side_Stack_Operable_Wall_6500:IDF 1.1 Foldevegg 6500x2800:2154531" | material: materials ("Light grey", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 3.3 145mm E30 (RN-95-NR)" | object type "Basic Wall:IVA 3.3 145mm E30 (RN-95-NR):3866097" | names: "Basic Wall:IVA 3.3 145mm E30 (RN-95-NR):2200940" | material: layers "Basic Wall:IVA 3.3 145mm E30 (RN-95-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCDOOR | type IFCDOORSTYLE "IDA 6.2 12x21M EI 30CS" | object type "IDA 6.2 12x21M EI 30CS" | names: "Dør Enkel_ Glassfelt:IDA 6.2 12x21M EI 30CS:2206635" | material: materials ("Lys grå", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 2.1 10x21M" | object type "IDT 2.1 10x21M" | names: "Dør Enkel:IDT 2.1 10x21M:2222006" | material: materials ("_White", "NCS S 0500-N", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 2.1 10x21M" | object type "IDT 2.1 10x21M" | names: "Dør Enkel:IDT 2.1 10x21M:2223619" | material: materials ("_White", "NCS S 0500-N", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "NUS - 0,0 - Kake" | object type "NUS - 0,0 - Kake" | names: "NUS - 0,0 - Kake:NUS - 0,0 - Kake:2233595" | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Other, Phasing
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 2.5 10x21M 33dB EI60S" | object type "IDT 2.5 10x21M 33dB EI60S" | names: "Dør Enkel:IDT 2.5 10x21M 33dB EI60S:2235152" | material: materials ("Light grey", "Lys grå", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDA 3.2 18x21M 33dB" | object type "IDA 3.2 18x21M 33dB" | names: "_Dør Dobbel_Ulike_Dørblader_Glassfelt2:IDA 3.2 18x21M 33dB:2235278" | material: materials ("Glass Klart", "Lys grå", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 8.1 125mm sjaktvegg EI60" | object type "Basic Wall:IVA 8.1 125mm sjaktvegg EI60:2855957" | names: "Basic Wall:IVA 8.1 125mm sjaktvegg EI60:2235676", "Basic Wall:IVA 8.1 125mm sjaktvegg EI60:7179844", "Basic Wall:IVA 8.1 125mm sjaktvegg EI60:7180132" | material: layers "Basic Wall:IVA 8.1 125mm sjaktvegg EI60" ("Branngips" 15., "Branngips" 15., "stender/isolasjon" 95.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 6.2 272mm 55dB EI60 (RN-95-30-95-NH)" | object type "Basic Wall:IVA 6.2 272mm 55dB EI60 (RN-95-30-95-NH):4826087" | names: "Basic Wall:IVA 6.2 272mm 55dB EI60 (RN-95-30-95-NH):2240092", "Basic Wall:IVA 6.2 272mm 55dB EI60 (RN-95-30-95-NH):4045437" | material: layers "Basic Wall:IVA 6.2 272mm 55dB EI60 (RN-95-30-95-NH)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 95., "Luftsjikt" 30., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          5 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVL 2.1 123mm (flis-leca) EI60" | object type "Basic Wall:IVL 2.1 123mm (flis-leca) EI60:4398624" | names: "Basic Wall:IVL 2.1 123mm (flis-leca) EI60:2242204", "Basic Wall:IVL 2.1 123mm (flis-leca) EI60:2280610", "Basic Wall:IVL 2.1 123mm (flis-leca) EI60:2371150" (+2 more) | material: layers "Basic Wall:IVL 2.1 123mm (flis-leca) EI60" ("Flis" 5., "Mur" 118.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 2.9 10x21M EI60S" | object type "IDT 2.9 10x21M EI60S" | names: "Dør Enkel:IDT 2.9 10x21M EI60S:2379978" | material: materials ("Light grey", "Lys grå", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCSLAB | object type "Floor:Betongdekke 350+ 120 dansegulv" | FLOOR | names: "Floor:Betongdekke 350+ 120 dansegulv:2406366" | material: layers "Floor:Betongdekke 350+ 120 dansegulv" ("<Unnamed>" 10., "Betong" 80., "Trinnlydplate" 30., "Betong" 350.) | property sets: Pset_SlabCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          2 x IFCSLAB | object type "Floor:Betongdekke 350 + avretting 65" | FLOOR | names: "Floor:Betongdekke 350 + avretting 65:2406772", "Floor:Betongdekke 350 + avretting 65:2406772:2" | material: layers "Floor:Betongdekke 350 + avretting 65" ("Betong" 35., "Betong avretting" 30., "Betong" 350.) | property sets: Pset_SlabCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCSLAB | object type "Floor:Betongdekke 350 + industriparkett, sløyd" | FLOOR | names: "Floor:Betongdekke 350 + industriparkett, sløyd:2410416" | material: layers "Floor:Betongdekke 350 + industriparkett, sløyd" ("Industriparkett" 28., "Sponplate" 22., "<Unnamed>" 12.5, "Betong avretting" 14.5, "Betong" 350.) | property sets: Pset_SlabCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Other
          4 x IFCWINDOW | type IFCWINDOWSTYLE "V13 12x16" | object type "V13 12x16" | names: "Vindu-Hengslet:V13 12x16:2425648", "Vindu-Hengslet:V13 12x16:2427845", "Vindu-Hengslet:V13 12x16:2428579" (+1 more) | material: materials ("Glass Klart", "NCS S 0502-Y", "Karm Malt") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "V15 24x16" | object type "V15 24x16" | names: "Fast vindu+ åpningsvindu:V15 24x16:2427850" | material: materials ("NCS S 0502-Y", "Glass Klart") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "V14 14x16" | object type "V14 14x16" | names: "Vindu-Fast:V14 14x16:2430034" | material: materials ("Glass Klart", "NCS S 0502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "V14 14x16" | object type "V14 14x16" | names: "Vindu-Fast:V14 14x16:2431102" | material: materials ("Glass Klart", "NCS S 0502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:YV 8.2 458mm gul platekledning EI60" | object type "Basic Wall:YV 8.2 458mm gul platekledning EI60:4470403" | names: "Basic Wall:YV 8.2 458mm gul platekledning EI60:2445283" | material: layers "Basic Wall:YV 8.2 458mm gul platekledning EI60" ("Cembrit Metro Amsterdam" 8., "Luftsjikt" 36., "Luftsjikt" 48., "Vindsperre" 9., "Stender isolert vegg" 296., "NO_Utlekting" 48., "Branngips" 15.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 2.5 10x21M 33dB EI60S" | object type "IDT 2.5 10x21M 33dB EI60S" | names: "Dør Enkel:IDT 2.5 10x21M 33dB EI60S:2467851" | material: materials ("Light grey", "Lys grå", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 2.5 10x21M 33dB EI60S" | object type "IDT 2.5 10x21M 33dB EI60S" | names: "Dør Enkel:IDT 2.5 10x21M 33dB EI60S:2467890" | material: materials ("Light grey", "Lys grå", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVL 1.1 118mm (leca) 34dB" | object type "Basic Wall:IVL 1.1 118mm (leca) 34dB:4134834" | names: "Basic Wall:IVL 1.1 118mm (leca) 34dB:2485947", "Basic Wall:IVL 1.1 118mm (leca) 34dB:3606985" | material: layers "Basic Wall:IVL 1.1 118mm (leca) 34dB" ("Mur" 118.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVL 1.1 118mm (leca) 44dB" | object type "Basic Wall:IVL 1.1 118mm (leca) 44dB:4134954" | names: "Basic Wall:IVL 1.1 118mm (leca) 44dB:2486042" | material: layers "Basic Wall:IVL 1.1 118mm (leca) 44dB" ("Mur" 118.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 2.1 10x21M" | object type "IDT 2.1 10x21M" | names: "Dør Enkel:IDT 2.1 10x21M:2486526" | material: materials ("_White", "NCS S 0500-N", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          2 x IFCDOOR | type IFCDOORSTYLE "IDT 2.1 10x21M" | object type "IDT 2.1 10x21M" | names: "Dør Enkel:IDT 2.1 10x21M:2486579", "Dør Enkel:IDT 2.1 10x21M:3605652" | material: materials ("_White", "NCS S 0500-N", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 2.1 10x21M" | object type "IDT 2.1 10x21M" | names: "Dør Enkel:IDT 2.1 10x21M:2487384" | material: materials ("_White", "NCS S 0500-N", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 2.1 10x21M" | object type "IDT 2.1 10x21M" | names: "Dør Enkel:IDT 2.1 10x21M:2488521" | material: materials ("Light grey", "NCS S 0500-N", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          2 x IFCWINDOW | type IFCWINDOWSTYLE "GF 3.6 6x21 33dB" | object type "GF 3.6 6x21 33dB" | names: "Vindu-Fast:GF 3.6 6x21 33dB:2525684", "Vindu-Fast:GF 3.6 6x21 33dB:2525730" | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "GF 3.6 6x21 33dB" | object type "GF 3.6 6x21 33dB" | names: "Vindu-Fast:GF 3.6 6x21 33dB:2525792" | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "GF 6.1 8x21 33dB" | object type "GF 6.1 8x21 33dB" | names: "Vindu-Fast:GF 6.1 8x21 33dB:2527002" | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "GF 2.2 9x21 33dB" | object type "GF 2.2 9x21 33dB" | names: "Vindu-Fast:GF 2.2 9x21 33dB:2527038" | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "GF 2.2 9x21 33dB" | object type "GF 2.2 9x21 33dB" | names: "Vindu-Fast:GF 2.2 9x21 33dB:2527134" | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "GF 2.2 9x21 33dB" | object type "GF 2.2 9x21 33dB" | names: "Vindu-Fast:GF 2.2 9x21 33dB:2527173" | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "GF 2.2 9x21 33dB" | object type "GF 2.2 9x21 33dB" | names: "Vindu-Fast:GF 2.2 9x21 33dB:2527217" | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "GF 2.2 9x21 33dB" | object type "GF 2.2 9x21 33dB" | names: "Vindu-Fast:GF 2.2 9x21 33dB:2527241" | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "GF 2.1 9x21 38dB" | object type "GF 2.1 9x21 38dB" | names: "Vindu-Fast:GF 2.1 9x21 38dB:2527441" | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "GF 5.3 5x21 33dB" | object type "GF 5.3 5x21 33dB" | names: "Vindu-Fast:GF 5.3 5x21 33dB:2527482" | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "GF 15.1 36x10 33dB" | object type "GF 15.1 36x10 33dB" | names: "Vindu-Fast:GF 15.1 36x10 33dB:2529032" | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "GF 8.1 7x7 58dB" | object type "GF 8.1 7x7 58dB" | names: "Vindu-Fast:GF 8.1 7x7 58dB:2529523" | material: materials ("Glass Klart", "NCS S 1002-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "GF 2.4 9x21 25dB E30" | object type "GF 2.4 9x21 25dB E30" | names: "Vindu-Fast:GF 2.4 9x21 25dB E30:2529908" | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "GF 2.3 9x21 25dB EI30" | object type "GF 2.3 9x21 25dB EI30" | names: "Vindu-Fast:GF 2.3 9x21 25dB EI30:2530890" | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "GF 3.1 6x21 25dB EI30" | object type "GF 3.1 6x21 25dB EI30" | names: "Vindu-Fast:GF 3.1 6x21 25dB EI30:2531956" | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "GF 4.3 33dB EI30" | object type "GF 4.3 33dB EI30" | names: "Vindu_2felt:GF 4.3 33dB EI30:2532106" | material: materials ("Karm Malt", "Glass Klart", "NCS S 3502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "GF 3.4 6x21 33dB E30" | object type "GF 3.4 6x21 33dB E30" | names: "Vindu-Fast:GF 3.4 6x21 33dB E30:2532146" | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          2 x IFCWINDOW | type IFCWINDOWSTYLE "GF 2.2 9x21 33dB" | object type "GF 2.2 9x21 33dB" | names: "Vindu-Fast:GF 2.2 9x21 33dB:2532505", "Vindu-Fast:GF 2.2 9x21 33dB:2532549" | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          4 x IFCWINDOW | type IFCWINDOWSTYLE "GF 2.2 9x21 33dB" | object type "GF 2.2 9x21 33dB" | names: "Vindu-Fast:GF 2.2 9x21 33dB:2532609", "Vindu-Fast:GF 2.2 9x21 33dB:2532682", "Vindu-Fast:GF 2.2 9x21 33dB:2532782" (+1 more) | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "GF 6.1 8x21 33dB" | object type "GF 6.1 8x21 33dB" | names: "Vindu-Fast:GF 6.1 8x21 33dB:2532752" | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          6 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:YV 7.3 410mm rød platekledning" | object type "Basic Wall:YV 7.3 410mm rød platekledning:2216522" | names: "Basic Wall:YV 7.3 410mm rød platekledning:2533885", "Basic Wall:YV 7.3 410mm rød platekledning:2534167", "Basic Wall:YV 7.3 410mm rød platekledning:2534283" (+3 more) | material: layers "Basic Wall:YV 7.3 410mm rød platekledning" ("Cembrit Metro Copenhagen" 8., "Luftsjikt" 36., "Vindsperre" 9., "Stender isolert vegg" 296., "NO_Utlekting" 48., "Robustgips" 12.5) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          5 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:YV 7.2 410mm grønn platekledning" | object type "Basic Wall:YV 7.2 410mm grønn platekledning:2569141" | names: "Basic Wall:YV 7.2 410mm grønn platekledning:2533952", "Basic Wall:YV 7.2 410mm grønn platekledning:2534068", "Basic Wall:YV 7.2 410mm grønn platekledning:3013398" (+2 more) | material: layers "Basic Wall:YV 7.2 410mm grønn platekledning" ("Cembrit Metro Hamburg" 8., "Luftsjikt" 36., "Vindsperre" 9., "Stender isolert vegg" 296., "NO_Utlekting" 48., "Robustgips" 12.5) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          2 x IFCWINDOW | type IFCWINDOWSTYLE "V25 12x30 36dB" | object type "V25 12x30 36dB" | names: "Vindu-Fast:V25 12x30 36dB:2535368", "Vindu-Fast:V25 12x30 36dB:2536143" | material: materials ("Glass Klart", "NCS S 0502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          5 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:YV 7.4 410mm gul platekledning" | object type "Basic Wall:YV 7.4 410mm gul platekledning:1741258" | names: "Basic Wall:YV 7.4 410mm gul platekledning:2537045", "Basic Wall:YV 7.4 410mm gul platekledning:2537132", "Basic Wall:YV 7.4 410mm gul platekledning:4194167" (+2 more) | material: layers "Basic Wall:YV 7.4 410mm gul platekledning" ("Cembrit Metro Amsterdam" 8., "Luftsjikt" 36., "Vindsperre" 9., "Stender isolert vegg" 296., "NO_Utlekting" 48., "Robustgips" 12.5) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCWINDOW | type IFCWINDOWSTYLE "VA1 12x24" | object type "VA1 12x24" | names: "Vindu-Fast:VA1 12x24:2537605" | material: materials ("Glass Klart", "NCS S 0502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "GF 7.4 15x21 EI60" | object type "GF 7.4 15x21 EI60" | names: "Vindu-Fast:GF 7.4 15x21 EI60:2552756" | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCROOF | object type "Basic Roof:Tak tre 246" | names: "Basic Roof:Tak tre 246:2558041" | parts: 1 IFCSLAB | property sets: Pset_RoofCommon, Pset_TFM, Constraints, Construction, Dimensions, Identity Data
          1 x IFCROOF | object type "Basic Roof:Tak tre 246 + spiler" | names: "Basic Roof:Tak tre 246 + spiler:2558158" | parts: 1 IFCSLAB | property sets: Pset_RoofCommon, Pset_TFM, Constraints, Construction, Dimensions, Other
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 3.9 10x21M 28dB" | object type "IDT 3.9 10x21M 28dB" | names: "Dør Enkel_ Glassfelt:IDT 3.9 10x21M 28dB:2571576" | material: materials ("Lys grå", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "GF 7.1 15x21 25dB" | object type "GF 7.1 15x21 25dB" | names: "Vindu-Fast:GF 7.1 15x21 25dB:2571640" | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          5 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:YV 20.1" | object type "Basic Wall:YV 20.1:5642374" | names: "Basic Wall:YV 20.1:2583217", "Basic Wall:YV 20.1:4882661", "Basic Wall:YV 20.1:4882753" (+2 more) | material: layers "Basic Wall:YV 20.1" ("Trekledning" 19., "Luftsjikt" 36., "Luftsjikt" 36., "Vindsperre" 9., "Stender isolert vegg" 148., "Kryssfiner" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:YV 20.3" | object type "Basic Wall:YV 20.3:5769428" | names: "Basic Wall:YV 20.3:2583220", "Basic Wall:YV 20.3:2583257", "Basic Wall:YV 20.3:2583258" | material: layers "Basic Wall:YV 20.3" ("Trekledning" 19., "Luftsjikt" 36., "Luftsjikt" 36., "Vindsperre" 9., "Stender isolert vegg" 148., "Baderomspanel" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IV 20.1" | object type "Basic Wall:IV 20.1:6302540" | names: "Basic Wall:IV 20.1:2583221" | material: layers "Basic Wall:IV 20.1" ("Baderomspanel" 10.2, "stender" 98., "Robustgips" 12.5) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCDOOR | type IFCDOORSTYLE "YDT 1.2 10x21M Isolert" | object type "YDT 1.2 10x21M Isolert" | names: "Dør Enkel:YDT 1.2 10x21M Isolert:2583745" | material: materials ("_White", "Lys grå", "Beslag") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          2 x IFCANNOTATION
          7 x IFCCOVERING | object type "Compound Ceiling:Lydhimling gips" | CEILING | names: "Compound Ceiling:Lydhimling gips:2599479", "Compound Ceiling:Lydhimling gips:3050935", "Compound Ceiling:Lydhimling gips:3053637" (+4 more) | material: layers "Compound Ceiling:Lydhimling gips" ("Himling Metallprofil" 48., "Gips" 12.5, "Gips" 12.5) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Other
          4 x IFCCOVERING | object type "Compound Ceiling:Himling System 600x600 Venus Kant A 42dB" | CEILING | names: "Compound Ceiling:Himling System 600x600 Venus Kant A 42dB:2599537", "Compound Ceiling:Himling System 600x600 Venus Kant A 42dB:3053015", "Compound Ceiling:Himling System 600x600 Venus Kant A 42dB:3053273" (+1 more) | material: layers "Compound Ceiling:Himling System 600x600 Venus Kant A 42dB" ("Himling Metallprofil" 38., "Himling System 600x600" 12.) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          7 x IFCCOVERING | object type "Compound Ceiling:Himling System 600x600 hygiene" | CEILING | names: "Compound Ceiling:Himling System 600x600 hygiene:2599647", "Compound Ceiling:Himling System 600x600 hygiene:2599709", "Compound Ceiling:Himling System 600x600 hygiene:2599730" (+4 more) | material: layers "Compound Ceiling:Himling System 600x600 hygiene" ("Himling Metallprofil" 38., "Himling System 600x600" 12.) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          34 x IFCCOVERING | object type "Compound Ceiling:Himling System 600x600" | CEILING | names: "Compound Ceiling:Himling System 600x600:2599746", "Compound Ceiling:Himling System 600x600:2599754", "Compound Ceiling:Himling System 600x600:2599770" (+31 more) | material: layers "Compound Ceiling:Himling System 600x600" ("Himling Metallprofil" 38., "Himling System 600x600" 12.) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Other
          2 x IFCCOVERING | object type "Compound Ceiling:Himling spiler" | CEILING | names: "Compound Ceiling:Himling spiler:2599840", "Compound Ceiling:Himling spiler:3085186" | material: layers "Compound Ceiling:Himling spiler" ("Himling Metallprofil" 48., "Spiler" 34.) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Other
          1 x IFCROOF | object type "Basic Roof:Tak tre (stål) 148:2058777" | names: "Basic Roof:Tak tre (stål) 148:2601127" | material: "stender" | property sets: Pset_RoofCommon, Pset_TFM, Constraints, Construction, Dimensions, Other
          2 x IFCWINDOW | type IFCWINDOWSTYLE "VA1 12x24" | object type "VA1 12x24" | names: "Vindu-Fast:VA1 12x24:2601155", "Vindu-Fast:VA1 12x24:3019389" | material: materials ("Glass Klart", "NCS S 0502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          2 x IFCSLAB | object type "Floor:Betongdekke 200" | FLOOR | names: "Floor:Betongdekke 200:2671357", "Floor:Betongdekke 200:4090351" | material: layers "Floor:Betongdekke 200" ("Betong" 200.) | property sets: Pset_SlabCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCROOF | object type "Basic Roof:Tak tre 223:6967508" | names: "Basic Roof:Tak tre 223:2671519" | material: "stender" | property sets: Pset_RoofCommon, Pset_TFM, Constraints, Construction, Dimensions, Other
          19 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:Sokkel pusset" | object type "Basic Wall:Sokkel pusset:2745482" | names: "Basic Wall:Sokkel pusset:2748042", "Basic Wall:Sokkel pusset:2748287", "Basic Wall:Sokkel pusset:2748494" (+16 more) | material: layers "Basic Wall:Sokkel pusset" ("Webertherm 260" 10., "NO_isolasjon" 100.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          2 x IFCWINDOW | type IFCWINDOWSTYLE "GF 3.2 6x21 38dB" | object type "GF 3.2 6x21 38dB" | names: "Vindu-Fast:GF 3.2 6x21 38dB:2751635", "Vindu-Fast:GF 3.2 6x21 38dB:3000160" | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 2.3 10x21M 33dB" | object type "IDT 2.3 10x21M 33dB" | names: "Dør Enkel:IDT 2.3 10x21M 33dB:2834668" | material: materials ("Terskel Tre", "Lys grå", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 3.2 145mm 34dB E30 (HN-95-NR)" | object type "Basic Wall:IVA 3.2 145mm 34dB E30 (HN-95-NR):3863579" | names: "Basic Wall:IVA 3.2 145mm 34dB E30 (HN-95-NR):2862879" | material: layers "Basic Wall:IVA 3.2 145mm 34dB E30 (HN-95-NR)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 2.4 134mm 44dB (R-95-NH)" | object type "Basic Wall:IVA 2.4 134mm 44dB (R-95-NH):4822545" | names: "Basic Wall:IVA 2.4 134mm 44dB (R-95-NH):2865540" | material: layers "Basic Wall:IVA 2.4 134mm 44dB (R-95-NH)" ("Robustgips" 13., "stender/isolasjon" 95., "Gips" 13., "Habito" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 13.1 126mm 48dB (HN-95+20+100-R)" | object type "Basic Wall:IVA 13.1 126mm 48dB (HN-95+20+100-R):7316740" | names: "Basic Wall:IVA 13.1 126mm 48dB (HN-95+20+100-R):2867164" | material: layers "Basic Wall:IVA 13.1 126mm 48dB (HN-95+20+100-R)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 95., "Luftsjikt" 20., "Massivtre" 100., "Branngips" 15.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVL 2.1 123mm (flis-leca) 44dB" | object type "Basic Wall:IVL 2.1 123mm (flis-leca) 44dB:3869632" | names: "Basic Wall:IVL 2.1 123mm (flis-leca) 44dB:2867406", "Basic Wall:IVL 2.1 123mm (flis-leca) 44dB:2868394" | material: layers "Basic Wall:IVL 2.1 123mm (flis-leca) 44dB" ("Flis" 5., "Mur" 118.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 4.3T 172mm 34dB (RN-120-NR)" | object type "Basic Wall:IVA 4.3T 172mm 34dB (RN-120-NR):6691836" | names: "Basic Wall:IVA 4.3T 172mm 34dB (RN-120-NR):2868671" | material: layers "Basic Wall:IVA 4.3T 172mm 34dB (RN-120-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 120., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 2.3T 134mm 34dB (R-95-NR)" | object type "Basic Wall:IVA 2.3T 134mm 34dB (R-95-NR):6701505" | names: "Basic Wall:IVA 2.3T 134mm 34dB (R-95-NR):2868861" | material: layers "Basic Wall:IVA 2.3T 134mm 34dB (R-95-NR)" ("Robustgips" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 3.2T 145mm 48dB EI60 (HN-95-NR)" | object type "Basic Wall:IVA 3.2T 145mm 48dB EI60 (HN-95-NR):6702539" | names: "Basic Wall:IVA 3.2T 145mm 48dB EI60 (HN-95-NR):2869074", "Basic Wall:IVA 3.2T 145mm 48dB EI60 (HN-95-NR):3435573" | material: layers "Basic Wall:IVA 3.2T 145mm 48dB EI60 (HN-95-NR)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 3.2T 145mm 44dB (HN-95-NR)" | object type "Basic Wall:IVA 3.2T 145mm 44dB (HN-95-NR):6703548" | names: "Basic Wall:IVA 3.2T 145mm 44dB (HN-95-NR):2869156" | material: layers "Basic Wall:IVA 3.2T 145mm 44dB (HN-95-NR)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 3.2T 145mm EI60 (HN-95-NR)" | object type "Basic Wall:IVA 3.2T 145mm EI60 (HN-95-NR):6703123" | names: "Basic Wall:IVA 3.2T 145mm EI60 (HN-95-NR):2869175", "Basic Wall:IVA 3.2T 145mm EI60 (HN-95-NR):3866457", "Basic Wall:IVA 3.2T 145mm EI60 (HN-95-NR):4044631" | material: layers "Basic Wall:IVA 3.2T 145mm EI60 (HN-95-NR)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 12.1 121mm (95-NR)" | object type "Basic Wall:IVA 12.1 121mm (95-NR):7206579" | names: "Basic Wall:IVA 12.1 121mm (95-NR):2882889" | material: layers "Basic Wall:IVA 12.1 121mm (95-NR)" ("Flis" 5., "Litex" 12., "Kryssfiner" 15., "stender/isolasjon" 95.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:YV 19.1 256mm EI60" | object type "Basic Wall:YV 19.1 256mm EI60:6291662" | names: "Basic Wall:YV 19.1 256mm EI60:2905274" | material: layers "Basic Wall:YV 19.1 256mm EI60" ("Trekledning" 19., "Luftsjikt" 48., "Luftsjikt" 36., "Vindsperre" 9., "Stender isolert vegg" 48., "Stender isolert vegg" 96.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          13 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Curtain Wall:YV 100 S" | object type "Curtain Wall:YV 100 S:305131" | names: "Curtain Wall:YV 100 S:2928051", "Curtain Wall:YV 100 S:2928179", "Curtain Wall:YV 100 S:2929985" (+10 more) | parts: 52 IFCMEMBER, 13 IFCPLATE | property sets: Pset_CurtainWallCommon, Pset_TFM, Constraints, Dimensions, Horizontal Grid, Identity Data
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:YV 3.1 306mm EI60" | object type "Basic Wall:YV 3.1 306mm EI60:2905012" | names: "Basic Wall:YV 3.1 306mm EI60:2980270", "Basic Wall:YV 3.1 306mm EI60:2980521" | material: layers "Basic Wall:YV 3.1 306mm EI60" ("Trekledning" 19., "Luftsjikt" 48., "Luftsjikt" 36., "Luftsjikt" 48., "Vindsperre" 9., "Stender isolert vegg" 146.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCDOOR | type IFCDOORSTYLE "YDA 1.2 16x21M EI 30S" | object type "YDA 1.2 16x21M EI 30S" | names: "_Dør Dobbel_Ulike_Dørblader_Glassfelt2:YDA 1.2 16x21M EI 30S:2980271" | material: materials ("Glass Klart", "Lys grå", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "YDA 1.2 16x21M EI 30S" | object type "YDA 1.2 16x21M EI 30S" | names: "_Dør Dobbel_Ulike_Dørblader_Glassfelt2:YDA 1.2 16x21M EI 30S:2980522" | material: materials ("Glass Klart", "Lys grå", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Curtain Wall:Glassfasade 6" | object type "Curtain Wall:Glassfasade 6:6185871" | names: "Curtain Wall:Glassfasade 6:3036779" | parts: 74 IFCMEMBER, 23 IFCPLATE, 1 IFCDOOR | property sets: Pset_CurtainWallCommon, Pset_TFM, Constraints, Dimensions, Horizontal Grid, Identity Data
          19 x IFCCOVERING | object type "Compound Ceiling:Himling System 600x1200" | CEILING | names: "Compound Ceiling:Himling System 600x1200:3049184", "Compound Ceiling:Himling System 600x1200:3049223", "Compound Ceiling:Himling System 600x1200:3049288" (+16 more) | material: layers "Compound Ceiling:Himling System 600x1200" ("Himling Metallprofil" 38., "Himling System 600x1200" 12.) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Other
          9 x IFCCOVERING | object type "Compound Ceiling:Himling System 600x600 hygiene korrosjonsklasse" | CEILING | names: "Compound Ceiling:Himling System 600x600 hygiene korrosjonsklasse:3050033", "Compound Ceiling:Himling System 600x600 hygiene korrosjonsklasse:3050070", "Compound Ceiling:Himling System 600x600 hygiene korrosjonsklasse:3050107" (+6 more) | material: layers "Compound Ceiling:Himling System 600x600 hygiene korrosjonsklasse" ("Himling Metallprofil" 38., "Himling System 600x600" 12.) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Other
          5 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 7.1 121mm Skjørt" | object type "Basic Wall:IVA 7.1 121mm Skjørt:2853494" | names: "Basic Wall:IVA 7.1 121mm Skjørt:3052611", "Basic Wall:IVA 7.1 121mm Skjørt:3053806", "Basic Wall:IVA 7.1 121mm Skjørt:3075364" (+2 more) | material: layers "Basic Wall:IVA 7.1 121mm Skjørt" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          11 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 7.2 108mm Skjørt" | object type "Basic Wall:IVA 7.2 108mm Skjørt:5366897" | names: "Basic Wall:IVA 7.2 108mm Skjørt:3054538", "Basic Wall:IVA 7.2 108mm Skjørt:3075047", "Basic Wall:IVA 7.2 108mm Skjørt:3075766" (+8 more) | material: layers "Basic Wall:IVA 7.2 108mm Skjørt" ("Gips" 13., "stender/isolasjon" 95.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          1 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Curtain Wall:GFA 2 38dB" | object type "Curtain Wall:GFA 2 38dB:2845368" | names: "Curtain Wall:GFA 2 38dB:3080384" | parts: 20 IFCMEMBER, 6 IFCPLATE, 1 IFCDOOR | property sets: Pset_CurtainWallCommon, Pset_TFM, Constraints, Dimensions, Horizontal Grid, Identity Data
          1 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Curtain Wall:GFA 1 38dB EI30S" | object type "Curtain Wall:GFA 1 38dB EI30S:4398633" | names: "Curtain Wall:GFA 1 38dB EI30S:3080439" | parts: 33 IFCMEMBER, 11 IFCPLATE, 1 IFCDOOR | property sets: Pset_CurtainWallCommon, Pset_TFM, Constraints, Dimensions, Horizontal Grid, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 9.1 10x21M" | object type "IDT 9.1 10x21M" | names: "Dør Enkel:IDT 9.1 10x21M:3427527" | material: materials ("_White", "Light grey", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 3.5 10x21M 38dB EI30S" | object type "IDT 3.5 10x21M 38dB EI30S" | names: "Dør Enkel_ Glassfelt:IDT 3.5 10x21M 38dB EI30S:3433322" | material: materials ("Lys grå", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 2.3 134mm 37dB (R-95-NR)" | object type "Basic Wall:IVA 2.3 134mm 37dB (R-95-NR):4820253" | names: "Basic Wall:IVA 2.3 134mm 37dB (R-95-NR):3448267" | material: layers "Basic Wall:IVA 2.3 134mm 37dB (R-95-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          1 x IFCWINDOW | type IFCWINDOWSTYLE "GF 8.2 58dB" | object type "GF 8.2 58dB" | names: "Vindu-Hengslet:GF 8.2 58dB:3566352" | material: materials ("Glass Klart", "NCS S 1002-Y", "Karm Malt") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCSLAB | object type "Floor:Betongdekke 350 + industriparkett, aula" | FLOOR | names: "Floor:Betongdekke 350 + industriparkett, aula:3603156" | material: layers "Floor:Betongdekke 350 + industriparkett, aula" ("Industriparkett" 28., "<Unnamed>" 62., "Trinnlydplate" 30., "Betong" 350.) | property sets: Pset_SlabCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCSLAB | object type "Floor:Betongdekke 350 + avretting 15" | names: "Floor:Betongdekke 350 + avretting 15:3603360" | parts: 2 IFCSLAB | property sets: Pset_SlabCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Other
          10 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:Flis" | object type "Basic Wall:Flis:3605862" | names: "Basic Wall:Flis:3610523", "Basic Wall:Flis:3610630", "Basic Wall:Flis:3837025" (+7 more) | material: layers "Basic Wall:Flis" ("Flis" 5.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 6.2 272mm 34dB (HN-95-60-95-NR)" | object type "Basic Wall:IVA 6.2 272mm 34dB (HN-95-60-95-NR):2856112" | names: "Basic Wall:IVA 6.2 272mm 34dB (HN-95-60-95-NR):3642321" | material: layers "Basic Wall:IVA 6.2 272mm 34dB (HN-95-60-95-NR)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 95., "Luftsjikt" 30., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 6.3 332mm 44dB (RN-95-90-95-NR)" | object type "Basic Wall:IVA 6.3 332mm 44dB (RN-95-90-95-NR):4827321" | names: "Basic Wall:IVA 6.3 332mm 44dB (RN-95-90-95-NR):3642862" | material: layers "Basic Wall:IVA 6.3 332mm 44dB (RN-95-90-95-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95., "Luftsjikt" 90., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVL 4.1 173mm leca + litex EI60" | object type "Basic Wall:IVL 4.1 173mm leca + litex EI60:6446981" | names: "Basic Wall:IVL 4.1 173mm leca + litex EI60:3644048" | material: layers "Basic Wall:IVL 4.1 173mm leca + litex EI60" ("<Unnamed>" 5., "Litex" 12., "Mur" 118.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 7.1 121mm 37dB EI30 (95-NR)" | object type "Basic Wall:IVA 7.1 121mm 37dB EI30 (95-NR):6023854" | names: "Basic Wall:IVA 7.1 121mm 37dB EI30 (95-NR):3652168", "Basic Wall:IVA 7.1 121mm 37dB EI30 (95-NR):3652196", "Basic Wall:IVA 7.1 121mm 37dB EI30 (95-NR):4045903" | material: layers "Basic Wall:IVA 7.1 121mm 37dB EI30 (95-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          1 x IFCDOOR | type IFCDOORSTYLE "IDA 9.1 12x21M EI60CS" | object type "IDA 9.1 12x21M EI60CS" | names: "Dør Enkel:IDA 9.1 12x21M EI60CS:3676346" | material: materials ("Light grey", "Karm Malt", "Lys grå") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDA 7.1 15x21M EI60CS" | object type "IDA 7.1 15x21M EI60CS" | names: "Enfløyet_aludør:IDA 7.1 15x21M EI60CS:3690402" | material: materials ("Karm Malt", "Lys grå", "Terskel Tre") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDA 3.5 18x21M 33dB EI30S" | object type "IDA 3.5 18x21M 33dB EI30S" | names: "Dør Dobbel_Ulike_Dørblader:IDA 3.5 18x21M 33dB EI30S:3705902" | material: materials ("Lys grå", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCBEAM | type IFCBEAMTYPE "IPE-Beams:IPE 200" | object type "IPE-Beams:IPE 200:3715116" | names: "IPE-Beams:IPE 200:3714985" | material: "Metal - Steel - 345 MPa" | property sets: BaseQuantities, Pset_BeamCommon, Pset_TFM, Constraints, Construction, Dimensions
          1 x IFCSLAB | object type "Floor:Betongdekke 350 + avretting 15" | FLOOR | names: "Floor:Betongdekke 350 + avretting 15:3761485" | material: layers "Floor:Betongdekke 350 + avretting 15" ("Betong avretting" 15., "Betong" 350.) | property sets: Pset_SlabCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCSLAB | object type "Floor:Betongdekke 300 + avretting og flis" | FLOOR | names: "Floor:Betongdekke 300 + avretting og flis:3768473" | material: materials ("Flis", "Betong avretting", "Betong") | property sets: Pset_SlabCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Other
          2 x IFCSLAB | object type "Floor:Betongdekke 220 + påstøp 80 + avretting" | FLOOR | names: "Floor:Betongdekke 220 + påstøp 80 + avretting:3774068", "Floor:Betongdekke 220 + påstøp 80 + avretting:4056892" | material: layers "Floor:Betongdekke 220 + påstøp 80 + avretting" ("Betong" 35., "Betong avretting" 30., "Betong påstøp" 80., "Betong" 220.) | property sets: Pset_SlabCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Other
          1 x IFCBEAM | type IFCBEAMTYPE "IPE330" | object type "IPE330" | names: "IPE-Beams_brannisolering:IPE330:3801341" | material: materials ("Metal - Steel - 345 MPa", "Brannisolering") | property sets: Pset_BeamCommon, Pset_TFM, BaseQuantities, Constraints, Construction, Dimensions
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 3.2T 145mm 34dB EI60 (HN-95-NR)" | object type "Basic Wall:IVA 3.2T 145mm 34dB EI60 (HN-95-NR):6703331" | names: "Basic Wall:IVA 3.2T 145mm 34dB EI60 (HN-95-NR):3866519" | material: layers "Basic Wall:IVA 3.2T 145mm 34dB EI60 (HN-95-NR)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          5 x IFCSLAB | object type "Floor:Betongdekke 250 m fall" | FLOOR | names: "Floor:Betongdekke 250 m fall:3875926", "Floor:Betongdekke 250 m fall:3879157", "Floor:Betongdekke 250 m fall:3949601" (+2 more) | material: materials ("Betong", "Betong"); layers "Floor:Betongdekke 250 m fall" ("Betong" 200., "Betong" 50.) | property sets: Pset_SlabCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Other
          1 x IFCSLAB | object type "Floor:Betongdekke 300" | FLOOR | names: "Floor:Betongdekke 300:3878971" | material: layers "Floor:Betongdekke 300" ("Betong" 300.) | property sets: Pset_SlabCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:110mm Heisvegg" | object type "Basic Wall:110mm Heisvegg:3943637" | names: "Basic Wall:110mm Heisvegg:3944653" | material: layers "Basic Wall:110mm Heisvegg" ("hvit malt" 110.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCWINDOW | type IFCWINDOWSTYLE "V22 14x14" | object type "V22 14x14" | names: "Vindu-Fast:V22 14x14:3951157" | material: materials ("Glass Klart", "NCS S 0502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCSLAB | object type "Floor:Betongdekke 150" | FLOOR | names: "Floor:Betongdekke 150:3953567" | material: layers "Floor:Betongdekke 150" ("Betong" 150.) | property sets: Pset_SlabCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Other
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IV 100" | object type "Basic Wall:IV 100:1838506" | names: "Basic Wall:IV 100:3971580" | material: layers "Basic Wall:IV 100" ("hvit malt" 100.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCDOOR | type IFCDOORSTYLE "YDS 2.1 13x21M" | object type "YDS 2.1 13x21M" | names: "Dør Enkel:YDS 2.1 13x21M:3971723" | material: materials ("Terskel Tre", "Dørblad Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "YDA 2.1 12x30 36dB" | object type "YDA 2.1 12x30 36dB" | names: "Dør Enkel_ Glassfelt_glassfelt over:YDA 2.1 12x30 36dB:3974002" | material: materials ("N_Windows - Glass", "RAL 9004", "Terskel Tre") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 2.8 10x21M EI30S" | object type "IDT 2.8 10x21M EI30S" | names: "Dør Enkel:IDT 2.8 10x21M EI30S:3988230" | material: materials ("Terskel Tre", "Lys grå", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:250mm" | object type "Basic Wall:250mm:3996120" | names: "Basic Wall:250mm:3996241", "Basic Wall:250mm:3996307" | material: layers "Basic Wall:250mm" ("hvit malt" 250.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 6.2T 272mm 48dB EI60 (HN-95-30-95-NR)" | object type "Basic Wall:IVA 6.2T 272mm 48dB EI60 (HN-95-30-95-NR):6703668" | names: "Basic Wall:IVA 6.2T 272mm 48dB EI60 (HN-95-30-95-NR):4034149" | material: layers "Basic Wall:IVA 6.2T 272mm 48dB EI60 (HN-95-30-95-NR)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 95., "Luftsjikt" 30., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 3.1 145mm 48dB EI60 (HN-95-NH)" | object type "Basic Wall:IVA 3.1 145mm 48dB EI60 (HN-95-NH):4821759" | names: "Basic Wall:IVA 3.1 145mm 48dB EI60 (HN-95-NH):4036274" | material: layers "Basic Wall:IVA 3.1 145mm 48dB EI60 (HN-95-NH)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Habito" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 6.2 342mm 48dB EI 60 (HN-95-100-95-NR)" | object type "Basic Wall:IVA 6.2 342mm 48dB EI 60 (HN-95-100-95-NR):4042113" | names: "Basic Wall:IVA 6.2 342mm 48dB EI 60 (HN-95-100-95-NR):4042026" | material: layers "Basic Wall:IVA 6.2 342mm 48dB EI 60 (HN-95-100-95-NR)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 95., "Luftsjikt" 100., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 3.2 145mm 44dB EI60 (HN-95-NR)" | object type "Basic Wall:IVA 3.2 145mm 44dB EI60 (HN-95-NR):2865591" | names: "Basic Wall:IVA 3.2 145mm 44dB EI60 (HN-95-NR):4045571" | material: layers "Basic Wall:IVA 3.2 145mm 44dB EI60 (HN-95-NR)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          4 x IFCSLAB | object type "Floor:Betongdekke 350 + 120 flytende gulv" | FLOOR | names: "Floor:Betongdekke 350 + 120 flytende gulv:4056116", "Floor:Betongdekke 350 + 120 flytende gulv:4996272", "Floor:Betongdekke 350 + 120 flytende gulv:7442124" (+1 more) | material: layers "Floor:Betongdekke 350 + 120 flytende gulv" ("Betong" 90., "<Unnamed>" 30., "Betong" 350.) | property sets: Pset_SlabCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Other
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:YV 11.1 266 Gesims Vindfang" | object type "Basic Wall:YV 11.1 266 Gesims Vindfang:4077506" | names: "Basic Wall:YV 11.1 266 Gesims Vindfang:4077571", "Basic Wall:YV 11.1 266 Gesims Vindfang:4077681" | material: layers "Basic Wall:YV 11.1 266 Gesims Vindfang" ("Cembrit Metro Copenhagen" 8., "Luftsjikt" 36., "Vindsperre" 9., "Stender isolert vegg" 198., "Kryssfiner" 15.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:YV 11.1 266 Gesims Vindfang 2" | object type "Basic Wall:YV 11.1 266 Gesims Vindfang 2:6898609" | names: "Basic Wall:YV 11.1 266 Gesims Vindfang 2:4077716" | material: layers "Basic Wall:YV 11.1 266 Gesims Vindfang 2" ("Cembrit Metro Copenhagen" 8., "Stender isolert vegg" 198.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 4.3 172mm 48dB (RN-120-NR)" | object type "Basic Wall:IVA 4.3 172mm 48dB (RN-120-NR):4079466" | names: "Basic Wall:IVA 4.3 172mm 48dB (RN-120-NR):4082173" | material: layers "Basic Wall:IVA 4.3 172mm 48dB (RN-120-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 120., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:YV 21.1" | object type "Basic Wall:YV 21.1:7047380" | names: "Basic Wall:YV 21.1:4090343", "Basic Wall:YV 21.1:4090444", "Basic Wall:YV 21.1:4090445" (+1 more) | material: layers "Basic Wall:YV 21.1" ("Trekledning" 19., "stender" 148.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCDOOR | type IFCDOORSTYLE "YDA 6.1 Skyvedører" | object type "YDA 6.1 Skyvedører" | names: "Doors-Sliding_Manusa_Biparting_sliding_fixed_INT:YDA 6.1 Skyvedører:4108057" | material: materials ("Aluminio Manusa", "Glass") | property sets: Pset_DoorCommon, Pset_ManufacturerTypeInformation, Pset_TFM, BaseQuantities, Constraints, Construction
          1 x IFCDOOR | type IFCDOORSTYLE "YDT 1.1 10x21M" | object type "YDT 1.1 10x21M" | names: "Dør Enkel:YDT 1.1 10x21M:4118873" | material: materials ("Terskel Tre", "Lys grå", "Karm Malt", "Trekledning") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:YV 15.1 150 EI60" | object type "Basic Wall:YV 15.1 150 EI60:4961661" | names: "Basic Wall:YV 15.1 150 EI60:4150458" | material: layers "Basic Wall:YV 15.1 150 EI60" ("<Unnamed>" 8., "<Unnamed>" 36., "Vindsperre" 9., "Vindsperre" 9., "stender" 98., "Vindsperre" 9., "<Unnamed>" 9., "<Unnamed>" 36., "<Unnamed>" 8., "<Unnamed>" 36., "<Unnamed>" 48.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:30mm" | object type "Basic Wall:30mm:4152099" | names: "Basic Wall:30mm:4152269", "Basic Wall:30mm:4152570", "Basic Wall:30mm:6953253" | material: layers "Basic Wall:30mm" ("hvit malt" 30.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 3.6 10x21M 38dB" | object type "IDT 3.6 10x21M 38dB" | names: "Dør Enkel_ Glassfelt:IDT 3.6 10x21M 38dB:4195455" | material: materials ("NCS S 2500-N", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 3.2 10x21M 28dB EI30S" | object type "IDT 3.2 10x21M 28dB EI30S" | names: "Dør Enkel_ Glassfelt:IDT 3.2 10x21M 28dB EI30S:4195576" | material: materials ("Lys grå", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "YDT 1.2 10x21M Isolert" | object type "YDT 1.2 10x21M Isolert" | names: "Dør Enkel:YDT 1.2 10x21M Isolert:4202873" | material: materials ("_White", "Lys grå", "Beslag") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:Bassabsorbent" | object type "Basic Wall:Bassabsorbent:4775288" | names: "Basic Wall:Bassabsorbent:4208952", "Basic Wall:Bassabsorbent:4775690" | material: layers "Basic Wall:Bassabsorbent" ("stender/isolasjon" 98.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IV 21.1" | object type "Basic Wall:IV 21.1:6861546" | names: "Basic Wall:IV 21.1:4214204" | material: layers "Basic Wall:IV 21.1" ("Kryssfiner" 12., "Stender isolert vegg" 148., "Kryssfiner" 12.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCDOOR | type IFCDOORSTYLE "YDP 1.1 2400 x 2100mm" | object type "YDP 1.1 2400 x 2100mm" | names: "M_Overhead-Sectional:YDP 1.1 2400 x 2100mm:4214299" | material: "Metal - Paint Finish - Ivory, Matte" | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          4 x IFCSTAIR | object type "Cast-In-Place Stair:Betongtrapp t=150 repo=200:306564" | names: "Cast-In-Place Stair:Stair:4250545", "Cast-In-Place Stair:Stair:4251515", "Cast-In-Place Stair:Stair:4428775" (+1 more) | parts: 8 IFCSLAB, 8 IFCSTAIRFLIGHT, 7 IFCRAILING | property sets: Pset_StairCommon, Pset_TFM, Constraints, Dimensions, Identity Data, Other
          1 x IFCDOOR | type IFCDOORSTYLE "IDA 1.1 10x21M" | object type "IDA 1.1 10x21M" | names: "Dør Enkel_ Glassfelt:IDA 1.1 10x21M:4270404" | material: materials ("hvit", "Glassfiberfylling", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDA 1.1 10x21M" | object type "IDA 1.1 10x21M" | names: "Dør Enkel_ Glassfelt:IDA 1.1 10x21M:4270571" | material: materials ("hvit", "Glassfiberfylling", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          3 x IFCCOVERING | object type "Compound Ceiling:Himling System 600x600 Master Gamma" | CEILING | names: "Compound Ceiling:Himling System 600x600 Master Gamma:4419259", "Compound Ceiling:Himling System 600x600 Master Gamma:4419272", "Compound Ceiling:Himling System 600x600 Master Gamma:4419285" | material: layers "Compound Ceiling:Himling System 600x600 Master Gamma" ("Himling Metallprofil" 38., "Himling System 600x600" 10.) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Other
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 6.1 15x21M 33dB" | object type "IDT 6.1 15x21M 33dB" | names: "_Dør Dobbel_Ulike_Dørblader_Glassfelt2:IDT 6.1 15x21M 33dB:4433797" | material: materials ("Glass Klart", "Lys grå", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "TV-skjerm" | object type "TV-skjerm" | names: "TV-skjerm:TV-skjerm:4441404" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
          1 x IFCDOOR | type IFCDOORSTYLE "1700 x 2100mm" | object type "1700 x 2100mm" | names: "M_Overhead-Rolling:1700 x 2100mm:4451019" | material: "Metal - Paint Finish - Ivory, Matte" | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          7 x IFCWALL | type IFCWALLTYPE "Basic Wall:IVSP 84mm SPILEVEGG" | object type "Basic Wall:IVSP 84mm SPILEVEGG:4800472" | names: "Basic Wall:IVSP 84mm SPILEVEGG:4451124", "Basic Wall:IVSP 84mm SPILEVEGG:4802079", "Basic Wall:IVSP 84mm SPILEVEGG:4802137" (+4 more) | material: materials ("NO_isolasjon", "Spiler"); layers "Basic Wall:IVSP 84mm SPILEVEGG" ("NO_isolasjon" 48., "<Unnamed>" 16., "Spiler" 34.) | property sets: Constraints, Dimensions, Other, Phasing, Structural, Text
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 6.2 15x21M 38dB" | object type "IDT 6.2 15x21M 38dB" | names: "_Dør Dobbel_Ulike_Dørblader_Glassfelt2:IDT 6.2 15x21M 38dB:4452497" | material: materials ("Glass Klart", "Lys grå", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "GF 2.2 9x21 33dB" | object type "GF 2.2 9x21 33dB" | names: "Vindu-Fast:GF 2.2 9x21 33dB:4452500" | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          7 x IFCSLAB | object type "Floor:Fotskraperist" | FLOOR | names: "Floor:Fotskraperist:4527148", "Floor:Fotskraperist:5309873", "Floor:Fotskraperist:5309873:2" (+4 more) | material: layers "Floor:Fotskraperist" ("Fotskraperist" 25.) | property sets: Pset_SlabCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "YDA 5.1 16x21M" | object type "YDA 5.1 16x21M" | names: "_Dør Dobbel_Ulike_Dørblader_Glassfelt:YDA 5.1 16x21M:4543202" | material: materials ("Glass Klart", "Lys grå", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 2" | object type "Generic Models 2" | names: "Generic Models 2:Generic Models 2:4575946" | material: "Lys grå" | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Other, Phasing
          2 x IFCROOF | type IFCCURTAINWALLTYPE "Sloped Glazing:Tak glass - Baldakintak" | object type "Sloped Glazing:Tak glass - Baldakintak:338" | names: "Sloped Glazing:Tak glass - Baldakintak:4575972", "Sloped Glazing:Tak glass - Baldakintak:4668049" | parts: 160 IFCMEMBER, 53 IFCPLATE | property sets: Pset_RoofCommon, Pset_TFM, Constraints, Construction, Dimensions, Grid 1
          1 x IFCROOF | object type "Basic Roof:Tak tre (stål) 198:4076687" | names: "Basic Roof:Tak tre (stål) 198:4578613" | material: "stender" | property sets: Pset_RoofCommon, Pset_TFM, Constraints, Construction, Dimensions, Identity Data
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 2" | object type "Generic Models 2" | names: "Generic Models 9:Generic Models 2:4605457" | material: "Lys grå" | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Other, Phasing
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 8.1T 125mm sjaktvegg EI60" | object type "Basic Wall:IVA 8.1T 125mm sjaktvegg EI60:6703020" | names: "Basic Wall:IVA 8.1T 125mm sjaktvegg EI60:4798490", "Basic Wall:IVA 8.1T 125mm sjaktvegg EI60:4798840", "Basic Wall:IVA 8.1T 125mm sjaktvegg EI60:4798860" | material: layers "Basic Wall:IVA 8.1T 125mm sjaktvegg EI60" ("Branngips" 15., "Branngips" 15., "stender/isolasjon" 95.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          1 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Curtain Wall:Glassfasade 5e" | object type "Curtain Wall:Glassfasade 5e:5695970" | names: "Curtain Wall:Glassfasade 5e:4856014" | parts: 30 IFCMEMBER, 7 IFCPLATE, 1 IFCDOOR | property sets: Pset_CurtainWallCommon, Pset_TFM, Constraints, Dimensions, Horizontal Grid, Identity Data
          1 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Curtain Wall:Glassfasade 4c" | object type "Curtain Wall:Glassfasade 4c:5696067" | names: "Curtain Wall:Glassfasade 4c:4856394" | parts: 26 IFCMEMBER, 6 IFCPLATE, 1 IFCDOOR | property sets: Pset_CurtainWallCommon, Pset_TFM, Constraints, Dimensions, Horizontal Grid, Identity Data
          1 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Curtain Wall:Glassfasade 3a" | object type "Curtain Wall:Glassfasade 3a:6086005" | names: "Curtain Wall:Glassfasade 3a:4856540" | parts: 32 IFCMEMBER, 9 IFCPLATE | property sets: Pset_CurtainWallCommon, Pset_TFM, Constraints, Dimensions, Horizontal Grid, Identity Data
          1 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Curtain Wall:Glassfasade 2a" | object type "Curtain Wall:Glassfasade 2a:6085896" | names: "Curtain Wall:Glassfasade 2a:4856862" | parts: 40 IFCMEMBER, 9 IFCPLATE, 1 IFCDOOR | property sets: Pset_CurtainWallCommon, Pset_TFM, Constraints, Dimensions, Horizontal Grid, Identity Data
          1 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Curtain Wall:Glassfasade 1c" | object type "Curtain Wall:Glassfasade 1c:1911982" | names: "Curtain Wall:Glassfasade 1c:4857050" | parts: 30 IFCMEMBER, 7 IFCPLATE | property sets: Pset_CurtainWallCommon, Pset_TFM, Constraints, Dimensions, Horizontal Grid, Identity Data
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 6.1 342mm (HN-95-100-95-NH)" | object type "Basic Wall:IVA 6.1 342mm (HN-95-100-95-NH):4857505" | names: "Basic Wall:IVA 6.1 342mm (HN-95-100-95-NH):4857675" | material: layers "Basic Wall:IVA 6.1 342mm (HN-95-100-95-NH)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 95., "Luftsjikt" 100., "stender/isolasjon" 95., "Gips" 13., "Habito" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCSTAIR | object type "Assembled Stair:Gitterrist:306561" | names: "Assembled Stair:Stair:4959975" | parts: 14 IFCMEMBER, 8 IFCRAILING, 2 IFCSLAB, 2 IFCSTAIRFLIGHT | property sets: Pset_StairCommon, Pset_TFM, Constraints, Dimensions, Other, Phasing
          1 x IFCSTAIR | object type "Assembled Stair:Ståltrapp:7605679" | names: "Assembled Stair:Stair:4960365" | parts: 9 IFCMEMBER, 4 IFCRAILING, 2 IFCSLAB, 2 IFCSTAIRFLIGHT | property sets: Pset_StairCommon, Pset_TFM, Constraints, Dimensions, Identity Data, Other
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:YV 14.1 371mm u/kledning" | object type "Basic Wall:YV 14.1 371mm u/kledning:5049812" | names: "Basic Wall:YV 14.1 371mm u/kledning:5027238", "Basic Wall:YV 14.1 371mm u/kledning:6072142" | material: layers "Basic Wall:YV 14.1 371mm u/kledning" ("RAL 9004" 5., "Vindsperre" 9., "Stender isolert vegg" 296., "NO_Utlekting" 48., "Gips" 12.5) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 6.3 252mm EI60 (RN-95-40-95-NR)" | object type "Basic Wall:IVA 6.3 252mm EI60 (RN-95-40-95-NR):5031793" | names: "Basic Wall:IVA 6.3 252mm EI60 (RN-95-40-95-NR):5032480" | material: layers "Basic Wall:IVA 6.3 252mm EI60 (RN-95-40-95-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95., "Luftsjikt" 20., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:YV 14.2 371mm u/kledning EI60" | object type "Basic Wall:YV 14.2 371mm u/kledning EI60:6771107" | names: "Basic Wall:YV 14.2 371mm u/kledning EI60:5055699" | material: layers "Basic Wall:YV 14.2 371mm u/kledning EI60" ("RAL 9004" 5., "Vindsperre" 9., "Stender isolert vegg" 296., "NO_Utlekting" 48., "Branngips" 15.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 3" | object type "Generic Models 3" | names: "Generic Models 7:Generic Models 3:5139434" | material: "Lys grå" | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Other, Phasing
          1 x IFCWINDOW | type IFCWINDOWSTYLE "GF 13.1 36x21 38dB" | object type "GF 13.1 36x21 38dB" | names: "Vindu_3felt:GF 13.1 36x21 38dB:5149291" | material: materials ("Karm Malt", "Glass Klart", "NCS S 3502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "GF 14.1" | object type "GF 14.1" | names: "Vindu_2felt:GF 14.1:5156029" | material: materials ("Karm Malt", "Glass Klart", "NCS S 3502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:YV 6.2 299mm grå platekledning basseng" | object type "Basic Wall:YV 6.2 299mm grå platekledning basseng:5306564" | names: "Basic Wall:YV 6.2 299mm grå platekledning basseng:5306358", "Basic Wall:YV 6.2 299mm grå platekledning basseng:5306701", "Basic Wall:YV 6.2 299mm grå platekledning basseng:5306777" | material: layers "Basic Wall:YV 6.2 299mm grå platekledning basseng" ("Cembrit Metro London" 8., "Luftsjikt" 36., "Vindsperre" 9., "Stender isolert vegg" 246.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          17 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVSP 84mm SPILEVEGG" | object type "Basic Wall:IVSP 84mm SPILEVEGG:4800472" | names: "Basic Wall:IVSP 84mm SPILEVEGG:5412010", "Basic Wall:IVSP 84mm SPILEVEGG:5412555", "Basic Wall:IVSP 84mm SPILEVEGG:5412687" (+14 more) | material: layers "Basic Wall:IVSP 84mm SPILEVEGG" ("NO_isolasjon" 48., "<Unnamed>" 16., "Spiler" 34.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCWINDOW | type IFCWINDOWSTYLE "V16 21x16" | object type "V16 21x16" | names: "Fast vindu+ åpningsvindu:V16 21x16:5422930" | material: materials ("NCS S 0502-Y", "Glass Klart") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          2 x IFCWINDOW | type IFCWINDOWSTYLE "V17 21x16" | object type "V17 21x16" | names: "Fast vindu+ åpningsvindu:V17 21x16:5423978", "Fast vindu+ åpningsvindu:V17 21x16:5425794" | material: materials ("NCS S 0502-Y", "Glass Klart") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          2 x IFCWINDOW | type IFCWINDOWSTYLE "V18 21x16" | object type "V18 21x16" | names: "Fast vindu+ åpningsvindu:V18 21x16:5427464", "Fast vindu+ åpningsvindu:V18 21x16:5427724" | material: materials ("NCS S 0502-Y", "Glass Klart") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "V19 21x16" | object type "V19 21x16" | names: "Fast vindu+ åpningsvindu:V19 21x16:5427952" | material: materials ("NCS S 0502-Y", "Glass Klart") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "V19 21x16" | object type "V19 21x16" | names: "Fast vindu+ åpningsvindu:V19 21x16:5428378" | material: materials ("NCS S 0502-Y", "Glass Klart") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "V20 19x16" | object type "V20 19x16" | names: "Fast vindu+ åpningsvindu:V20 19x16:5428885" | material: materials ("NCS S 0502-Y", "Glass Klart") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "V15 24x16" | object type "V15 24x16" | names: "Fast vindu+ åpningsvindu:V15 24x16:5429707" | material: materials ("NCS S 0502-Y", "Glass Klart") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          2 x IFCWINDOW | type IFCWINDOWSTYLE "V21 35x16" | object type "V21 35x16" | names: "Fast vindu+ åpningsvindu:V21 35x16:5430404", "Fast vindu+ åpningsvindu:V21 35x16:5430662" | material: materials ("NCS S 0502-Y", "Glass Klart") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "115x115mm" | object type "115x115mm" | names: "NO_Rektangulær tre Søyle:115x115mm:5621214" | material: "NO_Tømmer" | property sets: BaseQuantities, Pset_ColumnCommon, Pset_TFM, Constraints, Construction, Dimensions
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "115x115mm" | object type "115x115mm" | names: "NO_Rektangulær tre Søyle:115x115mm:5621422" | material: "NO_Tømmer" | property sets: BaseQuantities, Pset_ColumnCommon, Pset_TFM, Constraints, Dimensions, Other
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "115x115mm" | object type "115x115mm" | names: "NO_Rektangulær tre Søyle:115x115mm:5621531" | material: "NO_Tømmer" | property sets: BaseQuantities, Pset_ColumnCommon, Pset_TFM, Constraints, Construction, Dimensions
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "115x115mm" | object type "115x115mm" | names: "NO_Rektangulær tre Søyle:115x115mm:5621532" | material: "NO_Tømmer" | property sets: BaseQuantities, Pset_ColumnCommon, Pset_TFM, Constraints, Dimensions, Other
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "115x115mm" | object type "115x115mm" | names: "NO_Rektangulær tre Søyle:115x115mm:5621561" | material: "NO_Tømmer" | property sets: BaseQuantities, Pset_ColumnCommon, Pset_TFM, Constraints, Construction, Dimensions
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "115x115mm" | object type "115x115mm" | names: "NO_Rektangulær tre Søyle:115x115mm:5621562" | material: "NO_Tømmer" | property sets: BaseQuantities, Pset_ColumnCommon, Pset_TFM, Constraints, Dimensions, Identity Data
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "115x115mm" | object type "115x115mm" | names: "NO_Rektangulær tre Søyle:115x115mm:5621598" | material: "NO_Tømmer" | property sets: BaseQuantities, Pset_ColumnCommon, Pset_TFM, Constraints, Construction, Dimensions
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "115x115mm" | object type "115x115mm" | names: "NO_Rektangulær tre Søyle:115x115mm:5621599" | material: "NO_Tømmer" | property sets: BaseQuantities, Pset_ColumnCommon, Pset_TFM, Constraints, Dimensions, Identity Data
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "115x115mm" | object type "115x115mm" | names: "NO_Rektangulær tre Søyle:115x115mm:5621624" | material: "NO_Tømmer" | property sets: BaseQuantities, Pset_ColumnCommon, Pset_TFM, Constraints, Construction, Dimensions
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "115x115mm" | object type "115x115mm" | names: "NO_Rektangulær tre Søyle:115x115mm:5621625" | material: "NO_Tømmer" | property sets: BaseQuantities, Pset_ColumnCommon, Pset_TFM, Constraints, Construction, Dimensions
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "115x115mm" | object type "115x115mm" | names: "NO_Rektangulær tre Søyle:115x115mm:5621653" | material: "NO_Tømmer" | property sets: BaseQuantities, Pset_ColumnCommon, Pset_TFM, Constraints, Construction, Dimensions
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "115x115mm" | object type "115x115mm" | names: "NO_Rektangulær tre Søyle:115x115mm:5621654" | material: "NO_Tømmer" | property sets: BaseQuantities, Pset_ColumnCommon, Pset_TFM, Constraints, Dimensions, Identity Data
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "115x115mm" | object type "115x115mm" | names: "NO_Rektangulær tre Søyle:115x115mm:5621698" | material: "NO_Tømmer" | property sets: BaseQuantities, Pset_ColumnCommon, Pset_TFM, Constraints, Construction, Dimensions
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "115x115mm" | object type "115x115mm" | names: "NO_Rektangulær tre Søyle:115x115mm:5621759" | material: "NO_Tømmer" | property sets: BaseQuantities, Pset_ColumnCommon, Pset_TFM, Constraints, Construction, Dimensions
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "115x115mm" | object type "115x115mm" | names: "NO_Rektangulær tre Søyle:115x115mm:5621760" | material: "NO_Tømmer" | property sets: BaseQuantities, Pset_ColumnCommon, Pset_TFM, Constraints, Dimensions, Other
          3 x IFCROOF | object type "Basic Roof:Tak tre 250 uisolert" | names: "Basic Roof:Tak tre 250 uisolert:5622188", "Basic Roof:Tak tre 250 uisolert:5626747", "Basic Roof:Tak tre 250 uisolert:5771871" | parts: 3 IFCSLAB | property sets: Pset_RoofCommon, Pset_TFM, Constraints, Construction, Dimensions, Identity Data
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "96x130mm" | object type "96x130mm" | names: "NO_Rektangulær tre Søyle:96x130mm:5624928" | material: "NO_Tømmer" | property sets: BaseQuantities, Pset_ColumnCommon, Pset_TFM, Constraints, Construction, Dimensions
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "96x130mm" | object type "96x130mm" | names: "NO_Rektangulær tre Søyle:96x130mm:5625169" | material: "NO_Tømmer" | property sets: BaseQuantities, Pset_ColumnCommon, Pset_TFM, Constraints, Construction, Dimensions
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "96x130mm" | object type "96x130mm" | names: "NO_Rektangulær tre Søyle:96x130mm:5625237" | material: "NO_Tømmer" | property sets: BaseQuantities, Pset_ColumnCommon, Pset_TFM, Constraints, Construction, Dimensions
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "96x130mm" | object type "96x130mm" | names: "NO_Rektangulær tre Søyle:96x130mm:5625339" | material: "NO_Tømmer" | property sets: BaseQuantities, Pset_ColumnCommon, Pset_TFM, Constraints, Construction, Dimensions
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "96x130mm" | object type "96x130mm" | names: "NO_Rektangulær tre Søyle:96x130mm:5625453" | material: "NO_Tømmer" | property sets: BaseQuantities, Pset_ColumnCommon, Pset_TFM, Constraints, Construction, Dimensions
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "96x130mm" | object type "96x130mm" | names: "NO_Rektangulær tre Søyle:96x130mm:5625575" | material: "NO_Tømmer" | property sets: BaseQuantities, Pset_ColumnCommon, Pset_TFM, Constraints, Construction, Dimensions
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "96x130mm" | object type "96x130mm" | names: "NO_Rektangulær tre Søyle:96x130mm:5626483" | material: "NO_Tømmer" | property sets: BaseQuantities, Pset_ColumnCommon, Pset_TFM, Constraints, Construction, Dimensions
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "96x130mm" | object type "96x130mm" | names: "NO_Rektangulær tre Søyle:96x130mm:5626484" | material: "NO_Tømmer" | property sets: BaseQuantities, Pset_ColumnCommon, Pset_TFM, Constraints, Construction, Dimensions
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "96x130mm" | object type "96x130mm" | names: "NO_Rektangulær tre Søyle:96x130mm:5626526" | material: "NO_Tømmer" | property sets: BaseQuantities, Pset_ColumnCommon, Pset_TFM, Constraints, Construction, Dimensions
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "96x130mm" | object type "96x130mm" | names: "NO_Rektangulær tre Søyle:96x130mm:5626527" | material: "NO_Tømmer" | property sets: BaseQuantities, Pset_ColumnCommon, Pset_TFM, Constraints, Construction, Dimensions
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "96x130mm" | object type "96x130mm" | names: "NO_Rektangulær tre Søyle:96x130mm:5626616" | material: "NO_Tømmer" | property sets: BaseQuantities, Pset_ColumnCommon, Pset_TFM, Constraints, Construction, Dimensions
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Lysrigg" | object type "Lysrigg" | names: "lysrigg:Lysrigg:5636830", "lysrigg:Lysrigg:5637121" | material: "hvit malt" | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
          1 x IFCBEAM | type IFCBEAMTYPE "NOR-Bjelke-Tre-Stiplet:bjelke bod 2" | object type "NOR-Bjelke-Tre-Stiplet:bjelke bod 2:7419715" | names: "NOR-Bjelke-Tre-Stiplet:bjelke bod 2:5641896" | material: "Wood - Dimensional lumber" | property sets: BaseQuantities, Pset_BeamCommon, Pset_TFM, Constraints, Dimensions, Geometric Position
          1 x IFCROOF | object type "Basic Roof:Tak tre 250" | names: "Basic Roof:Tak tre 250:5644151" | parts: 1 IFCSLAB | property sets: Pset_RoofCommon, Pset_TFM, Constraints, Construction, Dimensions, Identity Data
          31 x IFCBEAM | type IFCBEAMTYPE "NOR-Bjelke-Tre-Stiplet:50x50" | object type "NOR-Bjelke-Tre-Stiplet:50x50:5644645" | names: "NOR-Bjelke-Tre-Stiplet:50x50:5644627", "NOR-Bjelke-Tre-Stiplet:50x50:5644693", "NOR-Bjelke-Tre-Stiplet:50x50:5644900" (+28 more) | material: "Wood - Dimensional lumber" | property sets: BaseQuantities, Pset_BeamCommon, Pset_TFM, Constraints, Dimensions, Geometric Position
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:YV 16.2 437mm grå platekledning" | object type "Basic Wall:YV 16.2 437mm grå platekledning:5693111" | names: "Basic Wall:YV 16.2 437mm grå platekledning:5668964" | material: layers "Basic Wall:YV 16.2 437mm grå platekledning" ("Cembrit Metro London" 8., "Luftsjikt" 36., "Vindsperre" 9., "Stender isolert vegg" 246., "Luftsjikt" 15., "stender/isolasjon" 98., "<Unnamed>" 12.5, "Robustgips" 12.5) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          2 x IFCWINDOW | type IFCWINDOWSTYLE "GF 14.2 12x21 33dB E30" | object type "GF 14.2 12x21 33dB E30" | names: "Vindu-Fast:GF 14.2 12x21 33dB E30:5676778", "Vindu-Fast:GF 14.2 12x21 33dB E30:5676924" | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWALL | type IFCWALLTYPE "Basic Wall:YV 16.1 437mm gul platekledning" | object type "Basic Wall:YV 16.1 437mm gul platekledning:5669055" | names: "Basic Wall:YV 16.1 437mm gul platekledning:5693070" | material: materials ("Cembrit Metro Amsterdam", "Luftsjikt", "Vindsperre", "Stender isolert vegg", "Luftsjikt", "Stender isolert vegg", "Robustgips") | property sets: Constraints, Dimensions, Other, Phasing, Structural, Text
          1 x IFCWALL | type IFCWALLTYPE "Basic Wall:YV 17.1 279 Vegg glassfelt" | object type "Basic Wall:YV 17.1 279 Vegg glassfelt:5715346" | names: "Basic Wall:YV 17.1 279 Vegg glassfelt:5717800" | material: materials ("Vindsperre", "Stender isolert vegg", "Stender isolert vegg", "Robustgips") | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:YV 5.1 233 Gesims Midtbygg" | object type "Basic Wall:YV 5.1 233 Gesims Midtbygg:2484317" | names: "Basic Wall:YV 5.1 233 Gesims Midtbygg:5718433" | material: layers "Basic Wall:YV 5.1 233 Gesims Midtbygg" ("Beslag" 5., "Vindsperre" 15., "<Unnamed>" 36., "<Unnamed>" 15., "Stender isolert vegg" 198., "Kryssfiner" 15.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCDOOR | type IFCDOORSTYLE "YDA 6.1 Skyvedører" | object type "YDA 6.1 Skyvedører" | names: "Doors-Sliding_Manusa_Biparting_sliding_fixed_INT:YDA 6.1 Skyvedører:5720315" | material: materials ("Aluminio Manusa", "Glass") | property sets: Pset_DoorCommon, Pset_ManufacturerTypeInformation, Pset_TFM, BaseQuantities, Constraints, Construction
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:YV 17.1 279 Vegg glassfelt" | object type "Basic Wall:YV 17.1 279 Vegg glassfelt:5715346" | names: "Basic Wall:YV 17.1 279 Vegg glassfelt:5750167" | material: layers "Basic Wall:YV 17.1 279 Vegg glassfelt" ("Vindsperre" 15., "Stender isolert vegg" 198., "Stender isolert vegg" 48., "Robustgips" 12.5) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:YV kle søyle" | object type "Basic Wall:YV kle søyle:5522497" | names: "Basic Wall:YV kle søyle:5750987", "Basic Wall:YV kle søyle:6073921" | material: layers "Basic Wall:YV kle søyle" ("Beslag" 5., "Vindsperre" 9., "Stender isolert vegg" 136.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          1 x IFCROOF | object type "Basic Roof:Tak tre 223 spilehimling" | names: "Basic Roof:Tak tre 223 spilehimling:5818769" | parts: 1 IFCSLAB | property sets: Pset_RoofCommon, Pset_TFM, Constraints, Construction, Dimensions, Identity Data
          1 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "Gutter:Takrenne:5043645" | object type "Gutter:Takrenne:5043645" | names: "Gutter:Takrenne:5818944" | property sets: Pset_DistributionFlowElementCommon, Constraints, Dimensions, Other, Phasing, Profile
          1 x IFCDOOR | type IFCDOORSTYLE "IDA 2.2 15x21M EI60SC" | object type "IDA 2.2 15x21M EI60SC" | names: "Dør Dobbel_Ulike_Dørblader:IDA 2.2 15x21M EI60SC:5866724" | material: materials ("Lys grå", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDA 6.1 12x21M EI60 CS" | object type "IDA 6.1 12x21M EI60 CS" | names: "Dør Enkel_ Glassfelt:IDA 6.1 12x21M EI60 CS:5876404" | material: materials ("Lys grå", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "2680 x 1275mm" | object type "2680 x 1275mm" | names: "M_Overhead-Rolling:2680 x 1275mm:5883834" | material: "Metal - Paint Finish - Ivory, Matte" | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDA 7.1 15x21M EI60CS" | object type "IDA 7.1 15x21M EI60CS" | names: "Enfløyet_aludør:IDA 7.1 15x21M EI60CS:5924061" | material: materials ("Karm Malt", "Lys grå", "Terskel Tre") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "YDA 4.1 14x21M" | object type "YDA 4.1 14x21M" | names: "Dør Enkel_ Glassfelt:YDA 4.1 14x21M:5953506" | material: materials ("Lys grå", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "YDA 4.1 14x21M" | object type "YDA 4.1 14x21M" | names: "Dør Enkel_ Glassfelt:YDA 4.1 14x21M:5953837" | material: materials ("Lys grå", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          12 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:YV 24.1 mellom glassvegger" | object type "Basic Wall:YV 24.1 mellom glassvegger:6034767" | names: "Basic Wall:YV 24.1 mellom glassvegger:6035004", "Basic Wall:YV 24.1 mellom glassvegger:6036173", "Basic Wall:YV 24.1 mellom glassvegger:6036687" (+9 more) | material: layers "Basic Wall:YV 24.1 mellom glassvegger" ("Beslag" 5., "Vindsperre" 9., "Stender isolert vegg" 123., "Stender isolert vegg" 48., "Gips" 12.5, "Robustgips" 12.5) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          1 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Curtain Wall:Glassfasade 3c" | object type "Curtain Wall:Glassfasade 3c:6086115" | names: "Curtain Wall:Glassfasade 3c:6035476" | parts: 7 IFCMEMBER, 2 IFCPLATE | property sets: Pset_CurtainWallCommon, Pset_TFM, Constraints, Dimensions, Horizontal Grid, Identity Data
          1 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Curtain Wall:Glassfasade 3b" | object type "Curtain Wall:Glassfasade 3b:6086064" | names: "Curtain Wall:Glassfasade 3b:6035911" | parts: 25 IFCMEMBER, 6 IFCPLATE | property sets: Pset_CurtainWallCommon, Pset_TFM, Constraints, Dimensions, Horizontal Grid, Identity Data
          1 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Curtain Wall:Glassfasade 4a" | object type "Curtain Wall:Glassfasade 4a:6086229" | names: "Curtain Wall:Glassfasade 4a:6036693" | parts: 10 IFCMEMBER, 2 IFCPLATE, 1 IFCDOOR | property sets: Pset_CurtainWallCommon, Pset_TFM, Constraints, Dimensions, Horizontal Grid, Identity Data
          1 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Curtain Wall:Glassfasade 4b" | object type "Curtain Wall:Glassfasade 4b:6086278" | names: "Curtain Wall:Glassfasade 4b:6037550" | parts: 7 IFCMEMBER, 2 IFCPLATE | property sets: Pset_CurtainWallCommon, Pset_TFM, Constraints, Dimensions, Horizontal Grid, Identity Data
          1 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Curtain Wall:Glassfasade 5a" | object type "Curtain Wall:Glassfasade 5a:6086473" | names: "Curtain Wall:Glassfasade 5a:6037879" | parts: 29 IFCMEMBER, 6 IFCPLATE | property sets: Pset_CurtainWallCommon, Pset_TFM, Constraints, Dimensions, Horizontal Grid, Identity Data
          1 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Curtain Wall:Glassfasade 5b" | object type "Curtain Wall:Glassfasade 5b:6086522" | names: "Curtain Wall:Glassfasade 5b:6038259" | parts: 29 IFCMEMBER, 6 IFCPLATE | property sets: Pset_CurtainWallCommon, Pset_TFM, Constraints, Dimensions, Horizontal Grid, Identity Data
          1 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Curtain Wall:Glassfasade 5c" | object type "Curtain Wall:Glassfasade 5c:6086571" | names: "Curtain Wall:Glassfasade 5c:6038530" | parts: 36 IFCMEMBER, 9 IFCPLATE | property sets: Pset_CurtainWallCommon, Pset_TFM, Constraints, Dimensions, Horizontal Grid, Identity Data
          1 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Curtain Wall:Glassfasade 5d" | object type "Curtain Wall:Glassfasade 5d:6086620" | names: "Curtain Wall:Glassfasade 5d:6038819" | parts: 35 IFCMEMBER, 8 IFCPLATE | property sets: Pset_CurtainWallCommon, Pset_TFM, Constraints, Dimensions, Horizontal Grid, Identity Data
          1 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Curtain Wall:Glassfasade 2b" | object type "Curtain Wall:Glassfasade 2b:5696223" | names: "Curtain Wall:Glassfasade 2b:6039741" | parts: 25 IFCMEMBER, 6 IFCPLATE, 1 IFCDOOR | property sets: Pset_CurtainWallCommon, Pset_TFM, Constraints, Dimensions, Horizontal Grid, Identity Data
          1 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Curtain Wall:Glassfasade 1b" | object type "Curtain Wall:Glassfasade 1b:6085796" | names: "Curtain Wall:Glassfasade 1b:6040561" | parts: 25 IFCMEMBER, 6 IFCPLATE | property sets: Pset_CurtainWallCommon, Pset_TFM, Constraints, Dimensions, Horizontal Grid, Identity Data
          1 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Curtain Wall:Glassfasade 1a" | object type "Curtain Wall:Glassfasade 1a:6085725" | names: "Curtain Wall:Glassfasade 1a:6040943" | parts: 15 IFCMEMBER, 4 IFCPLATE | property sets: Pset_CurtainWallCommon, Pset_TFM, Constraints, Dimensions, Horizontal Grid, Identity Data
        IFCSPACE "14" | long name "Area" | INTERNAL
        IFCSPACE "3" | long name "Area" | INTERNAL
        IFCSPACE "01024" | long name "forkontor" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | object type "Compound Ceiling:Himling System 600x600" | CEILING | names: "Compound Ceiling:Himling System 600x600:3051127" | material: layers "Compound Ceiling:Himling System 600x600" ("Himling Metallprofil" 38., "Himling System 600x600" 12.) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
        IFCSPACE "01035" | long name "avd.led" | INTERNAL
        IFCSPACE "01031" | long name "kontor" | INTERNAL
        IFCSPACE "01048" | long name "musikk" | INTERNAL
          contains 3 elements
            1 x IFCCOVERING | object type "Compound Ceiling:Himling System 600x600 Master Gamma" | CEILING | names: "Compound Ceiling:Himling System 600x600 Master Gamma:3645338" | material: layers "Compound Ceiling:Himling System 600x600 Master Gamma" ("Himling Metallprofil" 38., "Himling System 600x600" 10.) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Tavle 2m" | object type "Tavle 2m" | names: "Tavle:Tavle 2m:5297261" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Smartboard 2m" | object type "Smartboard 2m" | names: "Smartboard:Smartboard 2m:5297262" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
        IFCSPACE "01069" | long name "naturfag-kjemi" | INTERNAL
          contains 21 elements
            3 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Skap, resirkulering 450 x 450 x 692mm" | object type "Skap, resirkulering 450 x 450 x 692mm" | names: "Base Cabinet Single Door horisontalt håndtak:Skap, resirkulering 450 x 450 x 692mm:2450126", "Base Cabinet Single Door horisontalt håndtak:Skap, resirkulering 450 x 450 x 692mm:2450128", "Base Cabinet Single Door horisontalt håndtak:Skap, resirkulering 450 x 450 x 692mm:2450130" | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Other, Phasing
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Skap, resirkulering 450 x 450 x 692mm" | object type "Skap, resirkulering 450 x 450 x 692mm" | names: "Base Cabinet Single Door horisontalt håndtak:Skap, resirkulering 450 x 450 x 692mm:2450129" | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Other, Phasing
            1 x IFCFLOWTERMINAL | object type "Vaskerenne 1800mm, Krogsæter" | names: "intra_wash_throuh_wall_mounted_1800_mm:Vaskerenne 1800mm, Krogsæter:3641666" | material: materials ("f26d4e4b_a025_4dbf_b085_30ed485788cf", "4b4a701a_e8ab_4354_ac15_234043769b9c") | property sets: Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data, Mechanical
            1 x IFCFLOWTERMINAL | object type "Lab kum" | names: "N_Sink Kitchen-lab kum:Lab kum:4136389" | material: "Metal - Steel, Polished" | property sets: Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data, Other
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Demobenk, naturfag" | object type "Demobenk, naturfag" | names: "Benk_Naturfag:Demobenk, naturfag:4151897" | material: "hvit malt" | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Skap, demobenk naturfag 1200 x 600 x 860mm" | object type "Skap, demobenk naturfag 1200 x 600 x 860mm" | names: "N_Base Cabinet-Double Door-for sink:Skap, demobenk naturfag 1200 x 600 x 860mm:4151898" | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Other, Phasing
            4 x IFCFLOWTERMINAL | object type "Blandebatteri - Oras Saphira 1038F" | names: "Oras Saphira:Blandebatteri - Oras Saphira 1038F:4371435", "Oras Saphira:Blandebatteri - Oras Saphira 1038F:4371554", "Oras Saphira:Blandebatteri - Oras Saphira 1038F:4371795" (+1 more) | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Naturfagsbord" | object type "Naturfagsbord" | names: "M_Table spes equipment:Naturfagsbord:4404814", "M_Table spes equipment:Naturfagsbord:4405316" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_TFM, Constraints, Dimensions, Electrical - Loads
            2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Naturfagsbord" | object type "Naturfagsbord" | names: "M_Table spes equipment:Naturfagsbord:4405218", "M_Table spes equipment:Naturfagsbord:4405317" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_TFM, Constraints, Dimensions, Electrical - Loads
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Gasskap" | object type "Gasskap" | names: "Spesialutstyr spes equip:Gasskap:4406189" | material: "hvit malt" | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
            1 x IFCFLOWTERMINAL | object type "Haws nøddusjsøyle 8320 Axion ECO" | names: "Dusj:Haws nøddusjsøyle 8320 Axion ECO:5272756" | material: "Aluminum" | property sets: Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data, Other
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Tavle 2m" | object type "Tavle 2m" | names: "Tavle:Tavle 2m:5296800" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Smartboard 2m" | object type "Smartboard 2m" | names: "Smartboard:Smartboard 2m:5296801" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Underskap gasskap" | object type "Underskap gasskap" | names: "N_Base Cabinet-Double Door-for sink:Underskap gasskap:6533927" | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
        IFCSPACE "01050" | long name "øve" | INTERNAL
        IFCSPACE "01051" | long name "lager" | INTERNAL
        IFCSPACE "01058" | long name "M&H" | INTERNAL
          contains 68 elements
            2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Siemens induksjon" | object type "Siemens induksjon" | names: "N_Cook Top:Siemens induksjon:2013425", "N_Cook Top:Siemens induksjon:4126039" | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Benkeplate 625mm, Sigdal" | object type "Benkeplate 625mm, Sigdal" | names: "N_CounterTop:Benkeplate 625mm, Sigdal:2139256" | material: "hvit malt" | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Other, Phasing
            1 x IFCFLOWTERMINAL | object type "Kum kjøkken HC" | names: "M_Sink Kitchen-Double:Kum kjøkken HC:2139327" | material: "Metal - Steel, Polished" | property sets: Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data, Other
            1 x IFCFLOWTERMINAL | object type "Servant - Nautic 5556" | names: "Washbasin-GBG-Nautic_5556_Bolt_Bracket_Mounting:Servant - Nautic 5556:3653700" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            2 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Benkeplate 625mm" | object type "Benkeplate 625mm" | names: "N_CounterTop-L-w sink hole:Benkeplate 625mm:4126005", "N_CounterTop-L-w sink hole:Benkeplate 625mm:4126056" | material: "hvit malt" | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Other, Phasing
            2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Siemens induksjon" | object type "Siemens induksjon" | names: "N_Cook Top:Siemens induksjon:4126006", "N_Cook Top:Siemens induksjon:4126057" | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
            4 x IFCFLOWTERMINAL | object type "Kum kjøkken" | names: "M_Sink Kitchen-Double:Kum kjøkken:4126007", "M_Sink Kitchen-Double:Kum kjøkken:4126040", "M_Sink Kitchen-Double:Kum kjøkken:4126058" (+1 more) | material: "Metal - Steel, Polished" | property sets: Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data, Other
            3 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Skap, kjøkken 800 x 600 x 860mm" | object type "Skap, kjøkken 800 x 600 x 860mm" | names: "N_Base Cabinet-Double Door-for sink:Skap, kjøkken 800 x 600 x 860mm:4126008", "N_Base Cabinet-Double Door-for sink:Skap, kjøkken 800 x 600 x 860mm:4126059", "N_Base Cabinet-Double Door-for sink:Skap, kjøkken 800 x 600 x 860mm:4127233" | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Other, Phasing
            2 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Skap, kjøkken 600 x 600 x 860mm" | object type "Skap, kjøkken 600 x 600 x 860mm" | names: "N_Base Cabinet-3 drawers:Skap, kjøkken 600 x 600 x 860mm:4126009", "N_Base Cabinet-3 drawers:Skap, kjøkken 600 x 600 x 860mm:4126060" | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Other, Phasing
            5 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Skap, kjøkken 600 x 600 x 860mm" | object type "Skap, kjøkken 600 x 600 x 860mm" | names: "Base Cabinet Single Door:Skap, kjøkken 600 x 600 x 860mm:4126010", "Base Cabinet Single Door:Skap, kjøkken 600 x 600 x 860mm:4126061", "Base Cabinet Single Door:Skap, kjøkken 600 x 600 x 860mm:6137442" (+2 more) | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
            2 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Skap, kjøkken 400 x 600 x 860mm" | object type "Skap, kjøkken 400 x 600 x 860mm" | names: "Base Cabinet Single Door:Skap, kjøkken 400 x 600 x 860mm:4126011", "Base Cabinet Single Door:Skap, kjøkken 400 x 600 x 860mm:4126062" | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
            2 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Skap, kjøkken, hjørne 900 x 600 x 860mm" | object type "Skap, kjøkken, hjørne 900 x 600 x 860mm" | names: "N_Base Cabinet-Corner-Single Door:Skap, kjøkken, hjørne 900 x 600 x 860mm:4126013", "N_Base Cabinet-Corner-Single Door:Skap, kjøkken, hjørne 900 x 600 x 860mm:4126064" | material: "N_Cabinets" | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
            2 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Overskap 800 x 300 x 720mm" | object type "Overskap 800 x 300 x 720mm" | names: "N_Upper Cabinet-Double Door:Overskap 800 x 300 x 720mm:4126014", "N_Upper Cabinet-Double Door:Overskap 800 x 300 x 720mm:4126065" | material: "N_Cabinets" | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Other, Phasing
            2 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Overskap 300 x 300 x 700mm" | object type "Overskap 300 x 300 x 700mm" | names: "N_Upper Cabinet-Single Door:Overskap 300 x 300 x 700mm:4126015", "N_Upper Cabinet-Single Door:Overskap 300 x 300 x 700mm:4126066" | material: "N_Cabinets" | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
            3 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Overskap 600 x 300 x 700mm" | object type "Overskap 600 x 300 x 700mm" | names: "N_Upper Cabinet-Single Door:Overskap 600 x 300 x 700mm:4126017", "N_Upper Cabinet-Single Door:Overskap 600 x 300 x 700mm:4126068", "N_Upper Cabinet-Single Door:Overskap 600 x 300 x 700mm:6970876" | material: "N_Cabinets" | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Benkeplate 625mm" | object type "Benkeplate 625mm" | names: "N_CounterTop-L-w sink hole:Benkeplate 625mm:4126038" | material: "hvit malt" | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Skap, kjøkken 800 x 600 x 860mm" | object type "Skap, kjøkken 800 x 600 x 860mm" | names: "N_Base Cabinet-Double Door-for sink:Skap, kjøkken 800 x 600 x 860mm:4126041" | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
            2 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Skap, kjøkken 600 x 600 x 860mm" | object type "Skap, kjøkken 600 x 600 x 860mm" | names: "N_Base Cabinet-3 drawers:Skap, kjøkken 600 x 600 x 860mm:4126042", "N_Base Cabinet-3 drawers:Skap, kjøkken 600 x 600 x 860mm:6143047" | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Other, Phasing
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Skap, kjøkken 600 x 600 x 860mm" | object type "Skap, kjøkken 600 x 600 x 860mm" | names: "Base Cabinet Single Door:Skap, kjøkken 600 x 600 x 860mm:4126043" | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Other, Phasing
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Skap, kjøkken 400 x 600 x 860mm" | object type "Skap, kjøkken 400 x 600 x 860mm" | names: "Base Cabinet Single Door:Skap, kjøkken 400 x 600 x 860mm:4126044" | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Other, Phasing
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Skap, kjøkken, hjørne 900 x 600 x 860mm" | object type "Skap, kjøkken, hjørne 900 x 600 x 860mm" | names: "N_Base Cabinet-Corner-Single Door:Skap, kjøkken, hjørne 900 x 600 x 860mm:4126046" | material: "N_Cabinets" | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Other, Phasing
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Overskap 800 x 300 x 720mm" | object type "Overskap 800 x 300 x 720mm" | names: "N_Upper Cabinet-Double Door:Overskap 800 x 300 x 720mm:4126047" | material: "N_Cabinets" | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Other, Phasing
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Overskap 300 x 300 x 700mm" | object type "Overskap 300 x 300 x 700mm" | names: "N_Upper Cabinet-Single Door:Overskap 300 x 300 x 700mm:4126048" | material: "N_Cabinets" | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Other, Phasing
            2 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Overskap 600 x 300 x 700mm" | object type "Overskap 600 x 300 x 700mm" | names: "N_Upper Cabinet-Single Door:Overskap 600 x 300 x 700mm:4126050", "N_Upper Cabinet-Single Door:Overskap 600 x 300 x 700mm:6970807" | material: "N_Cabinets" | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Other, Phasing
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Asko oppvaskmaskin" | object type "Asko oppvaskmaskin" | names: "Dishwasher:Asko oppvaskmaskin:4127228" | material: materials ("N_Cabinets", "EQ-Cozinha-Maquinas", "EQ-Cozinha-Maquinas-Porta", "Default Light Source", "N_Cabinets - Handles") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Skap, resirkulering, sigdal" | object type "Skap, resirkulering, sigdal" | names: "Base Cabinet Single Door:Skap, resirkulering, sigdal:4127230" | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Other, Phasing
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Skap, resirkulering, sigdal" | object type "Skap, resirkulering, sigdal" | names: "Base Cabinet Single Door:Skap, resirkulering, sigdal:4127231" | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Other, Phasing
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Skap, kjøkken 600 x 500 x 860mm" | object type "Skap, kjøkken 600 x 500 x 860mm" | names: "N_Base Cabinet-3 drawers:Skap, kjøkken 600 x 500 x 860mm:4127234" | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Høyskap med ovn 600 x 600 x 2105mm" | object type "Høyskap med ovn 600 x 600 x 2105mm" | names: "M_Oven Tower Unit:Høyskap med ovn 600 x 600 x 2105mm:4138016" | material: "Glass" | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Siemens frittstående kjøleskap" | object type "Siemens frittstående kjøleskap" | names: "NO_Kjøleskap:Siemens frittstående kjøleskap:4145998" | material: materials ("Metal - Chrome", "Metal - Paint Finish - Ivory,Matte") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Siemens Frittstående fryseskap" | object type "Siemens Frittstående fryseskap" | names: "NO_Kjøleskap:Siemens Frittstående fryseskap:4146120" | material: materials ("Metal - Chrome", "Metal - Paint Finish - Ivory,Matte") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
            2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Siemens innebygget ovn" | object type "Siemens innebygget ovn" | names: "N_Oven-Built-in:Siemens innebygget ovn:4148959", "N_Oven-Built-in:Siemens innebygget ovn:4149071" | material: materials ("Glass", "EQ-Cozinha-Maquinas", "EQ-Cozinha-Maquinas-Porta") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Siemens innebygget ovn" | object type "Siemens innebygget ovn" | names: "N_Oven-Built-in:Siemens innebygget ovn:4149073" | material: materials ("Glass", "EQ-Cozinha-Maquinas", "EQ-Cozinha-Maquinas-Porta") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Benkeplate 625mm, Sigdal" | object type "Benkeplate 625mm, Sigdal" | names: "N_CounterTop:Benkeplate 625mm, Sigdal:4149343" | material: "hvit malt" | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Other, Phasing
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Høyskap, kjøkken 600 x 600 x 2100mm" | object type "Høyskap, kjøkken 600 x 600 x 2100mm" | names: "N_Tall Cabinet-Single Door:Høyskap, kjøkken 600 x 600 x 2100mm:4322013" | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Other, Phasing
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Tavle 2m" | object type "Tavle 2m" | names: "Tavle:Tavle 2m:5296695" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Smartboard 2m" | object type "Smartboard 2m" | names: "Smartboard:Smartboard 2m:5296696" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Skap, kjøkken 300 x 600 x 860mm" | object type "Skap, kjøkken 300 x 600 x 860mm" | names: "Base Cabinet Single Door:Skap, kjøkken 300 x 600 x 860mm:6729533" | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Other, Phasing
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Benkeplate 625mm, Sigdal" | object type "Benkeplate 625mm, Sigdal" | names: "N_CounterTop:Benkeplate 625mm, Sigdal:6970128" | material: "hvit malt" | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
            1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "Blandebatteri berøringsfri 1724FT" | object type "Blandebatteri berøringsfri 1724FT" | names: "1724FT(2013):Blandebatteri berøringsfri 1724FT:7586331" | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "Blandebatteri - Oras Saphira 1039F" | object type "Blandebatteri - Oras Saphira 1039F" | names: "Oras Saphira:Blandebatteri - Oras Saphira 1039F:7587928" | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            4 x IFCFLOWTERMINAL | object type "Blandebatteri - Oras Saphira 1038F" | names: "Oras Saphira:Blandebatteri - Oras Saphira 1038F:7588309", "Oras Saphira:Blandebatteri - Oras Saphira 1038F:7588378", "Oras Saphira:Blandebatteri - Oras Saphira 1038F:7588415" (+1 more) | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Benkeplate" | object type "Benkeplate" | names: "N_CounterTop:Benkeplate:7814541" | material: "hvit malt" | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Other, Phasing
        IFCSPACE "01028" | long name "kopi" | INTERNAL
          contains 18 elements
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Benkeplate 625mm, krogsæter" | object type "Benkeplate 625mm, krogsæter" | names: "N_CounterTop:Benkeplate 625mm, krogsæter:2434743" | material: "hvit malt" | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Other, Phasing
            6 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Hylle 300mm" | object type "Hylle 300mm" | names: "N_CounterTop:Hylle 300mm:2435002", "N_CounterTop:Hylle 300mm:5381480", "N_CounterTop:Hylle 300mm:6923492" (+3 more) | material: "hvit malt" | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Skap, krogsæter 600 x 600 x 860mm" | object type "Skap, krogsæter 600 x 600 x 860mm" | names: "Base Cabinet Single Door:Skap, krogsæter 600 x 600 x 860mm:2435450" | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
            1 x IFCCOVERING | object type "Compound Ceiling:Himling System 600x600" | CEILING | names: "Compound Ceiling:Himling System 600x600:3051233" | material: layers "Compound Ceiling:Himling System 600x600" ("Himling Metallprofil" 38., "Himling System 600x600" 12.) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Other
            6 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Hylle 300mm" | object type "Hylle 300mm" | names: "N_CounterTop:Hylle 300mm:6923488", "N_CounterTop:Hylle 300mm:6923489", "N_CounterTop:Hylle 300mm:6923495" (+3 more) | material: "hvit malt" | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Other, Phasing
            2 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Skap, krogsæter 1000 x 600 x 860mm" | object type "Skap, krogsæter 1000 x 600 x 860mm" | names: "N_Base Cabinet-Double Door-for sink:Skap, krogsæter 1000 x 600 x 860mm:6956807", "N_Base Cabinet-Double Door-for sink:Skap, krogsæter 1000 x 600 x 860mm:7234085" | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Other, Phasing
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Skap, krogsæter 1000 x 600 x 860mm" | object type "Skap, krogsæter 1000 x 600 x 860mm" | names: "N_Base Cabinet-Double Door-for sink:Skap, krogsæter 1000 x 600 x 860mm:6956810" | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Other, Phasing
        IFCSPACE "01045" | long name "møte" | INTERNAL
          contains 1 element
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "TV-skjerm" | object type "TV-skjerm" | names: "TV-skjerm:TV-skjerm:4452765" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
        IFCSPACE "01040" | long name "møte" | INTERNAL
          contains 2 elements
            1 x IFCCOVERING | object type "Compound Ceiling:Himling System 600x1200" | CEILING | names: "Compound Ceiling:Himling System 600x1200:3051373" | material: layers "Compound Ceiling:Himling System 600x1200" ("Himling Metallprofil" 38., "Himling System 600x1200" 12.) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "TV-skjerm" | object type "TV-skjerm" | names: "TV-skjerm:TV-skjerm:4452605" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
        IFCSPACE "01029" | long name "rektor" | INTERNAL
          contains 1 element
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "TV-skjerm" | object type "TV-skjerm" | names: "TV-skjerm:TV-skjerm:6714738" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
        IFCSPACE "01049" | long name "øve" | INTERNAL
        IFCSPACE "01006" | long name "lager" | INTERNAL
        IFCSPACE "01025" | long name "møte" | INTERNAL
          contains 1 element
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "TV-skjerm" | object type "TV-skjerm" | names: "TV-skjerm:TV-skjerm:4452822" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
        IFCSPACE "01068" | long name "forb" | INTERNAL
          contains 12 elements
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Benkeplate 625mm, krogsæter" | object type "Benkeplate 625mm, krogsæter" | names: "N_CounterTop:Benkeplate 625mm, krogsæter:2015854" | material: "hvit malt" | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Other, Phasing
            1 x IFCFLOWTERMINAL | object type "Lab kum" | names: "N_Sink Kitchen-lab kum:Lab kum:2142495" | material: "Metal - Steel, Polished" | property sets: Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data, Other
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Miele oppvaskmaskin" | object type "Miele oppvaskmaskin" | names: "Dishwasher:Miele oppvaskmaskin:2366691" | material: materials ("N_Cabinets", "EQ-Cozinha-Maquinas", "EQ-Cozinha-Maquinas-Porta", "Default Light Source", "N_Cabinets - Handles") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Overskap, krogsæter 600 x 300 x 720mm" | object type "Overskap, krogsæter 600 x 300 x 720mm" | names: "N_Upper Cabinet-Single Door:Overskap, krogsæter 600 x 300 x 720mm:2371659" | material: "N_Cabinets" | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Kjemikalieskap" | object type "Kjemikalieskap" | names: "Spesialutstyr spes equip:Kjemikalieskap:4408283" | material: "hvit malt" | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Overskap, krogsæter 600 x 300 x 720mm" | object type "Overskap, krogsæter 600 x 300 x 720mm" | names: "N_Upper Cabinet-Single Door:Overskap, krogsæter 600 x 300 x 720mm:6303536" | material: "N_Cabinets" | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Skuff, krogsæter 600 x 600 x 860mm" | object type "Skuff, krogsæter 600 x 600 x 860mm" | names: "N_Base Cabinet-3 drawers:Skuff, krogsæter 600 x 600 x 860mm:6318286" | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Skap, krogsæter 600 x 600 x 860mm" | object type "Skap, krogsæter 600 x 600 x 860mm" | names: "Base Cabinet Single Door:Skap, krogsæter 600 x 600 x 860mm:6318299" | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Other, Phasing
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Høyskap 500 x 600 x 2100mm" | object type "Høyskap 500 x 600 x 2100mm" | names: "N_Tall Cabinet-Single Door:Høyskap 500 x 600 x 2100mm:6596197" | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Skap, krogsæter 600 x 600 x 860mm" | object type "Skap, krogsæter 600 x 600 x 860mm" | names: "Base Cabinet Single Door:Skap, krogsæter 600 x 600 x 860mm:6884678" | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Høyskap 500 x 600 x 2100mm" | object type "Høyskap 500 x 600 x 2100mm" | names: "N_Tall Cabinet-Single Door:Høyskap 500 x 600 x 2100mm:6910774" | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Other, Phasing
            1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "Blandebatteri - Oras Saphira 1039F" | object type "Blandebatteri - Oras Saphira 1039F" | names: "Oras Saphira:Blandebatteri - Oras Saphira 1039F:7585144" | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
        IFCSPACE "01056" | long name "M&H" | INTERNAL
          contains 74 elements
            2 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Benkeplate 625mm" | object type "Benkeplate 625mm" | names: "N_CounterTop-L-w sink hole:Benkeplate 625mm:2013440", "N_CounterTop-L-w sink hole:Benkeplate 625mm:4125692" | material: "hvit malt" | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
            5 x IFCFLOWTERMINAL | object type "Kum kjøkken" | names: "M_Sink Kitchen-Double:Kum kjøkken:2013446", "M_Sink Kitchen-Double:Kum kjøkken:2450145", "M_Sink Kitchen-Double:Kum kjøkken:4125671" (+2 more) | material: "Metal - Steel, Polished" | property sets: Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data, Other
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Benkeplate 625mm, Sigdal" | object type "Benkeplate 625mm, Sigdal" | names: "N_CounterTop:Benkeplate 625mm, Sigdal:2142728" | material: "hvit malt" | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Other, Phasing
            3 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Skap, kjøkken 800 x 600 x 860mm" | object type "Skap, kjøkken 800 x 600 x 860mm" | names: "N_Base Cabinet-Double Door-for sink:Skap, kjøkken 800 x 600 x 860mm:2345407", "N_Base Cabinet-Double Door-for sink:Skap, kjøkken 800 x 600 x 860mm:2450152", "N_Base Cabinet-Double Door-for sink:Skap, kjøkken 800 x 600 x 860mm:4125695" | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
            2 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Skap, kjøkken 600 x 600 x 860mm" | object type "Skap, kjøkken 600 x 600 x 860mm" | names: "N_Base Cabinet-3 drawers:Skap, kjøkken 600 x 600 x 860mm:2345408", "N_Base Cabinet-3 drawers:Skap, kjøkken 600 x 600 x 860mm:4125696" | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Other, Phasing
            3 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Skap, kjøkken 600 x 600 x 860mm" | object type "Skap, kjøkken 600 x 600 x 860mm" | names: "Base Cabinet Single Door:Skap, kjøkken 600 x 600 x 860mm:2346384", "Base Cabinet Single Door:Skap, kjøkken 600 x 600 x 860mm:4125697", "Base Cabinet Single Door:Skap, kjøkken 600 x 600 x 860mm:6137347" | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Other, Phasing
            2 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Skap, kjøkken 400 x 600 x 860mm" | object type "Skap, kjøkken 400 x 600 x 860mm" | names: "Base Cabinet Single Door:Skap, kjøkken 400 x 600 x 860mm:2346385", "Base Cabinet Single Door:Skap, kjøkken 400 x 600 x 860mm:4125698" | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
            2 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Skap, kjøkken, hjørne 900 x 600 x 860mm" | object type "Skap, kjøkken, hjørne 900 x 600 x 860mm" | names: "N_Base Cabinet-Corner-Single Door:Skap, kjøkken, hjørne 900 x 600 x 860mm:2362298", "N_Base Cabinet-Corner-Single Door:Skap, kjøkken, hjørne 900 x 600 x 860mm:4125700" | material: "N_Cabinets" | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
            2 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Overskap 800 x 300 x 720mm" | object type "Overskap 800 x 300 x 720mm" | names: "N_Upper Cabinet-Double Door:Overskap 800 x 300 x 720mm:2363132", "N_Upper Cabinet-Double Door:Overskap 800 x 300 x 720mm:4125701" | material: "N_Cabinets" | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
            2 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Overskap 300 x 300 x 700mm" | object type "Overskap 300 x 300 x 700mm" | names: "N_Upper Cabinet-Single Door:Overskap 300 x 300 x 700mm:2363588", "N_Upper Cabinet-Single Door:Overskap 300 x 300 x 700mm:4125702" | material: "N_Cabinets" | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
            2 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Overskap 600 x 300 x 700mm" | object type "Overskap 600 x 300 x 700mm" | names: "N_Upper Cabinet-Single Door:Overskap 600 x 300 x 700mm:2364905", "N_Upper Cabinet-Single Door:Overskap 600 x 300 x 700mm:4125704" | material: "N_Cabinets" | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Other, Phasing
            2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Siemens induksjon" | object type "Siemens induksjon" | names: "N_Cook Top:Siemens induksjon:2450144", "N_Cook Top:Siemens induksjon:4125711" | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Benkeplate" | object type "Benkeplate" | names: "N_CounterTop:Benkeplate:2450146" | material: "hvit malt" | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Asko oppvaskmaskin" | object type "Asko oppvaskmaskin" | names: "Dishwasher:Asko oppvaskmaskin:2450147" | material: materials ("N_Cabinets", "EQ-Cozinha-Maquinas", "EQ-Cozinha-Maquinas-Porta", "Default Light Source", "N_Cabinets - Handles") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Skap, resirkulering, sigdal" | object type "Skap, resirkulering, sigdal" | names: "Base Cabinet Single Door:Skap, resirkulering, sigdal:2450149" | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Skap, resirkulering, sigdal" | object type "Skap, resirkulering, sigdal" | names: "Base Cabinet Single Door:Skap, resirkulering, sigdal:2450150" | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Skap, kjøkken 600 x 500 x 860mm" | object type "Skap, kjøkken 600 x 500 x 860mm" | names: "N_Base Cabinet-3 drawers:Skap, kjøkken 600 x 500 x 860mm:2450153" | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Other, Phasing
            1 x IFCFLOWTERMINAL | object type "Servant - Nautic 5556" | names: "Washbasin-GBG-Nautic_5556_Bolt_Bracket_Mounting:Servant - Nautic 5556:3653702" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            2 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Benkeplate 625mm" | object type "Benkeplate 625mm" | names: "N_CounterTop-L-w sink hole:Benkeplate 625mm:4125669", "N_CounterTop-L-w sink hole:Benkeplate 625mm:4125710" | material: "hvit malt" | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
            2 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Skap, kjøkken 800 x 600 x 860mm" | object type "Skap, kjøkken 800 x 600 x 860mm" | names: "N_Base Cabinet-Double Door-for sink:Skap, kjøkken 800 x 600 x 860mm:4125672", "N_Base Cabinet-Double Door-for sink:Skap, kjøkken 800 x 600 x 860mm:4125713" | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
            2 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Skap, kjøkken 600 x 600 x 860mm" | object type "Skap, kjøkken 600 x 600 x 860mm" | names: "N_Base Cabinet-3 drawers:Skap, kjøkken 600 x 600 x 860mm:4125673", "N_Base Cabinet-3 drawers:Skap, kjøkken 600 x 600 x 860mm:4125714" | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Other, Phasing
            2 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Skap, kjøkken 600 x 600 x 860mm" | object type "Skap, kjøkken 600 x 600 x 860mm" | names: "Base Cabinet Single Door:Skap, kjøkken 600 x 600 x 860mm:4125674", "Base Cabinet Single Door:Skap, kjøkken 600 x 600 x 860mm:4125715" | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
            2 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Skap, kjøkken 400 x 600 x 860mm" | object type "Skap, kjøkken 400 x 600 x 860mm" | names: "Base Cabinet Single Door:Skap, kjøkken 400 x 600 x 860mm:4125675", "Base Cabinet Single Door:Skap, kjøkken 400 x 600 x 860mm:4125716" | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
            2 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Skap, kjøkken, hjørne 900 x 600 x 860mm" | object type "Skap, kjøkken, hjørne 900 x 600 x 860mm" | names: "N_Base Cabinet-Corner-Single Door:Skap, kjøkken, hjørne 900 x 600 x 860mm:4125677", "N_Base Cabinet-Corner-Single Door:Skap, kjøkken, hjørne 900 x 600 x 860mm:4125718" | material: "N_Cabinets" | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Other, Phasing
            2 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Overskap 800 x 300 x 720mm" | object type "Overskap 800 x 300 x 720mm" | names: "N_Upper Cabinet-Double Door:Overskap 800 x 300 x 720mm:4125678", "N_Upper Cabinet-Double Door:Overskap 800 x 300 x 720mm:4125719" | material: "N_Cabinets" | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
            2 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Overskap 300 x 300 x 700mm" | object type "Overskap 300 x 300 x 700mm" | names: "N_Upper Cabinet-Single Door:Overskap 300 x 300 x 700mm:4125679", "N_Upper Cabinet-Single Door:Overskap 300 x 300 x 700mm:4125720" | material: "N_Cabinets" | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
            2 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Overskap 600 x 300 x 700mm" | object type "Overskap 600 x 300 x 700mm" | names: "N_Upper Cabinet-Single Door:Overskap 600 x 300 x 700mm:4125681", "N_Upper Cabinet-Single Door:Overskap 600 x 300 x 700mm:4125722" | material: "N_Cabinets" | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Siemens induksjon" | object type "Siemens induksjon" | names: "N_Cook Top:Siemens induksjon:4125693" | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Høyskap med ovn 600 x 600 x 2105mm" | object type "Høyskap med ovn 600 x 600 x 2105mm" | names: "M_Oven Tower Unit:Høyskap med ovn 600 x 600 x 2105mm:4138254" | material: "Glass" | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
            1 x IFCFLOWTERMINAL | object type "Kum mat og helse, vaskeri" | names: "N_Sink Kitchen-Single:Kum mat og helse, vaskeri:4139670" | material: "Metal - Steel, Polished" | property sets: Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data, Other
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Siemens Vaskemaskin, Sigdal" | object type "Siemens Vaskemaskin, Sigdal" | names: "N_Washing Machine:Siemens Vaskemaskin, Sigdal:4145620" | material: materials ("Glass", "EQ-Cozinha-Maquinas-Porta", "N_Cabinets", "EQ-Cozinha-Maquinas", "Default Light Source", "N_Cabinets - Handles") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Siemens Varmep.trommel Sigdal" | object type "Siemens Varmep.trommel Sigdal" | names: "N_Washing Machine:Siemens Varmep.trommel Sigdal:4145811" | material: materials ("Glass", "EQ-Cozinha-Maquinas-Porta", "N_Cabinets", "EQ-Cozinha-Maquinas", "Default Light Source", "N_Cabinets - Handles") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Siemens frittstående kjøleskap" | object type "Siemens frittstående kjøleskap" | names: "NO_Kjøleskap:Siemens frittstående kjøleskap:4146192" | material: materials ("Metal - Chrome", "Metal - Paint Finish - Ivory,Matte") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Siemens Frittstående fryseskap" | object type "Siemens Frittstående fryseskap" | names: "NO_Kjøleskap:Siemens Frittstående fryseskap:4146193" | material: materials ("Metal - Chrome", "Metal - Paint Finish - Ivory,Matte") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
            2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Siemens innebygget ovn" | object type "Siemens innebygget ovn" | names: "N_Oven-Built-in:Siemens innebygget ovn:4149061", "N_Oven-Built-in:Siemens innebygget ovn:4149067" | material: materials ("Glass", "EQ-Cozinha-Maquinas", "EQ-Cozinha-Maquinas-Porta") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
            2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Siemens innebygget ovn" | object type "Siemens innebygget ovn" | names: "N_Oven-Built-in:Siemens innebygget ovn:4149065", "N_Oven-Built-in:Siemens innebygget ovn:4149069" | material: materials ("Glass", "EQ-Cozinha-Maquinas", "EQ-Cozinha-Maquinas-Porta") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Høyskap, kjøkken 600 x 600 x 2100mm" | object type "Høyskap, kjøkken 600 x 600 x 2100mm" | names: "N_Tall Cabinet-Single Door:Høyskap, kjøkken 600 x 600 x 2100mm:4322010" | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Tavle 2m" | object type "Tavle 2m" | names: "Tavle:Tavle 2m:5296786" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Smartboard 2m" | object type "Smartboard 2m" | names: "Smartboard:Smartboard 2m:5296787" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Skap, kjøkken 900 x 600 x 860mm" | object type "Skap, kjøkken 900 x 600 x 860mm" | names: "N_Base Cabinet-Double Door-for sink:Skap, kjøkken 900 x 600 x 860mm:6971468" | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Other, Phasing
            1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "Blandebatteri berøringsfri 1724FT" | object type "Blandebatteri berøringsfri 1724FT" | names: "1724FT(2013):Blandebatteri berøringsfri 1724FT:7586246" | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            2 x IFCFLOWCONTROLLER | type IFCVALVETYPE "Blandebatteri - Oras Saphira 1039F" | object type "Blandebatteri - Oras Saphira 1039F" | names: "Oras Saphira:Blandebatteri - Oras Saphira 1039F:7587860", "Oras Saphira:Blandebatteri - Oras Saphira 1039F:7588232" | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            4 x IFCFLOWTERMINAL | object type "Blandebatteri - Oras Saphira 1038F" | names: "Oras Saphira:Blandebatteri - Oras Saphira 1038F:7587950", "Oras Saphira:Blandebatteri - Oras Saphira 1038F:7587981", "Oras Saphira:Blandebatteri - Oras Saphira 1038F:7588014" (+1 more) | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
        IFCSPACE "01064" | long name "Tre og metall" | INTERNAL | description "fast inventar?"
          contains 9 elements
            4 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Skap, resirkulering 300 x 450 x 690mm" | object type "Skap, resirkulering 300 x 450 x 690mm" | names: "Base Cabinet Single Door horisontalt håndtak:Skap, resirkulering 300 x 450 x 690mm:2450113", "Base Cabinet Single Door horisontalt håndtak:Skap, resirkulering 300 x 450 x 690mm:2450114", "Base Cabinet Single Door horisontalt håndtak:Skap, resirkulering 300 x 450 x 690mm:2450115" (+1 more) | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
            1 x IFCFLOWTERMINAL | object type "Vaskerenne 1200mm, Krogsæter" | names: "intra_wash_throuh_wall_mounted_1200_mm:Vaskerenne 1200mm, Krogsæter:3636065" | material: materials ("f26d4e4b_a025_4dbf_b085_30ed485788cf", "4b4a701a_e8ab_4354_ac15_234043769b9c") | property sets: Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data, Mechanical
            2 x IFCFLOWCONTROLLER | type IFCVALVETYPE "Blandebatteri berøringsfri 1724FT" | object type "Blandebatteri berøringsfri 1724FT" | names: "1724FT(2013):Blandebatteri berøringsfri 1724FT:4383539", "1724FT(2013):Blandebatteri berøringsfri 1724FT:4383541" | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Tavle 2m" | object type "Tavle 2m" | names: "Tavle:Tavle 2m:5296539" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Smartboard 2m" | object type "Smartboard 2m" | names: "Smartboard:Smartboard 2m:5296540" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
        IFCSPACE "01067" | long name "naturfag" | INTERNAL
          contains 19 elements
            1 x IFCFLOWTERMINAL | object type "Lab kum" | names: "N_Sink Kitchen-lab kum:Lab kum:2378496" | material: "Metal - Steel, Polished" | property sets: Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data, Other
            4 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Skap, resirkulering 450 x 450 x 860mm" | object type "Skap, resirkulering 450 x 450 x 860mm" | names: "Base Cabinet Single Door horisontalt håndtak:Skap, resirkulering 450 x 450 x 860mm:2450124", "Base Cabinet Single Door horisontalt håndtak:Skap, resirkulering 450 x 450 x 860mm:4377982", "Base Cabinet Single Door horisontalt håndtak:Skap, resirkulering 450 x 450 x 860mm:4377992" (+1 more) | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Other, Phasing
            1 x IFCFLOWTERMINAL | object type "Vaskerenne 1800mm, Krogsæter" | names: "intra_wash_throuh_wall_mounted_1800_mm:Vaskerenne 1800mm, Krogsæter:3641803" | material: materials ("f26d4e4b_a025_4dbf_b085_30ed485788cf", "4b4a701a_e8ab_4354_ac15_234043769b9c") | property sets: Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data, Mechanical
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Demobenk, naturfag" | object type "Demobenk, naturfag" | names: "Benk_Naturfag:Demobenk, naturfag:4151169" | material: "hvit malt" | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Other, Phasing
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Skap, demobenk naturfag 1200 x 600 x 860mm" | object type "Skap, demobenk naturfag 1200 x 600 x 860mm" | names: "N_Base Cabinet-Double Door-for sink:Skap, demobenk naturfag 1200 x 600 x 860mm:4151506" | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Other, Phasing
            4 x IFCFLOWTERMINAL | object type "Blandebatteri - Oras Saphira 1038F" | names: "Oras Saphira:Blandebatteri - Oras Saphira 1038F:4371868", "Oras Saphira:Blandebatteri - Oras Saphira 1038F:4371869", "Oras Saphira:Blandebatteri - Oras Saphira 1038F:4371870" (+1 more) | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Naturfagsbord" | object type "Naturfagsbord" | names: "M_Table spes equipment:Naturfagsbord:4407039", "M_Table spes equipment:Naturfagsbord:4407083" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_TFM, Constraints, Dimensions, Electrical - Loads
            2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Naturfagsbord" | object type "Naturfagsbord" | names: "M_Table spes equipment:Naturfagsbord:4407040", "M_Table spes equipment:Naturfagsbord:4407084" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_TFM, Constraints, Dimensions, Electrical - Loads
            1 x IFCFLOWTERMINAL | object type "Haws nøddusjsøyle 8320 Axion ECO" | names: "Dusj:Haws nøddusjsøyle 8320 Axion ECO:5272702" | material: "Aluminum" | property sets: Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data, Other
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Tavle 2m" | object type "Tavle 2m" | names: "Tavle:Tavle 2m:5296868" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Smartboard 2m" | object type "Smartboard 2m" | names: "Smartboard:Smartboard 2m:5296869" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
        IFCSPACE "01061" | long name "design tekno" | INTERNAL
          contains 2 elements
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Tavle 2m" | object type "Tavle 2m" | names: "Tavle:Tavle 2m:5294278" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Smartboard 2m" | object type "Smartboard 2m" | names: "Smartboard:Smartboard 2m:5296373" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
        IFCSPACE "01062" | long name "tegne-keramikk" | INTERNAL
          contains 11 elements
            4 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Skap, resirkulering 300 x 450 x 690mm" | object type "Skap, resirkulering 300 x 450 x 690mm" | names: "Base Cabinet Single Door horisontalt håndtak:Skap, resirkulering 300 x 450 x 690mm:2450118", "Base Cabinet Single Door horisontalt håndtak:Skap, resirkulering 300 x 450 x 690mm:4383565", "Base Cabinet Single Door horisontalt håndtak:Skap, resirkulering 300 x 450 x 690mm:4383566" (+1 more) | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Other, Phasing
            1 x IFCFLOWTERMINAL | object type "Vaskerenne 1800mm, Krogsæter" | names: "intra_wash_throuh_wall_mounted_1800_mm:Vaskerenne 1800mm, Krogsæter:3633894" | material: materials ("f26d4e4b_a025_4dbf_b085_30ed485788cf", "4b4a701a_e8ab_4354_ac15_234043769b9c") | property sets: Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data, Mechanical
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "dreieskive560x720x540" | object type "dreieskive560x720x540" | names: "Dreieskive:dreieskive560x720x540:4122443" | material: "hvit malt" | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Gipsutskiller" | object type "Gipsutskiller" | names: "Spesialutstyr:Gipsutskiller:4122746" | material: "hvit malt" | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
            2 x IFCFLOWCONTROLLER | type IFCVALVETYPE "Blandebatteri berøringsfri 1724FT" | object type "Blandebatteri berøringsfri 1724FT" | names: "1724FT(2013):Blandebatteri berøringsfri 1724FT:4383568", "1724FT(2013):Blandebatteri berøringsfri 1724FT:4383569" | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWTERMINAL | object type "Blandebatteri - Oras Saphira 1038F" | names: "Oras Saphira:Blandebatteri - Oras Saphira 1038F:4383571" | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Whiteboard 2,5m" | object type "Whiteboard 2,5m" | names: "Tavle:Whiteboard 2,5m:4459982" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
        IFCSPACE "01057" | long name "lager" | INTERNAL
        IFCSPACE "01059" | long name "tekstil" | INTERNAL
          contains 13 elements
            5 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Sybord" | object type "Sybord" | names: "Elevbord-sybord:Sybord:2437925", "Elevbord-sybord:Sybord:4386820", "Elevbord-sybord:Sybord:4386830" (+2 more) | material: materials ("Farge sort", "Paint Hvit(1)") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
            4 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Skap, resirkulering 300 x 450 x 860mm" | object type "Skap, resirkulering 300 x 450 x 860mm" | names: "Base Cabinet Single Door horisontalt håndtak:Skap, resirkulering 300 x 450 x 860mm:2450105", "Base Cabinet Single Door horisontalt håndtak:Skap, resirkulering 300 x 450 x 860mm:2450106", "Base Cabinet Single Door horisontalt håndtak:Skap, resirkulering 300 x 450 x 860mm:2450107" (+1 more) | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Other, Phasing
            1 x IFCFLOWTERMINAL | object type "Vaskerenne 1200mm, Krogsæter" | names: "intra_wash_throuh_wall_mounted_1200_mm:Vaskerenne 1200mm, Krogsæter:3641486" | material: materials ("f26d4e4b_a025_4dbf_b085_30ed485788cf", "4b4a701a_e8ab_4354_ac15_234043769b9c") | property sets: Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data, Mechanical
            1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "Blandebatteri berøringsfri 1724FT" | object type "Blandebatteri berøringsfri 1724FT" | names: "1724FT(2013):Blandebatteri berøringsfri 1724FT:4386966" | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWTERMINAL | object type "Blandebatteri - Oras Saphira 1038F" | names: "Oras Saphira:Blandebatteri - Oras Saphira 1038F:4386968" | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Whiteboard 2,5m" | object type "Whiteboard 2,5m" | names: "Tavle:Whiteboard 2,5m:4412678" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
        IFCSPACE "01043" | long name "drift" | INTERNAL
        IFCSPACE "01042" | long name "helse" | INTERNAL
          contains 7 elements
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Benkeplate 625mm, Sigdal" | object type "Benkeplate 625mm, Sigdal" | names: "N_CounterTop:Benkeplate 625mm, Sigdal:2432436" | material: "hvit malt" | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Skap, kjøkken 500 x 600 x 860mm" | object type "Skap, kjøkken 500 x 600 x 860mm" | names: "Base Cabinet Single Door horisontalt håndtak:Skap, kjøkken 500 x 600 x 860mm:2432901" | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Overskap 1000 x 300 x 720mm" | object type "Overskap 1000 x 300 x 720mm" | names: "N_Upper Cabinet-Double Door:Overskap 1000 x 300 x 720mm:2438601" | material: "N_Cabinets" | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Siemens Kjøleskap under benk" | object type "Siemens Kjøleskap under benk" | names: "NO_Kjøleskap_lite:Siemens Kjøleskap under benk:4383662" | material: materials ("Metal - Chrome", "Metal - Paint Finish - Ivory,Matte") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
            1 x IFCFLOWTERMINAL | object type "Kum helse" | names: "N_Sink Kitchen-Single:Kum helse:4383826" | material: "Metal - Steel, Polished" | property sets: Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data, Other
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "TV-skjerm" | object type "TV-skjerm" | names: "TV-skjerm:TV-skjerm:6715056" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
            1 x IFCFLOWTERMINAL | object type "Blandebatteri - Oras Saphira 1038F" | names: "Oras Saphira:Blandebatteri - Oras Saphira 1038F:7584275" | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
        IFCSPACE "01039" | long name "vente" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | object type "Compound Ceiling:Himling System 600x600" | CEILING | names: "Compound Ceiling:Himling System 600x600:4834309" | material: layers "Compound Ceiling:Himling System 600x600" ("Himling Metallprofil" 38., "Himling System 600x600" 12.) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
        IFCSPACE "01044" | long name "hcwc" | INTERNAL
          contains 5 elements
            1 x IFCFLOWTERMINAL | object type "Gulvstående toalett - Nautic 1546" | names: "WC-GBG-Nautic_1546-Floor_Standing:Gulvstående toalett - Nautic 1546:1710340" | material: materials ("Gustavsberg Chrome - Polished", "Gustavsberg Porcelain - White", "Gustavsberg Plastic - White") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWTERMINAL | object type "Servant HCWC - 7119" | names: "Washbasin-GBG-7119_Bolt_Mounting:Servant HCWC - 7119:3628343" | material: "Gustavsberg Porcelain - White" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "Blandebatteri berøringsfri 1724FT" | object type "Blandebatteri berøringsfri 1724FT" | names: "1724FT(2013):Blandebatteri berøringsfri 1724FT:7590028" | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Armstøtte veggmontert" | object type "Armstøtte veggmontert" | names: "WC_Armrest-GBG-1712_Wall_Mounted:Armstøtte veggmontert:7603372", "WC_Armrest-GBG-1712_Wall_Mounted:Armstøtte veggmontert:7603391" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_TFM, Constraints, Dimensions, Electrical - Loads
        IFCSPACE "01142" | long name "basseng" | INTERNAL
        IFCSPACE "01146" | long name "rengj" | INTERNAL
          contains 2 elements
            1 x IFCFLOWTERMINAL | object type "Utslagsvask" | names: "intra_gub1_bucket_sink_wall_mounted:Utslagsvask:5297974" | material: "f26d4e4b_a025_4dbf_b085_30ed485788cf" | property sets: Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data, Mechanical
            1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "Blandebatteri 3970" | object type "Blandebatteri 3970" | names: "Oras Saga:Blandebatteri 3970:7601786" | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
        IFCSPACE "01123" | long name "garderobe" | INTERNAL
          contains 11 elements
            7 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Vegghengt benk" | object type "Vegghengt benk" | names: "Benk:Vegghengt benk:5291161", "Benk:Vegghengt benk:5291267", "Benk:Vegghengt benk:6913306" (+4 more) | material: "hvit malt" | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Vegghengt benk" | object type "Vegghengt benk" | names: "Benk:Vegghengt benk:6932681" | material: "hvit malt" | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Other, Phasing
            2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "gard skap 5rom 30cm" | object type "gard skap 5rom 30cm" | names: "Locker_Metal_Hadrian_Replacement-Front:gard skap 5rom 30cm:6947893", "Locker_Metal_Hadrian_Replacement-Front:gard skap 5rom 30cm:6948177" | material: materials ("Gul avdeling", "Steel - Hadrian - Black") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_TFM, Constraints, Construction, Dimensions
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "gard skap 5rom 30cm" | object type "gard skap 5rom 30cm" | names: "Locker_Metal_Hadrian_Replacement-Front:gard skap 5rom 30cm:6948163" | material: materials ("Gul avdeling", "Steel - Hadrian - Black") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_TFM, Constraints, Construction, Dimensions
        IFCSPACE "01128" | long name "dusj" | INTERNAL
          contains 5 elements
            4 x IFCFLOWTERMINAL | object type "Delabie Sportsdusj 714700-S2" | names: "Dusj:Delabie Sportsdusj 714700-S2:5271371", "Dusj:Delabie Sportsdusj 714700-S2:5271372", "Dusj:Delabie Sportsdusj 714700-S2:5271373" (+1 more) | material: "Aluminum" | property sets: Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data, Other
            1 x IFCFLOWTERMINAL | object type "Delabie dusjpanel 749350" | names: "Dusj:Delabie dusjpanel 749350:5271375" | material: "Aluminum" | property sets: Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data, Other
        IFCSPACE "01124" | long name "dusj" | INTERNAL
          contains 5 elements
            1 x IFCFLOWTERMINAL | object type "Delabie dusjpanel 749350" | names: "Dusj:Delabie dusjpanel 749350:5271117" | material: "Aluminum" | property sets: Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data, Other
            4 x IFCFLOWTERMINAL | object type "Delabie Sportsdusj 714700-S2" | names: "Dusj:Delabie Sportsdusj 714700-S2:5271188", "Dusj:Delabie Sportsdusj 714700-S2:5271207", "Dusj:Delabie Sportsdusj 714700-S2:5271231" (+1 more) | material: "Aluminum" | property sets: Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data, Other
        IFCSPACE "01011" | long name "garderobe" | INTERNAL
          contains 1 element
            1 x IFCFLOWTERMINAL | object type "Servant - Nautic 5556" | names: "Washbasin-GBG-Nautic_5556_Bolt_Bracket_Mounting:Servant - Nautic 5556:3649458" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
        IFCSPACE "01127" | long name "hcgard" | INTERNAL
          contains 7 elements
            1 x IFCFLOWTERMINAL | object type "Gulvstående toalett - Nautic 1546" | names: "WC-GBG-Nautic_1546-Floor_Standing:Gulvstående toalett - Nautic 1546:2114971" | material: materials ("Gustavsberg Chrome - Polished", "Gustavsberg Porcelain - White", "Gustavsberg Plastic - White") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWTERMINAL | object type "Servant HCWC - 7119" | names: "Washbasin-GBG-7119_Bolt_Mounting:Servant HCWC - 7119:3627755" | material: "Gustavsberg Porcelain - White" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Armstøtte veggmontert" | object type "Armstøtte veggmontert" | names: "WC_Armrest-GBG-1712_Wall_Mounted:Armstøtte veggmontert:3639020" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_TFM, Constraints, Dimensions, Electrical - Loads
            1 x IFCFLOWTERMINAL | object type "Dusjhode - Oras Apollo 530" | names: "Dusj:Dusjhode - Oras Apollo 530:5271791" | material: "Aluminum" | property sets: Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data, Other
            1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "Blandebatteri berøringsfri 1724FT" | object type "Blandebatteri berøringsfri 1724FT" | names: "1724FT(2013):Blandebatteri berøringsfri 1724FT:7589620" | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "Blandebatteri dusj 7267" | object type "Blandebatteri dusj 7267" | names: "Oras Oramix:Blandebatteri dusj 7267:7600436" | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Armstøtte veggmontert" | object type "Armstøtte veggmontert" | names: "WC_Armrest-GBG-1712_Wall_Mounted:Armstøtte veggmontert:7603213" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_TFM, Constraints, Dimensions, Electrical - Loads
        IFCSPACE "01148" | long name "hcwc" | INTERNAL
          contains 6 elements
            1 x IFCFLOWTERMINAL | object type "Gulvstående toalett - Nautic 1546" | names: "WC-GBG-Nautic_1546-Floor_Standing:Gulvstående toalett - Nautic 1546:2568927" | material: materials ("Gustavsberg Chrome - Polished", "Gustavsberg Porcelain - White", "Gustavsberg Plastic - White") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCCOVERING | object type "Compound Ceiling:Himling System 600x600 hygiene korrosjonsklasse" | CEILING | names: "Compound Ceiling:Himling System 600x600 hygiene korrosjonsklasse:3050549" | material: layers "Compound Ceiling:Himling System 600x600 hygiene korrosjonsklasse" ("Himling Metallprofil" 38., "Himling System 600x600" 12.) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Other
            1 x IFCFLOWTERMINAL | object type "Servant HCWC - 7119" | names: "Washbasin-GBG-7119_Bolt_Mounting:Servant HCWC - 7119:3628254" | material: "Gustavsberg Porcelain - White" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "Blandebatteri berøringsfri 1724FT" | object type "Blandebatteri berøringsfri 1724FT" | names: "1724FT(2013):Blandebatteri berøringsfri 1724FT:7589790" | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Armstøtte veggmontert" | object type "Armstøtte veggmontert" | names: "WC_Armrest-GBG-1712_Wall_Mounted:Armstøtte veggmontert:7603683", "WC_Armrest-GBG-1712_Wall_Mounted:Armstøtte veggmontert:7603701" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_TFM, Constraints, Dimensions, Electrical - Loads
        IFCSPACE "01149" | long name "lager" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | object type "Compound Ceiling:Himling System 600x600 hygiene korrosjonsklasse" | CEILING | names: "Compound Ceiling:Himling System 600x600 hygiene korrosjonsklasse:3050668" | material: layers "Compound Ceiling:Himling System 600x600 hygiene korrosjonsklasse" ("Himling Metallprofil" 38., "Himling System 600x600" 12.) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Other
        IFCSPACE "01002" | long name "kantine" | INTERNAL
          contains 17 elements
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Hylle 350mm" | object type "Hylle 350mm" | names: "N_CounterTop:Hylle 350mm:2436199" | material: "hvit malt" | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Skap, resirkulering 300 x 460 x 825mm" | object type "Skap, resirkulering 300 x 460 x 825mm" | names: "Base Cabinet Single Door:Skap, resirkulering 300 x 460 x 825mm:2450566" | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
            2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Siemens mikro, 20L" | object type "Siemens mikro, 20L" | names: "Microwave_-_classic_amp_simple_13218:Siemens mikro, 20L:6138087", "Microwave_-_classic_amp_simple_13218:Siemens mikro, 20L:6138274" | material: materials ("Glass - black", "Metal - Aluminium", "Metal - Firring") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
            4 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Skap, resirkulering 400 x 460 x 825mm" | object type "Skap, resirkulering 400 x 460 x 825mm" | names: "Base Cabinet Single Door:Skap, resirkulering 400 x 460 x 825mm:7158588", "Base Cabinet Single Door:Skap, resirkulering 400 x 460 x 825mm:7158589", "Base Cabinet Single Door:Skap, resirkulering 400 x 460 x 825mm:7159029" (+1 more) | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
            3 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Skap, resirkulering 300 x 460 x 825mm" | object type "Skap, resirkulering 300 x 460 x 825mm" | names: "Base Cabinet Single Door:Skap, resirkulering 300 x 460 x 825mm:7158590", "Base Cabinet Single Door:Skap, resirkulering 300 x 460 x 825mm:7158591", "Base Cabinet Single Door:Skap, resirkulering 300 x 460 x 825mm:7159031" | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Other, Phasing
            2 x IFCFLOWTERMINAL | object type "Kum kantine" | names: "Utslagsvask:Kum kantine:7159897", "Utslagsvask:Kum kantine:7159925" | material: "Metal - Aluminium" | property sets: Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data, Other
            2 x IFCFLOWTERMINAL | object type "Delabie flaskefyller" | names: "M_Tap_2:Delabie flaskefyller:7578278", "M_Tap_2:Delabie flaskefyller:7579926" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            2 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Benkeplate kildesortering" | object type "Benkeplate kildesortering" | names: "N_CounterTop:Benkeplate kildesortering:7720702", "N_CounterTop:Benkeplate kildesortering:7721222" | material: "hvit malt" | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
        IFCSPACE "01109" | long name "lærerarbeid" | INTERNAL
        IFCSPACE "01110" | long name "aktivitetsrom" | INTERNAL
        IFCSPACE "01111" | long name "hjemmeområde" | INTERNAL | description "sas"
          contains 27 elements
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Siemens induksjon" | object type "Siemens induksjon" | names: "N_Cook Top:Siemens induksjon:2013458" | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
            1 x IFCFLOWTERMINAL | object type "Kum kjøkken 2" | names: "N_Sink Kitchen-Double uneven:Kum kjøkken 2:2013459" | material: "Metal - Steel, Polished" | property sets: Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data, Other
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Benkeplate 625mm, Sigdal" | object type "Benkeplate 625mm, Sigdal" | names: "N_CounterTop:Benkeplate 625mm, Sigdal:2013461" | material: "hvit malt" | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
            4 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Skap, resirkulering 300 x 450 x 690mm" | object type "Skap, resirkulering 300 x 450 x 690mm" | names: "Base Cabinet Single Door horisontalt håndtak:Skap, resirkulering 300 x 450 x 690mm:2450792", "Base Cabinet Single Door horisontalt håndtak:Skap, resirkulering 300 x 450 x 690mm:2450793", "Base Cabinet Single Door horisontalt håndtak:Skap, resirkulering 300 x 450 x 690mm:2450794" (+1 more) | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Siemens Kombiskap, hvit,186 cm" | object type "Siemens Kombiskap, hvit,186 cm" | names: "N_Refrigerator-Freezer:Siemens Kombiskap, hvit,186 cm:2451579" | material: "N_Cabinets" | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "OPPV.MASK, FRITTSTÅENDE, 60 CM" | object type "OPPV.MASK, FRITTSTÅENDE, 60 CM" | names: "Dishwasher:OPPV.MASK, FRITTSTÅENDE, 60 CM:2469295" | material: materials ("N_Cabinets", "EQ-Cozinha-Maquinas", "EQ-Cozinha-Maquinas-Porta", "Default Light Source", "N_Cabinets - Handles") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Skap, kjøkken 800 x 600 x 860mm" | object type "Skap, kjøkken 800 x 600 x 860mm" | names: "N_Base Cabinet-Double Door-for sink:Skap, kjøkken 800 x 600 x 860mm:2469462" | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
            2 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Skap, kjøkken 600 x 600 x 860mm" | object type "Skap, kjøkken 600 x 600 x 860mm" | names: "N_Base Cabinet-3 drawers:Skap, kjøkken 600 x 600 x 860mm:2469535", "N_Base Cabinet-3 drawers:Skap, kjøkken 600 x 600 x 860mm:2469609" | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Siemens innebygget ovn" | object type "Siemens innebygget ovn" | names: "N_Oven-Built-in:Siemens innebygget ovn:2564428" | material: materials ("Glass", "EQ-Cozinha-Maquinas", "EQ-Cozinha-Maquinas-Porta") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Overskap 800 x 300 x 600mm" | object type "Overskap 800 x 300 x 600mm" | names: "N_Upper Cabinet-Double Door:Overskap 800 x 300 x 600mm:2564651" | material: "N_Cabinets" | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
            4 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Overskap 600 x 300 x 600mm" | object type "Overskap 600 x 300 x 600mm" | names: "N_Upper Cabinet-Single Door:Overskap 600 x 300 x 600mm:2564725", "N_Upper Cabinet-Single Door:Overskap 600 x 300 x 600mm:2564796", "N_Upper Cabinet-Single Door:Overskap 600 x 300 x 600mm:2564839" (+1 more) | material: "N_Cabinets" | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Other, Phasing
            1 x IFCFLOWTERMINAL | object type "Vaskerenne 1200mm, Krogsæter" | names: "intra_wash_throuh_wall_mounted_1200_mm:Vaskerenne 1200mm, Krogsæter:3641586" | material: materials ("f26d4e4b_a025_4dbf_b085_30ed485788cf", "4b4a701a_e8ab_4354_ac15_234043769b9c") | property sets: Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data, Mechanical
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Siemens mikro, 60skap" | object type "Siemens mikro, 60skap" | names: "Microwave_-_classic_amp_simple_13218:Siemens mikro, 60skap:4486010" | material: materials ("Glass - black", "Metal - Aluminium", "Metal - Firring") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
            2 x IFCFLOWCONTROLLER | type IFCVALVETYPE "Blandebatteri berøringsfri 1724FT" | object type "Blandebatteri berøringsfri 1724FT" | names: "1724FT(2013):Blandebatteri berøringsfri 1724FT:4487399", "1724FT(2013):Blandebatteri berøringsfri 1724FT:4487618" | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Skap, kjøkken 600 x 600 x 860mm" | object type "Skap, kjøkken 600 x 600 x 860mm" | names: "Base Cabinet Single Door:Skap, kjøkken 600 x 600 x 860mm:4493403" | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Overskap 600 x 300 x 600mm" | object type "Overskap 600 x 300 x 600mm" | names: "N_Upper Cabinet-Single Door:Overskap 600 x 300 x 600mm:4493404" | material: "N_Cabinets" | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Other, Phasing
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Tavle 2m" | object type "Tavle 2m" | names: "Tavle:Tavle 2m:5297038" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Smartboard 2m" | object type "Smartboard 2m" | names: "Smartboard:Smartboard 2m:5297039" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
            1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "Blandebatteri - Oras Saphira 1039F" | object type "Blandebatteri - Oras Saphira 1039F" | names: "Oras Saphira:Blandebatteri - Oras Saphira 1039F:7588762" | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
        IFCSPACE "01114" | long name "gruppe" | INTERNAL
          contains 2 elements
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Tavle 2m" | object type "Tavle 2m" | names: "Tavle:Tavle 2m:5296891" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Smartboard 2m" | object type "Smartboard 2m" | names: "Smartboard:Smartboard 2m:5296892" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
        IFCSPACE "01113" | long name "gruppe" | INTERNAL
          contains 2 elements
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Tavle 2m" | object type "Tavle 2m" | names: "Tavle:Tavle 2m:5296973" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Smartboard 2m" | object type "Smartboard 2m" | names: "Smartboard:Smartboard 2m:5296974" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
        IFCSPACE "01108" | long name "gruppe" | INTERNAL
          contains 2 elements
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Tavle 2m" | object type "Tavle 2m" | names: "Tavle:Tavle 2m:5297184" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Smartboard 2m" | object type "Smartboard 2m" | names: "Smartboard:Smartboard 2m:5297185" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
        IFCSPACE "01100" | long name "trapp" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | object type "Compound Ceiling:Himling System 600x600" | CEILING | names: "Compound Ceiling:Himling System 600x600:4435080" | material: layers "Compound Ceiling:Himling System 600x600" ("Himling Metallprofil" 38., "Himling System 600x600" 12.) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
        IFCSPACE "01118" | long name "lager" | INTERNAL
        IFCSPACE "01115" | long name "garderobe" | INTERNAL
          contains 20 elements
            10 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Båsgarderobe 400 x 350 x 2000mm" | object type "Båsgarderobe 400 x 350 x 2000mm" | names: "høyskap:Båsgarderobe 400 x 350 x 2000mm:5378897", "høyskap:Båsgarderobe 400 x 350 x 2000mm:5379086", "høyskap:Båsgarderobe 400 x 350 x 2000mm:5379144" (+7 more) | material: "N_Cabinets" | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
            10 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Båsgarderobe 400 x 350 x 2000mm" | object type "Båsgarderobe 400 x 350 x 2000mm" | names: "høyskap:Båsgarderobe 400 x 350 x 2000mm:5379056", "høyskap:Båsgarderobe 400 x 350 x 2000mm:5379115", "høyskap:Båsgarderobe 400 x 350 x 2000mm:5379173" (+7 more) | material: "N_Cabinets" | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
        IFCSPACE "01119" | long name "sanserom" | INTERNAL
        IFCSPACE "01117" | long name "stelle" | INTERNAL
          contains 9 elements
            1 x IFCFLOWTERMINAL | object type "Gulvstående toalett - Nautic 1546" | names: "WC-GBG-Nautic_1546-Floor_Standing:Gulvstående toalett - Nautic 1546:1785299" | material: materials ("Gustavsberg Chrome - Polished", "Gustavsberg Porcelain - White", "Gustavsberg Plastic - White") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWTERMINAL | object type "Servant HCWC - 7119" | names: "Washbasin-GBG-7119_Bolt_Mounting:Servant HCWC - 7119:3627903" | material: "Gustavsberg Porcelain - White" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Siemens Vaskemaskin, Sigdal" | object type "Siemens Vaskemaskin, Sigdal" | names: "N_Washing Machine:Siemens Vaskemaskin, Sigdal:4184262" | material: materials ("Glass", "EQ-Cozinha-Maquinas-Porta", "N_Cabinets", "EQ-Cozinha-Maquinas", "Default Light Source", "N_Cabinets - Handles") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Siemens Varmep.trommel Sigdal" | object type "Siemens Varmep.trommel Sigdal" | names: "N_Washing Machine:Siemens Varmep.trommel Sigdal:4184459" | material: materials ("Glass", "EQ-Cozinha-Maquinas-Porta", "N_Cabinets", "EQ-Cozinha-Maquinas", "Default Light Source", "N_Cabinets - Handles") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
            1 x IFCFLOWTERMINAL | object type "Dusjhode - Oras Apollo 530" | names: "Dusj:Dusjhode - Oras Apollo 530:5271423" | material: "Aluminum" | property sets: Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data, Other
            1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "Blandebatteri berøringsfri 1724FT" | object type "Blandebatteri berøringsfri 1724FT" | names: "1724FT(2013):Blandebatteri berøringsfri 1724FT:7589451" | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "Blandebatteri dusj 7267" | object type "Blandebatteri dusj 7267" | names: "Oras Oramix:Blandebatteri dusj 7267:7600288" | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Armstøtte veggmontert" | object type "Armstøtte veggmontert" | names: "WC_Armrest-GBG-1712_Wall_Mounted:Armstøtte veggmontert:7603245", "WC_Armrest-GBG-1712_Wall_Mounted:Armstøtte veggmontert:7603265" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_TFM, Constraints, Dimensions, Electrical - Loads
        IFCSPACE "01103" | long name "gard/toal" | INTERNAL
          contains 4 elements
            2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "gard skap 5rom 30cm" | object type "gard skap 5rom 30cm" | names: "Locker_Metal_Hadrian_Replacement-Front:gard skap 5rom 30cm:2572076", "Locker_Metal_Hadrian_Replacement-Front:gard skap 5rom 30cm:2572077" | material: materials ("Gul avdeling", "hvit malt") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_TFM, Constraints, Construction, Dimensions
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Hattehylle360mm" | object type "Hattehylle360mm" | names: "NO_Hattehylle med stang:Hattehylle360mm:5369651" | material: "Wood - Birch, Natural" | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Skohylle" | object type "Skohylle" | names: "N_CounterTop:Skohylle:5369835" | material: "hvit malt" | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
        IFCSPACE "01116" | long name "lager" | INTERNAL
          contains 1 element
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Rullestol-ikon" | object type "Rullestol-ikon" | names: "Rullestol-ikon:Rullestol-ikon:2194314" | material: "Paint - White" | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Identity Data, Other
        IFCSPACE "01104" | long name "kopi" | INTERNAL
        IFCSPACE "01005" | long name "lager" | INTERNAL
        IFCSPACE "01143" | long name "vakt/forrom" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | object type "Compound Ceiling:Himling System 600x600 hygiene korrosjonsklasse" | CEILING | names: "Compound Ceiling:Himling System 600x600 hygiene korrosjonsklasse:4602264" | material: layers "Compound Ceiling:Himling System 600x600 hygiene korrosjonsklasse" ("Himling Metallprofil" 38., "Himling System 600x600" 12.) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
        IFCSPACE "01145" | long name "lærer" | INTERNAL
          contains 10 elements
            1 x IFCFLOWTERMINAL | object type "Gulvstående toalett - Nautic 1500" | names: "WC-GBG-Nautic_1546-Floor_Standing:Gulvstående toalett - Nautic 1500:2568261" | material: materials ("Gustavsberg Chrome - Polished", "Gustavsberg Porcelain - White", "Gustavsberg Plastic - White") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "gard skap 5rom 30cm" | object type "gard skap 5rom 30cm" | names: "Locker_Metal_Hadrian_Replacement-Front:gard skap 5rom 30cm:2568478", "Locker_Metal_Hadrian_Replacement-Front:gard skap 5rom 30cm:2568479" | material: materials ("Gul avdeling", "hvit malt") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_TFM, Constraints, Construction, Dimensions
            1 x IFCFLOWTERMINAL | object type "Servant HCWC - Nautic 5560" | names: "Washbasin-GBG-7119_Bolt_Mounting:Servant HCWC - Nautic 5560:3628134" | material: "Gustavsberg Porcelain - White" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWTERMINAL | object type "Dusjhode - Oras Apollo 530" | names: "Dusj:Dusjhode - Oras Apollo 530:5271670" | material: "Aluminum" | property sets: Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data, Other
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Vegghengt benk" | object type "Vegghengt benk" | names: "Benk:Vegghengt benk:7237000" | material: "hvit malt" | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
            1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "Blandebatteri berøringsfri 1724FT" | object type "Blandebatteri berøringsfri 1724FT" | names: "1724FT(2013):Blandebatteri berøringsfri 1724FT:7589936" | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "Blandebatteri dusj 7264" | object type "Blandebatteri dusj 7264" | names: "Oras Oramix:Blandebatteri dusj 7264:7600824" | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Armstøtte veggmontert" | object type "Armstøtte veggmontert" | names: "WC_Armrest-GBG-1712_Wall_Mounted:Armstøtte veggmontert:7603750", "WC_Armrest-GBG-1712_Wall_Mounted:Armstøtte veggmontert:7603817" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_TFM, Constraints, Dimensions, Electrical - Loads
        IFCSPACE "01144" | long name "lærer" | INTERNAL
          contains 10 elements
            1 x IFCFLOWTERMINAL | object type "Gulvstående toalett - Nautic 1500" | names: "WC-GBG-Nautic_1546-Floor_Standing:Gulvstående toalett - Nautic 1500:2568770" | material: materials ("Gustavsberg Chrome - Polished", "Gustavsberg Porcelain - White", "Gustavsberg Plastic - White") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "gard skap 5rom 30cm" | object type "gard skap 5rom 30cm" | names: "Locker_Metal_Hadrian_Replacement-Front:gard skap 5rom 30cm:2568774", "Locker_Metal_Hadrian_Replacement-Front:gard skap 5rom 30cm:2568775" | material: materials ("Gul avdeling", "hvit malt") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_TFM, Constraints, Construction, Dimensions
            1 x IFCFLOWTERMINAL | object type "Servant HCWC - Nautic 5560" | names: "Washbasin-GBG-7119_Bolt_Mounting:Servant HCWC - Nautic 5560:3628083" | material: "Gustavsberg Porcelain - White" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWTERMINAL | object type "Dusjhode - Oras Apollo 530" | names: "Dusj:Dusjhode - Oras Apollo 530:5271721" | material: "Aluminum" | property sets: Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data, Other
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Vegghengt benk" | object type "Vegghengt benk" | names: "Benk:Vegghengt benk:7236552" | material: "hvit malt" | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Other, Phasing
            1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "Blandebatteri berøringsfri 1724FT" | object type "Blandebatteri berøringsfri 1724FT" | names: "1724FT(2013):Blandebatteri berøringsfri 1724FT:7589895" | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "Blandebatteri dusj 7264" | object type "Blandebatteri dusj 7264" | names: "Oras Oramix:Blandebatteri dusj 7264:7600961" | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Armstøtte veggmontert" | object type "Armstøtte veggmontert" | names: "WC_Armrest-GBG-1712_Wall_Mounted:Armstøtte veggmontert:7603857", "WC_Armrest-GBG-1712_Wall_Mounted:Armstøtte veggmontert:7603910" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_TFM, Constraints, Dimensions, Electrical - Loads
        IFCSPACE "01129" | long name "hcwc" | INTERNAL
          contains 5 elements
            1 x IFCFLOWTERMINAL | object type "Gulvstående toalett - Nautic 1546" | names: "WC-GBG-Nautic_1546-Floor_Standing:Gulvstående toalett - Nautic 1546:3613315" | material: materials ("Gustavsberg Chrome - Polished", "Gustavsberg Porcelain - White", "Gustavsberg Plastic - White") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWTERMINAL | object type "Servant HCWC - 7119" | names: "Washbasin-GBG-7119_Bolt_Mounting:Servant HCWC - 7119:3627661" | material: "Gustavsberg Porcelain - White" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "Blandebatteri berøringsfri 1724FT" | object type "Blandebatteri berøringsfri 1724FT" | names: "1724FT(2013):Blandebatteri berøringsfri 1724FT:7589533" | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Armstøtte veggmontert" | object type "Armstøtte veggmontert" | names: "WC_Armrest-GBG-1712_Wall_Mounted:Armstøtte veggmontert:7603240" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_TFM, Constraints, Dimensions, Electrical - Loads
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Armstøtte veggmontert" | object type "Armstøtte veggmontert" | names: "WC_Armrest-GBG-1712_Wall_Mounted:Armstøtte veggmontert:7603242" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_TFM, Constraints, Dimensions, Electrical - Loads
        IFCSPACE "01066" | long name "maskinrom" | INTERNAL
          contains 3 elements
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Båndsag" | object type "Båndsag" | names: "Spesialutstyr:Båndsag:4397305" | material: "hvit malt" | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Avretter" | object type "Avretter" | names: "Spesialutstyr:Avretter:4397488" | material: "hvit malt" | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Sponavsug" | object type "Sponavsug" | names: "Spesialutstyr spes equip:Sponavsug:6133257" | material: "hvit malt" | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
        IFCSPACE "01063" | long name "ovn" | INTERNAL
          contains 16 elements
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Keramikkovn" | object type "Keramikkovn" | names: "Spesialutstyr:Keramikkovn:4394019" | material: "hvit malt" | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
            10 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Eskoleia småvarereol 1000 x 400mm" | object type "Eskoleia småvarereol 1000 x 400mm" | names: "M_Light Shelf Interior:Eskoleia småvarereol 1000 x 400mm:6903138", "M_Light Shelf Interior:Eskoleia småvarereol 1000 x 400mm:6903453", "M_Light Shelf Interior:Eskoleia småvarereol 1000 x 400mm:6903474" (+7 more) | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Other, Phasing
            5 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Eskoleia småvarereol 1000 x 400mm" | object type "Eskoleia småvarereol 1000 x 400mm" | names: "M_Light Shelf Interior:Eskoleia småvarereol 1000 x 400mm:6933157", "M_Light Shelf Interior:Eskoleia småvarereol 1000 x 400mm:6933158", "M_Light Shelf Interior:Eskoleia småvarereol 1000 x 400mm:6933159" (+2 more) | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Other, Phasing
        IFCSPACE "01125" | long name "hcwc" | INTERNAL
          contains 5 elements
            1 x IFCFLOWTERMINAL | object type "Gulvstående toalett - Nautic 1546" | names: "WC-GBG-Nautic_1546-Floor_Standing:Gulvstående toalett - Nautic 1546:2111914" | material: materials ("Gustavsberg Chrome - Polished", "Gustavsberg Porcelain - White", "Gustavsberg Plastic - White") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWTERMINAL | object type "Servant HCWC - 7119" | names: "Washbasin-GBG-7119_Bolt_Mounting:Servant HCWC - 7119:3627830" | material: "Gustavsberg Porcelain - White" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "Blandebatteri berøringsfri 1724FT" | object type "Blandebatteri berøringsfri 1724FT" | names: "1724FT(2013):Blandebatteri berøringsfri 1724FT:7589690" | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Armstøtte veggmontert" | object type "Armstøtte veggmontert" | names: "WC_Armrest-GBG-1712_Wall_Mounted:Armstøtte veggmontert:7603039", "WC_Armrest-GBG-1712_Wall_Mounted:Armstøtte veggmontert:7603062" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_TFM, Constraints, Dimensions, Electrical - Loads
        IFCSPACE "01015" | long name "hcwc" | INTERNAL
          contains 5 elements
            1 x IFCFLOWTERMINAL | object type "Gulvstående toalett - Nautic 1546" | names: "WC-GBG-Nautic_1546-Floor_Standing:Gulvstående toalett - Nautic 1546:3094845" | material: materials ("Gustavsberg Chrome - Polished", "Gustavsberg Porcelain - White", "Gustavsberg Plastic - White") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWTERMINAL | object type "Servant HCWC - 7119" | names: "Washbasin-GBG-7119_Bolt_Mounting:Servant HCWC - 7119:3627969" | material: "Gustavsberg Porcelain - White" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "Blandebatteri berøringsfri 1724FT" | object type "Blandebatteri berøringsfri 1724FT" | names: "1724FT(2013):Blandebatteri berøringsfri 1724FT:7590187" | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Armstøtte veggmontert" | object type "Armstøtte veggmontert" | names: "WC_Armrest-GBG-1712_Wall_Mounted:Armstøtte veggmontert:7603490", "WC_Armrest-GBG-1712_Wall_Mounted:Armstøtte veggmontert:7603506" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_TFM, Constraints, Dimensions, Electrical - Loads
        IFCSPACE "01054" | long name "IKT-server" | INTERNAL
        IFCSPACE "01026" | long name "forrom" | INTERNAL
        IFCSPACE "01038" | long name "rådg" | INTERNAL
          contains 1 element
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "TV-skjerm" | object type "TV-skjerm" | names: "TV-skjerm:TV-skjerm:6714879" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
        IFCSPACE "01070" | long name "lager" | INTERNAL
        IFCSPACE "01041" | long name "helse hvil" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | object type "Compound Ceiling:Himling System 600x600" | CEILING | names: "Compound Ceiling:Himling System 600x600:3051135" | material: layers "Compound Ceiling:Himling System 600x600" ("Himling Metallprofil" 38., "Himling System 600x600" 12.) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Other
        IFCSPACE "01004" | long name "bakscene" | INTERNAL
        IFCSPACE "01036" | long name "avd.led" | INTERNAL
        IFCSPACE "01033" | long name "avd.led" | INTERNAL
        IFCSPACE "01034" | long name "avd.led" | INTERNAL
        IFCSPACE "01037" | long name "rådg" | INTERNAL
        IFCSPACE "01101" | long name "EL" | INTERNAL
        IFCSPACE "01091" | long name "EL" | INTERNAL
        IFCSPACE "01020" | long name "trapp" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | object type "Compound Ceiling:Himling System 600x600" | CEILING | names: "Compound Ceiling:Himling System 600x600:4418810" | material: layers "Compound Ceiling:Himling System 600x600" ("Himling Metallprofil" 38., "Himling System 600x600" 12.) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
        IFCSPACE "01140" | long name "trapp" | INTERNAL
          contains 2 elements
            2 x IFCCOVERING | object type "Compound Ceiling:Himling System 600x600" | CEILING | names: "Compound Ceiling:Himling System 600x600:4433159", "Compound Ceiling:Himling System 600x600:7495429" | material: layers "Compound Ceiling:Himling System 600x600" ("Himling Metallprofil" 38., "Himling System 600x600" 12.) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
        IFCSPACE "01032" | long name "spes.ped" | INTERNAL
        IFCSPACE "01003" | long name "aula - nedre del" | INTERNAL
          contains 3 elements
            1 x IFCCOVERING | object type "Compound Ceiling:Himling System 600x1200" | CEILING | names: "Compound Ceiling:Himling System 600x1200:7438092" | material: layers "Compound Ceiling:Himling System 600x1200" ("Himling Metallprofil" 38., "Himling System 600x1200" 12.) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
            1 x IFCCOVERING | object type "Compound Ceiling:Fast gipshimling" | CEILING | names: "Compound Ceiling:Fast gipshimling:7504587" | material: layers "Compound Ceiling:Fast gipshimling" ("Himling Metallprofil" 95., "Himling fast gips" 12.5, "Himling fast gips" 12.5) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Other
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "AV rack" | object type "AV rack" | names: "AVrack:AV rack:7718372" | material: materials ("Cabinets", "Cabinets - Handles", "Cabinets - Panel") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
        IFCSPACE "01010" | long name "kjøkken" | INTERNAL
          contains 38 elements
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Benkeplate 625mm, Sigdal" | object type "Benkeplate 625mm, Sigdal" | names: "N_CounterTop:Benkeplate 625mm, Sigdal:2074527" | material: "hvit malt" | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
            2 x IFCFLOWTERMINAL | object type "Kum kjøkken 3" | names: "N_Sink Kitchen-lab kum:Kum kjøkken 3:2332593", "N_Sink Kitchen-lab kum:Kum kjøkken 3:4476092" | material: "Metal - Steel, Polished" | property sets: Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data, Other
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Siemens induksjon" | object type "Siemens induksjon" | names: "N_Cook Top:Siemens induksjon:2332673" | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Benkeplate 625mm, Sigdal" | object type "Benkeplate 625mm, Sigdal" | names: "N_CounterTop:Benkeplate 625mm, Sigdal:2427008" | material: "hvit malt" | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Other, Phasing
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Asko oppvaskmaskin" | object type "Asko oppvaskmaskin" | names: "Dishwasher:Asko oppvaskmaskin:2436579" | material: materials ("N_Cabinets", "EQ-Cozinha-Maquinas", "EQ-Cozinha-Maquinas-Porta", "Default Light Source", "N_Cabinets - Handles") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Benkeplate 625mm, Sigdal" | object type "Benkeplate 625mm, Sigdal" | names: "N_CounterTop:Benkeplate 625mm, Sigdal:2437010" | material: "hvit malt" | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Other, Phasing
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Overskap 300 x 300 x 700mm" | object type "Overskap 300 x 300 x 700mm" | names: "N_Upper Cabinet-Single Door:Overskap 300 x 300 x 700mm:2565263" | material: "N_Cabinets" | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Other, Phasing
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Overskap, hjørne 600 x 300 x 720mm" | object type "Overskap, hjørne 600 x 300 x 720mm" | names: "N_Upper Cabinet-Corner-Single Door:Overskap, hjørne 600 x 300 x 720mm:2565537" | material: "N_Cabinets" | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Other, Phasing
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Siemens innebygget ovn" | object type "Siemens innebygget ovn" | names: "N_Oven-Built-in:Siemens innebygget ovn:2565814" | material: materials ("Glass", "EQ-Cozinha-Maquinas", "EQ-Cozinha-Maquinas-Porta") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Skap, kjøkken, hjørne 900 x 600 x 860mm" | object type "Skap, kjøkken, hjørne 900 x 600 x 860mm" | names: "N_Base Cabinet-Corner-Single Door:Skap, kjøkken, hjørne 900 x 600 x 860mm:2565925" | material: "N_Cabinets" | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Other, Phasing
            3 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Overskap 600 x 300 x 700mm" | object type "Overskap 600 x 300 x 700mm" | names: "N_Upper Cabinet-Single Door:Overskap 600 x 300 x 700mm:2566231", "N_Upper Cabinet-Single Door:Overskap 600 x 300 x 700mm:4467960", "N_Upper Cabinet-Single Door:Overskap 600 x 300 x 700mm:4491795" | material: "N_Cabinets" | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Other, Phasing
            2 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Overskap 400 x 300 x 700mm" | object type "Overskap 400 x 300 x 700mm" | names: "N_Upper Cabinet-Single Door:Overskap 400 x 300 x 700mm:2566428", "N_Upper Cabinet-Single Door:Overskap 400 x 300 x 700mm:4468034" | material: "N_Cabinets" | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Other, Phasing
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Skap, kjøkken 600 x 500 x 860mm" | object type "Skap, kjøkken 600 x 500 x 860mm" | names: "N_Base Cabinet-3 drawers:Skap, kjøkken 600 x 500 x 860mm:2566555" | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Other, Phasing
            3 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Skap, kjøken 400 x 600 x 860mm" | object type "Skap, kjøken 400 x 600 x 860mm" | names: "N_Base Cabinet-3 drawers:Skap, kjøken 400 x 600 x 860mm:2566618", "N_Base Cabinet-3 drawers:Skap, kjøken 400 x 600 x 860mm:3649798", "N_Base Cabinet-3 drawers:Skap, kjøken 400 x 600 x 860mm:4474712" | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
            3 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Skap, kjøkken 600 x 600 x 860mm" | object type "Skap, kjøkken 600 x 600 x 860mm" | names: "Base Cabinet Single Door:Skap, kjøkken 600 x 600 x 860mm:2567277", "Base Cabinet Single Door:Skap, kjøkken 600 x 600 x 860mm:3649788", "Base Cabinet Single Door:Skap, kjøkken 600 x 600 x 860mm:4474714" | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Other, Phasing
            2 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Overskap 600 x 300 x 700mm" | object type "Overskap 600 x 300 x 700mm" | names: "N_Upper Cabinet-Single Door:Overskap 600 x 300 x 700mm:2567838", "N_Upper Cabinet-Single Door:Overskap 600 x 300 x 700mm:4469149" | material: "N_Cabinets" | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Other, Phasing
            1 x IFCFLOWTERMINAL | object type "Servant - Nautic 5556" | names: "Washbasin-GBG-Nautic_5556_Bolt_Bracket_Mounting:Servant - Nautic 5556:3649653" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Overskap 400 x 300 x 700mm" | object type "Overskap 400 x 300 x 700mm" | names: "N_Upper Cabinet-Single Door:Overskap 400 x 300 x 700mm:4474721" | material: "N_Cabinets" | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Other, Phasing
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Overskap 300 x 300 x 700mm" | object type "Overskap 300 x 300 x 700mm" | names: "N_Upper Cabinet-Single Door:Overskap 300 x 300 x 700mm:4474723" | material: "N_Cabinets" | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Other, Phasing
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Benkeplate, sigdal" | object type "Benkeplate, sigdal" | names: "N_CounterTop:Benkeplate, sigdal:4474728" | material: "hvit malt" | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Skap, kjøkken 600 x 350 x 860mm" | object type "Skap, kjøkken 600 x 350 x 860mm" | names: "Base Cabinet Single Door:Skap, kjøkken 600 x 350 x 860mm:4474729" | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Other, Phasing
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Skap, kjøkken 600 x 350 x 860mm" | object type "Skap, kjøkken 600 x 350 x 860mm" | names: "Base Cabinet Single Door:Skap, kjøkken 600 x 350 x 860mm:4474731" | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Kjøleskap_plass for" | object type "Kjøleskap_plass for" | names: "høyskap:Kjøleskap_plass for:4483866" | material: "N_Cabinets" | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Overskap 500 x 300 x 700mm" | object type "Overskap 500 x 300 x 700mm" | names: "N_Upper Cabinet-Single Door:Overskap 500 x 300 x 700mm:4492490" | material: "N_Cabinets" | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Other, Phasing
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Siemens mikro, 20L" | object type "Siemens mikro, 20L" | names: "Microwave_-_classic_amp_simple_13218:Siemens mikro, 20L:4493409" | material: materials ("Glass - black", "Metal - Aluminium", "Metal - Firring") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Kjøleskap_plass for" | object type "Kjøleskap_plass for" | names: "høyskap:Kjøleskap_plass for:4494764" | material: "N_Cabinets" | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
            1 x IFCCOVERING | object type "Compound Ceiling:Himling System 600x600 hygiene" | CEILING | names: "Compound Ceiling:Himling System 600x600 hygiene:4834345" | material: layers "Compound Ceiling:Himling System 600x600 hygiene" ("Himling Metallprofil" 38., "Himling System 600x600" 12.) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Other
            1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "Blandebatteri - Oras Saphira 1039F" | object type "Blandebatteri - Oras Saphira 1039F" | names: "Oras Saphira:Blandebatteri - Oras Saphira 1039F:7588566" | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWTERMINAL | object type "Blandebatteri - Oras Saphira 1038F" | names: "Oras Saphira:Blandebatteri - Oras Saphira 1038F:7588682" | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
        IFCSPACE "01008" | long name "lager" | INTERNAL
          contains 18 elements
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Siemens frittstående kjøleskap" | object type "Siemens frittstående kjøleskap" | names: "NO_Kjøleskap:Siemens frittstående kjøleskap:4328608" | material: materials ("Metal - Chrome", "Metal - Paint Finish - Ivory,Matte") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Siemens Frittstående fryseskap" | object type "Siemens Frittstående fryseskap" | names: "NO_Kjøleskap:Siemens Frittstående fryseskap:4328714" | material: materials ("Metal - Chrome", "Metal - Paint Finish - Ivory,Matte") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
            8 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Eskoleia småvarereol 800 x 400mm" | object type "Eskoleia småvarereol 800 x 400mm" | names: "M_Light Shelf Interior:Eskoleia småvarereol 800 x 400mm:6911530", "M_Light Shelf Interior:Eskoleia småvarereol 800 x 400mm:6911531", "M_Light Shelf Interior:Eskoleia småvarereol 800 x 400mm:6911579" (+5 more) | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
            8 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Eskoleia småvarereol 800 x 400mm" | object type "Eskoleia småvarereol 800 x 400mm" | names: "M_Light Shelf Interior:Eskoleia småvarereol 800 x 400mm:7362357", "M_Light Shelf Interior:Eskoleia småvarereol 800 x 400mm:7362359", "M_Light Shelf Interior:Eskoleia småvarereol 800 x 400mm:7362361" (+5 more) | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
        IFCSPACE "01007" | long name "lager" | INTERNAL
        IFCSPACE "01009" | long name "lager" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | object type "Compound Ceiling:Himling System 600x600" | CEILING | names: "Compound Ceiling:Himling System 600x600:4473586" | material: layers "Compound Ceiling:Himling System 600x600" ("Himling Metallprofil" 38., "Himling System 600x600" 12.) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Other
        IFCSPACE "01122" | long name "sluse" | INTERNAL
        IFCSPACE "01013" | long name "wc" | INTERNAL
          contains 3 elements
            1 x IFCFLOWTERMINAL | object type "Servant - Ecco 50x35" | names: "Ecco:Servant - Ecco 50x35:3626796" | material: materials ("Gustavsberg Chrome - Polished", "Gustavsberg Porcelain - White") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWTERMINAL | object type "Vegghengt toalett" | names: "WC-GBG-Nautic_1522-Wall_Mounted:Vegghengt toalett:4798676" | material: materials ("Gustavsberg Chrome - Polished", "Gustavsberg Porcelain - White (with C+)", "Gustavsberg Plastic - White") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "Blandebatteri berøringsfri 1724FT" | object type "Blandebatteri berøringsfri 1724FT" | names: "1724FT(2013):Blandebatteri berøringsfri 1724FT:7575396" | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
        IFCSPACE "01130" | long name "garderobe" | INTERNAL
          contains 11 elements
            7 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Vegghengt benk" | object type "Vegghengt benk" | names: "Benk:Vegghengt benk:6913533", "Benk:Vegghengt benk:6913534", "Benk:Vegghengt benk:6913535" (+4 more) | material: "hvit malt" | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Vegghengt benk" | object type "Vegghengt benk" | names: "Benk:Vegghengt benk:6932723" | material: "hvit malt" | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
            2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "gard skap 5rom 30cm" | object type "gard skap 5rom 30cm" | names: "Locker_Metal_Hadrian_Replacement-Front:gard skap 5rom 30cm:6948203", "Locker_Metal_Hadrian_Replacement-Front:gard skap 5rom 30cm:6948205" | material: materials ("Gul avdeling", "Steel - Hadrian - Black") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_TFM, Constraints, Construction, Dimensions
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "gard skap 5rom 30cm" | object type "gard skap 5rom 30cm" | names: "Locker_Metal_Hadrian_Replacement-Front:gard skap 5rom 30cm:6948204" | material: materials ("Gul avdeling", "Steel - Hadrian - Black") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_TFM, Constraints, Construction, Dimensions
        IFCSPACE "01126" | long name "gang" | INTERNAL
        IFCSPACE "01060" | long name "lager" | INTERNAL
          contains 17 elements
            15 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Stålhylle, krogsæter 900 x 400mm" | object type "Stålhylle, krogsæter 900 x 400mm" | names: "M_Light Shelf Interior:Stålhylle, krogsæter 900 x 400mm:4410623", "M_Light Shelf Interior:Stålhylle, krogsæter 900 x 400mm:4410624", "M_Light Shelf Interior:Stålhylle, krogsæter 900 x 400mm:4410625" (+12 more) | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Other, Phasing
            2 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "høyskap 800" | object type "høyskap 800" | names: "Høyskap dobbelt casework:høyskap 800:6889389", "Høyskap dobbelt casework:høyskap 800:6889390" | material: "Elevreol 2" | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
        IFCSPACE "01065" | long name "lager" | INTERNAL
          contains 1 element
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Kjemikalieskap maling" | object type "Kjemikalieskap maling" | names: "Spesialutstyr spes equip:Kjemikalieskap maling:6301430" | material: "hvit malt" | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
        IFCSPACE "4" | long name "Area" | INTERNAL
        IFCSPACE "01055" | long name "bk" | INTERNAL
          contains 2 elements
            1 x IFCFLOWTERMINAL | object type "Utslagsvask" | names: "intra_gub1_bucket_sink_wall_mounted:Utslagsvask:3638174" | material: "f26d4e4b_a025_4dbf_b085_30ed485788cf" | property sets: Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data, Mechanical
            1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "Blandebatteri 3970" | object type "Blandebatteri 3970" | names: "Oras Saga:Blandebatteri 3970:7601718" | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
        IFCSPACE "01052" | long name "lager" | INTERNAL
        IFCSPACE "01102" | long name "IKT" | INTERNAL
        IFCSPACE "01021" | long name "EL" | INTERNAL
        IFCSPACE "01001" | long name "vf" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | object type "Compound Ceiling:Himling spiler" | CEILING | names: "Compound Ceiling:Himling spiler:6454088" | material: layers "Compound Ceiling:Himling spiler" ("Himling Metallprofil" 48., "Spiler" 34.) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Other
        IFCSPACE "01014" | long name "wc" | INTERNAL
          contains 4 elements
            1 x IFCCOVERING | object type "Compound Ceiling:Himling System 600x600" | CEILING | names: "Compound Ceiling:Himling System 600x600:2599738" | material: layers "Compound Ceiling:Himling System 600x600" ("Himling Metallprofil" 38., "Himling System 600x600" 12.) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Other
            1 x IFCFLOWTERMINAL | object type "Vegghengt toalett" | names: "WC-GBG-Nautic_1522-Wall_Mounted:Vegghengt toalett:3618545" | material: materials ("Gustavsberg Chrome - Polished", "Gustavsberg Porcelain - White (with C+)", "Gustavsberg Plastic - White") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWTERMINAL | object type "Servant - Ecco 50x35" | names: "Ecco:Servant - Ecco 50x35:3626818" | material: materials ("Gustavsberg Chrome - Polished", "Gustavsberg Porcelain - White") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "Blandebatteri berøringsfri 1724FT" | object type "Blandebatteri berøringsfri 1724FT" | names: "1724FT(2013):Blandebatteri berøringsfri 1724FT:7575323" | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
        IFCSPACE "01012" | long name "wc" | INTERNAL
          contains 3 elements
            1 x IFCFLOWTERMINAL | object type "Servant - Ecco 50x35" | names: "Ecco:Servant - Ecco 50x35:3626588" | material: materials ("Gustavsberg Chrome - Polished", "Gustavsberg Porcelain - White") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWTERMINAL | object type "Vegghengt toalett" | names: "WC-GBG-Nautic_1522-Wall_Mounted:Vegghengt toalett:4798716" | material: materials ("Gustavsberg Chrome - Polished", "Gustavsberg Porcelain - White (with C+)", "Gustavsberg Plastic - White") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "Blandebatteri berøringsfri 1724FT" | object type "Blandebatteri berøringsfri 1724FT" | names: "1724FT(2013):Blandebatteri berøringsfri 1724FT:7575465" | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
        IFCSPACE "01017" | long name "heis" | INTERNAL
        IFCSPACE "01022" | long name "korridor" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | object type "Compound Ceiling:Himling System 600x1200" | CEILING | names: "Compound Ceiling:Himling System 600x1200:3051602" | material: layers "Compound Ceiling:Himling System 600x1200" ("Himling Metallprofil" 38., "Himling System 600x1200" 12.) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
        IFCSPACE "01023" | long name "forrom" | INTERNAL
          contains 4 elements
            1 x IFCCOVERING | object type "Compound Ceiling:Himling System 600x1200" | CEILING | names: "Compound Ceiling:Himling System 600x1200:3786856" | material: layers "Compound Ceiling:Himling System 600x1200" ("Himling Metallprofil" 38., "Himling System 600x1200" 12.) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Benkeplate 265mm, krogsæter" | object type "Benkeplate 265mm, krogsæter" | names: "N_CounterTop:Benkeplate 265mm, krogsæter:7788325" | material: "hvit malt" | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Benkeplate 265mm, krogsæter" | object type "Benkeplate 265mm, krogsæter" | names: "N_CounterTop:Benkeplate 265mm, krogsæter:7788516" | material: "hvit malt" | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Other, Phasing
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Benkeplate 265mm, krogsæter" | object type "Benkeplate 265mm, krogsæter" | names: "N_CounterTop:Benkeplate 265mm, krogsæter:7788671" | material: "hvit malt" | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
        IFCSPACE "01027" | long name "wc" | INTERNAL
          contains 4 elements
            1 x IFCCOVERING | object type "Compound Ceiling:Himling System 600x600" | CEILING | names: "Compound Ceiling:Himling System 600x600:3051322" | material: layers "Compound Ceiling:Himling System 600x600" ("Himling Metallprofil" 38., "Himling System 600x600" 12.) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Other
            1 x IFCFLOWTERMINAL | object type "Servant - Ecco 50x35" | names: "Ecco:Servant - Ecco 50x35:3630998" | material: materials ("Gustavsberg Chrome - Polished", "Gustavsberg Porcelain - White") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWTERMINAL | object type "Vegghengt toalett" | names: "WC-GBG-Nautic_1522-Wall_Mounted:Vegghengt toalett:3642975" | material: materials ("Gustavsberg Chrome - Polished", "Gustavsberg Porcelain - White (with C+)", "Gustavsberg Plastic - White") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "Blandebatteri berøringsfri 1724FT" | object type "Blandebatteri berøringsfri 1724FT" | names: "1724FT(2013):Blandebatteri berøringsfri 1724FT:7574960" | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
        IFCSPACE "01030" | long name "korridor" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | object type "Compound Ceiling:Himling System 600x1200" | CEILING | names: "Compound Ceiling:Himling System 600x1200:3051147" | material: layers "Compound Ceiling:Himling System 600x1200" ("Himling Metallprofil" 38., "Himling System 600x1200" 12.) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
        IFCSPACE "01046" | long name "disp" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | object type "Compound Ceiling:Himling System 600x600" | CEILING | names: "Compound Ceiling:Himling System 600x600:3051249" | material: layers "Compound Ceiling:Himling System 600x600" ("Himling Metallprofil" 38., "Himling System 600x600" 12.) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
        IFCSPACE "01047" | long name "korridor" | INTERNAL
          contains 2 elements
            1 x IFCCOVERING | object type "Compound Ceiling:Himling System 600x1200" | CEILING | names: "Compound Ceiling:Himling System 600x1200:4834334" | material: layers "Compound Ceiling:Himling System 600x1200" ("Himling Metallprofil" 38., "Himling System 600x1200" 12.) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Other
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Inkubator" | object type "Inkubator" | names: "Spesialutstyr:Inkubator:6302160" | material: "hvit malt" | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
        IFCSPACE "01053" | long name "sluse" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | object type "Compound Ceiling:Himling System 600x600" | CEILING | names: "Compound Ceiling:Himling System 600x600:2599529" | material: layers "Compound Ceiling:Himling System 600x600" ("Himling Metallprofil" 38., "Himling System 600x600" 12.) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Other
        IFCSPACE "01090" | long name "trapp" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | object type "Compound Ceiling:Himling System 600x600" | CEILING | names: "Compound Ceiling:Himling System 600x600:4418820" | material: layers "Compound Ceiling:Himling System 600x600" ("Himling Metallprofil" 38., "Himling System 600x600" 12.) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
        IFCSPACE "01093" | long name "wc" | INTERNAL
          contains 4 elements
            1 x IFCCOVERING | object type "Compound Ceiling:Himling System 600x600" | CEILING | names: "Compound Ceiling:Himling System 600x600:3051919" | material: layers "Compound Ceiling:Himling System 600x600" ("Himling Metallprofil" 38., "Himling System 600x600" 12.) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Other
            1 x IFCFLOWTERMINAL | object type "Servant - Ecco 50x35" | names: "Ecco:Servant - Ecco 50x35:3631199" | material: materials ("Gustavsberg Chrome - Polished", "Gustavsberg Porcelain - White") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWTERMINAL | object type "Vegghengt toalett" | names: "WC-GBG-Nautic_1522-Wall_Mounted:Vegghengt toalett:3647746" | material: materials ("Gustavsberg Chrome - Polished", "Gustavsberg Porcelain - White (with C+)", "Gustavsberg Plastic - White") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "Blandebatteri berøringsfri 1724FT" | object type "Blandebatteri berøringsfri 1724FT" | names: "1724FT(2013):Blandebatteri berøringsfri 1724FT:7574901" | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
        IFCSPACE "01094" | long name "wc" | INTERNAL
          contains 4 elements
            1 x IFCCOVERING | object type "Compound Ceiling:Himling System 600x600" | CEILING | names: "Compound Ceiling:Himling System 600x600:3051911" | material: layers "Compound Ceiling:Himling System 600x600" ("Himling Metallprofil" 38., "Himling System 600x600" 12.) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
            1 x IFCFLOWTERMINAL | object type "Servant - Ecco 50x35" | names: "Ecco:Servant - Ecco 50x35:3631136" | material: materials ("Gustavsberg Chrome - Polished", "Gustavsberg Porcelain - White") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWTERMINAL | object type "Vegghengt toalett" | names: "WC-GBG-Nautic_1522-Wall_Mounted:Vegghengt toalett:3647571" | material: materials ("Gustavsberg Chrome - Polished", "Gustavsberg Porcelain - White (with C+)", "Gustavsberg Plastic - White") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "Blandebatteri berøringsfri 1724FT" | object type "Blandebatteri berøringsfri 1724FT" | names: "1724FT(2013):Blandebatteri berøringsfri 1724FT:7574861" | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
        IFCSPACE "01095" | long name "wc" | INTERNAL
          contains 4 elements
            1 x IFCCOVERING | object type "Compound Ceiling:Himling System 600x600" | CEILING | names: "Compound Ceiling:Himling System 600x600:3051903" | material: layers "Compound Ceiling:Himling System 600x600" ("Himling Metallprofil" 38., "Himling System 600x600" 12.) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Other
            1 x IFCFLOWTERMINAL | object type "Servant - Ecco 50x35" | names: "Ecco:Servant - Ecco 50x35:3631085" | material: materials ("Gustavsberg Chrome - Polished", "Gustavsberg Porcelain - White") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWTERMINAL | object type "Vegghengt toalett" | names: "WC-GBG-Nautic_1522-Wall_Mounted:Vegghengt toalett:3647719" | material: materials ("Gustavsberg Chrome - Polished", "Gustavsberg Porcelain - White (with C+)", "Gustavsberg Plastic - White") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "Blandebatteri berøringsfri 1724FT" | object type "Blandebatteri berøringsfri 1724FT" | names: "1724FT(2013):Blandebatteri berøringsfri 1724FT:7574402" | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
        IFCSPACE "01092" | long name "korridor/sluse" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | object type "Compound Ceiling:Himling System 600x1200" | CEILING | names: "Compound Ceiling:Himling System 600x1200:3051939" | material: layers "Compound Ceiling:Himling System 600x1200" ("Himling Metallprofil" 38., "Himling System 600x1200" 12.) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Other
        IFCSPACE "01107" | long name "fellesområde" | INTERNAL
        IFCSPACE "01120" | long name "korridor" | INTERNAL
          contains 2 elements
            2 x IFCCOVERING | object type "Compound Ceiling:Himling System 600x1200" | CEILING | names: "Compound Ceiling:Himling System 600x1200:3054453", "Compound Ceiling:Himling System 600x1200:4474471" | material: layers "Compound Ceiling:Himling System 600x1200" ("Himling Metallprofil" 38., "Himling System 600x1200" 12.) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
        IFCSPACE "01105" | long name "wc" | INTERNAL
          contains 4 elements
            1 x IFCCOVERING | object type "Compound Ceiling:Himling System 600x600" | CEILING | names: "Compound Ceiling:Himling System 600x600:3049745" | material: layers "Compound Ceiling:Himling System 600x600" ("Himling Metallprofil" 38., "Himling System 600x600" 12.) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Other
            1 x IFCFLOWTERMINAL | object type "Servant - Ecco 50x35" | names: "Ecco:Servant - Ecco 50x35:3631409" | material: materials ("Gustavsberg Chrome - Polished", "Gustavsberg Porcelain - White") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWTERMINAL | object type "Vegghengt toalett" | names: "WC-GBG-Nautic_1522-Wall_Mounted:Vegghengt toalett:3642661" | material: materials ("Gustavsberg Chrome - Polished", "Gustavsberg Porcelain - White (with C+)", "Gustavsberg Plastic - White") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "Blandebatteri berøringsfri 1724FT" | object type "Blandebatteri berøringsfri 1724FT" | names: "1724FT(2013):Blandebatteri berøringsfri 1724FT:7575110" | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
        IFCSPACE "01106" | long name "wc" | INTERNAL
          contains 4 elements
            1 x IFCCOVERING | object type "Compound Ceiling:Himling System 600x600" | CEILING | names: "Compound Ceiling:Himling System 600x600:3049708" | material: layers "Compound Ceiling:Himling System 600x600" ("Himling Metallprofil" 38., "Himling System 600x600" 12.) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Other
            1 x IFCFLOWTERMINAL | object type "Servant - Ecco 50x35" | names: "Ecco:Servant - Ecco 50x35:3631326" | material: materials ("Gustavsberg Chrome - Polished", "Gustavsberg Porcelain - White") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWTERMINAL | object type "Vegghengt toalett" | names: "WC-GBG-Nautic_1522-Wall_Mounted:Vegghengt toalett:3642556" | material: materials ("Gustavsberg Chrome - Polished", "Gustavsberg Porcelain - White (with C+)", "Gustavsberg Plastic - White") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "Blandebatteri berøringsfri 1724FT" | object type "Blandebatteri berøringsfri 1724FT" | names: "1724FT(2013):Blandebatteri berøringsfri 1724FT:7575057" | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
        IFCSPACE "01141" | long name "korridor" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | object type "Compound Ceiling:Himling System 600x1200" | CEILING | names: "Compound Ceiling:Himling System 600x1200:3054753" | material: layers "Compound Ceiling:Himling System 600x1200" ("Himling Metallprofil" 38., "Himling System 600x1200" 12.) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
        IFCSPACE "01121" | long name "korridor" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | object type "Compound Ceiling:Himling System 600x1200" | CEILING | names: "Compound Ceiling:Himling System 600x1200:3049671" | material: layers "Compound Ceiling:Himling System 600x1200" ("Himling Metallprofil" 38., "Himling System 600x1200" 12.) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Other
        IFCSPACE "01152" | long name "sjakt" | INTERNAL
        IFCSPACE "01131" | long name "bk" | INTERNAL
          contains 2 elements
            1 x IFCFLOWTERMINAL | object type "Utslagsvask" | names: "intra_gub1_bucket_sink_wall_mounted:Utslagsvask:3639123" | material: "f26d4e4b_a025_4dbf_b085_30ed485788cf" | property sets: Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data, Mechanical
            1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "Blandebatteri 3970" | object type "Blandebatteri 3970" | names: "Oras Saga:Blandebatteri 3970:7601640" | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
        IFCSPACE "01096" | long name "sluse" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | object type "Compound Ceiling:Himling System 600x1200" | CEILING | names: "Compound Ceiling:Himling System 600x1200:2599959" | material: layers "Compound Ceiling:Himling System 600x1200" ("Himling Metallprofil" 38., "Himling System 600x1200" 12.) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
        IFCSPACE "01150" | long name "sjakt" | INTERNAL
        IFCSPACE "01147" | long name "forrom" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | object type "Compound Ceiling:Himling System 600x600 hygiene korrosjonsklasse" | CEILING | names: "Compound Ceiling:Himling System 600x600 hygiene korrosjonsklasse:3050586" | material: layers "Compound Ceiling:Himling System 600x600 hygiene korrosjonsklasse" ("Himling Metallprofil" 38., "Himling System 600x600" 12.) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
        IFCSPACE "01161" | long name "temperert sykkelbod" | INTERNAL
        IFCSPACE "01162" | long name "vaktm" | INTERNAL
        IFCSPACE "2" | long name "Area" | INTERNAL
        IFCSPACE "01153" | long name "sjakt" | INTERNAL
        IFCSPACE "01160" | long name "sykkelparkering" | INTERNAL
        IFCSPACE "20" | long name "Area" | INTERNAL
        IFCSPACE "4" | long name "Area" | INTERNAL
        IFCSPACE "6" | long name "Area" | INTERNAL
        IFCSPACE "7" | long name "Area" | INTERNAL
        IFCSPACE "6" | long name "Area" | INTERNAL
        IFCSPACE "7" | long name "Area" | INTERNAL
        IFCSPACE "8" | long name "Area" | INTERNAL
        IFCSPACE "9" | long name "Area" | INTERNAL
        IFCSPACE "10" | long name "Area" | INTERNAL
        IFCSPACE "11" | long name "Area" | INTERNAL
        IFCSPACE "01170" | long name "Utebod-Nat-M&H" | INTERNAL
        IFCSPACE "01171" | long name "sykkelparkering" | INTERNAL
        IFCSPACE "01163" | long name "Vaskerom sykkel" | INTERNAL
          contains 1 element
            1 x IFCFLOWTERMINAL | object type "Spyling sykler" | names: "Vann:Spyling sykler:5272853" | material: "Aluminum" | property sets: Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data, Other
        IFCSPACE "14" | long name "Area" | INTERNAL
        IFCSPACE "21" | long name "Area" | INTERNAL
      IFCBUILDINGSTOREY "Plan 02" | long name "Plan 02" | elevation 3999.99999999709
        contains 671 elements
          7 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:YV 1.1 517mm" | object type "Basic Wall:YV 1.1 517mm:1735105" | names: "Basic Wall:YV 1.1 517mm:1663810", "Basic Wall:YV 1.1 517mm:1696951", "Basic Wall:YV 1.1 517mm:1700386" (+4 more) | material: layers "Basic Wall:YV 1.1 517mm" ("Trekledning" 19., "Luftsjikt" 48., "Luftsjikt" 36., "Luftsjikt" 48., "Vindsperre" 9., "Stender isolert vegg" 296., "NO_Utlekting" 48., "Robustgips" 12.5) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          2 x IFCSLAB | object type "Floor:Betongdekke 320 + 30 avretting" | FLOOR | names: "Floor:Betongdekke 320 + 30 avretting:1663900", "Floor:Betongdekke 320 + 30 avretting:2409771" | material: layers "Floor:Betongdekke 320 + 30 avretting" ("Betong avretting" 30., "Betong" 320.) | property sets: Pset_SlabCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          8 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 3.3 145mm 48dB EI60 (RN-95-NR)" | object type "Basic Wall:IVA 3.3 145mm 48dB EI60 (RN-95-NR):2860483" | names: "Basic Wall:IVA 3.3 145mm 48dB EI60 (RN-95-NR):1696687", "Basic Wall:IVA 3.3 145mm 48dB EI60 (RN-95-NR):1782274", "Basic Wall:IVA 3.3 145mm 48dB EI60 (RN-95-NR):1835963" (+5 more) | material: layers "Basic Wall:IVA 3.3 145mm 48dB EI60 (RN-95-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          10 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 2.3 134mm 34dB (R-95-NR)" | object type "Basic Wall:IVA 2.3 134mm 34dB (R-95-NR):4809032" | names: "Basic Wall:IVA 2.3 134mm 34dB (R-95-NR):1698947", "Basic Wall:IVA 2.3 134mm 34dB (R-95-NR):1825614", "Basic Wall:IVA 2.3 134mm 34dB (R-95-NR):1866286" (+7 more) | material: layers "Basic Wall:IVA 2.3 134mm 34dB (R-95-NR)" ("Robustgips" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          5 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 1.1T 121mm 44dB (H-95-H)" | object type "Basic Wall:IVA 1.1T 121mm 44dB (H-95-H):6691464" | names: "Basic Wall:IVA 1.1T 121mm 44dB (H-95-H):1700390", "Basic Wall:IVA 1.1T 121mm 44dB (H-95-H):1904134", "Basic Wall:IVA 1.1T 121mm 44dB (H-95-H):2069230" (+2 more) | material: layers "Basic Wall:IVA 1.1T 121mm 44dB (H-95-H)" ("Habito" 13., "stender/isolasjon" 95., "Habito" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          27 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 1.1 121mm 44dB (H-95-H)" | object type "Basic Wall:IVA 1.1 121mm 44dB (H-95-H):4807508" | names: "Basic Wall:IVA 1.1 121mm 44dB (H-95-H):1700429", "Basic Wall:IVA 1.1 121mm 44dB (H-95-H):1720482", "Basic Wall:IVA 1.1 121mm 44dB (H-95-H):1904147" (+24 more) | material: layers "Basic Wall:IVA 1.1 121mm 44dB (H-95-H)" ("Habito" 13., "stender/isolasjon" 95., "Habito" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 3.3T 145mm 48dB (RN-95-NR)" | object type "Basic Wall:IVA 3.3T 145mm 48dB (RN-95-NR):6701502" | names: "Basic Wall:IVA 3.3T 145mm 48dB (RN-95-NR):1700439", "Basic Wall:IVA 3.3T 145mm 48dB (RN-95-NR):4046256" | material: layers "Basic Wall:IVA 3.3T 145mm 48dB (RN-95-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          1 x IFCDOOR | type IFCDOORSTYLE "IDA 7.1 15x21M EI60CS" | object type "IDA 7.1 15x21M EI60CS" | names: "Enfløyet_aludør:IDA 7.1 15x21M EI60CS:1700923" | material: materials ("Karm Malt", "Lys grå", "Terskel Tre") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          2 x IFCDOOR | type IFCDOORSTYLE "IDA 7.1 15x21M EI60CS" | object type "IDA 7.1 15x21M EI60CS" | names: "Enfløyet_aludør:IDA 7.1 15x21M EI60CS:1700924", "Enfløyet_aludør:IDA 7.1 15x21M EI60CS:2539298" | material: materials ("Karm Malt", "Lys grå", "Terskel Tre") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          2 x IFCDOOR | type IFCDOORSTYLE "IDA 6.2 12x21M EI 30CS" | object type "IDA 6.2 12x21M EI 30CS" | names: "Dør Enkel_ Glassfelt:IDA 6.2 12x21M EI 30CS:1700926", "Dør Enkel_ Glassfelt:IDA 6.2 12x21M EI 30CS:1848774" | material: materials ("Lys grå", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          4 x IFCDOOR | type IFCDOORSTYLE "IDT 1.2 8x21M 33dB" | object type "IDT 1.2 8x21M 33dB" | names: "Dør Enkel:IDT 1.2 8x21M 33dB:1725481", "Dør Enkel:IDT 1.2 8x21M 33dB:1881850", "Dør Enkel:IDT 1.2 8x21M 33dB:2172911" (+1 more) | material: materials ("Terskel Tre", "NCS S 0500-N", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          8 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 2.1 134mm 48dB (H-95-NH)" | object type "Basic Wall:IVA 2.1 134mm 48dB (H-95-NH):4807019" | names: "Basic Wall:IVA 2.1 134mm 48dB (H-95-NH):1726620", "Basic Wall:IVA 2.1 134mm 48dB (H-95-NH):1781370", "Basic Wall:IVA 2.1 134mm 48dB (H-95-NH):1825609" (+5 more) | material: layers "Basic Wall:IVA 2.1 134mm 48dB (H-95-NH)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 95., "Habito" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          14 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 3.3 145mm EI60 (RN-95-NR)" | object type "Basic Wall:IVA 3.3 145mm EI60 (RN-95-NR):2850935" | names: "Basic Wall:IVA 3.3 145mm EI60 (RN-95-NR):1727393", "Basic Wall:IVA 3.3 145mm EI60 (RN-95-NR):1737417", "Basic Wall:IVA 3.3 145mm EI60 (RN-95-NR):1847862" (+11 more) | material: layers "Basic Wall:IVA 3.3 145mm EI60 (RN-95-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 1.1 121mm 34dB (H-95-H)" | object type "Basic Wall:IVA 1.1 121mm 34dB (H-95-H):4819050" | names: "Basic Wall:IVA 1.1 121mm 34dB (H-95-H):1728453", "Basic Wall:IVA 1.1 121mm 34dB (H-95-H):5416387" | material: layers "Basic Wall:IVA 1.1 121mm 34dB (H-95-H)" ("Habito" 13., "stender/isolasjon" 95., "Habito" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:YV 3.1 306mm EI60" | object type "Basic Wall:YV 3.1 306mm EI60:2905012" | names: "Basic Wall:YV 3.1 306mm EI60:1728541", "Basic Wall:YV 3.1 306mm EI60:2905601", "Basic Wall:YV 3.1 306mm EI60:3026546" | material: layers "Basic Wall:YV 3.1 306mm EI60" ("Trekledning" 19., "Luftsjikt" 48., "Luftsjikt" 36., "Luftsjikt" 48., "Vindsperre" 9., "Stender isolert vegg" 146.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCDOOR | type IFCDOORSTYLE "IDA 2.2 15x21M EI60SC" | object type "IDA 2.2 15x21M EI60SC" | names: "Dør Dobbel_Ulike_Dørblader:IDA 2.2 15x21M EI60SC:1728746" | material: materials ("Lys grå", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          2 x IFCWINDOW | type IFCWINDOWSTYLE "V23 14x14" | object type "V23 14x14" | names: "Vindu-Hengslet:V23 14x14:1761672", "Vindu-Hengslet:V23 14x14:2392852" | material: materials ("Glass Klart", "NCS S 0502-Y", "Karm Malt") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 2.1 134mm 44dB (H-95-NH)" | object type "Basic Wall:IVA 2.1 134mm 44dB (H-95-NH):4808479" | names: "Basic Wall:IVA 2.1 134mm 44dB (H-95-NH):1772801", "Basic Wall:IVA 2.1 134mm 44dB (H-95-NH):1904143" | material: layers "Basic Wall:IVA 2.1 134mm 44dB (H-95-NH)" ("Habito" 13., "stender/isolasjon" 95., "Gips" 13., "Habito" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 2.3 10x21M 33dB" | object type "IDT 2.3 10x21M 33dB" | names: "Dør Enkel:IDT 2.3 10x21M 33dB:1779794" | material: materials ("Terskel Tre", "Lys grå", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 11.1 193mm 48dB (RN-95-NR)" | object type "Basic Wall:IVA 11.1 193mm 48dB (RN-95-NR):6718454" | names: "Basic Wall:IVA 11.1 193mm 48dB (RN-95-NR):1780829" | material: layers "Basic Wall:IVA 11.1 193mm 48dB (RN-95-NR)" ("Robustgips" 13., "<Unnamed>" 13., "<Unnamed>" 10., "stender/isolasjon" 98., "<Unnamed>" 20., "<Unnamed>" 48., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCDOOR | type IFCDOORSTYLE "IDF 2.1 Foldevegg 8000x2800" | object type "IDF 2.1 Foldevegg 8000x2800" | names: "Side_Stack_Operable_Wall_8000:IDF 2.1 Foldevegg 8000x2800:1780830" | material: materials ("Light grey", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 3.3T 145mm 48dB EI60 (RN-95-NR)" | object type "Basic Wall:IVA 3.3T 145mm 48dB EI60 (RN-95-NR):6691651" | names: "Basic Wall:IVA 3.3T 145mm 48dB EI60 (RN-95-NR):1781147", "Basic Wall:IVA 3.3T 145mm 48dB EI60 (RN-95-NR):1904045" | material: layers "Basic Wall:IVA 3.3T 145mm 48dB EI60 (RN-95-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          13 x IFCDOOR | type IFCDOORSTYLE "IDT 3.6 10x21M 38dB" | object type "IDT 3.6 10x21M 38dB" | names: "Dør Enkel_ Glassfelt:IDT 3.6 10x21M 38dB:1781401", "Dør Enkel_ Glassfelt:IDT 3.6 10x21M 38dB:1825699", "Dør Enkel_ Glassfelt:IDT 3.6 10x21M 38dB:1858179" (+10 more) | material: materials ("NCS S 2500-N", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 3.3 145mm 48dB EI30 (RN-95-NR) 2" | object type "Basic Wall:IVA 3.3 145mm 48dB EI30 (RN-95-NR) 2:6214229" | names: "Basic Wall:IVA 3.3 145mm 48dB EI30 (RN-95-NR) 2:1825525" | material: layers "Basic Wall:IVA 3.3 145mm 48dB EI30 (RN-95-NR) 2" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:YV 9.1 500mm uisolert" | object type "Basic Wall:YV 9.1 500mm uisolert:4333404" | names: "Basic Wall:YV 9.1 500mm uisolert:1825526" | material: layers "Basic Wall:YV 9.1 500mm uisolert" ("Trekledning" 19., "Luftsjikt" 48., "Luftsjikt" 36., "Luftsjikt" 48., "Vindsperre" 9., "stender" 296., "Luftsjikt" 36., "Cembrit Metro Amsterdam" 8.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          10 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 3.3 145mm 34dB (RN-95-NR)" | object type "Basic Wall:IVA 3.3 145mm 34dB (RN-95-NR):2849806" | names: "Basic Wall:IVA 3.3 145mm 34dB (RN-95-NR):1825563", "Basic Wall:IVA 3.3 145mm 34dB (RN-95-NR):1825728", "Basic Wall:IVA 3.3 145mm 34dB (RN-95-NR):1925054" (+7 more) | material: layers "Basic Wall:IVA 3.3 145mm 34dB (RN-95-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          9 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 3.3 145mm 48dB (RN-95-NR)" | object type "Basic Wall:IVA 3.3 145mm 48dB (RN-95-NR):2849733" | names: "Basic Wall:IVA 3.3 145mm 48dB (RN-95-NR):1825615", "Basic Wall:IVA 3.3 145mm 48dB (RN-95-NR):1825705", "Basic Wall:IVA 3.3 145mm 48dB (RN-95-NR):1825724" (+6 more) | material: layers "Basic Wall:IVA 3.3 145mm 48dB (RN-95-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          13 x IFCDOOR | type IFCDOORSTYLE "IDT 3.6 10x21M 38dB" | object type "IDT 3.6 10x21M 38dB" | names: "Dør Enkel_ Glassfelt:IDT 3.6 10x21M 38dB:1825698", "Dør Enkel_ Glassfelt:IDT 3.6 10x21M 38dB:1904148", "Dør Enkel_ Glassfelt:IDT 3.6 10x21M 38dB:1904159" (+10 more) | material: materials ("NCS S 2500-N", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 4.3 172mm 48dB EI60 (RN-120-NR)" | object type "Basic Wall:IVA 4.3 172mm 48dB EI60 (RN-120-NR):4410969" | names: "Basic Wall:IVA 4.3 172mm 48dB EI60 (RN-120-NR):1825704" | material: layers "Basic Wall:IVA 4.3 172mm 48dB EI60 (RN-120-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 120., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:YV 8.3 458mm gul platekledning EI60" | object type "Basic Wall:YV 8.3 458mm gul platekledning EI60:6744466" | names: "Basic Wall:YV 8.3 458mm gul platekledning EI60:1834005" | material: layers "Basic Wall:YV 8.3 458mm gul platekledning EI60" ("Cembrit Metro Amsterdam" 8., "Luftsjikt" 36., "Luftsjikt" 48., "Vindsperre" 9., "Stender isolert vegg" 296., "NO_Utlekting" 48., "Gips" 12.5, "Gips" 12.5) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:YV 7.5 410mm gul platekledning EI60" | object type "Basic Wall:YV 7.5 410mm gul platekledning EI60:2905155" | names: "Basic Wall:YV 7.5 410mm gul platekledning EI60:1834137" | material: layers "Basic Wall:YV 7.5 410mm gul platekledning EI60" ("Cembrit Metro Amsterdam" 8., "Luftsjikt" 36., "Vindsperre" 9., "Stender isolert vegg" 296., "NO_Utlekting" 48., "Branngips" 15.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCDOOR | type IFCDOORSTYLE "YDA 5.2 16x21M EI 30S" | object type "YDA 5.2 16x21M EI 30S" | names: "_Dør Dobbel_Ulike_Dørblader_Glassfelt:YDA 5.2 16x21M EI 30S:1835036" | material: materials ("Glass Klart", "Lys grå", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 4.1 172mm 34dB (HN-120-NH)" | object type "Basic Wall:IVA 4.1 172mm 34dB (HN-120-NH):4860180" | names: "Basic Wall:IVA 4.1 172mm 34dB (HN-120-NH):1837645" | material: layers "Basic Wall:IVA 4.1 172mm 34dB (HN-120-NH)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 120., "Gips" 13., "Habito" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 6.1 302mm 34dB (HN-95-60-95-NH)" | object type "Basic Wall:IVA 6.1 302mm 34dB (HN-95-60-95-NH):4828119" | names: "Basic Wall:IVA 6.1 302mm 34dB (HN-95-60-95-NH):1837646", "Basic Wall:IVA 6.1 302mm 34dB (HN-95-60-95-NH):4034682" | material: layers "Basic Wall:IVA 6.1 302mm 34dB (HN-95-60-95-NH)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 95., "Luftsjikt" 60., "stender/isolasjon" 95., "Gips" 13., "Habito" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 6.1 15x21M 33dB" | object type "IDT 6.1 15x21M 33dB" | names: "_Dør Dobbel_Ulike_Dørblader_Glassfelt2:IDT 6.1 15x21M 33dB:1837647" | material: materials ("Glass Klart", "Lys grå", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 1.1T 121mm 34dB (H-95-H)" | object type "Basic Wall:IVA 1.1T 121mm 34dB (H-95-H):6702432" | names: "Basic Wall:IVA 1.1T 121mm 34dB (H-95-H):1837946", "Basic Wall:IVA 1.1T 121mm 34dB (H-95-H):2083372", "Basic Wall:IVA 1.1T 121mm 34dB (H-95-H):2083464" | material: layers "Basic Wall:IVA 1.1T 121mm 34dB (H-95-H)" ("Habito" 13., "stender/isolasjon" 95., "Habito" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 3.3 10x21M 33dB" | object type "IDT 3.3 10x21M 33dB" | names: "Dør Enkel_ Glassfelt:IDT 3.3 10x21M 33dB:1841845" | material: materials ("Lys grå", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDA 6.2 12x21M EI 30CS" | object type "IDA 6.2 12x21M EI 30CS" | names: "Dør Enkel_ Glassfelt:IDA 6.2 12x21M EI 30CS:1848683" | material: materials ("Lys grå", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          2 x IFCDOOR | type IFCDOORSTYLE "IDA 3.1 18x21M 33db EI30S" | object type "IDA 3.1 18x21M 33db EI30S" | names: "_Dør Dobbel_Ulike_Dørblader_Glassfelt:IDA 3.1 18x21M 33db EI30S:1852022", "_Dør Dobbel_Ulike_Dørblader_Glassfelt:IDA 3.1 18x21M 33db EI30S:2069215" | material: materials ("Glass Klart", "Lys grå", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          17 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 7.1 121mm 37dB EI30 (95-NR)" | object type "Basic Wall:IVA 7.1 121mm 37dB EI30 (95-NR):6023854" | names: "Basic Wall:IVA 7.1 121mm 37dB EI30 (95-NR):1857416", "Basic Wall:IVA 7.1 121mm 37dB EI30 (95-NR):2184218", "Basic Wall:IVA 7.1 121mm 37dB EI30 (95-NR):2347970" (+14 more) | material: layers "Basic Wall:IVA 7.1 121mm 37dB EI30 (95-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 2.3 10x21M 33dB" | object type "IDT 2.3 10x21M 33dB" | names: "Dør Enkel:IDT 2.3 10x21M 33dB:1857757" | material: materials ("Terskel Tre", "Lys grå", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          2 x IFCDOOR | type IFCDOORSTYLE "IDT 3.3 10x21M 33dB" | object type "IDT 3.3 10x21M 33dB" | names: "Dør Enkel_ Glassfelt:IDT 3.3 10x21M 33dB:1863225", "Dør Enkel_ Glassfelt:IDT 3.3 10x21M 33dB:3088168" | material: materials ("Lys grå", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 2.1 10x21M" | object type "IDT 2.1 10x21M" | names: "Dør Enkel:IDT 2.1 10x21M:1866280" | material: materials ("_White", "NCS S 0500-N", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDA 3.1 18x21M 33db EI30S" | object type "IDA 3.1 18x21M 33db EI30S" | names: "_Dør Dobbel_Ulike_Dørblader_Glassfelt:IDA 3.1 18x21M 33db EI30S:1870405" | material: materials ("Glass Klart", "Lys grå", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 1.3 121mm 34dB (R-95-R)" | object type "Basic Wall:IVA 1.3 121mm 34dB (R-95-R):4808382" | names: "Basic Wall:IVA 1.3 121mm 34dB (R-95-R):1870768", "Basic Wall:IVA 1.3 121mm 34dB (R-95-R):1881846", "Basic Wall:IVA 1.3 121mm 34dB (R-95-R):4816573" (+1 more) | material: layers "Basic Wall:IVA 1.3 121mm 34dB (R-95-R)" ("Robustgips" 13., "stender/isolasjon" 95., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 8.1T 125mm sjaktvegg 48dB EI60" | object type "Basic Wall:IVA 8.1T 125mm sjaktvegg 48dB EI60:6702676" | names: "Basic Wall:IVA 8.1T 125mm sjaktvegg 48dB EI60:1872423" | material: layers "Basic Wall:IVA 8.1T 125mm sjaktvegg 48dB EI60" ("Branngips" 15., "Branngips" 15., "stender/isolasjon" 95.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 4.3 172mm 34dB (RN-120-NR)" | object type "Basic Wall:IVA 4.3 172mm 34dB (RN-120-NR):4859885" | names: "Basic Wall:IVA 4.3 172mm 34dB (RN-120-NR):1881845", "Basic Wall:IVA 4.3 172mm 34dB (RN-120-NR):2275791", "Basic Wall:IVA 4.3 172mm 34dB (RN-120-NR):3846919" | material: layers "Basic Wall:IVA 4.3 172mm 34dB (RN-120-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 120., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 1.2 121mm 34dB (R-95-H)" | object type "Basic Wall:IVA 1.2 121mm 34dB (R-95-H):4824661" | names: "Basic Wall:IVA 1.2 121mm 34dB (R-95-H):1881847" | material: layers "Basic Wall:IVA 1.2 121mm 34dB (R-95-H)" ("Habito" 13., "stender/isolasjon" 95., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 7.1 121mm 37dB (95-NR)" | object type "Basic Wall:IVA 7.1 121mm 37dB (95-NR):6445986" | names: "Basic Wall:IVA 7.1 121mm 37dB (95-NR):1881848", "Basic Wall:IVA 7.1 121mm 37dB (95-NR):3847509" | material: layers "Basic Wall:IVA 7.1 121mm 37dB (95-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          2 x IFCDOOR | type IFCDOORSTYLE "IDT 1.2 8x21M 33dB" | object type "IDT 1.2 8x21M 33dB" | names: "Dør Enkel:IDT 1.2 8x21M 33dB:1881849", "Dør Enkel:IDT 1.2 8x21M 33dB:1881851" | material: materials ("Terskel Tre", "NCS S 0500-N", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 1.1 8x21M" | object type "IDT 1.1 8x21M" | names: "Dør Enkel:IDT 1.1 8x21M:1881980" | material: materials ("Terskel Tre", "Lys grå", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 2.1T 134mm 44dB (H-95-NH)" | object type "Basic Wall:IVA 2.1T 134mm 44dB (H-95-NH):6702437" | names: "Basic Wall:IVA 2.1T 134mm 44dB (H-95-NH):1884499" | material: layers "Basic Wall:IVA 2.1T 134mm 44dB (H-95-NH)" ("Habito" 13., "stender/isolasjon" 95., "Gips" 13., "Habito" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 3.6 10x21M 38dB" | object type "IDT 3.6 10x21M 38dB" | names: "Dør Enkel_ Glassfelt:IDT 3.6 10x21M 38dB:1886980" | material: materials ("NCS S 2500-N", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          4 x IFCWINDOW | type IFCWINDOWSTYLE "V3 18x22" | object type "V3 18x22" | names: "Vindu-Fast:V3 18x22:1892833", "Vindu-Fast:V3 18x22:1895999", "Vindu-Fast:V3 18x22:2399566" (+1 more) | material: materials ("N_Windows - Glass", "NCS S 0502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          6 x IFCWINDOW | type IFCWINDOWSTYLE "V4 23x22" | object type "V4 23x22" | names: "Vindu-Fast:V4 23x22:1896885", "Vindu-Fast:V4 23x22:1897872", "Vindu-Fast:V4 23x22:1926043" (+3 more) | material: materials ("Glass Klart", "NCS S 0502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "V22 14x14" | object type "V22 14x14" | names: "Vindu-Fast:V22 14x14:1897688" | material: materials ("Glass Klart", "NCS S 0502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          3 x IFCWINDOW | type IFCWINDOWSTYLE "V1 12x22" | object type "V1 12x22" | names: "Vindu-Hengslet_1200 opening:V1 12x22:1898390", "Vindu-Hengslet_1200 opening:V1 12x22:1899682", "Vindu-Hengslet_1200 opening:V1 12x22:1899684" | material: materials ("NCS S 0502-Y", "Glass Klart") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          4 x IFCWINDOW | type IFCWINDOWSTYLE "V1 12x22" | object type "V1 12x22" | names: "Vindu-Hengslet_1200 opening:V1 12x22:1898690", "Vindu-Hengslet_1200 opening:V1 12x22:2258110", "Vindu-Hengslet_1200 opening:V1 12x22:2259432" (+1 more) | material: materials ("NCS S 0502-Y", "Glass Klart") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          3 x IFCWINDOW | type IFCWINDOWSTYLE "V3 18x22" | object type "V3 18x22" | names: "Vindu-Fast:V3 18x22:1899683", "Vindu-Fast:V3 18x22:2258481", "Vindu-Fast:V3 18x22:2260402" | material: materials ("N_Windows - Glass", "NCS S 0502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          4 x IFCWINDOW | type IFCWINDOWSTYLE "V4 23x22" | object type "V4 23x22" | names: "Vindu-Fast:V4 23x22:1899685", "Vindu-Fast:V4 23x22:2257995", "Vindu-Fast:V4 23x22:2258672" (+1 more) | material: materials ("Glass Klart", "NCS S 0502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "V22 14x14" | object type "V22 14x14" | names: "Vindu-Fast:V22 14x14:1901278" | material: materials ("Glass Klart", "NCS S 0502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDA 3.1 18x21M 33db EI30S" | object type "IDA 3.1 18x21M 33db EI30S" | names: "_Dør Dobbel_Ulike_Dørblader_Glassfelt:IDA 3.1 18x21M 33db EI30S:1904044" | material: materials ("Glass Klart", "Lys grå", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 2.1T 134mm 48dB (H-95-NH)" | object type "Basic Wall:IVA 2.1T 134mm 48dB (H-95-NH):6691061" | names: "Basic Wall:IVA 2.1T 134mm 48dB (H-95-NH):1904128", "Basic Wall:IVA 2.1T 134mm 48dB (H-95-NH):2161148", "Basic Wall:IVA 2.1T 134mm 48dB (H-95-NH):4806748" | material: layers "Basic Wall:IVA 2.1T 134mm 48dB (H-95-NH)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 95., "Habito" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          4 x IFCDOOR | type IFCDOORSTYLE "IDT 3.6 10x21M 38dB" | object type "IDT 3.6 10x21M 38dB" | names: "Dør Enkel_ Glassfelt:IDT 3.6 10x21M 38dB:1904138", "Dør Enkel_ Glassfelt:IDT 3.6 10x21M 38dB:1904139", "Dør Enkel_ Glassfelt:IDT 3.6 10x21M 38dB:2996292" (+1 more) | material: materials ("NCS S 2500-N", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 3.6 10x21M 38dB" | object type "IDT 3.6 10x21M 38dB" | names: "Dør Enkel_ Glassfelt:IDT 3.6 10x21M 38dB:1904144" | material: materials ("NCS S 2500-N", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 3.6 10x21M 38dB" | object type "IDT 3.6 10x21M 38dB" | names: "Dør Enkel_ Glassfelt:IDT 3.6 10x21M 38dB:1904145" | material: materials ("NCS S 2500-N", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 3.1 F 145mm 48dB (HN-95-NH)" | object type "Basic Wall:IVA 3.1 F 145mm 48dB (HN-95-NH):7123985" | names: "Basic Wall:IVA 3.1 F 145mm 48dB (HN-95-NH):1904150" | material: layers "Basic Wall:IVA 3.1 F 145mm 48dB (HN-95-NH)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Habito" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 1.1 F 121mm 44dB (H-95-H)" | object type "Basic Wall:IVA 1.1 F 121mm 44dB (H-95-H):7123743" | names: "Basic Wall:IVA 1.1 F 121mm 44dB (H-95-H):1904153" | material: layers "Basic Wall:IVA 1.1 F 121mm 44dB (H-95-H)" ("Habito" 13., "stender/isolasjon" 95., "Habito" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 3.6 10x21M 38dB" | object type "IDT 3.6 10x21M 38dB" | names: "Dør Enkel_ Glassfelt:IDT 3.6 10x21M 38dB:1904154" | material: materials ("NCS S 2500-N", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 2.1 134mm 34dB (H-95-NH)" | object type "Basic Wall:IVA 2.1 134mm 34dB (H-95-NH):4843176" | names: "Basic Wall:IVA 2.1 134mm 34dB (H-95-NH):1904997" | material: layers "Basic Wall:IVA 2.1 134mm 34dB (H-95-NH)" ("Habito" 13., "stender/isolasjon" 95., "Gips" 13., "Habito" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 2.3T 134mm 34dB (R-95-NR)" | object type "Basic Wall:IVA 2.3T 134mm 34dB (R-95-NR):6701505" | names: "Basic Wall:IVA 2.3T 134mm 34dB (R-95-NR):1913527", "Basic Wall:IVA 2.3T 134mm 34dB (R-95-NR):2083460" | material: layers "Basic Wall:IVA 2.3T 134mm 34dB (R-95-NR)" ("Robustgips" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCBUILDINGELEMENTPROXY | object type "Model Text:350mm Arial 2" | names: "Model Text:350mm Arial 2" | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Graphics, Identity Data
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 6.3 272mm 55dB EI60 (RN-95-30-95-NR)" | object type "Basic Wall:IVA 6.3 272mm 55dB EI60 (RN-95-30-95-NR):2851985" | names: "Basic Wall:IVA 6.3 272mm 55dB EI60 (RN-95-30-95-NR):1925732", "Basic Wall:IVA 6.3 272mm 55dB EI60 (RN-95-30-95-NR):2147852", "Basic Wall:IVA 6.3 272mm 55dB EI60 (RN-95-30-95-NR):2575347" (+1 more) | material: layers "Basic Wall:IVA 6.3 272mm 55dB EI60 (RN-95-30-95-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95., "Luftsjikt" 30., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCCOVERING | object type "Compound Ceiling:Himling spiler" | CEILING | names: "Compound Ceiling:Himling spiler:1929856" | material: layers "Compound Ceiling:Himling spiler" ("Himling Metallprofil" 48., "Spiler" 34.) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 5.2 15x21M EI60S" | object type "IDT 5.2 15x21M EI60S" | names: "Dør Dobbel:IDT 5.2 15x21M EI60S:1937235" | material: materials ("NCS S 1000-N", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          3 x IFCDOOR | type IFCDOORSTYLE "IDT 5.2 15x21M EI60S" | object type "IDT 5.2 15x21M EI60S" | names: "Dør Dobbel:IDT 5.2 15x21M EI60S:1937292", "Dør Dobbel:IDT 5.2 15x21M EI60S:2180852", "Dør Dobbel:IDT 5.2 15x21M EI60S:2181750" | material: materials ("NCS S 1000-N", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IV 50 - skillevegg" | object type "Basic Wall:IV 50 - skillevegg:425527" | names: "Basic Wall:IV 50 - skillevegg:1939986", "Basic Wall:IV 50 - skillevegg:2147854", "Basic Wall:IV 50 - skillevegg:2276115" | material: layers "Basic Wall:IV 50 - skillevegg" ("<Unnamed>" 50.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 3.3 10x21M 33dB" | object type "IDT 3.3 10x21M 33dB" | names: "Dør Enkel_ Glassfelt:IDT 3.3 10x21M 33dB:1941435" | material: materials ("Lys grå", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 10.1 193mm 48dB (RN-95-NR)" | object type "Basic Wall:IVA 10.1 193mm 48dB (RN-95-NR):6681277" | names: "Basic Wall:IVA 10.1 193mm 48dB (RN-95-NR):2031438" | material: layers "Basic Wall:IVA 10.1 193mm 48dB (RN-95-NR)" ("Robustgips" 13., "<Unnamed>" 13., "Gips" 13., "<Unnamed>" 10., "stender/isolasjon" 98., "<Unnamed>" 10., "<Unnamed>" 13., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCDOOR | type IFCDOORSTYLE "IDF 3.1 Foldevegg 9700x2500" | object type "IDF 3.1 Foldevegg 9700x2500" | names: "Side_Stack_Operable_Wall_h2500_w9700:IDF 3.1 Foldevegg 9700x2500:2031491" | material: materials ("Light grey", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "GFA 3 8x27 38dB" | object type "GFA 3 8x27 38dB" | names: "Vindu-Fast:GFA 3 8x27 38dB:2067745" | material: materials ("Glass Klart", "RAL 9004") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCSLAB | object type "Floor:Betongdekke 320+100+50" | FLOOR | names: "Floor:Betongdekke 320+100+50:2068595" | material: layers "Floor:Betongdekke 320+100+50" ("Betong" 50., "NO_isolasjon" 100., "Betong" 320.) | property sets: Pset_SlabCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 1.1 121mm (H-95-H)" | object type "Basic Wall:IVA 1.1 121mm (H-95-H):4814431" | names: "Basic Wall:IVA 1.1 121mm (H-95-H):2069251", "Basic Wall:IVA 1.1 121mm (H-95-H):2098245", "Basic Wall:IVA 1.1 121mm (H-95-H):2098679" | material: layers "Basic Wall:IVA 1.1 121mm (H-95-H)" ("Habito" 13., "stender/isolasjon" 95., "Habito" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 4.3T 172mm 34dB (RN-120-NR)" | object type "Basic Wall:IVA 4.3T 172mm 34dB (RN-120-NR):6691836" | names: "Basic Wall:IVA 4.3T 172mm 34dB (RN-120-NR):2083367" | material: layers "Basic Wall:IVA 4.3T 172mm 34dB (RN-120-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 120., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 3.2T 145mm 48dB EI60 (HN-95-NR)" | object type "Basic Wall:IVA 3.2T 145mm 48dB EI60 (HN-95-NR):6702539" | names: "Basic Wall:IVA 3.2T 145mm 48dB EI60 (HN-95-NR):2083368", "Basic Wall:IVA 3.2T 145mm 48dB EI60 (HN-95-NR):2589357", "Basic Wall:IVA 3.2T 145mm 48dB EI60 (HN-95-NR):2985989" | material: layers "Basic Wall:IVA 3.2T 145mm 48dB EI60 (HN-95-NR)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 6.3T 302mm EI 30 (RN-95-60-95-NR)" | object type "Basic Wall:IVA 6.3T 302mm EI 30 (RN-95-60-95-NR):6702607" | names: "Basic Wall:IVA 6.3T 302mm EI 30 (RN-95-60-95-NR):2083371" | material: layers "Basic Wall:IVA 6.3T 302mm EI 30 (RN-95-60-95-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95., "Luftsjikt" 60., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          3 x IFCDOOR | type IFCDOORSTYLE "IDT 1.2 8x21M 33dB" | object type "IDT 1.2 8x21M 33dB" | names: "Dør Enkel:IDT 1.2 8x21M 33dB:2083373", "Dør Enkel:IDT 1.2 8x21M 33dB:2083380", "Dør Enkel:IDT 1.2 8x21M 33dB:2083471" | material: materials ("Terskel Tre", "NCS S 0500-N", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          3 x IFCDOOR | type IFCDOORSTYLE "IDT 1.2 8x21M 33dB" | object type "IDT 1.2 8x21M 33dB" | names: "Dør Enkel:IDT 1.2 8x21M 33dB:2083379", "Dør Enkel:IDT 1.2 8x21M 33dB:2083465", "Dør Enkel:IDT 1.2 8x21M 33dB:2083472" | material: materials ("Terskel Tre", "NCS S 0500-N", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 1.3T 121mm 34dB (R-95-R)" | object type "Basic Wall:IVA 1.3T 121mm 34dB (R-95-R):6691719" | names: "Basic Wall:IVA 1.3T 121mm 34dB (R-95-R):2083461" | material: layers "Basic Wall:IVA 1.3T 121mm 34dB (R-95-R)" ("Robustgips" 13., "stender/isolasjon" 95., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 6.3T 272mm 48dB EI60 (RN-95-30-95-NR)" | object type "Basic Wall:IVA 6.3T 272mm 48dB EI60 (RN-95-30-95-NR):6702429" | names: "Basic Wall:IVA 6.3T 272mm 48dB EI60 (RN-95-30-95-NR):2083463" | material: layers "Basic Wall:IVA 6.3T 272mm 48dB EI60 (RN-95-30-95-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95., "Luftsjikt" 30., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 6.1 302mm (HN-95-60-95-NH)" | object type "Basic Wall:IVA 6.1 302mm (HN-95-60-95-NH):3658349" | names: "Basic Wall:IVA 6.1 302mm (HN-95-60-95-NH):2089930" | material: layers "Basic Wall:IVA 6.1 302mm (HN-95-60-95-NH)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 95., "Luftsjikt" 60., "stender/isolasjon" 95., "Gips" 13., "Habito" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 3.1 145mm 48dB (HN-95-NH)" | object type "Basic Wall:IVA 3.1 145mm 48dB (HN-95-NH):4820944" | names: "Basic Wall:IVA 3.1 145mm 48dB (HN-95-NH):2094431", "Basic Wall:IVA 3.1 145mm 48dB (HN-95-NH):7123971" | material: layers "Basic Wall:IVA 3.1 145mm 48dB (HN-95-NH)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Habito" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 3.3 145mm 44dB (RN-95-NR)" | object type "Basic Wall:IVA 3.3 145mm 44dB (RN-95-NR):4816971" | names: "Basic Wall:IVA 3.3 145mm 44dB (RN-95-NR):2096685", "Basic Wall:IVA 3.3 145mm 44dB (RN-95-NR):5063590" | material: layers "Basic Wall:IVA 3.3 145mm 44dB (RN-95-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          2 x IFCDOOR | type IFCDOORSTYLE "IDT 3.6 10x21M 38dB" | object type "IDT 3.6 10x21M 38dB" | names: "Dør Enkel_ Glassfelt:IDT 3.6 10x21M 38dB:2097868", "Dør Enkel_ Glassfelt:IDT 3.6 10x21M 38dB:2099270" | material: materials ("NCS S 2500-N", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 3.3 10x21M 33dB" | object type "IDT 3.3 10x21M 33dB" | names: "Dør Enkel_ Glassfelt:IDT 3.3 10x21M 33dB:2099229" | material: materials ("Lys grå", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 3.3 10x21M 33dB" | object type "IDT 3.3 10x21M 33dB" | names: "Dør Enkel_ Glassfelt:IDT 3.3 10x21M 33dB:2105557" | material: materials ("Lys grå", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          2 x IFCDOOR | type IFCDOORSTYLE "IDT 1.1 8x21M" | object type "IDT 1.1 8x21M" | names: "Dør Enkel:IDT 1.1 8x21M:2136594", "Dør Enkel:IDT 1.1 8x21M:2182396" | material: materials ("Terskel Tre", "Lys grå", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 1.1 8x21M" | object type "IDT 1.1 8x21M" | names: "Dør Enkel:IDT 1.1 8x21M:2147861" | material: materials ("Terskel Tre", "Lys grå", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          2 x IFCDOOR | type IFCDOORSTYLE "IDT 1.1 8x21M" | object type "IDT 1.1 8x21M" | names: "Dør Enkel:IDT 1.1 8x21M:2147862", "Dør Enkel:IDT 1.1 8x21M:2182349" | material: materials ("Terskel Tre", "Lys grå", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 7.3 121mm 37dB EI30 (95-NH)" | object type "Basic Wall:IVA 7.3 121mm 37dB EI30 (95-NH):6248387" | names: "Basic Wall:IVA 7.3 121mm 37dB EI30 (95-NH):2147923", "Basic Wall:IVA 7.3 121mm 37dB EI30 (95-NH):2181595" | material: layers "Basic Wall:IVA 7.3 121mm 37dB EI30 (95-NH)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 1.3 121mm (R-95-R)" | object type "Basic Wall:IVA 1.3 121mm (R-95-R):4815917" | names: "Basic Wall:IVA 1.3 121mm (R-95-R):2150344", "Basic Wall:IVA 1.3 121mm (R-95-R):3427154" | material: layers "Basic Wall:IVA 1.3 121mm (R-95-R)" ("Robustgips" 13., "stender/isolasjon" 95., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 6.3 302mm 48dB (RN-95-60-95-NR)" | object type "Basic Wall:IVA 6.3 302mm 48dB (RN-95-60-95-NR):3868042" | names: "Basic Wall:IVA 6.3 302mm 48dB (RN-95-60-95-NR):2171852" | material: layers "Basic Wall:IVA 6.3 302mm 48dB (RN-95-60-95-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95., "Luftsjikt" 60., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          5 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 3.3T 145mm EI60 (RN-95-NR)" | object type "Basic Wall:IVA 3.3T 145mm EI60 (RN-95-NR):6701511" | names: "Basic Wall:IVA 3.3T 145mm EI60 (RN-95-NR):2178585", "Basic Wall:IVA 3.3T 145mm EI60 (RN-95-NR):2178759", "Basic Wall:IVA 3.3T 145mm EI60 (RN-95-NR):2178829" (+2 more) | material: layers "Basic Wall:IVA 3.3T 145mm EI60 (RN-95-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 5.2 15x21M EI60S" | object type "IDT 5.2 15x21M EI60S" | names: "Dør Dobbel:IDT 5.2 15x21M EI60S:2179297" | material: materials ("NCS S 1000-N", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 5.2 15x21M EI60S" | object type "IDT 5.2 15x21M EI60S" | names: "Dør Dobbel:IDT 5.2 15x21M EI60S:2179356" | material: materials ("NCS S 1000-N", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          2 x IFCDOOR | type IFCDOORSTYLE "IDT 3.6 10x21M 38dB" | object type "IDT 3.6 10x21M 38dB" | names: "Dør Enkel_ Glassfelt:IDT 3.6 10x21M 38dB:2186885", "Dør Enkel_ Glassfelt:IDT 3.6 10x21M 38dB:2187020" | material: materials ("NCS S 2500-N", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 3.3 10x21M 33dB" | object type "IDT 3.3 10x21M 33dB" | names: "Dør Enkel_ Glassfelt:IDT 3.3 10x21M 33dB:2187413" | material: materials ("Lys grå", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 2.1 10x21M" | object type "IDT 2.1 10x21M" | names: "Dør Enkel:IDT 2.1 10x21M:2187712" | material: materials ("_White", "NCS S 0500-N", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 2.1 10x21M" | object type "IDT 2.1 10x21M" | names: "Dør Enkel:IDT 2.1 10x21M:2187786" | material: materials ("_White", "NCS S 0500-N", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 2.3 10x21M 33dB" | object type "IDT 2.3 10x21M 33dB" | names: "Dør Enkel:IDT 2.3 10x21M 33dB:2188261" | material: materials ("Terskel Tre", "Lys grå", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 8.1 125mm sjaktvegg 37dB EI60" | object type "Basic Wall:IVA 8.1 125mm sjaktvegg 37dB EI60:2857583" | names: "Basic Wall:IVA 8.1 125mm sjaktvegg 37dB EI60:2229620" | material: layers "Basic Wall:IVA 8.1 125mm sjaktvegg 37dB EI60" ("Branngips" 15., "Branngips" 15., "stender/isolasjon" 95.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 3.3 145mm 37dB EI60 (RN-95-NR)" | object type "Basic Wall:IVA 3.3 145mm 37dB EI60 (RN-95-NR):4823028" | names: "Basic Wall:IVA 3.3 145mm 37dB EI60 (RN-95-NR):2229651", "Basic Wall:IVA 3.3 145mm 37dB EI60 (RN-95-NR):4046476", "Basic Wall:IVA 3.3 145mm 37dB EI60 (RN-95-NR):4046526" | material: layers "Basic Wall:IVA 3.3 145mm 37dB EI60 (RN-95-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 3.2 145mm 37dB EI60 (HN-95-NR)" | object type "Basic Wall:IVA 3.2 145mm 37dB EI60 (HN-95-NR):2850426" | names: "Basic Wall:IVA 3.2 145mm 37dB EI60 (HN-95-NR):2231094" | material: layers "Basic Wall:IVA 3.2 145mm 37dB EI60 (HN-95-NR)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          2 x IFCWINDOW | type IFCWINDOWSTYLE "V2 12x22" | object type "V2 12x22" | names: "Vindu-Fast:V2 12x22:2275275", "Vindu-Fast:V2 12x22:2836494" | material: materials ("Glass Klart", "NCS S 0502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 1.1 8x21M" | object type "IDT 1.1 8x21M" | names: "Dør Enkel:IDT 1.1 8x21M:2275999" | material: materials ("Terskel Tre", "Lys grå", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          2 x IFCSLAB | object type "Floor:Betongdekke 420+ isolasjon 100 + betong 50" | FLOOR | names: "Floor:Betongdekke 420+ isolasjon 100 + betong 50:2368008", "Floor:Betongdekke 420+ isolasjon 100 + betong 50:4449980" | material: layers "Floor:Betongdekke 420+ isolasjon 100 + betong 50" ("Betong" 50., "NO_isolasjon" 100., "Betong" 420.) | property sets: Pset_SlabCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Other
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 8.1 125mm sjaktvegg EI60" | object type "Basic Wall:IVA 8.1 125mm sjaktvegg EI60:2855957" | names: "Basic Wall:IVA 8.1 125mm sjaktvegg EI60:2371232" | material: layers "Basic Wall:IVA 8.1 125mm sjaktvegg EI60" ("Branngips" 15., "Branngips" 15., "stender/isolasjon" 95.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          2 x IFCWINDOW | type IFCWINDOWSTYLE "V22 14x14" | object type "V22 14x14" | names: "Vindu-Fast:V22 14x14:2393061", "Vindu-Fast:V22 14x14:2421968" | material: materials ("Glass Klart", "NCS S 0502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "V5 8x22" | object type "V5 8x22" | names: "Vindu-Fast:V5 8x22:2399390" | material: materials ("Glass Klart", "NCS S 0502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          38 x IFCCOVERING | object type "Compound Ceiling:Himling System 600x1200" | CEILING | names: "Compound Ceiling:Himling System 600x1200:2410560", "Compound Ceiling:Himling System 600x1200:2410966", "Compound Ceiling:Himling System 600x1200:2411445" (+35 more) | material: layers "Compound Ceiling:Himling System 600x1200" ("Himling Metallprofil" 38., "Himling System 600x1200" 12.) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          14 x IFCCOVERING | object type "Compound Ceiling:Himling System 600x600" | CEILING | names: "Compound Ceiling:Himling System 600x600:2411015", "Compound Ceiling:Himling System 600x600:2411625", "Compound Ceiling:Himling System 600x600:2592221" (+11 more) | material: layers "Compound Ceiling:Himling System 600x600" ("Himling Metallprofil" 38., "Himling System 600x600" 12.) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          12 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 7.2 108mm Skjørt" | object type "Basic Wall:IVA 7.2 108mm Skjørt:5366897" | names: "Basic Wall:IVA 7.2 108mm Skjørt:2411316", "Basic Wall:IVA 7.2 108mm Skjørt:2780932", "Basic Wall:IVA 7.2 108mm Skjørt:3043849" (+9 more) | material: layers "Basic Wall:IVA 7.2 108mm Skjørt" ("Gips" 13., "stender/isolasjon" 95.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCWINDOW | type IFCWINDOWSTYLE "V1 12x22" | object type "V1 12x22" | names: "Vindu-Hengslet_1200 opening:V1 12x22:2416707" | material: materials ("NCS S 0502-Y", "Glass Klart") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "V23 14x14" | object type "V23 14x14" | names: "Vindu-Hengslet:V23 14x14:2424325" | material: materials ("Glass Klart", "NCS S 0502-Y", "Karm Malt") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          3 x IFCWINDOW | type IFCWINDOWSTYLE "GF 1.3 12x21 38dB" | object type "GF 1.3 12x21 38dB" | names: "Vindu-Fast:GF 1.3 12x21 38dB:2493195", "Vindu-Fast:GF 1.3 12x21 38dB:2493273", "Vindu-Fast:GF 1.3 12x21 38dB:2996294" | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "GF 3.3 6x21 44dB" | object type "GF 3.3 6x21 44dB" | names: "Vindu-Fast:GF 3.3 6x21 44dB:2493355" | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          6 x IFCWINDOW | type IFCWINDOWSTYLE "GF 1.1 12x21 33dB" | object type "GF 1.1 12x21 33dB" | names: "Vindu-Fast:GF 1.1 12x21 33dB:2493862", "Vindu-Fast:GF 1.1 12x21 33dB:2498568", "Vindu-Fast:GF 1.1 12x21 33dB:2504791" (+3 more) | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          15 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:YV 7.3 410mm rød platekledning" | object type "Basic Wall:YV 7.3 410mm rød platekledning:2216522" | names: "Basic Wall:YV 7.3 410mm rød platekledning:2495136", "Basic Wall:YV 7.3 410mm rød platekledning:2496271", "Basic Wall:YV 7.3 410mm rød platekledning:2496445" (+12 more) | material: layers "Basic Wall:YV 7.3 410mm rød platekledning" ("Cembrit Metro Copenhagen" 8., "Luftsjikt" 36., "Vindsperre" 9., "Stender isolert vegg" 296., "NO_Utlekting" 48., "Robustgips" 12.5) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          9 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:YV 7.4 410mm gul platekledning" | object type "Basic Wall:YV 7.4 410mm gul platekledning:1741258" | names: "Basic Wall:YV 7.4 410mm gul platekledning:2495411", "Basic Wall:YV 7.4 410mm gul platekledning:2498001", "Basic Wall:YV 7.4 410mm gul platekledning:2498274" (+6 more) | material: layers "Basic Wall:YV 7.4 410mm gul platekledning" ("Cembrit Metro Amsterdam" 8., "Luftsjikt" 36., "Vindsperre" 9., "Stender isolert vegg" 296., "NO_Utlekting" 48., "Robustgips" 12.5) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          12 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:YV 7.2 410mm grønn platekledning" | object type "Basic Wall:YV 7.2 410mm grønn platekledning:2569141" | names: "Basic Wall:YV 7.2 410mm grønn platekledning:2496208", "Basic Wall:YV 7.2 410mm grønn platekledning:2496416", "Basic Wall:YV 7.2 410mm grønn platekledning:2496458" (+9 more) | material: layers "Basic Wall:YV 7.2 410mm grønn platekledning" ("Cembrit Metro Hamburg" 8., "Luftsjikt" 36., "Vindsperre" 9., "Stender isolert vegg" 296., "NO_Utlekting" 48., "Robustgips" 12.5) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          3 x IFCWINDOW | type IFCWINDOWSTYLE "GF 3.2 6x21 38dB" | object type "GF 3.2 6x21 38dB" | names: "Vindu-Fast:GF 3.2 6x21 38dB:2498596", "Vindu-Fast:GF 3.2 6x21 38dB:2498656", "Vindu-Fast:GF 3.2 6x21 38dB:2499673" | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "GF 4.2 18x21 33dB" | object type "GF 4.2 18x21 33dB" | names: "Vindu-Fast:GF 4.2 18x21 33dB:2498708" | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "GF 4.2 18x21 33dB" | object type "GF 4.2 18x21 33dB" | names: "Vindu-Fast:GF 4.2 18x21 33dB:2499363" | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "GF 1.1 12x21 33dB" | object type "GF 1.1 12x21 33dB" | names: "Vindu-Fast:GF 1.1 12x21 33dB:2500259" | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          8 x IFCWINDOW | type IFCWINDOWSTYLE "GF 1.3 12x21 38dB" | object type "GF 1.3 12x21 38dB" | names: "Vindu-Fast:GF 1.3 12x21 38dB:2500325", "Vindu-Fast:GF 1.3 12x21 38dB:2504855", "Vindu-Fast:GF 1.3 12x21 38dB:2504883" (+5 more) | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "GF 4.1 18x21 38dB" | object type "GF 4.1 18x21 38dB" | names: "Vindu-Fast:GF 4.1 18x21 38dB:2500740" | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "GF 10.2 8x27 38dB" | object type "GF 10.2 8x27 38dB" | names: "Vindu-Fast:GF 10.2 8x27 38dB:2500909" | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "GF 4.2 18x21 33dB" | object type "GF 4.2 18x21 33dB" | names: "Vindu-Fast:GF 4.2 18x21 33dB:2501801" | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          2 x IFCWINDOW | type IFCWINDOWSTYLE "GF 2.2 9x21 33dB" | object type "GF 2.2 9x21 33dB" | names: "Vindu-Fast:GF 2.2 9x21 33dB:2504598", "Vindu-Fast:GF 2.2 9x21 33dB:2504761" | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "GF 10.2 8x27 38dB" | object type "GF 10.2 8x27 38dB" | names: "Vindu-Fast:GF 10.2 8x27 38dB:2504695" | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "GF 1.1 12x21 33dB" | object type "GF 1.1 12x21 33dB" | names: "Vindu-Fast:GF 1.1 12x21 33dB:2504942" | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          2 x IFCWINDOW | type IFCWINDOWSTYLE "GF 3.3 6x21 44dB" | object type "GF 3.3 6x21 44dB" | names: "Vindu-Fast:GF 3.3 6x21 44dB:2505781", "Vindu-Fast:GF 3.3 6x21 44dB:2836551" | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          2 x IFCWINDOW | type IFCWINDOWSTYLE "GF 11.1 12x27 33dB" | object type "GF 11.1 12x27 33dB" | names: "Vindu-Fast:GF 11.1 12x27 33dB:2505892", "Vindu-Fast:GF 11.1 12x27 33dB:2994244" | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "GF 2.2 9x21 33dB" | object type "GF 2.2 9x21 33dB" | names: "Vindu-Fast:GF 2.2 9x21 33dB:2506361" | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "GF 6.1 8x21 33dB" | object type "GF 6.1 8x21 33dB" | names: "Vindu-Fast:GF 6.1 8x21 33dB:2506671" | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "GF 1.1 12x21 33dB" | object type "GF 1.1 12x21 33dB" | names: "Vindu-Fast:GF 1.1 12x21 33dB:2506898" | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "GF 7.2 15x21 38dB" | object type "GF 7.2 15x21 38dB" | names: "Vindu-Fast:GF 7.2 15x21 38dB:2506998" | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "GF 3.6 6x21 33dB" | object type "GF 3.6 6x21 33dB" | names: "Vindu-Fast:GF 3.6 6x21 33dB:2507587" | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "GF 7.2 15x21 38dB" | object type "GF 7.2 15x21 38dB" | names: "Vindu-Fast:GF 7.2 15x21 38dB:2507681" | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "GF 1.3 12x21 38dB" | object type "GF 1.3 12x21 38dB" | names: "Vindu-Fast:GF 1.3 12x21 38dB:2507723" | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "GF 4.1 18x21 38dB" | object type "GF 4.1 18x21 38dB" | names: "Vindu-Fast:GF 4.1 18x21 38dB:2508145" | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "GF 2.2 9x21 33dB" | object type "GF 2.2 9x21 33dB" | names: "Vindu-Fast:GF 2.2 9x21 33dB:2508462" | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "GF 1.1 12x21 33dB" | object type "GF 1.1 12x21 33dB" | names: "Vindu-Fast:GF 1.1 12x21 33dB:2569729" | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCANNOTATION
          1 x IFCCOVERING | object type "Compound Ceiling:Fast gipshimling" | CEILING | names: "Compound Ceiling:Fast gipshimling:2600619" | material: layers "Compound Ceiling:Fast gipshimling" ("Himling Metallprofil" 95., "Himling fast gips" 12.5, "Himling fast gips" 12.5) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "GF 1.3 12x21 38dB" | object type "GF 1.3 12x21 38dB" | names: "Vindu-Fast:GF 1.3 12x21 38dB:2836552" | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "GF 3.2 6x21 38dB" | object type "GF 3.2 6x21 38dB" | names: "Vindu-Fast:GF 3.2 6x21 38dB:2846481" | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 5.1 212mm 34 dB (HN-160-NR)" | object type "Basic Wall:IVA 5.1 212mm 34 dB (HN-160-NR):3884061" | names: "Basic Wall:IVA 5.1 212mm 34 dB (HN-160-NR):2856295" | material: layers "Basic Wall:IVA 5.1 212mm 34 dB (HN-160-NR)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 160., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 2.4 134mm 34dB (R-95-NH)" | object type "Basic Wall:IVA 2.4 134mm 34dB (R-95-NH):4844120" | names: "Basic Wall:IVA 2.4 134mm 34dB (R-95-NH):2856783" | material: layers "Basic Wall:IVA 2.4 134mm 34dB (R-95-NH)" ("Robustgips" 13., "stender/isolasjon" 95., "Gips" 13., "Habito" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 4.1T 172mm 34dB (HN-120-NH)" | object type "Basic Wall:IVA 4.1T 172mm 34dB (HN-120-NH):6783070" | names: "Basic Wall:IVA 4.1T 172mm 34dB (HN-120-NH):2861423" | material: layers "Basic Wall:IVA 4.1T 172mm 34dB (HN-120-NH)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 120., "Gips" 13., "Habito" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 6.3 376mm 34dB (RN-95-134-95-NR)" | object type "Basic Wall:IVA 6.3 376mm 34dB (RN-95-134-95-NR):2872477" | names: "Basic Wall:IVA 6.3 376mm 34dB (RN-95-134-95-NR):2875045" | material: layers "Basic Wall:IVA 6.3 376mm 34dB (RN-95-134-95-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95., "Luftsjikt" 198., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          3 x IFCWALL | type IFCWALLTYPE "Basic Wall:YV 1.1 517mm" | object type "Basic Wall:YV 1.1 517mm:1735105" | names: "Basic Wall:YV 1.1 517mm:2905786", "Basic Wall:YV 1.1 517mm:2905897", "Basic Wall:YV 1.1 517mm:4333381" | material: layers "Basic Wall:YV 1.1 517mm" ("Trekledning" 19., "Luftsjikt" 48., "Luftsjikt" 36., "Luftsjikt" 48., "Vindsperre" 9., "Stender isolert vegg" 296., "NO_Utlekting" 48., "Robustgips" 12.5) | property sets: Constraints, Dimensions, Other, Phasing, Structural, Text
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 3.3 F 145mm 48dB (RN-95-NR)" | object type "Basic Wall:IVA 3.3 F 145mm 48dB (RN-95-NR):7123846" | names: "Basic Wall:IVA 3.3 F 145mm 48dB (RN-95-NR):2907734" | material: layers "Basic Wall:IVA 3.3 F 145mm 48dB (RN-95-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCWINDOW | type IFCWINDOWSTYLE "GF 1.4 12x21 44dB" | object type "GF 1.4 12x21 44dB" | names: "Vindu-Fast:GF 1.4 12x21 44dB:2992305" | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          2 x IFCWINDOW | type IFCWINDOWSTYLE "GF 1.1 12x21 33dB" | object type "GF 1.1 12x21 33dB" | names: "Vindu-Fast:GF 1.1 12x21 33dB:2994099", "Vindu-Fast:GF 1.1 12x21 33dB:2994979" | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "GF 2.1 9x21 38dB" | object type "GF 2.1 9x21 38dB" | names: "Vindu-Fast:GF 2.1 9x21 38dB:2995137" | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 6.1 302mm 44dB (HN-95-30-95-NH)" | object type "Basic Wall:IVA 6.1 302mm 44dB (HN-95-30-95-NH):3855970" | names: "Basic Wall:IVA 6.1 302mm 44dB (HN-95-30-95-NH):2995705" | material: layers "Basic Wall:IVA 6.1 302mm 44dB (HN-95-30-95-NH)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 95., "Luftsjikt" 60., "stender/isolasjon" 95., "Gips" 13., "Habito" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 3.6 10x21M 38dB" | object type "IDT 3.6 10x21M 38dB" | names: "Dør Enkel_ Glassfelt:IDT 3.6 10x21M 38dB:2996291" | material: materials ("NCS S 2500-N", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "GF 1.1 12x21 33dB" | object type "GF 1.1 12x21 33dB" | names: "Vindu-Fast:GF 1.1 12x21 33dB:2996295" | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "GF 9.1 11x26.5 33dB" | object type "GF 9.1 11x26.5 33dB" | names: "Vindu-Fast:GF 9.1 11x26.5 33dB:2996296" | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "GF 16.1 5x31 38dB" | object type "GF 16.1 5x31 38dB" | names: "Vindu-Fast:GF 16.1 5x31 38dB:2997461" | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "GF 1.1 12x21 33dB" | object type "GF 1.1 12x21 33dB" | names: "Vindu-Fast:GF 1.1 12x21 33dB:2998472" | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          4 x IFCWINDOW | type IFCWINDOWSTYLE "GF 12.1 6x31 38dB" | object type "GF 12.1 6x31 38dB" | names: "Vindu-Fast:GF 12.1 6x31 38dB:2998710", "Vindu-Fast:GF 12.1 6x31 38dB:3384739", "Vindu-Fast:GF 12.1 6x31 38dB:3385492" (+1 more) | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCSLAB | object type "Floor:Amfi repos" | FLOOR | names: "Floor:Amfi repos:3021519" | material: layers "Floor:Amfi repos" ("Massivtre" 250.) | property sets: Pset_SlabCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Other
          4 x IFCSLAB | object type "Floor:Betongdekke 320 + 80 påstøp + 10 avretting" | FLOOR | names: "Floor:Betongdekke 320 + 80 påstøp + 10 avretting:3021655", "Floor:Betongdekke 320 + 80 påstøp + 10 avretting:4439102", "Floor:Betongdekke 320 + 80 påstøp + 10 avretting:4439551" (+1 more) | material: layers "Floor:Betongdekke 320 + 80 påstøp + 10 avretting" ("Betong avretting" 10., "Betong påstøp" 80., "Betong" 320.) | property sets: Pset_SlabCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Other
          1 x IFCDOOR | type IFCDOORSTYLE "1700 x 2100mm" | object type "1700 x 2100mm" | names: "M_Overhead-Rolling:1700 x 2100mm:3038740" | material: "Metal - Paint Finish - Ivory, Matte" | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 3.3 145mm E30 (RN-95-NR)" | object type "Basic Wall:IVA 3.3 145mm E30 (RN-95-NR):3866097" | names: "Basic Wall:IVA 3.3 145mm E30 (RN-95-NR):3038741" | material: layers "Basic Wall:IVA 3.3 145mm E30 (RN-95-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          1 x IFCCOVERING | object type "Compound Ceiling:Himling System 600x600 hygiene" | CEILING | names: "Compound Ceiling:Himling System 600x600 hygiene:3045654" | material: layers "Compound Ceiling:Himling System 600x600 hygiene" ("Himling Metallprofil" 38., "Himling System 600x600" 12.) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "GF 7.4 15x21 EI60" | object type "GF 7.4 15x21 EI60" | names: "Vindu-Fast:GF 7.4 15x21 EI60:3078166" | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 2.3 10x21M 33dB" | object type "IDT 2.3 10x21M 33dB" | names: "Dør Enkel:IDT 2.3 10x21M 33dB:3087980" | material: materials ("Terskel Tre", "Lys grå", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 2.3 10x21M 33dB" | object type "IDT 2.3 10x21M 33dB" | names: "Dør Enkel:IDT 2.3 10x21M 33dB:3087981" | material: materials ("Terskel Tre", "Lys grå", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "GF 2.2 9x21 33dB" | object type "GF 2.2 9x21 33dB" | names: "Vindu-Fast:GF 2.2 9x21 33dB:3088169" | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "GF 12.1 6x31 38dB" | object type "GF 12.1 6x31 38dB" | names: "Vindu-Fast:GF 12.1 6x31 38dB:3212641" | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "GF 12.1 6x31 38dB" | object type "GF 12.1 6x31 38dB" | names: "Vindu-Fast:GF 12.1 6x31 38dB:3217776" | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "GF 10.1 8x27 33dB" | object type "GF 10.1 8x27 33dB" | names: "Vindu-Fast:GF 10.1 8x27 33dB:3382692" | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 2.1 10x21M" | object type "IDT 2.1 10x21M" | names: "Dør Enkel:IDT 2.1 10x21M:3443650" | material: materials ("_White", "NCS S 0500-N", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          2 x IFCWINDOW | type IFCWINDOWSTYLE "V3 18x22" | object type "V3 18x22" | names: "Vindu-Fast:V3 18x22:3466359", "Vindu-Fast:V3 18x22:4272092" | material: materials ("N_Windows - Glass", "NCS S 0502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          5 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 7.1 121mm Skjørt" | object type "Basic Wall:IVA 7.1 121mm Skjørt:2853494" | names: "Basic Wall:IVA 7.1 121mm Skjørt:3514054", "Basic Wall:IVA 7.1 121mm Skjørt:3859437", "Basic Wall:IVA 7.1 121mm Skjørt:3882754" (+2 more) | material: layers "Basic Wall:IVA 7.1 121mm Skjørt" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          6 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 7.1 121mm (95-NR)" | object type "Basic Wall:IVA 7.1 121mm (95-NR):6248452" | names: "Basic Wall:IVA 7.1 121mm (95-NR):3514351", "Basic Wall:IVA 7.1 121mm (95-NR):3514430", "Basic Wall:IVA 7.1 121mm (95-NR):3887634" (+3 more) | material: layers "Basic Wall:IVA 7.1 121mm (95-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 6.2 272mm 48dB EI60 (HN-95-30-95-NR)" | object type "Basic Wall:IVA 6.2 272mm 48dB EI60 (HN-95-30-95-NR):4826408" | names: "Basic Wall:IVA 6.2 272mm 48dB EI60 (HN-95-30-95-NR):3658770" | material: layers "Basic Wall:IVA 6.2 272mm 48dB EI60 (HN-95-30-95-NR)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 95., "Luftsjikt" 30., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          1 x IFCDOOR | type IFCDOORSTYLE "IDA 10.1 14x21M E30CS" | object type "IDA 10.1 14x21M E30CS" | names: "Dør Enkel:IDA 10.1 14x21M E30CS:3697547" | material: materials ("Light grey", "Karm Malt", "Lys grå") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCSLAB | object type "Floor:Betongdekke 400 + 80 påstøp + 10 avretting" | FLOOR | names: "Floor:Betongdekke 400 + 80 påstøp + 10 avretting:3939993" | material: layers "Floor:Betongdekke 400 + 80 påstøp + 10 avretting" ("Betong avretting" 10., "Betong påstøp" 80., "Betong" 400.) | property sets: Pset_SlabCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:110mm Heisvegg" | object type "Basic Wall:110mm Heisvegg:3943637" | names: "Basic Wall:110mm Heisvegg:3944655" | material: layers "Basic Wall:110mm Heisvegg" ("hvit malt" 110.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          3 x IFCCOVERING | object type "Compound Ceiling:Lydhimling gips" | CEILING | names: "Compound Ceiling:Lydhimling gips:3989341", "Compound Ceiling:Lydhimling gips:4269468", "Compound Ceiling:Lydhimling gips:6059863" | material: layers "Compound Ceiling:Lydhimling gips" ("Himling Metallprofil" 48., "Gips" 12.5, "Gips" 12.5) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Other
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 3.3 10x21M 33dB" | object type "IDT 3.3 10x21M 33dB" | names: "Dør Enkel_ Glassfelt:IDT 3.3 10x21M 33dB:4000707" | material: materials ("Lys grå", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 7.1T 121mm (95-NR)" | object type "Basic Wall:IVA 7.1T 121mm (95-NR):6702427" | names: "Basic Wall:IVA 7.1T 121mm (95-NR):4154038", "Basic Wall:IVA 7.1T 121mm (95-NR):4154039" | material: layers "Basic Wall:IVA 7.1T 121mm (95-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 3.3 10x21M 33dB" | object type "IDT 3.3 10x21M 33dB" | names: "Dør Enkel_ Glassfelt:IDT 3.3 10x21M 33dB:4202122" | material: materials ("Lys grå", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "V5 8x22" | object type "V5 8x22" | names: "Vindu-Fast:V5 8x22:4272094" | material: materials ("Glass Klart", "NCS S 0502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:YV 9.2 536mm uisolert" | object type "Basic Wall:YV 9.2 536mm uisolert:6597558" | names: "Basic Wall:YV 9.2 536mm uisolert:4333764" | material: layers "Basic Wall:YV 9.2 536mm uisolert" ("Trekledning" 19., "Luftsjikt" 48., "Luftsjikt" 36., "Luftsjikt" 48., "Vindsperre" 9., "stender" 296., "<Unnamed>" 36., "Luftsjikt" 36., "Cembrit Metro Amsterdam" 8.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 4.3 172mm 48dB (RN-120-NR)" | object type "Basic Wall:IVA 4.3 172mm 48dB (RN-120-NR):4079466" | names: "Basic Wall:IVA 4.3 172mm 48dB (RN-120-NR):4410967" | material: layers "Basic Wall:IVA 4.3 172mm 48dB (RN-120-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 120., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          2 x IFCSTAIR | object type "Cast-In-Place Stair:Betongtrapp t=150 repo=200:306564" | names: "Cast-In-Place Stair:Stair:4430332", "Cast-In-Place Stair:Stair:4433002" | parts: 4 IFCSLAB, 4 IFCSTAIRFLIGHT, 2 IFCRAILING | property sets: Pset_StairCommon, Pset_TFM, Constraints, Dimensions, Identity Data, Other
          1 x IFCSLAB | object type "Floor:Betongdekke 265+80+20+50" | FLOOR | names: "Floor:Betongdekke 265+80+20+50:4439291" | material: layers "Floor:Betongdekke 265+80+20+50" ("Betong avretting" 50., "Spaceloft" 20., "Betong påstøp" 80., "Betong" 265.) | property sets: Pset_SlabCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Other
          1 x IFCSLAB | object type "Floor:Betongdekke 420 + påstøp 80+ spaceloft 20 + betong 50" | FLOOR | names: "Floor:Betongdekke 420 + påstøp 80+ spaceloft 20 + betong 50:4439452" | material: layers "Floor:Betongdekke 420 + påstøp 80+ spaceloft 20 + betong 50" ("Betong" 50., "Spaceloft" 20., "Betong" 80., "Betong" 420.) | property sets: Pset_SlabCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          2 x IFCSLAB | object type "Floor:Betongdekke 265 + 80 påstøp + 10 avretting" | FLOOR | names: "Floor:Betongdekke 265 + 80 påstøp + 10 avretting:4439872", "Floor:Betongdekke 265 + 80 påstøp + 10 avretting:4455507" | material: layers "Floor:Betongdekke 265 + 80 påstøp + 10 avretting" ("Betong avretting" 10., "Betong påstøp" 80., "Betong" 265.) | property sets: Pset_SlabCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Other
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 7.1 13x21M 38dB" | object type "IDT 7.1 13x21M 38dB" | names: "Dør Dobbel_Ulike_Dørblader:IDT 7.1 13x21M 38dB:4801842" | material: materials ("Lys grå", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          18 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVSP 84mm SPILEVEGG" | object type "Basic Wall:IVSP 84mm SPILEVEGG:4800472" | names: "Basic Wall:IVSP 84mm SPILEVEGG:4803256", "Basic Wall:IVSP 84mm SPILEVEGG:4803318", "Basic Wall:IVSP 84mm SPILEVEGG:4803362" (+15 more) | material: layers "Basic Wall:IVSP 84mm SPILEVEGG" ("NO_isolasjon" 48., "<Unnamed>" 16., "Spiler" 34.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          1 x IFCWINDOW | type IFCWINDOWSTYLE "GFA 3 8x27 38dB" | object type "GFA 3 8x27 38dB" | names: "Vindu-Fast:GFA 3 8x27 38dB:4804571" | material: materials ("Glass Klart", "RAL 9004") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCBUILDINGELEMENTPROXY | object type "Model Text:400mm Arial" | names: "Model Text:400mm Arial" | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Graphics, Identity Data
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 6.3 252mm EI60 (RN-95-40-95-NR)" | object type "Basic Wall:IVA 6.3 252mm EI60 (RN-95-40-95-NR):5031793" | names: "Basic Wall:IVA 6.3 252mm EI60 (RN-95-40-95-NR):5031724" | material: layers "Basic Wall:IVA 6.3 252mm EI60 (RN-95-40-95-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95., "Luftsjikt" 20., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          1 x IFCWINDOW | type IFCWINDOWSTYLE "GF 1.3 12x21 38dB" | object type "GF 1.3 12x21 38dB" | names: "Vindu-Fast:GF 1.3 12x21 38dB:5046262" | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "GF 13.1 36x21 38dB" | object type "GF 13.1 36x21 38dB" | names: "Vindu_3felt:GF 13.1 36x21 38dB:5153882" | material: materials ("Karm Malt", "Glass Klart", "NCS S 3502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          4 x IFCWINDOW | type IFCWINDOWSTYLE "V7 24x22" | object type "V7 24x22" | names: "Vindu 3 felt:V7 24x22:5436093", "Vindu 3 felt:V7 24x22:5447258", "Vindu 3 felt:V7 24x22:5447942" (+1 more) | material: materials ("NCS S 0502-Y", "N_Windows - Glass") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          2 x IFCWINDOW | type IFCWINDOWSTYLE "V11 35x22" | object type "V11 35x22" | names: "Vindu 3 felt:V11 35x22:5444204", "Vindu 3 felt:V11 35x22:5465449" | material: materials ("NO_Aluminium", "NCS S 0502-Y", "N_Windows - Glass") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          3 x IFCWINDOW | type IFCWINDOWSTYLE "V9 30x22" | object type "V9 30x22" | names: "Vindu 3 felt:V9 30x22:5444681", "Vindu 3 felt:V9 30x22:5447190", "Vindu 3 felt:V9 30x22:5448169" | material: materials ("NCS S 0502-Y", "N_Windows - Glass") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "V10 30x22" | object type "V10 30x22" | names: "Vindu 3 felt:V10 30x22:5444956" | material: materials ("NCS S 0502-Y", "N_Windows - Glass") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          2 x IFCWINDOW | type IFCWINDOWSTYLE "V9 30x22" | object type "V9 30x22" | names: "Vindu 3 felt:V9 30x22:5445253", "Vindu 3 felt:V9 30x22:5446585" | material: materials ("NCS S 0502-Y", "N_Windows - Glass") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          2 x IFCWINDOW | type IFCWINDOWSTYLE "V8 27x22" | object type "V8 27x22" | names: "Vindu 3 felt:V8 27x22:5445842", "Vindu 3 felt:V8 27x22:5445970" | material: materials ("NCS S 0502-Y", "N_Windows - Glass") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          4 x IFCWINDOW | type IFCWINDOWSTYLE "V6 24x22" | object type "V6 24x22" | names: "Vindu 3 felt:V6 24x22:5446097", "Vindu 3 felt:V6 24x22:5446268", "Vindu 3 felt:V6 24x22:5446392" (+1 more) | material: materials ("NCS S 0502-Y", "N_Windows - Glass") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          6 x IFCWINDOW | type IFCWINDOWSTYLE "V7 24x22" | object type "V7 24x22" | names: "Vindu 3 felt:V7 24x22:5446726", "Vindu 3 felt:V7 24x22:5446860", "Vindu 3 felt:V7 24x22:5447015" (+3 more) | material: materials ("NCS S 0502-Y", "N_Windows - Glass") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "V10 30x22" | object type "V10 30x22" | names: "Vindu 3 felt:V10 30x22:5447393" | material: materials ("NCS S 0502-Y", "N_Windows - Glass") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          2 x IFCWINDOW | type IFCWINDOWSTYLE "V12 35x22" | object type "V12 35x22" | names: "Vindu 3 felt:V12 35x22:5463949", "Vindu 3 felt:V12 35x22:5464775" | material: materials ("NO_Aluminium", "NCS S 0502-Y", "N_Windows - Glass") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          5 x IFCWINDOW | type IFCWINDOWSTYLE "V11 35x22" | object type "V11 35x22" | names: "Vindu 3 felt:V11 35x22:5464245", "Vindu 3 felt:V11 35x22:5464381", "Vindu 3 felt:V11 35x22:5464682" (+2 more) | material: materials ("NO_Aluminium", "NCS S 0502-Y", "N_Windows - Glass") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          2 x IFCWINDOW | type IFCWINDOWSTYLE "V12 35x22" | object type "V12 35x22" | names: "Vindu 3 felt:V12 35x22:5464550", "Vindu 3 felt:V12 35x22:5466633" | material: materials ("NO_Aluminium", "NCS S 0502-Y", "N_Windows - Glass") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "V6 24x22" | object type "V6 24x22" | names: "Vindu 3 felt:V6 24x22:5472792" | material: materials ("NCS S 0502-Y", "N_Windows - Glass") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:Rekkverksvegg" | object type "Basic Wall:Rekkverksvegg:5603317" | names: "Basic Wall:Rekkverksvegg:5603411", "Basic Wall:Rekkverksvegg:5607243" | material: layers "Basic Wall:Rekkverksvegg" ("Farge sort" 6.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          9 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:YV stolpe" | object type "Basic Wall:YV stolpe:5563726" | names: "Basic Wall:YV stolpe:5761711", "Basic Wall:YV stolpe:5761836", "Basic Wall:YV stolpe:5761874" (+6 more) | material: layers "Basic Wall:YV stolpe" ("Vindsperre" 9., "Stender isolert vegg" 98., "Gips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 8.1 18x21M 33dB" | object type "IDT 8.1 18x21M 33dB" | names: "_Dør Dobbel_Ulike_Dørblader_Glassfelt2:IDT 8.1 18x21M 33dB:6481045" | material: materials ("Glass Klart", "Lys grå", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          2 x IFCDOOR | type IFCDOORSTYLE "Luke 600" | object type "Luke 600" | names: "Luke600:Luke 600:6609756", "Luke600:Luke 600:6622567" | material: materials ("Light grey", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          2 x IFCDOOR | type IFCDOORSTYLE "Luke 600" | object type "Luke 600" | names: "Luke600:Luke 600:6623186", "Luke600:Luke 600:6623547" | material: materials ("Light grey", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          4 x IFCBEAM | type IFCBEAMTYPE "NOR-Bjelke-Tre-Stiplet:50x50" | object type "NOR-Bjelke-Tre-Stiplet:50x50:5644645" | names: "NOR-Bjelke-Tre-Stiplet:50x50:6647639", "NOR-Bjelke-Tre-Stiplet:50x50:6647666", "NOR-Bjelke-Tre-Stiplet:50x50:7415693" (+1 more) | material: "Wood - Dimensional lumber" | property sets: BaseQuantities, Pset_BeamCommon, Pset_TFM, Constraints, Dimensions, Geometric Position
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 3.2 145mm 48dB EI60 (HN-95-NR)" | object type "Basic Wall:IVA 3.2 145mm 48dB EI60 (HN-95-NR):4821417" | names: "Basic Wall:IVA 3.2 145mm 48dB EI60 (HN-95-NR):6673909", "Basic Wall:IVA 3.2 145mm 48dB EI60 (HN-95-NR):6673912" | material: layers "Basic Wall:IVA 3.2 145mm 48dB EI60 (HN-95-NR)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          1 x IFCWALL | type IFCWALLTYPE "Basic Wall:YV 1.2 517mm EI60" | object type "Basic Wall:YV 1.2 517mm EI60:6727771" | names: "Basic Wall:YV 1.2 517mm EI60:6727707" | material: materials ("Trekledning", "Luftsjikt", "Luftsjikt", "Luftsjikt", "Vindsperre", "Stender isolert vegg", "Vapor / Moisture Barriers - Damp-proofing", "NO_Utlekting", "Branngips") | property sets: Constraints, Dimensions, Other, Phasing, Structural, Text
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 3.1T 145mm 48dB EI60 (HN-95-NH)" | object type "Basic Wall:IVA 3.1T 145mm 48dB EI60 (HN-95-NH):6783138" | names: "Basic Wall:IVA 3.1T 145mm 48dB EI60 (HN-95-NH):6822092" | material: layers "Basic Wall:IVA 3.1T 145mm 48dB EI60 (HN-95-NH)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Habito" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:Skranke" | object type "Basic Wall:Skranke:6952733" | names: "Basic Wall:Skranke:6889376", "Basic Wall:Skranke:6952292" | material: layers "Basic Wall:Skranke" ("Baderomsinnredning Benkeplate" 100.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:30mm" | object type "Basic Wall:30mm:4152099" | names: "Basic Wall:30mm:6952543" | material: layers "Basic Wall:30mm" ("hvit malt" 30.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:18mm 2" | object type "Basic Wall:18mm 2:6904286" | names: "Basic Wall:18mm 2:7123639", "Basic Wall:18mm 2:7123640" | material: layers "Basic Wall:18mm 2" ("Laminate, Ivory, Matte" 18.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Projector" | object type "Projector" | names: "Spesialutstyr:Projector:7148148" | material: "hvit malt" | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 3.3T 145mm 48dB EI60 (RN-95-NNNR)" | object type "Basic Wall:IVA 3.3T 145mm 48dB EI60 (RN-95-NNNR):7239474" | names: "Basic Wall:IVA 3.3T 145mm 48dB EI60 (RN-95-NNNR):7239435" | material: layers "Basic Wall:IVA 3.3T 145mm 48dB EI60 (RN-95-NNNR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Gips" 13., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:Bassabsorbent 2" | object type "Basic Wall:Bassabsorbent 2:7503742" | names: "Basic Wall:Bassabsorbent 2:7504318" | material: layers "Basic Wall:Bassabsorbent 2" ("Metal - Steel" 10.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          22 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:Flis" | object type "Basic Wall:Flis:3605862" | names: "Basic Wall:Flis:7607442", "Basic Wall:Flis:7607472", "Basic Wall:Flis:7607544" (+19 more) | material: layers "Basic Wall:Flis" ("Flis" 5.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          4 x IFCRAILING | object type "Railing:Glassfelt - h=1000 bro" | names: "Railing:Glassfelt - h=1000 bro:2068610", "Railing:Glassfelt - h=1000 bro:2068741", "Railing:Glassfelt - h=1000 bro:3078809" (+1 more) | material: materials ("Glass Klart", "Lys grå") | property sets: Pset_RailingCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Other
          2 x IFCRAILING | object type "Railing:Handrail - h=1000" | names: "Railing:Handrail - h=1000:5306053", "Railing:Handrail - h=1000:7454507" | property sets: Pset_RailingCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCRAILING | object type "Railing:Handrail - vestibyle" | names: "Railing:Handrail - vestibyle:6605920" | property sets: Pset_RailingCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Other
        IFCSPACE "15" | long name "Area" | INTERNAL
        IFCSPACE "02030" | long name "fellesområde" | INTERNAL
          contains 10 elements
            1 x IFCFLOWTERMINAL | object type "Vaskerenne 1200mm" | names: "intra_wash_throuh_wall_mounted_1200_mm:Vaskerenne 1200mm:3640668" | material: materials ("f26d4e4b_a025_4dbf_b085_30ed485788cf", "4b4a701a_e8ab_4354_ac15_234043769b9c") | property sets: Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data, Mechanical
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Tavle 2m" | object type "Tavle 2m" | names: "Tavle:Tavle 2m:4358241" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
            2 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Skap, resirkulering 400 x 400 x 825mm" | object type "Skap, resirkulering 400 x 400 x 825mm" | names: "Base Cabinet Single Door:Skap, resirkulering 400 x 400 x 825mm:7158329", "Base Cabinet Single Door:Skap, resirkulering 400 x 400 x 825mm:7158330" | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
            2 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Skap, resirkulering 300 x 400 x 825mm" | object type "Skap, resirkulering 300 x 400 x 825mm" | names: "Base Cabinet Single Door:Skap, resirkulering 300 x 400 x 825mm:7158331", "Base Cabinet Single Door:Skap, resirkulering 300 x 400 x 825mm:7158332" | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
            1 x IFCFLOWTERMINAL | object type "Delabie flaskefyller" | names: "M_Tap_2:Delabie flaskefyller:7581083" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            2 x IFCFLOWCONTROLLER | type IFCVALVETYPE "Blandebatteri berøringsfri 1724FT" | object type "Blandebatteri berøringsfri 1724FT" | names: "1724FT(2013):Blandebatteri berøringsfri 1724FT:7581565", "1724FT(2013):Blandebatteri berøringsfri 1724FT:7581650" | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Benkeplate kildesortering 2" | object type "Benkeplate kildesortering 2" | names: "N_CounterTop:Benkeplate kildesortering 2:7722038" | material: "hvit malt" | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
        IFCSPACE "02032" | long name "klasse" | INTERNAL
          contains 4 elements
            1 x IFCCOVERING | object type "Compound Ceiling:Himling System 600x1200" | CEILING | names: "Compound Ceiling:Himling System 600x1200:3043772" | material: layers "Compound Ceiling:Himling System 600x1200" ("Himling Metallprofil" 38., "Himling System 600x1200" 12.) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Other
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "PC-skap" | object type "PC-skap" | names: "Spesialutstyr:PC-skap:3379484" | material: "hvit malt" | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Tavle 2m" | object type "Tavle 2m" | names: "Tavle:Tavle 2m:5299857" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Smartboard 2m" | object type "Smartboard 2m" | names: "Smartboard:Smartboard 2m:5299858" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
        IFCSPACE "02047" | long name "lærergard" | INTERNAL
          contains 7 elements
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Hattehylle360mm" | object type "Hattehylle360mm" | names: "NO_Hattehylle med stang:Hattehylle360mm:5347009" | material: "Wood - Birch, Natural" | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Skohylle" | object type "Skohylle" | names: "N_CounterTop:Skohylle:5347142" | material: "hvit malt" | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Other, Phasing
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Tørkeskap" | object type "Tørkeskap" | names: "Spesialutstyr spes equip:Tørkeskap:6479372" | material: "hvit malt" | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Tørkeskap" | object type "Tørkeskap" | names: "Spesialutstyr spes equip:Tørkeskap:6479373" | material: "hvit malt" | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
            3 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "gard skap 30cm 3" | object type "gard skap 30cm 3" | names: "Locker_Metal_Hadrian_Replacement-Front:gard skap 30cm 3:7182925", "Locker_Metal_Hadrian_Replacement-Front:gard skap 30cm 3:7182927", "Locker_Metal_Hadrian_Replacement-Front:gard skap 30cm 3:7182928" | material: materials ("Gul avdeling", "Steel - Hadrian - Black") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_TFM, Constraints, Construction, Dimensions
        IFCSPACE "02024" | long name "wc" | INTERNAL
          contains 3 elements
            1 x IFCFLOWTERMINAL | object type "Vegghengt toalett" | names: "WC-GBG-Nautic_1522-Wall_Mounted:Vegghengt toalett:3623944" | material: materials ("Gustavsberg Chrome - Polished", "Gustavsberg Porcelain - White (with C+)", "Gustavsberg Plastic - White") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWTERMINAL | object type "Servant - Ecco 50x35" | names: "Ecco:Servant - Ecco 50x35:3630194" | material: materials ("Gustavsberg Chrome - Polished", "Gustavsberg Porcelain - White") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "Blandebatteri berøringsfri 1724FT" | object type "Blandebatteri berøringsfri 1724FT" | names: "1724FT(2013):Blandebatteri berøringsfri 1724FT:7577453" | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
        IFCSPACE "02039" | long name "personal" | INTERNAL
          contains 24 elements
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Siemens induksjon" | object type "Siemens induksjon" | names: "N_Cook Top:Siemens induksjon:1943234" | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Skap, kjøkken 600 x 600 x 860mm" | object type "Skap, kjøkken 600 x 600 x 860mm" | names: "Base Cabinet Single Door:Skap, kjøkken 600 x 600 x 860mm:1943236" | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Other, Phasing
            1 x IFCFLOWTERMINAL | object type "Kum kjøkken" | names: "M_Sink Kitchen-Double:Kum kjøkken:1943239" | material: "Metal - Steel, Polished" | property sets: Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data, Other
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "OPPV.MASK, FRITTSTÅENDE, 60 CM" | object type "OPPV.MASK, FRITTSTÅENDE, 60 CM" | names: "Dishwasher:OPPV.MASK, FRITTSTÅENDE, 60 CM:2470491" | material: materials ("N_Cabinets", "EQ-Cozinha-Maquinas", "EQ-Cozinha-Maquinas-Porta", "Default Light Source", "N_Cabinets - Handles") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Siemens frittstående kombiskap" | object type "Siemens frittstående kombiskap" | names: "N_Refrigerator-Freezer:Siemens frittstående kombiskap:2470687" | material: "N_Cabinets" | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
            2 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Skap, kjøkken 600 x 600 x 860mm" | object type "Skap, kjøkken 600 x 600 x 860mm" | names: "N_Base Cabinet-3 drawers:Skap, kjøkken 600 x 600 x 860mm:2470977", "N_Base Cabinet-3 drawers:Skap, kjøkken 600 x 600 x 860mm:2471008" | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Other, Phasing
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Overskap 800 x 300 x 720mm" | object type "Overskap 800 x 300 x 720mm" | names: "N_Upper Cabinet-Double Door:Overskap 800 x 300 x 720mm:2471048" | material: "N_Cabinets" | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Skap, kjøkken 800 x 600 x 860mm" | object type "Skap, kjøkken 800 x 600 x 860mm" | names: "N_Base Cabinet-Double Door-for sink:Skap, kjøkken 800 x 600 x 860mm:2471096" | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
            5 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Overskap 600 x 300 x 700mm" | object type "Overskap 600 x 300 x 700mm" | names: "N_Upper Cabinet-Single Door:Overskap 600 x 300 x 700mm:2561632", "N_Upper Cabinet-Single Door:Overskap 600 x 300 x 700mm:2561701", "N_Upper Cabinet-Single Door:Overskap 600 x 300 x 700mm:2561864" (+2 more) | material: "N_Cabinets" | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Skap, kjøkken 600 x 600 x 860mm" | object type "Skap, kjøkken 600 x 600 x 860mm" | names: "Base Cabinet Single Door:Skap, kjøkken 600 x 600 x 860mm:2563308" | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Other, Phasing
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Siemens innebygget ovn" | object type "Siemens innebygget ovn" | names: "N_Oven-Built-in:Siemens innebygget ovn:2563715" | material: materials ("Glass", "EQ-Cozinha-Maquinas", "EQ-Cozinha-Maquinas-Porta") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
            2 x IFCCOVERING | object type "Compound Ceiling:Himling System 600x1200" | CEILING | names: "Compound Ceiling:Himling System 600x1200:2600839", "Compound Ceiling:Himling System 600x1200:3859583" | material: layers "Compound Ceiling:Himling System 600x1200" ("Himling Metallprofil" 38., "Himling System 600x1200" 12.) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
            2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Siemens mikro, 60skap" | object type "Siemens mikro, 60skap" | names: "Microwave_-_classic_amp_simple_13218:Siemens mikro, 60skap:4491013", "Microwave_-_classic_amp_simple_13218:Siemens mikro, 60skap:4491257" | material: materials ("Glass - black", "Metal - Aluminium", "Metal - Firring") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Overskap 600 x 300 x 700mm" | object type "Overskap 600 x 300 x 700mm" | names: "N_Upper Cabinet-Single Door:Overskap 600 x 300 x 700mm:4493408" | material: "N_Cabinets" | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Siemens frittstående kombiskap" | object type "Siemens frittstående kombiskap" | names: "N_Refrigerator-Freezer:Siemens frittstående kombiskap:6137613" | material: "N_Cabinets" | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
            1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "Blandebatteri - Oras Saphira 1039F" | object type "Blandebatteri - Oras Saphira 1039F" | names: "Oras Saphira:Blandebatteri - Oras Saphira 1039F:7588816" | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Benkeplate 625mm, Sigdal" | object type "Benkeplate 625mm, Sigdal" | names: "N_CounterTop:Benkeplate 625mm, Sigdal:7630609" | material: "hvit malt" | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
        IFCSPACE "02130" | long name "gruppe" | INTERNAL
          contains 3 elements
            1 x IFCCOVERING | object type "Compound Ceiling:Himling System 600x1200" | CEILING | names: "Compound Ceiling:Himling System 600x1200:3043681" | material: layers "Compound Ceiling:Himling System 600x1200" ("Himling Metallprofil" 38., "Himling System 600x1200" 12.) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "TV-skjerm" | object type "TV-skjerm" | names: "TV-skjerm:TV-skjerm:4453027" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Tavle 2m" | object type "Tavle 2m" | names: "Tavle:Tavle 2m:4453223" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
        IFCSPACE "02111" | long name "klasse" | INTERNAL
          contains 3 elements
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "PC-skap" | object type "PC-skap" | names: "Spesialutstyr:PC-skap:3379476" | material: "hvit malt" | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Tavle 2m" | object type "Tavle 2m" | names: "Tavle:Tavle 2m:5298755" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Smartboard 2m" | object type "Smartboard 2m" | names: "Smartboard:Smartboard 2m:5298756" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
        IFCSPACE "02128" | long name "klasse" | INTERNAL
          contains 3 elements
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "PC-skap" | object type "PC-skap" | names: "Spesialutstyr:PC-skap:3377794" | material: "hvit malt" | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Tavle 2m" | object type "Tavle 2m" | names: "Tavle:Tavle 2m:5298568" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Smartboard 2m" | object type "Smartboard 2m" | names: "Smartboard:Smartboard 2m:5298569" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
        IFCSPACE "02124" | long name "fellesområde" | INTERNAL
          contains 11 elements
            2 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Skap, resirkulering 400 x 400 x 825mm" | object type "Skap, resirkulering 400 x 400 x 825mm" | names: "Base Cabinet Single Door:Skap, resirkulering 400 x 400 x 825mm:2168335", "Base Cabinet Single Door:Skap, resirkulering 400 x 400 x 825mm:2168336" | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
            2 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Skap, resirkulering 300 x 400 x 825mm" | object type "Skap, resirkulering 300 x 400 x 825mm" | names: "Base Cabinet Single Door:Skap, resirkulering 300 x 400 x 825mm:2168337", "Base Cabinet Single Door:Skap, resirkulering 300 x 400 x 825mm:2168338" | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Other, Phasing
            1 x IFCFLOWTERMINAL | object type "Vaskerenne 1200mm" | names: "intra_wash_throuh_wall_mounted_1200_mm:Vaskerenne 1200mm:3640995" | material: materials ("f26d4e4b_a025_4dbf_b085_30ed485788cf", "4b4a701a_e8ab_4354_ac15_234043769b9c") | property sets: Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data, Mechanical
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Tavle 2m" | object type "Tavle 2m" | names: "Tavle:Tavle 2m:4325812" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
            1 x IFCCOVERING | object type "Compound Ceiling:Himling System 600x1200" | CEILING | names: "Compound Ceiling:Himling System 600x1200:4434218" | material: layers "Compound Ceiling:Himling System 600x1200" ("Himling Metallprofil" 38., "Himling System 600x1200" 12.) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
            1 x IFCFLOWTERMINAL | object type "Delabie flaskefyller" | names: "M_Tap_2:Delabie flaskefyller:7580925" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            2 x IFCFLOWCONTROLLER | type IFCVALVETYPE "Blandebatteri berøringsfri 1724FT" | object type "Blandebatteri berøringsfri 1724FT" | names: "1724FT(2013):Blandebatteri berøringsfri 1724FT:7581704", "1724FT(2013):Blandebatteri berøringsfri 1724FT:7581785" | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Benkeplate kildesortering 2" | object type "Benkeplate kildesortering 2" | names: "N_CounterTop:Benkeplate kildesortering 2:7721551" | material: "hvit malt" | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
        IFCSPACE "02127" | long name "gruppe" | INTERNAL
          contains 2 elements
            1 x IFCCOVERING | object type "Compound Ceiling:Himling System 600x1200" | CEILING | names: "Compound Ceiling:Himling System 600x1200:3046913" | material: layers "Compound Ceiling:Himling System 600x1200" ("Himling Metallprofil" 38., "Himling System 600x1200" 12.) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Other
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Tavle 2m" | object type "Tavle 2m" | names: "Tavle:Tavle 2m:4358691" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
        IFCSPACE "02106" | long name "gruppe" | INTERNAL
          contains 2 elements
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Tavle 2m" | object type "Tavle 2m" | names: "Tavle:Tavle 2m:4359654" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "TV-skjerm" | object type "TV-skjerm" | names: "TV-skjerm:TV-skjerm:4453346" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
        IFCSPACE "02107" | long name "klasse" | INTERNAL
          contains 3 elements
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "PC-skap" | object type "PC-skap" | names: "Spesialutstyr:PC-skap:2715936" | material: "hvit malt" | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Tavle 2m" | object type "Tavle 2m" | names: "Tavle:Tavle 2m:5298937" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Smartboard 2m" | object type "Smartboard 2m" | names: "Smartboard:Smartboard 2m:5298938" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
        IFCSPACE "02125" | long name "klasse" | INTERNAL
          contains 3 elements
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "PC-skap" | object type "PC-skap" | names: "Spesialutstyr:PC-skap:3379481" | material: "hvit malt" | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Tavle 2m" | object type "Tavle 2m" | names: "Tavle:Tavle 2m:5298684" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Smartboard 2m" | object type "Smartboard 2m" | names: "Smartboard:Smartboard 2m:5298685" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
        IFCSPACE "02110" | long name "klasse" | INTERNAL
          contains 3 elements
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "PC-skap" | object type "PC-skap" | names: "Spesialutstyr:PC-skap:3379479" | material: "hvit malt" | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Tavle 2m" | object type "Tavle 2m" | names: "Tavle:Tavle 2m:5298825" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Smartboard 2m" | object type "Smartboard 2m" | names: "Smartboard:Smartboard 2m:5298826" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
        IFCSPACE "02105" | long name "fellesområde" | INTERNAL
          contains 10 elements
            1 x IFCFLOWTERMINAL | object type "Vaskerenne 1200mm" | names: "intra_wash_throuh_wall_mounted_1200_mm:Vaskerenne 1200mm:3640882" | material: materials ("f26d4e4b_a025_4dbf_b085_30ed485788cf", "4b4a701a_e8ab_4354_ac15_234043769b9c") | property sets: Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data, Mechanical
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Tavle 2m" | object type "Tavle 2m" | names: "Tavle:Tavle 2m:4358239" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
            2 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Skap, resirkulering 400 x 400 x 825mm" | object type "Skap, resirkulering 400 x 400 x 825mm" | names: "Base Cabinet Single Door:Skap, resirkulering 400 x 400 x 825mm:7158066", "Base Cabinet Single Door:Skap, resirkulering 400 x 400 x 825mm:7158067" | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
            2 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Skap, resirkulering 300 x 400 x 825mm" | object type "Skap, resirkulering 300 x 400 x 825mm" | names: "Base Cabinet Single Door:Skap, resirkulering 300 x 400 x 825mm:7158068", "Base Cabinet Single Door:Skap, resirkulering 300 x 400 x 825mm:7158069" | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Other, Phasing
            1 x IFCFLOWTERMINAL | object type "Delabie flaskefyller" | names: "M_Tap_2:Delabie flaskefyller:7580977" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            2 x IFCFLOWCONTROLLER | type IFCVALVETYPE "Blandebatteri berøringsfri 1724FT" | object type "Blandebatteri berøringsfri 1724FT" | names: "1724FT(2013):Blandebatteri berøringsfri 1724FT:7581873", "1724FT(2013):Blandebatteri berøringsfri 1724FT:7581946" | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Benkeplate kildesortering 2" | object type "Benkeplate kildesortering 2" | names: "N_CounterTop:Benkeplate kildesortering 2:7721717" | material: "hvit malt" | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Other, Phasing
        IFCSPACE "02108" | long name "gruppe" | INTERNAL
          contains 1 element
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Tavle 2m" | object type "Tavle 2m" | names: "Tavle:Tavle 2m:4359458" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
        IFCSPACE "02119" | long name "lærerarbeid" | INTERNAL
        IFCSPACE "02149" | long name "bibliotek" | INTERNAL
          contains 5 elements
            2 x IFCCOVERING | object type "Compound Ceiling:Himling System 600x1200" | CEILING | names: "Compound Ceiling:Himling System 600x1200:4436096", "Compound Ceiling:Himling System 600x1200:4436928" | material: layers "Compound Ceiling:Himling System 600x1200" ("Himling Metallprofil" 38., "Himling System 600x1200" 12.) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Other
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Benkeplate 265mm, krogsæter" | object type "Benkeplate 265mm, krogsæter" | names: "N_CounterTop:Benkeplate 265mm, krogsæter:7788957" | material: "hvit malt" | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Other, Phasing
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Benkeplate 265mm, krogsæter" | object type "Benkeplate 265mm, krogsæter" | names: "N_CounterTop:Benkeplate 265mm, krogsæter:7789148" | material: "hvit malt" | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Other, Phasing
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Benkeplate 265mm, krogsæter" | object type "Benkeplate 265mm, krogsæter" | names: "N_CounterTop:Benkeplate 265mm, krogsæter:7789224" | material: "hvit malt" | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
        IFCSPACE "02129" | long name "klasse" | INTERNAL
          contains 3 elements
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "PC-skap" | object type "PC-skap" | names: "Spesialutstyr:PC-skap:3378122" | material: "hvit malt" | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Tavle 2m" | object type "Tavle 2m" | names: "Tavle:Tavle 2m:5298448" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Smartboard 2m" | object type "Smartboard 2m" | names: "Smartboard:Smartboard 2m:5298449" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
        IFCSPACE "02150" | long name "elevtjenester/møte" | INTERNAL
          contains 1 element
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Tavle 2,5m" | object type "Tavle 2,5m" | names: "Tavle:Tavle 2,5m:4359896" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
        IFCSPACE "02112" | long name "møterom" | INTERNAL
          contains 1 element
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Tavle 2m" | object type "Tavle 2m" | names: "Tavle:Tavle 2m:4359210" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
        IFCSPACE "02003" | long name "aula-øvre del" | INTERNAL
          contains 3 elements
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Mixebord" | object type "Mixebord" | names: "Mixebord:Mixebord:5503313" | material: materials ("Default", "hvit malt") | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Other, Phasing
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Lysrigg" | object type "Lysrigg" | names: "lysrigg:Lysrigg:6131495" | material: "hvit malt" | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Rullestol-ikon" | object type "Rullestol-ikon" | names: "Rullestol-ikon:Rullestol-ikon:6131984" | material: "Paint - White" | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Other, Phasing
        IFCSPACE "02109" | long name "gruppe" | INTERNAL
          contains 1 element
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Tavle 2m" | object type "Tavle 2m" | names: "Tavle:Tavle 2m:4359622" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
        IFCSPACE "02067" | long name "gruppe" | INTERNAL
          contains 2 elements
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Tavle 2m" | object type "Tavle 2m" | names: "Tavle:Tavle 2m:4360631" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "TV-skjerm" | object type "TV-skjerm" | names: "TV-skjerm:TV-skjerm:4453759" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
        IFCSPACE "02058" | long name "lærerarbeid" | INTERNAL
        IFCSPACE "02066" | long name "klasse" | INTERNAL
          contains 3 elements
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "PC-skap" | object type "PC-skap" | names: "Spesialutstyr:PC-skap:3379498" | material: "hvit malt" | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Tavle 2m" | object type "Tavle 2m" | names: "Tavle:Tavle 2m:5299254" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Smartboard 2m" | object type "Smartboard 2m" | names: "Smartboard:Smartboard 2m:5299255" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
        IFCSPACE "02062" | long name "klasse" | INTERNAL
          contains 3 elements
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "PC-skap" | object type "PC-skap" | names: "Spesialutstyr:PC-skap:3379506" | material: "hvit malt" | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Tavle 2m" | object type "Tavle 2m" | names: "Tavle:Tavle 2m:5299506" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Smartboard 2m" | object type "Smartboard 2m" | names: "Smartboard:Smartboard 2m:5299507" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
        IFCSPACE "02035" | long name "klasse" | INTERNAL
          contains 4 elements
            1 x IFCCOVERING | object type "Compound Ceiling:Himling System 600x1200" | CEILING | names: "Compound Ceiling:Himling System 600x1200:3043953" | material: layers "Compound Ceiling:Himling System 600x1200" ("Himling Metallprofil" 38., "Himling System 600x1200" 12.) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "PC-skap" | object type "PC-skap" | names: "Spesialutstyr:PC-skap:3379486" | material: "hvit malt" | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Tavle 2m" | object type "Tavle 2m" | names: "Tavle:Tavle 2m:5299771" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Smartboard 2m" | object type "Smartboard 2m" | names: "Smartboard:Smartboard 2m:5299772" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
        IFCSPACE "02064" | long name "gruppe" | INTERNAL
          contains 1 element
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Tavle 1,5m" | object type "Tavle 1,5m" | names: "Tavle:Tavle 1,5m:4496955" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
        IFCSPACE "02068" | long name "mottak" | INTERNAL
          contains 3 elements
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "PC-skap" | object type "PC-skap" | names: "Spesialutstyr:PC-skap:3387542" | material: "hvit malt" | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Tavle 2m" | object type "Tavle 2m" | names: "Tavle:Tavle 2m:5299133" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Smartboard 2m" | object type "Smartboard 2m" | names: "Smartboard:Smartboard 2m:5299134" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
        IFCSPACE "02065" | long name "klasse" | INTERNAL
          contains 3 elements
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "PC-skap" | object type "PC-skap" | names: "Spesialutstyr:PC-skap:3379501" | material: "hvit malt" | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Tavle 2m" | object type "Tavle 2m" | names: "Tavle:Tavle 2m:5299342" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Smartboard 2m" | object type "Smartboard 2m" | names: "Smartboard:Smartboard 2m:5299343" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
        IFCSPACE "02061" | long name "fellesområde" | INTERNAL
          contains 10 elements
            1 x IFCFLOWTERMINAL | object type "Vaskerenne 1200mm" | names: "intra_wash_throuh_wall_mounted_1200_mm:Vaskerenne 1200mm:3640750" | material: materials ("f26d4e4b_a025_4dbf_b085_30ed485788cf", "4b4a701a_e8ab_4354_ac15_234043769b9c") | property sets: Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data, Mechanical
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Tavle 2m" | object type "Tavle 2m" | names: "Tavle:Tavle 2m:4358240" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
            2 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Skap, resirkulering 400 x 400 x 825mm" | object type "Skap, resirkulering 400 x 400 x 825mm" | names: "Base Cabinet Single Door:Skap, resirkulering 400 x 400 x 825mm:7158179", "Base Cabinet Single Door:Skap, resirkulering 400 x 400 x 825mm:7158180" | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
            2 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Skap, resirkulering 300 x 400 x 825mm" | object type "Skap, resirkulering 300 x 400 x 825mm" | names: "Base Cabinet Single Door:Skap, resirkulering 300 x 400 x 825mm:7158181", "Base Cabinet Single Door:Skap, resirkulering 300 x 400 x 825mm:7158182" | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Other, Phasing
            1 x IFCFLOWTERMINAL | object type "Delabie flaskefyller" | names: "M_Tap_2:Delabie flaskefyller:7581165" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            2 x IFCFLOWCONTROLLER | type IFCVALVETYPE "Blandebatteri berøringsfri 1724FT" | object type "Blandebatteri berøringsfri 1724FT" | names: "1724FT(2013):Blandebatteri berøringsfri 1724FT:7581258", "1724FT(2013):Blandebatteri berøringsfri 1724FT:7581325" | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Benkeplate kildesortering 2" | object type "Benkeplate kildesortering 2" | names: "N_CounterTop:Benkeplate kildesortering 2:7721918" | material: "hvit malt" | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
        IFCSPACE "02063" | long name "gruppe" | INTERNAL
          contains 1 element
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Tavle 2m" | object type "Tavle 2m" | names: "Tavle:Tavle 2m:4360817" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
        IFCSPACE "02031" | long name "gruppe" | INTERNAL
          contains 2 elements
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Tavle 2m" | object type "Tavle 2m" | names: "Tavle:Tavle 2m:4360161" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "TV-skjerm" | object type "TV-skjerm" | names: "TV-skjerm:TV-skjerm:4453609" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
        IFCSPACE "02036" | long name "klasse" | INTERNAL
          contains 3 elements
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "PC-skap" | object type "PC-skap" | names: "Spesialutstyr:PC-skap:3379489" | material: "hvit malt" | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Tavle 2m" | object type "Tavle 2m" | names: "Tavle:Tavle 2m:5299653" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Smartboard 2m" | object type "Smartboard 2m" | names: "Smartboard:Smartboard 2m:5299654" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
        IFCSPACE "02048" | long name "sjakt" | INTERNAL
        IFCSPACE "02053" | long name "kopi" | INTERNAL
        IFCSPACE "02148" | long name "gruppe" | INTERNAL
        IFCSPACE "02059" | long name "hcwc" | INTERNAL
          contains 5 elements
            1 x IFCFLOWTERMINAL | object type "Gulvstående toalett - Nautic 1546" | names: "WC-GBG-Nautic_1546-Floor_Standing:Gulvstående toalett - Nautic 1546:1825739" | material: materials ("Gustavsberg Chrome - Polished", "Gustavsberg Porcelain - White", "Gustavsberg Plastic - White") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWTERMINAL | object type "Servant HCWC - 7119" | names: "Washbasin-GBG-7119_Bolt_Mounting:Servant HCWC - 7119:3628691" | material: "Gustavsberg Porcelain - White" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "Blandebatteri berøringsfri 1724FT" | object type "Blandebatteri berøringsfri 1724FT" | names: "1724FT(2013):Blandebatteri berøringsfri 1724FT:7589216" | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Armstøtte veggmontert" | object type "Armstøtte veggmontert" | names: "WC_Armrest-GBG-1712_Wall_Mounted:Armstøtte veggmontert:7602919", "WC_Armrest-GBG-1712_Wall_Mounted:Armstøtte veggmontert:7602936" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_TFM, Constraints, Dimensions, Electrical - Loads
        IFCSPACE "02113" | long name "hcwc" | INTERNAL
          contains 5 elements
            1 x IFCFLOWTERMINAL | object type "Gulvstående toalett - Nautic 1546" | names: "WC-GBG-Nautic_1546-Floor_Standing:Gulvstående toalett - Nautic 1546:1908234" | material: materials ("Gustavsberg Chrome - Polished", "Gustavsberg Porcelain - White", "Gustavsberg Plastic - White") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWTERMINAL | object type "Servant HCWC - 7119" | names: "Washbasin-GBG-7119_Bolt_Mounting:Servant HCWC - 7119:3628794" | material: "Gustavsberg Porcelain - White" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "Blandebatteri berøringsfri 1724FT" | object type "Blandebatteri berøringsfri 1724FT" | names: "1724FT(2013):Blandebatteri berøringsfri 1724FT:7589366" | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Armstøtte veggmontert" | object type "Armstøtte veggmontert" | names: "WC_Armrest-GBG-1712_Wall_Mounted:Armstøtte veggmontert:7602666", "WC_Armrest-GBG-1712_Wall_Mounted:Armstøtte veggmontert:7602678" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_TFM, Constraints, Dimensions, Electrical - Loads
        IFCSPACE "02040" | long name "lærergard" | INTERNAL
          contains 8 elements
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Skohylle" | object type "Skohylle" | names: "N_CounterTop:Skohylle:5346002" | material: "hvit malt" | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Hattehylle360mm" | object type "Hattehylle360mm" | names: "NO_Hattehylle med stang:Hattehylle360mm:5346814" | material: "Wood - Birch, Natural" | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Tørkeskap" | object type "Tørkeskap" | names: "Spesialutstyr spes equip:Tørkeskap:6479367" | material: "hvit malt" | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Tørkeskap" | object type "Tørkeskap" | names: "Spesialutstyr spes equip:Tørkeskap:6479370" | material: "hvit malt" | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
            4 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "gard skap 30cm 3" | object type "gard skap 30cm 3" | names: "Locker_Metal_Hadrian_Replacement-Front:gard skap 30cm 3:7182932", "Locker_Metal_Hadrian_Replacement-Front:gard skap 30cm 3:7182933", "Locker_Metal_Hadrian_Replacement-Front:gard skap 30cm 3:7182934" (+1 more) | material: materials ("Gul avdeling", "Steel - Hadrian - Black") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_TFM, Constraints, Construction, Dimensions
        IFCSPACE "02045" | long name "wc" | INTERNAL
          contains 3 elements
            1 x IFCFLOWTERMINAL | object type "Vegghengt toalett" | names: "WC-GBG-Nautic_1522-Wall_Mounted:Vegghengt toalett:3624685" | material: materials ("Gustavsberg Chrome - Polished", "Gustavsberg Porcelain - White (with C+)", "Gustavsberg Plastic - White") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWTERMINAL | object type "Servant - Ecco 50x35" | names: "Ecco:Servant - Ecco 50x35:3630682" | material: materials ("Gustavsberg Chrome - Polished", "Gustavsberg Porcelain - White") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "Blandebatteri berøringsfri 1724FT" | object type "Blandebatteri berøringsfri 1724FT" | names: "1724FT(2013):Blandebatteri berøringsfri 1724FT:7577038" | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
        IFCSPACE "02126" | long name "gruppe" | INTERNAL
          contains 2 elements
            1 x IFCCOVERING | object type "Compound Ceiling:Himling System 600x1200" | CEILING | names: "Compound Ceiling:Himling System 600x1200:2601933" | material: layers "Compound Ceiling:Himling System 600x1200" ("Himling Metallprofil" 38., "Himling System 600x1200" 12.) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Tavle 2m" | object type "Tavle 2m" | names: "Tavle:Tavle 2m:4358983" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
        IFCSPACE "02044" | long name "dusj" | INTERNAL
          contains 3 elements
            1 x IFCFLOWTERMINAL | object type "Dusjhode - Oras Apollo 530" | names: "Dusj:Dusjhode - Oras Apollo 530:5271553" | material: "Aluminum" | property sets: Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data, Other
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Vegghengt benk" | object type "Vegghengt benk" | names: "Benk:Vegghengt benk:5348883" | material: "hvit malt" | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
            1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "Blandebatteri dusj 7264" | object type "Blandebatteri dusj 7264" | names: "Oras Oramix:Blandebatteri dusj 7264:7600732" | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
        IFCSPACE "02102" | long name "IKT" | INTERNAL
        IFCSPACE "02091" | long name "EL" | INTERNAL
        IFCSPACE "02140" | long name "trapp" | INTERNAL
          contains 2 elements
            2 x IFCCOVERING | object type "Compound Ceiling:Himling System 600x600" | CEILING | names: "Compound Ceiling:Himling System 600x600:4433230", "Compound Ceiling:Himling System 600x600:7495781" | material: layers "Compound Ceiling:Himling System 600x600" ("Himling Metallprofil" 38., "Himling System 600x600" 12.) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Other
        IFCSPACE "02100" | long name "trapp" | INTERNAL
          contains 2 elements
            2 x IFCCOVERING | object type "Compound Ceiling:Himling System 600x600" | CEILING | names: "Compound Ceiling:Himling System 600x600:4435087", "Compound Ceiling:Himling System 600x600:7495931" | material: layers "Compound Ceiling:Himling System 600x600" ("Himling Metallprofil" 38., "Himling System 600x600" 12.) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
        IFCSPACE "02090" | long name "trapp" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | object type "Compound Ceiling:Himling System 600x600" | CEILING | names: "Compound Ceiling:Himling System 600x600:3924626" | material: layers "Compound Ceiling:Himling System 600x600" ("Himling Metallprofil" 38., "Himling System 600x600" 12.) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
        IFCSPACE "02020" | long name "trapp" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | object type "Compound Ceiling:Himling System 600x600" | CEILING | names: "Compound Ceiling:Himling System 600x600:3924590" | material: layers "Compound Ceiling:Himling System 600x600" ("Himling Metallprofil" 38., "Himling System 600x600" 12.) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
        IFCSPACE "02122" | long name "lærerarbeid" | INTERNAL
        IFCSPACE "02121" | long name "stille" | INTERNAL
        IFCSPACE "02123" | long name "garderobe" | INTERNAL
          contains 46 elements
            9 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Elevskap" | object type "Elevskap" | names: "Lockers x 2:Elevskap:3367075", "Lockers x 2:Elevskap:3371862", "Lockers x 2:Elevskap:3371889" (+6 more) | material: materials ("Paint - Grey", "Skapdør 2", "Gul avdeling") | property sets: Pset_TFM, Constraints, Dimensions, Materials and Finishes, Other, Phasing
            9 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Elevskap" | object type "Elevskap" | names: "Lockers x 2:Elevskap:3371825", "Lockers x 2:Elevskap:3371887", "Lockers x 2:Elevskap:3371890" (+6 more) | material: materials ("Paint - Grey", "Skapdør 3", "Skapdør 2") | property sets: Pset_TFM, Constraints, Dimensions, Materials and Finishes, Other, Phasing
            9 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Elevskap" | object type "Elevskap" | names: "Lockers x 2:Elevskap:3371861", "Lockers x 2:Elevskap:3371888", "Lockers x 2:Elevskap:3371919" (+6 more) | material: materials ("Paint - Grey", "Gul avdeling", "Skapdør 3") | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
            6 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Elevskap" | object type "Elevskap" | names: "Lockers x 2:Elevskap:3376174", "Lockers x 2:Elevskap:3376177", "Lockers x 2:Elevskap:3376180" (+3 more) | material: materials ("Paint - Grey", "Gul avdeling", "Skapdør 3") | property sets: Pset_TFM, Constraints, Dimensions, Materials and Finishes, Other, Phasing
            6 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Elevskap" | object type "Elevskap" | names: "Lockers x 2:Elevskap:3376175", "Lockers x 2:Elevskap:3376178", "Lockers x 2:Elevskap:3376181" (+3 more) | material: materials ("Paint - Grey", "Skapdør 2", "Gul avdeling") | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
            6 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Elevskap" | object type "Elevskap" | names: "Lockers x 2:Elevskap:3376176", "Lockers x 2:Elevskap:3376179", "Lockers x 2:Elevskap:3376182" (+3 more) | material: materials ("Paint - Grey", "Skapdør 3", "Skapdør 2") | property sets: Pset_TFM, Constraints, Dimensions, Materials and Finishes, Other, Phasing
            1 x IFCCOVERING | object type "Compound Ceiling:Lydhimling gips" | CEILING | names: "Compound Ceiling:Lydhimling gips:4706180" | material: layers "Compound Ceiling:Lydhimling gips" ("Himling Metallprofil" 48., "Gips" 12.5, "Gips" 12.5) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
        IFCSPACE "02144" | long name "wc" | INTERNAL
          contains 3 elements
            1 x IFCFLOWTERMINAL | object type "Servant - Ecco 50x35" | names: "Ecco:Servant - Ecco 50x35:3630018" | material: materials ("Gustavsberg Chrome - Polished", "Gustavsberg Porcelain - White") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWTERMINAL | object type "Vegghengt toalett" | names: "WC-GBG-Nautic_1522-Wall_Mounted:Vegghengt toalett:3658578" | material: materials ("Gustavsberg Chrome - Polished", "Gustavsberg Porcelain - White (with C+)", "Gustavsberg Plastic - White") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "Blandebatteri berøringsfri 1724FT" | object type "Blandebatteri berøringsfri 1724FT" | names: "1724FT(2013):Blandebatteri berøringsfri 1724FT:7576388" | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
        IFCSPACE "02104" | long name "garderobe" | INTERNAL
          contains 45 elements
            9 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Elevskap" | object type "Elevskap" | names: "Lockers x 2:Elevskap:3374437", "Lockers x 2:Elevskap:3374438", "Lockers x 2:Elevskap:3374439" (+6 more) | material: materials ("Paint - Grey", "_White") | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
            36 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Elevskap" | object type "Elevskap" | names: "Lockers x 2:Elevskap:3374446", "Lockers x 2:Elevskap:3374447", "Lockers x 2:Elevskap:3374448" (+33 more) | material: materials ("Paint - Grey", "_White") | property sets: Pset_TFM, Constraints, Dimensions, Materials and Finishes, Other, Phasing
        IFCSPACE "02115" | long name "wc" | INTERNAL
          contains 3 elements
            1 x IFCFLOWTERMINAL | object type "Servant - Ecco 50x35" | names: "Ecco:Servant - Ecco 50x35:3629722" | material: materials ("Gustavsberg Chrome - Polished", "Gustavsberg Porcelain - White") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWTERMINAL | object type "Vegghengt toalett" | names: "WC-GBG-Nautic_1522-Wall_Mounted:Vegghengt toalett:3659155" | material: materials ("Gustavsberg Chrome - Polished", "Gustavsberg Porcelain - White (with C+)", "Gustavsberg Plastic - White") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "Blandebatteri berøringsfri 1724FT" | object type "Blandebatteri berøringsfri 1724FT" | names: "1724FT(2013):Blandebatteri berøringsfri 1724FT:7576535" | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
        IFCSPACE "02120" | long name "kopi" | INTERNAL
        IFCSPACE "02052" | long name "lærerarbeid" | INTERNAL
        IFCSPACE "02054" | long name "stille" | INTERNAL
        IFCSPACE "02029" | long name "garderobe" | INTERNAL
          contains 45 elements
            27 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Elevskap" | object type "Elevskap" | names: "Lockers x 2:Elevskap:3375132", "Lockers x 2:Elevskap:3375133", "Lockers x 2:Elevskap:3375134" (+24 more) | material: materials ("Paint - Grey", "_White") | property sets: Pset_TFM, Constraints, Dimensions, Materials and Finishes, Other, Phasing
            18 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Elevskap" | object type "Elevskap" | names: "Lockers x 2:Elevskap:3375141", "Lockers x 2:Elevskap:3375142", "Lockers x 2:Elevskap:3375143" (+15 more) | material: materials ("Paint - Grey", "_White") | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
        IFCSPACE "02060" | long name "garderobe" | INTERNAL
          contains 52 elements
            25 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Elevskap" | object type "Elevskap" | names: "Lockers x 2:Elevskap:3374746", "Lockers x 2:Elevskap:3374747", "Lockers x 2:Elevskap:3374748" (+22 more) | material: materials ("Paint - Grey", "_White") | property sets: Pset_TFM, Constraints, Dimensions, Materials and Finishes, Other, Phasing
            27 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Elevskap" | object type "Elevskap" | names: "Lockers x 2:Elevskap:3374755", "Lockers x 2:Elevskap:3374756", "Lockers x 2:Elevskap:3374757" (+24 more) | material: materials ("Paint - Grey", "_White") | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
        IFCSPACE "02050" | long name "hcwc" | INTERNAL
          contains 7 elements
            1 x IFCFLOWTERMINAL | object type "Gulvstående toalett - Nautic 1546" | names: "WC-GBG-Nautic_1546-Floor_Standing:Gulvstående toalett - Nautic 1546:2147921" | material: materials ("Gustavsberg Chrome - Polished", "Gustavsberg Porcelain - White", "Gustavsberg Plastic - White") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWTERMINAL | object type "Servant HCWC - 7119" | names: "Washbasin-GBG-7119_Bolt_Mounting:Servant HCWC - 7119:3882745" | material: "Gustavsberg Porcelain - White" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWTERMINAL | object type "Dusjhode - Oras Apollo 530" | names: "Dusj:Dusjhode - Oras Apollo 530:5271605" | material: "Aluminum" | property sets: Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data, Other
            1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "Blandebatteri berøringsfri 1724FT" | object type "Blandebatteri berøringsfri 1724FT" | names: "1724FT(2013):Blandebatteri berøringsfri 1724FT:7589296" | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "Blandebatteri dusj 7267" | object type "Blandebatteri dusj 7267" | names: "Oras Oramix:Blandebatteri dusj 7267:7600560" | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Armstøtte veggmontert" | object type "Armstøtte veggmontert" | names: "WC_Armrest-GBG-1712_Wall_Mounted:Armstøtte veggmontert:7602773", "WC_Armrest-GBG-1712_Wall_Mounted:Armstøtte veggmontert:7602803" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_TFM, Constraints, Dimensions, Electrical - Loads
        IFCSPACE "02041" | long name "dusj" | INTERNAL
          contains 3 elements
            1 x IFCFLOWTERMINAL | object type "Dusjhode - Oras Apollo 530" | names: "Dusj:Dusjhode - Oras Apollo 530:5271522" | material: "Aluminum" | property sets: Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data, Other
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Vegghengt benk" | object type "Vegghengt benk" | names: "Benk:Vegghengt benk:5348695" | material: "hvit malt" | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
            1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "Blandebatteri dusj 7264" | object type "Blandebatteri dusj 7264" | names: "Oras Oramix:Blandebatteri dusj 7264:7600651" | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
        IFCSPACE "02042" | long name "wc" | INTERNAL
          contains 3 elements
            1 x IFCFLOWTERMINAL | object type "Vegghengt toalett" | names: "WC-GBG-Nautic_1522-Wall_Mounted:Vegghengt toalett:3624292" | material: materials ("Gustavsberg Chrome - Polished", "Gustavsberg Porcelain - White (with C+)", "Gustavsberg Plastic - White") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWTERMINAL | object type "Servant - Ecco 50x35" | names: "Ecco:Servant - Ecco 50x35:3630532" | material: materials ("Gustavsberg Chrome - Polished", "Gustavsberg Porcelain - White") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "Blandebatteri berøringsfri 1724FT" | object type "Blandebatteri berøringsfri 1724FT" | names: "1724FT(2013):Blandebatteri berøringsfri 1724FT:7577093" | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
        IFCSPACE "02049" | long name "bk" | INTERNAL
          contains 2 elements
            1 x IFCFLOWTERMINAL | object type "Utslagsvask" | names: "intra_gub1_bucket_sink_wall_mounted:Utslagsvask:3639851" | material: "f26d4e4b_a025_4dbf_b085_30ed485788cf" | property sets: Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data, Mechanical
            1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "Blandebatteri 3970" | object type "Blandebatteri 3970" | names: "Oras Saga:Blandebatteri 3970:7601588" | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
        IFCSPACE "02101" | long name "EL" | INTERNAL
        IFCSPACE "02142" | long name "disp" | INTERNAL
        IFCSPACE "02021" | long name "EL" | INTERNAL
        IFCSPACE "02043" | long name "wc" | INTERNAL
          contains 3 elements
            1 x IFCFLOWTERMINAL | object type "Vegghengt toalett" | names: "WC-GBG-Nautic_1522-Wall_Mounted:Vegghengt toalett:3624401" | material: materials ("Gustavsberg Chrome - Polished", "Gustavsberg Porcelain - White (with C+)", "Gustavsberg Plastic - White") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWTERMINAL | object type "Servant - Ecco 50x35" | names: "Ecco:Servant - Ecco 50x35:3630568" | material: materials ("Gustavsberg Chrome - Polished", "Gustavsberg Porcelain - White") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "Blandebatteri berøringsfri 1724FT" | object type "Blandebatteri berøringsfri 1724FT" | names: "1724FT(2013):Blandebatteri berøringsfri 1724FT:7577120" | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
        IFCSPACE "02046" | long name "wc" | INTERNAL
          contains 3 elements
            1 x IFCFLOWTERMINAL | object type "Vegghengt toalett" | names: "WC-GBG-Nautic_1522-Wall_Mounted:Vegghengt toalett:3624568" | material: materials ("Gustavsberg Chrome - Polished", "Gustavsberg Porcelain - White (with C+)", "Gustavsberg Plastic - White") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWTERMINAL | object type "Servant - Ecco 50x35" | names: "Ecco:Servant - Ecco 50x35:3938616" | material: materials ("Gustavsberg Chrome - Polished", "Gustavsberg Porcelain - White") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "Blandebatteri berøringsfri 1724FT" | object type "Blandebatteri berøringsfri 1724FT" | names: "1724FT(2013):Blandebatteri berøringsfri 1724FT:7576961" | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
        IFCSPACE "02056" | long name "wc" | INTERNAL
          contains 3 elements
            1 x IFCFLOWTERMINAL | object type "Vegghengt toalett" | names: "WC-GBG-Nautic_1522-Wall_Mounted:Vegghengt toalett:3624861" | material: materials ("Gustavsberg Chrome - Polished", "Gustavsberg Porcelain - White (with C+)", "Gustavsberg Plastic - White") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWTERMINAL | object type "Servant - Ecco 50x35" | names: "Ecco:Servant - Ecco 50x35:4697596" | material: materials ("Gustavsberg Chrome - Polished", "Gustavsberg Porcelain - White") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "Blandebatteri berøringsfri 1724FT" | object type "Blandebatteri berøringsfri 1724FT" | names: "1724FT(2013):Blandebatteri berøringsfri 1724FT:7576893" | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
        IFCSPACE "02002" | long name "kantine -øvre del" | INTERNAL
          contains 7 elements
            1 x IFCFLOWTERMINAL | object type "Kum kantine" | names: "Utslagsvask:Kum kantine:2558997" | material: "Metal - Aluminium" | property sets: Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data, Other
            2 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Skap, resirkulering 400 x 460 x 825mm" | object type "Skap, resirkulering 400 x 460 x 825mm" | names: "Base Cabinet Single Door:Skap, resirkulering 400 x 460 x 825mm:7159511", "Base Cabinet Single Door:Skap, resirkulering 400 x 460 x 825mm:7159512" | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Other, Phasing
            2 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Skap, resirkulering 300 x 460 x 825mm" | object type "Skap, resirkulering 300 x 460 x 825mm" | names: "Base Cabinet Single Door:Skap, resirkulering 300 x 460 x 825mm:7159513", "Base Cabinet Single Door:Skap, resirkulering 300 x 460 x 825mm:7159514" | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Other, Phasing
            1 x IFCFLOWTERMINAL | object type "Delabie flaskefyller" | names: "M_Tap_2:Delabie flaskefyller:7580049" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Benkeplate kildesortering" | object type "Benkeplate kildesortering" | names: "N_CounterTop:Benkeplate kildesortering:7721393" | material: "hvit malt" | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
        IFCSPACE "02143" | long name "sluse/korr" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | object type "Compound Ceiling:Himling System 600x1200" | CEILING | names: "Compound Ceiling:Himling System 600x1200:3045386" | material: layers "Compound Ceiling:Himling System 600x1200" ("Himling Metallprofil" 38., "Himling System 600x1200" 12.) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
        IFCSPACE "02017" | long name "heis" | INTERNAL
        IFCSPACE "02092" | long name "sjakt" | INTERNAL
        IFCSPACE "02055" | long name "sjakt" | INTERNAL
        IFCSPACE "02057" | long name "wc" | INTERNAL
          contains 4 elements
            1 x IFCCOVERING | object type "Compound Ceiling:Himling System 600x600" | CEILING | names: "Compound Ceiling:Himling System 600x600:3044642" | material: layers "Compound Ceiling:Himling System 600x600" ("Himling Metallprofil" 38., "Himling System 600x600" 12.) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
            1 x IFCFLOWTERMINAL | object type "Vegghengt toalett" | names: "WC-GBG-Nautic_1522-Wall_Mounted:Vegghengt toalett:3624907" | material: materials ("Gustavsberg Chrome - Polished", "Gustavsberg Porcelain - White (with C+)", "Gustavsberg Plastic - White") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWTERMINAL | object type "Servant - Ecco 50x35" | names: "Ecco:Servant - Ecco 50x35:3630806" | material: materials ("Gustavsberg Chrome - Polished", "Gustavsberg Porcelain - White") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "Blandebatteri berøringsfri 1724FT" | object type "Blandebatteri berøringsfri 1724FT" | names: "1724FT(2013):Blandebatteri berøringsfri 1724FT:7576666" | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
        IFCSPACE "02023" | long name "sluse/korr" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | object type "Compound Ceiling:Himling System 600x1200" | CEILING | names: "Compound Ceiling:Himling System 600x1200:3044971" | material: layers "Compound Ceiling:Himling System 600x1200" ("Himling Metallprofil" 38., "Himling System 600x1200" 12.) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
        IFCSPACE "02022" | long name "sjakt" | INTERNAL
        IFCSPACE "02025" | long name "wc" | INTERNAL
          contains 4 elements
            1 x IFCCOVERING | object type "Compound Ceiling:Himling System 600x600" | CEILING | names: "Compound Ceiling:Himling System 600x600:3044949" | material: layers "Compound Ceiling:Himling System 600x600" ("Himling Metallprofil" 38., "Himling System 600x600" 12.) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Other
            1 x IFCFLOWTERMINAL | object type "Vegghengt toalett" | names: "WC-GBG-Nautic_1522-Wall_Mounted:Vegghengt toalett:3623970" | material: materials ("Gustavsberg Chrome - Polished", "Gustavsberg Porcelain - White (with C+)", "Gustavsberg Plastic - White") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWTERMINAL | object type "Servant - Ecco 50x35" | names: "Ecco:Servant - Ecco 50x35:3630251" | material: materials ("Gustavsberg Chrome - Polished", "Gustavsberg Porcelain - White") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "Blandebatteri berøringsfri 1724FT" | object type "Blandebatteri berøringsfri 1724FT" | names: "1724FT(2013):Blandebatteri berøringsfri 1724FT:7577228" | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
        IFCSPACE "02026" | long name "wc" | INTERNAL
          contains 4 elements
            1 x IFCCOVERING | object type "Compound Ceiling:Himling System 600x600" | CEILING | names: "Compound Ceiling:Himling System 600x600:3044915" | material: layers "Compound Ceiling:Himling System 600x600" ("Himling Metallprofil" 38., "Himling System 600x600" 12.) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
            1 x IFCFLOWTERMINAL | object type "Vegghengt toalett" | names: "WC-GBG-Nautic_1522-Wall_Mounted:Vegghengt toalett:3624043" | material: materials ("Gustavsberg Chrome - Polished", "Gustavsberg Porcelain - White (with C+)", "Gustavsberg Plastic - White") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWTERMINAL | object type "Servant - Ecco 50x35" | names: "Ecco:Servant - Ecco 50x35:3630312" | material: materials ("Gustavsberg Chrome - Polished", "Gustavsberg Porcelain - White") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "Blandebatteri berøringsfri 1724FT" | object type "Blandebatteri berøringsfri 1724FT" | names: "1724FT(2013):Blandebatteri berøringsfri 1724FT:7577378" | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
        IFCSPACE "02027" | long name "wc" | INTERNAL
          contains 4 elements
            1 x IFCCOVERING | object type "Compound Ceiling:Himling System 600x600" | CEILING | names: "Compound Ceiling:Himling System 600x600:3044863" | material: layers "Compound Ceiling:Himling System 600x600" ("Himling Metallprofil" 38., "Himling System 600x600" 12.) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Other
            1 x IFCFLOWTERMINAL | object type "Vegghengt toalett" | names: "WC-GBG-Nautic_1522-Wall_Mounted:Vegghengt toalett:3624117" | material: materials ("Gustavsberg Chrome - Polished", "Gustavsberg Porcelain - White (with C+)", "Gustavsberg Plastic - White") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWTERMINAL | object type "Servant - Ecco 50x35" | names: "Ecco:Servant - Ecco 50x35:3630374" | material: materials ("Gustavsberg Chrome - Polished", "Gustavsberg Porcelain - White") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "Blandebatteri berøringsfri 1724FT" | object type "Blandebatteri berøringsfri 1724FT" | names: "1724FT(2013):Blandebatteri berøringsfri 1724FT:7577301" | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
        IFCSPACE "02028" | long name "sjakt" | INTERNAL
        IFCSPACE "02037" | long name "korridor" | INTERNAL
          contains 12 elements
            1 x IFCCOVERING | object type "Compound Ceiling:Himling System 600x1200" | CEILING | names: "Compound Ceiling:Himling System 600x1200:2600749" | material: layers "Compound Ceiling:Himling System 600x1200" ("Himling Metallprofil" 38., "Himling System 600x1200" 12.) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Ladeskap - sykkel" | object type "Ladeskap - sykkel" | names: "Spesialutstyr spes equip:Ladeskap - sykkel:4997808" | material: "hvit malt" | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
            2 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Skap, resirkulering 400 x 400 x 825mm" | object type "Skap, resirkulering 400 x 400 x 825mm" | names: "Base Cabinet Single Door:Skap, resirkulering 400 x 400 x 825mm:7158463", "Base Cabinet Single Door:Skap, resirkulering 400 x 400 x 825mm:7158464" | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Other, Phasing
            2 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Skap, resirkulering 300 x 400 x 825mm" | object type "Skap, resirkulering 300 x 400 x 825mm" | names: "Base Cabinet Single Door:Skap, resirkulering 300 x 400 x 825mm:7158465", "Base Cabinet Single Door:Skap, resirkulering 300 x 400 x 825mm:7158466" | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Other, Phasing
            3 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Corpus 800" | object type "Corpus 800" | names: "Locker_Metal_Hadrian_Replacement-Front:Corpus 800:7217252", "Locker_Metal_Hadrian_Replacement-Front:Corpus 800:7217434", "Locker_Metal_Hadrian_Replacement-Front:Corpus 800:7217460" | material: materials ("Gul avdeling", "Steel - Hadrian - Black") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_TFM, Constraints, Construction, Dimensions
            2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Corpus 800" | object type "Corpus 800" | names: "Locker_Metal_Hadrian_Replacement-Front:Corpus 800:7217420", "Locker_Metal_Hadrian_Replacement-Front:Corpus 800:7217447" | material: materials ("Gul avdeling", "Steel - Hadrian - Black") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_TFM, Constraints, Construction, Dimensions
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Benkeplate kildesortering 2" | object type "Benkeplate kildesortering 2" | names: "N_CounterTop:Benkeplate kildesortering 2:7722404" | material: "hvit malt" | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Other, Phasing
        IFCSPACE "02038" | long name "personal/møte" | INTERNAL
          contains 1 element
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Whiteboard 3m" | object type "Whiteboard 3m" | names: "Tavle:Whiteboard 3m:4458115" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
        IFCSPACE "02051" | long name "korridor" | INTERNAL
          contains 11 elements
            2 x IFCCOVERING | object type "Compound Ceiling:Himling System 600x1200" | CEILING | names: "Compound Ceiling:Himling System 600x1200:3044389", "Compound Ceiling:Himling System 600x1200:4461232" | material: layers "Compound Ceiling:Himling System 600x1200" ("Himling Metallprofil" 38., "Himling System 600x1200" 12.) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Other
            9 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Elevskap" | object type "Elevskap" | names: "Lockers x 2:Elevskap:3384918", "Lockers x 2:Elevskap:3384919", "Lockers x 2:Elevskap:3384920" (+6 more) | material: materials ("Paint - Grey", "_White") | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
        IFCSPACE "02093" | long name "sluse/korr" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | object type "Compound Ceiling:Himling System 600x1200" | CEILING | names: "Compound Ceiling:Himling System 600x1200:3046226" | material: layers "Compound Ceiling:Himling System 600x1200" ("Himling Metallprofil" 38., "Himling System 600x1200" 12.) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Other
        IFCSPACE "02103" | long name "sluse/korr" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | object type "Compound Ceiling:Himling System 600x1200" | CEILING | names: "Compound Ceiling:Himling System 600x1200:2592110" | material: layers "Compound Ceiling:Himling System 600x1200" ("Himling Metallprofil" 38., "Himling System 600x1200" 12.) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Other
        IFCSPACE "02116" | long name "wc" | INTERNAL
          contains 4 elements
            1 x IFCCOVERING | object type "Compound Ceiling:Himling System 600x600" | CEILING | names: "Compound Ceiling:Himling System 600x600:2410973" | material: layers "Compound Ceiling:Himling System 600x600" ("Himling Metallprofil" 38., "Himling System 600x600" 12.) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
            1 x IFCFLOWTERMINAL | object type "Servant - Ecco 50x35" | names: "Ecco:Servant - Ecco 50x35:3629758" | material: materials ("Gustavsberg Chrome - Polished", "Gustavsberg Porcelain - White") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWTERMINAL | object type "Vegghengt toalett" | names: "WC-GBG-Nautic_1522-Wall_Mounted:Vegghengt toalett:3659080" | material: materials ("Gustavsberg Chrome - Polished", "Gustavsberg Porcelain - White (with C+)", "Gustavsberg Plastic - White") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "Blandebatteri berøringsfri 1724FT" | object type "Blandebatteri berøringsfri 1724FT" | names: "1724FT(2013):Blandebatteri berøringsfri 1724FT:7576492" | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
        IFCSPACE "02117" | long name "wc" | INTERNAL
          contains 4 elements
            1 x IFCCOVERING | object type "Compound Ceiling:Himling System 600x600" | CEILING | names: "Compound Ceiling:Himling System 600x600:2410983" | material: layers "Compound Ceiling:Himling System 600x600" ("Himling Metallprofil" 38., "Himling System 600x600" 12.) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
            1 x IFCFLOWTERMINAL | object type "Vegghengt toalett" | names: "WC-GBG-Nautic_1522-Wall_Mounted:Vegghengt toalett:3623768" | material: materials ("Gustavsberg Chrome - Polished", "Gustavsberg Porcelain - White (with C+)", "Gustavsberg Plastic - White") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWTERMINAL | object type "Servant - Ecco 50x35" | names: "Ecco:Servant - Ecco 50x35:3629811" | material: materials ("Gustavsberg Chrome - Polished", "Gustavsberg Porcelain - White") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "Blandebatteri berøringsfri 1724FT" | object type "Blandebatteri berøringsfri 1724FT" | names: "1724FT(2013):Blandebatteri berøringsfri 1724FT:7576592" | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
        IFCSPACE "02118" | long name "sjakt" | INTERNAL
        IFCSPACE "02114" | long name "korridor" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | object type "Compound Ceiling:Himling System 600x1200" | CEILING | names: "Compound Ceiling:Himling System 600x1200:2602320" | material: layers "Compound Ceiling:Himling System 600x1200" ("Himling Metallprofil" 38., "Himling System 600x1200" 12.) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Other
        IFCSPACE "02141" | long name "EL" | INTERNAL
        IFCSPACE "02145" | long name "wc" | INTERNAL
          contains 4 elements
            1 x IFCCOVERING | object type "Compound Ceiling:Himling System 600x600" | CEILING | names: "Compound Ceiling:Himling System 600x600:3048220" | material: layers "Compound Ceiling:Himling System 600x600" ("Himling Metallprofil" 38., "Himling System 600x600" 12.) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Other
            1 x IFCFLOWTERMINAL | object type "Servant - Ecco 50x35" | names: "Ecco:Servant - Ecco 50x35:3629965" | material: materials ("Gustavsberg Chrome - Polished", "Gustavsberg Porcelain - White") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWTERMINAL | object type "Vegghengt toalett" | names: "WC-GBG-Nautic_1522-Wall_Mounted:Vegghengt toalett:3658515" | material: materials ("Gustavsberg Chrome - Polished", "Gustavsberg Porcelain - White (with C+)", "Gustavsberg Plastic - White") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "Blandebatteri berøringsfri 1724FT" | object type "Blandebatteri berøringsfri 1724FT" | names: "1724FT(2013):Blandebatteri berøringsfri 1724FT:7576226" | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
        IFCSPACE "02146" | long name "wc" | INTERNAL
          contains 4 elements
            1 x IFCCOVERING | object type "Compound Ceiling:Himling System 600x600" | CEILING | names: "Compound Ceiling:Himling System 600x600:3048284" | material: layers "Compound Ceiling:Himling System 600x600" ("Himling Metallprofil" 38., "Himling System 600x600" 12.) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
            1 x IFCFLOWTERMINAL | object type "Servant - Ecco 50x35" | names: "Ecco:Servant - Ecco 50x35:3629946" | material: materials ("Gustavsberg Chrome - Polished", "Gustavsberg Porcelain - White") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWTERMINAL | object type "Vegghengt toalett" | names: "WC-GBG-Nautic_1522-Wall_Mounted:Vegghengt toalett:3658497" | material: materials ("Gustavsberg Chrome - Polished", "Gustavsberg Porcelain - White (with C+)", "Gustavsberg Plastic - White") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "Blandebatteri berøringsfri 1724FT" | object type "Blandebatteri berøringsfri 1724FT" | names: "1724FT(2013):Blandebatteri berøringsfri 1724FT:7576321" | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
        IFCSPACE "02151" | long name "bk" | INTERNAL
          contains 2 elements
            1 x IFCFLOWTERMINAL | object type "Utslagsvask" | names: "intra_gub1_bucket_sink_wall_mounted:Utslagsvask:3639958" | material: "f26d4e4b_a025_4dbf_b085_30ed485788cf" | property sets: Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data, Mechanical
            1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "Blandebatteri 3970" | object type "Blandebatteri 3970" | names: "Oras Saga:Blandebatteri 3970:7601416" | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
        IFCSPACE "02152" | long name "sjakt" | INTERNAL
        IFCSPACE "02069" | long name "dusj" | INTERNAL
          contains 3 elements
            1 x IFCCOVERING | object type "Compound Ceiling:Himling System 600x600 hygiene" | CEILING | names: "Compound Ceiling:Himling System 600x600 hygiene:3045525" | material: layers "Compound Ceiling:Himling System 600x600 hygiene" ("Himling Metallprofil" 38., "Himling System 600x600" 12.) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
            1 x IFCFLOWTERMINAL | object type "Dusjhode" | names: "Dusj:Dusjhode:5271499" | material: "Aluminum" | property sets: Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data, Other
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Vegghengt benk" | object type "Vegghengt benk" | names: "Benk:Vegghengt benk:5397658" | material: "hvit malt" | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Other, Phasing
        IFCSPACE "02055" | long name "sjakt" | INTERNAL
        IFCSPACE "3" | long name "Area" | INTERNAL
        IFCSPACE "02034" | long name "gruppe" | INTERNAL
          contains 1 element
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Tavle 2m" | object type "Tavle 2m" | names: "Tavle:Tavle 2m:4360299" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
        IFCSPACE "02033" | long name "gruppe" | INTERNAL
          contains 2 elements
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Tavle 2m" | object type "Tavle 2m" | names: "Tavle:Tavle 2m:4360544" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "TV-skjerm" | object type "TV-skjerm" | names: "TV-skjerm:TV-skjerm:4473306" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
        IFCSPACE "12" | long name "Area" | INTERNAL
      IFCBUILDINGSTOREY "Plan 03" | long name "Plan 03" | elevation 8059.99999999973
        contains 341 elements
          3 x IFCSLAB | object type "Floor:Betongdekke 320 + 80 påstøp + 10 avretting" | FLOOR | names: "Floor:Betongdekke 320 + 80 påstøp + 10 avretting:1663916", "Floor:Betongdekke 320 + 80 påstøp + 10 avretting:4440744", "Floor:Betongdekke 320 + 80 påstøp + 10 avretting:4440744:2" | material: layers "Floor:Betongdekke 320 + 80 påstøp + 10 avretting" ("Betong avretting" 10., "Betong påstøp" 80., "Betong" 320.) | property sets: Pset_SlabCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Other
          5 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 3.3T 145mm EI60 (RN-95-NR)" | object type "Basic Wall:IVA 3.3T 145mm EI60 (RN-95-NR):6701511" | names: "Basic Wall:IVA 3.3T 145mm EI60 (RN-95-NR):1700403", "Basic Wall:IVA 3.3T 145mm EI60 (RN-95-NR):1700440", "Basic Wall:IVA 3.3T 145mm EI60 (RN-95-NR):2190120" (+2 more) | material: layers "Basic Wall:IVA 3.3T 145mm EI60 (RN-95-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          2 x IFCSLAB | object type "Floor:Betongdekke 320 + 30 avretting" | FLOOR | names: "Floor:Betongdekke 320 + 30 avretting:1700417", "Floor:Betongdekke 320 + 30 avretting:1700417:2" | material: layers "Floor:Betongdekke 320 + 30 avretting" ("Betong avretting" 30., "Betong" 320.) | property sets: Pset_SlabCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Other
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 11.1 193mm 48dB (RN-95-NR)" | object type "Basic Wall:IVA 11.1 193mm 48dB (RN-95-NR):6718454" | names: "Basic Wall:IVA 11.1 193mm 48dB (RN-95-NR):1700902" | material: layers "Basic Wall:IVA 11.1 193mm 48dB (RN-95-NR)" ("Robustgips" 13., "<Unnamed>" 13., "<Unnamed>" 10., "stender/isolasjon" 98., "<Unnamed>" 20., "<Unnamed>" 48., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 3.3 145mm EI60 (RN-95-NR)" | object type "Basic Wall:IVA 3.3 145mm EI60 (RN-95-NR):2850935" | names: "Basic Wall:IVA 3.3 145mm EI60 (RN-95-NR):1700905", "Basic Wall:IVA 3.3 145mm EI60 (RN-95-NR):1971745", "Basic Wall:IVA 3.3 145mm EI60 (RN-95-NR):1971748" (+1 more) | material: layers "Basic Wall:IVA 3.3 145mm EI60 (RN-95-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          14 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 1.1 121mm 44dB (H-95-H)" | object type "Basic Wall:IVA 1.1 121mm 44dB (H-95-H):4807508" | names: "Basic Wall:IVA 1.1 121mm 44dB (H-95-H):1700916", "Basic Wall:IVA 1.1 121mm 44dB (H-95-H):1919229", "Basic Wall:IVA 1.1 121mm 44dB (H-95-H):1919237" (+11 more) | material: layers "Basic Wall:IVA 1.1 121mm 44dB (H-95-H)" ("Habito" 13., "stender/isolasjon" 95., "Habito" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCDOOR | type IFCDOORSTYLE "IDA 7.1 15x21M EI60CS" | object type "IDA 7.1 15x21M EI60CS" | names: "Enfløyet_aludør:IDA 7.1 15x21M EI60CS:1700918" | material: materials ("Karm Malt", "Lys grå", "Terskel Tre") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDA 7.1 15x21M EI60CS" | object type "IDA 7.1 15x21M EI60CS" | names: "Enfløyet_aludør:IDA 7.1 15x21M EI60CS:1700920" | material: materials ("Karm Malt", "Lys grå", "Terskel Tre") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          2 x IFCROOF | object type "Basic Roof:Tak betong 320 + påstøp 80 + 150" | names: "Basic Roof:Tak betong 320 + påstøp 80 + 150:1703529", "Basic Roof:Tak betong 320 + påstøp 80 + 150:2082229" | parts: 2 IFCSLAB | property sets: Pset_RoofCommon, Pset_TFM, Constraints, Construction, Dimensions, Identity Data
          6 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:YV 1.1 517mm" | object type "Basic Wall:YV 1.1 517mm:1735105" | names: "Basic Wall:YV 1.1 517mm:1736839", "Basic Wall:YV 1.1 517mm:1736840", "Basic Wall:YV 1.1 517mm:1736841" (+3 more) | material: layers "Basic Wall:YV 1.1 517mm" ("Trekledning" 19., "Luftsjikt" 48., "Luftsjikt" 36., "Luftsjikt" 48., "Vindsperre" 9., "Stender isolert vegg" 296., "NO_Utlekting" 48., "Robustgips" 12.5) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 2.1 134mm 48dB (H-95-NH)" | object type "Basic Wall:IVA 2.1 134mm 48dB (H-95-NH):4807019" | names: "Basic Wall:IVA 2.1 134mm 48dB (H-95-NH):1771554", "Basic Wall:IVA 2.1 134mm 48dB (H-95-NH):4810905" | material: layers "Basic Wall:IVA 2.1 134mm 48dB (H-95-NH)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 95., "Habito" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 3.3 145mm 37dB EI60 (RN-95-NR)" | object type "Basic Wall:IVA 3.3 145mm 37dB EI60 (RN-95-NR):4823028" | names: "Basic Wall:IVA 3.3 145mm 37dB EI60 (RN-95-NR):1855846", "Basic Wall:IVA 3.3 145mm 37dB EI60 (RN-95-NR):2235682", "Basic Wall:IVA 3.3 145mm 37dB EI60 (RN-95-NR):4383422" | material: layers "Basic Wall:IVA 3.3 145mm 37dB EI60 (RN-95-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 3.3 145mm 48dB EI60 (RN-95-NR)" | object type "Basic Wall:IVA 3.3 145mm 48dB EI60 (RN-95-NR):2860483" | names: "Basic Wall:IVA 3.3 145mm 48dB EI60 (RN-95-NR):1915458" | material: layers "Basic Wall:IVA 3.3 145mm 48dB EI60 (RN-95-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCDOOR | type IFCDOORSTYLE "IDA 3.1 18x21M 33db EI30S" | object type "IDA 3.1 18x21M 33db EI30S" | names: "_Dør Dobbel_Ulike_Dørblader_Glassfelt:IDA 3.1 18x21M 33db EI30S:1915514" | material: materials ("Glass Klart", "Lys grå", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 3.3T 145mm 48dB EI60 (RN-95-NR)" | object type "Basic Wall:IVA 3.3T 145mm 48dB EI60 (RN-95-NR):6691651" | names: "Basic Wall:IVA 3.3T 145mm 48dB EI60 (RN-95-NR):1915854", "Basic Wall:IVA 3.3T 145mm 48dB EI60 (RN-95-NR):4207330" | material: layers "Basic Wall:IVA 3.3T 145mm 48dB EI60 (RN-95-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCDOOR | type IFCDOORSTYLE "IDA 3.1 18x21M 33db EI30S" | object type "IDA 3.1 18x21M 33db EI30S" | names: "_Dør Dobbel_Ulike_Dørblader_Glassfelt:IDA 3.1 18x21M 33db EI30S:1915951" | material: materials ("Glass Klart", "Lys grå", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDF 2.1 Foldevegg 8000x2800" | object type "IDF 2.1 Foldevegg 8000x2800" | names: "Side_Stack_Operable_Wall_8000:IDF 2.1 Foldevegg 8000x2800:1916249" | material: materials ("Light grey", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          5 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 3.3 145mm 48dB (RN-95-NR)" | object type "Basic Wall:IVA 3.3 145mm 48dB (RN-95-NR):2849733" | names: "Basic Wall:IVA 3.3 145mm 48dB (RN-95-NR):1916504", "Basic Wall:IVA 3.3 145mm 48dB (RN-95-NR):1919485", "Basic Wall:IVA 3.3 145mm 48dB (RN-95-NR):1919487" (+2 more) | material: layers "Basic Wall:IVA 3.3 145mm 48dB (RN-95-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          2 x IFCDOOR | type IFCDOORSTYLE "IDT 3.6 10x21M 38dB" | object type "IDT 3.6 10x21M 38dB" | names: "Dør Enkel_ Glassfelt:IDT 3.6 10x21M 38dB:1919231", "Dør Enkel_ Glassfelt:IDT 3.6 10x21M 38dB:1919255" | material: materials ("NCS S 2500-N", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 2.2 134mm 34dB (H-95-NR)" | object type "Basic Wall:IVA 2.2 134mm 34dB (H-95-NR):4823696" | names: "Basic Wall:IVA 2.2 134mm 34dB (H-95-NR):1919240" | material: layers "Basic Wall:IVA 2.2 134mm 34dB (H-95-NR)" ("Habito" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          7 x IFCDOOR | type IFCDOORSTYLE "IDT 3.6 10x21M 38dB" | object type "IDT 3.6 10x21M 38dB" | names: "Dør Enkel_ Glassfelt:IDT 3.6 10x21M 38dB:1919258", "Dør Enkel_ Glassfelt:IDT 3.6 10x21M 38dB:1919259", "Dør Enkel_ Glassfelt:IDT 3.6 10x21M 38dB:1919523" (+4 more) | material: materials ("NCS S 2500-N", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          5 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 1.1T 121mm 44dB (H-95-H)" | object type "Basic Wall:IVA 1.1T 121mm 44dB (H-95-H):6691464" | names: "Basic Wall:IVA 1.1T 121mm 44dB (H-95-H):1919492", "Basic Wall:IVA 1.1T 121mm 44dB (H-95-H):1919495", "Basic Wall:IVA 1.1T 121mm 44dB (H-95-H):1919498" (+2 more) | material: layers "Basic Wall:IVA 1.1T 121mm 44dB (H-95-H)" ("Habito" 13., "stender/isolasjon" 95., "Habito" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 2.1T 134mm 48dB (H-95-NH)" | object type "Basic Wall:IVA 2.1T 134mm 48dB (H-95-NH):6691061" | names: "Basic Wall:IVA 2.1T 134mm 48dB (H-95-NH):1919493", "Basic Wall:IVA 2.1T 134mm 48dB (H-95-NH):2162667", "Basic Wall:IVA 2.1T 134mm 48dB (H-95-NH):4755193" | material: layers "Basic Wall:IVA 2.1T 134mm 48dB (H-95-NH)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 95., "Habito" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          4 x IFCDOOR | type IFCDOORSTYLE "IDT 3.6 10x21M 38dB" | object type "IDT 3.6 10x21M 38dB" | names: "Dør Enkel_ Glassfelt:IDT 3.6 10x21M 38dB:1919504", "Dør Enkel_ Glassfelt:IDT 3.6 10x21M 38dB:2988445", "Dør Enkel_ Glassfelt:IDT 3.6 10x21M 38dB:2988446" (+1 more) | material: materials ("NCS S 2500-N", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 6.1 302mm 44dB (HN-95-30-95-NH)" | object type "Basic Wall:IVA 6.1 302mm 44dB (HN-95-30-95-NH):3855970" | names: "Basic Wall:IVA 6.1 302mm 44dB (HN-95-30-95-NH):1919518" | material: layers "Basic Wall:IVA 6.1 302mm 44dB (HN-95-30-95-NH)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 95., "Luftsjikt" 60., "stender/isolasjon" 95., "Gips" 13., "Habito" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 2.1 134mm 44dB (H-95-NH)" | object type "Basic Wall:IVA 2.1 134mm 44dB (H-95-NH):4808479" | names: "Basic Wall:IVA 2.1 134mm 44dB (H-95-NH):1919519", "Basic Wall:IVA 2.1 134mm 44dB (H-95-NH):4810811" | material: layers "Basic Wall:IVA 2.1 134mm 44dB (H-95-NH)" ("Habito" 13., "stender/isolasjon" 95., "Gips" 13., "Habito" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 5.2 15x21M EI60S" | object type "IDT 5.2 15x21M EI60S" | names: "Dør Dobbel:IDT 5.2 15x21M EI60S:1971746" | material: materials ("NCS S 1000-N", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 5.2 15x21M EI60S" | object type "IDT 5.2 15x21M EI60S" | names: "Dør Dobbel:IDT 5.2 15x21M EI60S:1971747" | material: materials ("NCS S 1000-N", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 6.2T 272mm 55dB EI60 (HN-95-30-95-NR)" | object type "Basic Wall:IVA 6.2T 272mm 55dB EI60 (HN-95-30-95-NR):6822742" | names: "Basic Wall:IVA 6.2T 272mm 55dB EI60 (HN-95-30-95-NR):2100542" | material: layers "Basic Wall:IVA 6.2T 272mm 55dB EI60 (HN-95-30-95-NR)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 95., "Luftsjikt" 30., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 4.3T 172mm 34dB (RN-120-NR)" | object type "Basic Wall:IVA 4.3T 172mm 34dB (RN-120-NR):6691836" | names: "Basic Wall:IVA 4.3T 172mm 34dB (RN-120-NR):2100543" | material: layers "Basic Wall:IVA 4.3T 172mm 34dB (RN-120-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 120., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 6.2T 272mm 48dB EI60 (HN-95-60-95-NR)" | object type "Basic Wall:IVA 6.2T 272mm 48dB EI60 (HN-95-60-95-NR):6783710" | names: "Basic Wall:IVA 6.2T 272mm 48dB EI60 (HN-95-60-95-NR):2100545" | material: layers "Basic Wall:IVA 6.2T 272mm 48dB EI60 (HN-95-60-95-NR)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 95., "Luftsjikt" 60., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 1.1T 121mm 34dB (H-95-H)" | object type "Basic Wall:IVA 1.1T 121mm 34dB (H-95-H):6702432" | names: "Basic Wall:IVA 1.1T 121mm 34dB (H-95-H):2100546", "Basic Wall:IVA 1.1T 121mm 34dB (H-95-H):2100559" | material: layers "Basic Wall:IVA 1.1T 121mm 34dB (H-95-H)" ("Habito" 13., "stender/isolasjon" 95., "Habito" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          3 x IFCDOOR | type IFCDOORSTYLE "IDT 1.2 8x21M 33dB" | object type "IDT 1.2 8x21M 33dB" | names: "Dør Enkel:IDT 1.2 8x21M 33dB:2100547", "Dør Enkel:IDT 1.2 8x21M 33dB:2100554", "Dør Enkel:IDT 1.2 8x21M 33dB:2100566" | material: materials ("Terskel Tre", "NCS S 0500-N", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          3 x IFCDOOR | type IFCDOORSTYLE "IDT 1.2 8x21M 33dB" | object type "IDT 1.2 8x21M 33dB" | names: "Dør Enkel:IDT 1.2 8x21M 33dB:2100553", "Dør Enkel:IDT 1.2 8x21M 33dB:2100560", "Dør Enkel:IDT 1.2 8x21M 33dB:2100567" | material: materials ("Terskel Tre", "NCS S 0500-N", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 6.2T 272mm 48dB EI60 (HN-95-30-95-NR)" | object type "Basic Wall:IVA 6.2T 272mm 48dB EI60 (HN-95-30-95-NR):6703668" | names: "Basic Wall:IVA 6.2T 272mm 48dB EI60 (HN-95-30-95-NR):2100555", "Basic Wall:IVA 6.2T 272mm 48dB EI60 (HN-95-30-95-NR):2100558" | material: layers "Basic Wall:IVA 6.2T 272mm 48dB EI60 (HN-95-30-95-NR)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 95., "Luftsjikt" 30., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 1.3T 121mm 34dB (R-95-R)" | object type "Basic Wall:IVA 1.3T 121mm 34dB (R-95-R):6691719" | names: "Basic Wall:IVA 1.3T 121mm 34dB (R-95-R):2100556" | material: layers "Basic Wall:IVA 1.3T 121mm 34dB (R-95-R)" ("Robustgips" 13., "stender/isolasjon" 95., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 4.1T 172mm 34dB (HN-120-NH)" | object type "Basic Wall:IVA 4.1T 172mm 34dB (HN-120-NH):6783070" | names: "Basic Wall:IVA 4.1T 172mm 34dB (HN-120-NH):2100626" | material: layers "Basic Wall:IVA 4.1T 172mm 34dB (HN-120-NH)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 120., "Gips" 13., "Habito" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 6.1T 272mm 55dB EI60 (HN-95-30-95-NH)" | object type "Basic Wall:IVA 6.1T 272mm 55dB EI60 (HN-95-30-95-NH):6822634" | names: "Basic Wall:IVA 6.1T 272mm 55dB EI60 (HN-95-30-95-NH):2100699" | material: layers "Basic Wall:IVA 6.1T 272mm 55dB EI60 (HN-95-30-95-NH)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 95., "Luftsjikt" 30., "stender/isolasjon" 95., "Gips" 13., "Habito" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 7.1 121mm 37dB EI30 (95-NR)" | object type "Basic Wall:IVA 7.1 121mm 37dB EI30 (95-NR):6023854" | names: "Basic Wall:IVA 7.1 121mm 37dB EI30 (95-NR):2101750", "Basic Wall:IVA 7.1 121mm 37dB EI30 (95-NR):2347768" | material: layers "Basic Wall:IVA 7.1 121mm 37dB EI30 (95-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 1.1 121mm 34dB (H-95-H)" | object type "Basic Wall:IVA 1.1 121mm 34dB (H-95-H):4819050" | names: "Basic Wall:IVA 1.1 121mm 34dB (H-95-H):2102524", "Basic Wall:IVA 1.1 121mm 34dB (H-95-H):4049794" | material: layers "Basic Wall:IVA 1.1 121mm 34dB (H-95-H)" ("Habito" 13., "stender/isolasjon" 95., "Habito" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 3.1T 145mm 48dB EI60 (HN-95-NH)" | object type "Basic Wall:IVA 3.1T 145mm 48dB EI60 (HN-95-NH):6783138" | names: "Basic Wall:IVA 3.1T 145mm 48dB EI60 (HN-95-NH):2137694", "Basic Wall:IVA 3.1T 145mm 48dB EI60 (HN-95-NH):4207329" | material: layers "Basic Wall:IVA 3.1T 145mm 48dB EI60 (HN-95-NH)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Habito" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 1.1 121mm (H-95-H)" | object type "Basic Wall:IVA 1.1 121mm (H-95-H):4814431" | names: "Basic Wall:IVA 1.1 121mm (H-95-H):2168668" | material: layers "Basic Wall:IVA 1.1 121mm (H-95-H)" ("Habito" 13., "stender/isolasjon" 95., "Habito" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 6.1 302mm (HN-95-60-95-NH)" | object type "Basic Wall:IVA 6.1 302mm (HN-95-60-95-NH):3658349" | names: "Basic Wall:IVA 6.1 302mm (HN-95-60-95-NH):2168669" | material: layers "Basic Wall:IVA 6.1 302mm (HN-95-60-95-NH)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 95., "Luftsjikt" 60., "stender/isolasjon" 95., "Gips" 13., "Habito" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 5.2 15x21M EI60S" | object type "IDT 5.2 15x21M EI60S" | names: "Dør Dobbel:IDT 5.2 15x21M EI60S:2190610" | material: materials ("NCS S 1000-N", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 5.2 15x21M EI60S" | object type "IDT 5.2 15x21M EI60S" | names: "Dør Dobbel:IDT 5.2 15x21M EI60S:2190704" | material: materials ("NCS S 1000-N", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "V24 20x20" | object type "V24 20x20" | names: "Vindu-Fast:V24 20x20:2217007" | material: materials ("Glass Klart", "NCS S 0502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "V24 20x20" | object type "V24 20x20" | names: "Vindu-Fast:V24 20x20:2217110" | material: materials ("Glass Klart", "NCS S 0502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 8.1 125mm sjaktvegg 37dB EI60" | object type "Basic Wall:IVA 8.1 125mm sjaktvegg 37dB EI60:2857583" | names: "Basic Wall:IVA 8.1 125mm sjaktvegg 37dB EI60:2235681" | material: layers "Basic Wall:IVA 8.1 125mm sjaktvegg 37dB EI60" ("Branngips" 15., "Branngips" 15., "stender/isolasjon" 95.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 3.2 145mm 37dB EI60 (HN-95-NR)" | object type "Basic Wall:IVA 3.2 145mm 37dB EI60 (HN-95-NR):2850426" | names: "Basic Wall:IVA 3.2 145mm 37dB EI60 (HN-95-NR):2235683" | material: layers "Basic Wall:IVA 3.2 145mm 37dB EI60 (HN-95-NR)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          1 x IFCSLAB | object type "Floor:Betongdekke 400 + 30 avretting" | FLOOR | names: "Floor:Betongdekke 400 + 30 avretting:2369486" | material: layers "Floor:Betongdekke 400 + 30 avretting" ("Betong avretting" 30., "Betong" 400.) | property sets: Pset_SlabCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:YV 12.1 411 Ventilasjonsrom" | object type "Basic Wall:YV 12.1 411 Ventilasjonsrom:5093016" | names: "Basic Wall:YV 12.1 411 Ventilasjonsrom:2383912", "Basic Wall:YV 12.1 411 Ventilasjonsrom:5402836", "Basic Wall:YV 12.1 411 Ventilasjonsrom:5404973" (+1 more) | material: layers "Basic Wall:YV 12.1 411 Ventilasjonsrom" ("Spiler ute" 19., "Luftsjikt" 36., "Luftsjikt" 36., "Vindsperre" 9., "Stender isolert vegg" 250., "Stender isolert vegg" 48., "Habito" 12.5, "Habito" 12.5) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:YV 12.1 411 Ventilasjonsrom EI 60" | object type "Basic Wall:YV 12.1 411 Ventilasjonsrom EI 60:5093156" | names: "Basic Wall:YV 12.1 411 Ventilasjonsrom EI 60:2384554", "Basic Wall:YV 12.1 411 Ventilasjonsrom EI 60:6268552" | material: layers "Basic Wall:YV 12.1 411 Ventilasjonsrom EI 60" ("Spiler ute" 19., "Luftsjikt" 36., "Luftsjikt" 36., "Vindsperre" 9., "Stender isolert vegg" 250., "Stender isolert vegg" 48., "Habito" 12.5, "Habito" 12.5) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCDOOR | type IFCDOORSTYLE "YDS 1.2 15x21M EI 60S" | object type "YDS 1.2 15x21M EI 60S" | names: "_Dør Dobbel_Ulike_Dørblader:YDS 1.2 15x21M EI 60S:2389213" | material: materials ("Lys grå", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "YDS 1.1 15x21M" | object type "YDS 1.1 15x21M" | names: "_Dør Dobbel_Ulike_Dørblader:YDS 1.1 15x21M:2389269" | material: materials ("Lys grå", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "V3 18x22" | object type "V3 18x22" | names: "Vindu-Fast:V3 18x22:2424976" | material: materials ("N_Windows - Glass", "NCS S 0502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          2 x IFCWINDOW | type IFCWINDOWSTYLE "V1 12x22" | object type "V1 12x22" | names: "Vindu-Hengslet_1200 opening:V1 12x22:2424977", "Vindu-Hengslet_1200 opening:V1 12x22:2424993" | material: materials ("NCS S 0502-Y", "Glass Klart") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "V2 12x22" | object type "V2 12x22" | names: "Vindu-Fast:V2 12x22:2424980" | material: materials ("Glass Klart", "NCS S 0502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "V1 12x22" | object type "V1 12x22" | names: "Vindu-Hengslet_1200 opening:V1 12x22:2424981" | material: materials ("NCS S 0502-Y", "Glass Klart") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "V3 18x22" | object type "V3 18x22" | names: "Vindu-Fast:V3 18x22:2424982" | material: materials ("N_Windows - Glass", "NCS S 0502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          4 x IFCWINDOW | type IFCWINDOWSTYLE "V4 23x22" | object type "V4 23x22" | names: "Vindu-Fast:V4 23x22:2424986", "Vindu-Fast:V4 23x22:2424991", "Vindu-Fast:V4 23x22:2425289" (+1 more) | material: materials ("Glass Klart", "NCS S 0502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "V23 14x14" | object type "V23 14x14" | names: "Vindu-Hengslet:V23 14x14:2424987" | material: materials ("Glass Klart", "NCS S 0502-Y", "Karm Malt") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "V23 14x14" | object type "V23 14x14" | names: "Vindu-Hengslet:V23 14x14:2424994" | material: materials ("Glass Klart", "NCS S 0502-Y", "Karm Malt") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "V22 14x14" | object type "V22 14x14" | names: "Vindu-Fast:V22 14x14:2425414" | material: materials ("Glass Klart", "NCS S 0502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "V22 14x14" | object type "V22 14x14" | names: "Vindu-Fast:V22 14x14:2425504" | material: materials ("Glass Klart", "NCS S 0502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "V3 18x22" | object type "V3 18x22" | names: "Vindu-Fast:V3 18x22:2425505" | material: materials ("N_Windows - Glass", "NCS S 0502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "V22 14x14" | object type "V22 14x14" | names: "Vindu-Fast:V22 14x14:2425508" | material: materials ("Glass Klart", "NCS S 0502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          5 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:YV 4.1 373 Gesims" | object type "Basic Wall:YV 4.1 373 Gesims:2482013" | names: "Basic Wall:YV 4.1 373 Gesims:2482335", "Basic Wall:YV 4.1 373 Gesims:2482475", "Basic Wall:YV 4.1 373 Gesims:2482566" (+2 more) | material: layers "Basic Wall:YV 4.1 373 Gesims" ("Trekledning" 19., "Luftsjikt" 48., "Luftsjikt" 36., "Luftsjikt" 48., "Vindsperre" 9., "Stender isolert vegg" 198., "Kryssfiner" 15.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          6 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:YV 7.4 410mm gul platekledning" | object type "Basic Wall:YV 7.4 410mm gul platekledning:1741258" | names: "Basic Wall:YV 7.4 410mm gul platekledning:2514577", "Basic Wall:YV 7.4 410mm gul platekledning:2514942", "Basic Wall:YV 7.4 410mm gul platekledning:2516308" (+3 more) | material: layers "Basic Wall:YV 7.4 410mm gul platekledning" ("Cembrit Metro Amsterdam" 8., "Luftsjikt" 36., "Vindsperre" 9., "Stender isolert vegg" 296., "NO_Utlekting" 48., "Robustgips" 12.5) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          6 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:YV 7.3 410mm rød platekledning" | object type "Basic Wall:YV 7.3 410mm rød platekledning:2216522" | names: "Basic Wall:YV 7.3 410mm rød platekledning:2514791", "Basic Wall:YV 7.3 410mm rød platekledning:2515025", "Basic Wall:YV 7.3 410mm rød platekledning:2516398" (+3 more) | material: layers "Basic Wall:YV 7.3 410mm rød platekledning" ("Cembrit Metro Copenhagen" 8., "Luftsjikt" 36., "Vindsperre" 9., "Stender isolert vegg" 296., "NO_Utlekting" 48., "Robustgips" 12.5) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:YV 7.2 410mm grønn platekledning" | object type "Basic Wall:YV 7.2 410mm grønn platekledning:2569141" | names: "Basic Wall:YV 7.2 410mm grønn platekledning:2514860", "Basic Wall:YV 7.2 410mm grønn platekledning:2518586", "Basic Wall:YV 7.2 410mm grønn platekledning:2519346" | material: layers "Basic Wall:YV 7.2 410mm grønn platekledning" ("Cembrit Metro Hamburg" 8., "Luftsjikt" 36., "Vindsperre" 9., "Stender isolert vegg" 296., "NO_Utlekting" 48., "Robustgips" 12.5) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          4 x IFCWINDOW | type IFCWINDOWSTYLE "GF 3.2 6x21 38dB" | object type "GF 3.2 6x21 38dB" | names: "Vindu-Fast:GF 3.2 6x21 38dB:2519856", "Vindu-Fast:GF 3.2 6x21 38dB:2990848", "Vindu-Fast:GF 3.2 6x21 38dB:3867925" (+1 more) | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          5 x IFCWINDOW | type IFCWINDOWSTYLE "GF 1.1 12x21 33dB" | object type "GF 1.1 12x21 33dB" | names: "Vindu-Fast:GF 1.1 12x21 33dB:2520638", "Vindu-Fast:GF 1.1 12x21 33dB:2520739", "Vindu-Fast:GF 1.1 12x21 33dB:2521440" (+2 more) | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "GF 1.3 12x21 38dB" | object type "GF 1.3 12x21 38dB" | names: "Vindu-Fast:GF 1.3 12x21 38dB:2520815" | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          3 x IFCWINDOW | type IFCWINDOWSTYLE "GF 1.3 12x21 38dB" | object type "GF 1.3 12x21 38dB" | names: "Vindu-Fast:GF 1.3 12x21 38dB:2523541", "Vindu-Fast:GF 1.3 12x21 38dB:2988447", "Vindu-Fast:GF 1.3 12x21 38dB:2988697" | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "GF 3.3 6x21 44dB" | object type "GF 3.3 6x21 44dB" | names: "Vindu-Fast:GF 3.3 6x21 44dB:2523913" | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 2.1 10x21M" | object type "IDT 2.1 10x21M" | names: "Dør Enkel:IDT 2.1 10x21M:2550978" | material: materials ("_White", "NCS S 0500-N", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDS 3.1 18x21M 38dB EI60S" | object type "IDS 3.1 18x21M 38dB EI60S" | names: "Dør Dobbel:IDS 3.1 18x21M 38dB EI60S:2551141" | material: materials ("Lys grå", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDS 3.1 18x21M 38dB EI60S" | object type "IDS 3.1 18x21M 38dB EI60S" | names: "Dør Dobbel:IDS 3.1 18x21M 38dB EI60S:2551181" | material: materials ("Lys grå", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 8.1 125mm sjaktvegg EI60" | object type "Basic Wall:IVA 8.1 125mm sjaktvegg EI60:2855957" | names: "Basic Wall:IVA 8.1 125mm sjaktvegg EI60:2596351" | material: layers "Basic Wall:IVA 8.1 125mm sjaktvegg EI60" ("Branngips" 15., "Branngips" 15., "stender/isolasjon" 95.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          1 x IFCANNOTATION
          6 x IFCCOVERING | object type "Compound Ceiling:Himling System 600x600" | CEILING | names: "Compound Ceiling:Himling System 600x600:2602846", "Compound Ceiling:Himling System 600x600:3048419", "Compound Ceiling:Himling System 600x600:3048426" (+3 more) | material: layers "Compound Ceiling:Himling System 600x600" ("Himling Metallprofil" 38., "Himling System 600x600" 12.) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          5 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 7.2 108mm Skjørt" | object type "Basic Wall:IVA 7.2 108mm Skjørt:5366897" | names: "Basic Wall:IVA 7.2 108mm Skjørt:2781316", "Basic Wall:IVA 7.2 108mm Skjørt:3212118", "Basic Wall:IVA 7.2 108mm Skjørt:3380806" (+2 more) | material: layers "Basic Wall:IVA 7.2 108mm Skjørt" ("Gips" 13., "stender/isolasjon" 95.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 2.2T 134mm 34dB (H-95-NR)" | object type "Basic Wall:IVA 2.2T 134mm 34dB (H-95-NR):6783331" | names: "Basic Wall:IVA 2.2T 134mm 34dB (H-95-NR):2852417" | material: layers "Basic Wall:IVA 2.2T 134mm 34dB (H-95-NR)" ("Habito" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 2.3T 134mm 34dB (R-95-NR)" | object type "Basic Wall:IVA 2.3T 134mm 34dB (R-95-NR):6701505" | names: "Basic Wall:IVA 2.3T 134mm 34dB (R-95-NR):2852780", "Basic Wall:IVA 2.3T 134mm 34dB (R-95-NR):6783271" | material: layers "Basic Wall:IVA 2.3T 134mm 34dB (R-95-NR)" ("Robustgips" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 2.3 134mm 34dB (R-95-NR)" | object type "Basic Wall:IVA 2.3 134mm 34dB (R-95-NR):4809032" | names: "Basic Wall:IVA 2.3 134mm 34dB (R-95-NR):2854167" | material: layers "Basic Wall:IVA 2.3 134mm 34dB (R-95-NR)" ("Robustgips" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 6.2 272mm 55dB EI60 (RN-95-30-95-NH)" | object type "Basic Wall:IVA 6.2 272mm 55dB EI60 (RN-95-30-95-NH):4826087" | names: "Basic Wall:IVA 6.2 272mm 55dB EI60 (RN-95-30-95-NH):2854325" | material: layers "Basic Wall:IVA 6.2 272mm 55dB EI60 (RN-95-30-95-NH)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 95., "Luftsjikt" 30., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:YV 3.1 306mm EI60" | object type "Basic Wall:YV 3.1 306mm EI60:2905012" | names: "Basic Wall:YV 3.1 306mm EI60:2906062", "Basic Wall:YV 3.1 306mm EI60:2906316", "Basic Wall:YV 3.1 306mm EI60:4635161" | material: layers "Basic Wall:YV 3.1 306mm EI60" ("Trekledning" 19., "Luftsjikt" 48., "Luftsjikt" 36., "Luftsjikt" 48., "Vindsperre" 9., "Stender isolert vegg" 146.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:YV 22.1" | object type "Basic Wall:YV 22.1:7219441" | names: "Basic Wall:YV 22.1:2906140" | material: layers "Basic Wall:YV 22.1" ("Trekledning" 19., "Luftsjikt" 48., "Luftsjikt" 36., "Luftsjikt" 48., "Vindsperre" 9., "Stender isolert vegg" 296., "NO_Utlekting" 48., "Habito" 12.5, "Habito" 12.5) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 3.6 10x21M 38dB" | object type "IDT 3.6 10x21M 38dB" | names: "Dør Enkel_ Glassfelt:IDT 3.6 10x21M 38dB:2987831" | material: materials ("NCS S 2500-N", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "GF 1.1 12x21 33dB" | object type "GF 1.1 12x21 33dB" | names: "Vindu-Fast:GF 1.1 12x21 33dB:2987832" | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 3.6 10x21M 38dB" | object type "IDT 3.6 10x21M 38dB" | names: "Dør Enkel_ Glassfelt:IDT 3.6 10x21M 38dB:2988444" | material: materials ("NCS S 2500-N", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "GF 1.1 12x21 33dB" | object type "GF 1.1 12x21 33dB" | names: "Vindu-Fast:GF 1.1 12x21 33dB:2988448" | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "GF 9.1 11x26.5 33dB" | object type "GF 9.1 11x26.5 33dB" | names: "Vindu-Fast:GF 9.1 11x26.5 33dB:2988449" | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 2.3 10x21M 33dB" | object type "IDT 2.3 10x21M 33dB" | names: "Dør Enkel:IDT 2.3 10x21M 33dB:2997367" | material: materials ("Terskel Tre", "Lys grå", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          2 x IFCDOOR | type IFCDOORSTYLE "IDT 3.3 10x21M 33dB" | object type "IDT 3.3 10x21M 33dB" | names: "Dør Enkel_ Glassfelt:IDT 3.3 10x21M 33dB:2997368", "Dør Enkel_ Glassfelt:IDT 3.3 10x21M 33dB:2997369" | material: materials ("Lys grå", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 2.3 10x21M 33dB" | object type "IDT 2.3 10x21M 33dB" | names: "Dør Enkel:IDT 2.3 10x21M 33dB:2997375" | material: materials ("Terskel Tre", "Lys grå", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 2.3 10x21M 33dB" | object type "IDT 2.3 10x21M 33dB" | names: "Dør Enkel:IDT 2.3 10x21M 33dB:2997376" | material: materials ("Terskel Tre", "Lys grå", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "GF 4.2 18x21 33dB" | object type "GF 4.2 18x21 33dB" | names: "Vindu-Fast:GF 4.2 18x21 33dB:2997389" | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 3.6 10x21M 38dB" | object type "IDT 3.6 10x21M 38dB" | names: "Dør Enkel_ Glassfelt:IDT 3.6 10x21M 38dB:2998549" | material: materials ("NCS S 2500-N", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          19 x IFCCOVERING | object type "Compound Ceiling:Himling System 600x1200" | CEILING | names: "Compound Ceiling:Himling System 600x1200:3047729", "Compound Ceiling:Himling System 600x1200:3047736", "Compound Ceiling:Himling System 600x1200:3047743" (+16 more) | material: layers "Compound Ceiling:Himling System 600x1200" ("Himling Metallprofil" 38., "Himling System 600x1200" 12.) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "GF 12.1 6x31 38dB" | object type "GF 12.1 6x31 38dB" | names: "Vindu-Fast:GF 12.1 6x31 38dB:3380385" | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "GF 12.1 6x31 38dB" | object type "GF 12.1 6x31 38dB" | names: "Vindu-Fast:GF 12.1 6x31 38dB:3380386" | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "GF 16.1 5x31 38dB" | object type "GF 16.1 5x31 38dB" | names: "Vindu-Fast:GF 16.1 5x31 38dB:3381397" | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "GF 12.1 6x31 38dB" | object type "GF 12.1 6x31 38dB" | names: "Vindu-Fast:GF 12.1 6x31 38dB:3381504" | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "GF 10.1 8x27 33dB" | object type "GF 10.1 8x27 33dB" | names: "Vindu-Fast:GF 10.1 8x27 33dB:3382939" | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 3.3T 145mm 48dB (RN-95-NR)" | object type "Basic Wall:IVA 3.3T 145mm 48dB (RN-95-NR):6701502" | names: "Basic Wall:IVA 3.3T 145mm 48dB (RN-95-NR):3445952" | material: layers "Basic Wall:IVA 3.3T 145mm 48dB (RN-95-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:110mm Heisvegg" | object type "Basic Wall:110mm Heisvegg:3943637" | names: "Basic Wall:110mm Heisvegg:3944657" | material: layers "Basic Wall:110mm Heisvegg" ("hvit malt" 110.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 3.6 10x21M 38dB" | object type "IDT 3.6 10x21M 38dB" | names: "Dør Enkel_ Glassfelt:IDT 3.6 10x21M 38dB:4003185" | material: materials ("NCS S 2500-N", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 3.6 10x21M 38dB" | object type "IDT 3.6 10x21M 38dB" | names: "Dør Enkel_ Glassfelt:IDT 3.6 10x21M 38dB:4003197" | material: materials ("NCS S 2500-N", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "GF 2.1 9x21 38dB" | object type "GF 2.1 9x21 38dB" | names: "Vindu-Fast:GF 2.1 9x21 38dB:4003198" | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "GF 2.1 9x21 38dB" | object type "GF 2.1 9x21 38dB" | names: "Vindu-Fast:GF 2.1 9x21 38dB:4003205" | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 7.3 121mm 37dB EI30 (95-NH)" | object type "Basic Wall:IVA 7.3 121mm 37dB EI30 (95-NH):6248387" | names: "Basic Wall:IVA 7.3 121mm 37dB EI30 (95-NH):4049786", "Basic Wall:IVA 7.3 121mm 37dB EI30 (95-NH):4049919" | material: layers "Basic Wall:IVA 7.3 121mm 37dB EI30 (95-NH)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCWINDOW | type IFCWINDOWSTYLE "GF 4.2 18x21 33dB" | object type "GF 4.2 18x21 33dB" | names: "Vindu-Fast:GF 4.2 18x21 33dB:4200771" | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "GF 1.4 12x21 44dB" | object type "GF 1.4 12x21 44dB" | names: "Vindu-Fast:GF 1.4 12x21 44dB:4200772" | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCROOF | object type "Basic Roof:Tak betong 320 + iso over og under" | names: "Basic Roof:Tak betong 320 + iso over og under:4334037" | parts: 1 IFCSLAB | property sets: Pset_RoofCommon, Pset_TFM, Constraints, Construction, Dimensions, Other
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 3.3 145mm 34dB (RN-95-NR)" | object type "Basic Wall:IVA 3.3 145mm 34dB (RN-95-NR):2849806" | names: "Basic Wall:IVA 3.3 145mm 34dB (RN-95-NR):4383295" | material: layers "Basic Wall:IVA 3.3 145mm 34dB (RN-95-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          1 x IFCSLAB | object type "Floor:Betongdekke 400 + 80 påstøp + 10 avretting" | FLOOR | names: "Floor:Betongdekke 400 + 80 påstøp + 10 avretting:4440486" | material: layers "Floor:Betongdekke 400 + 80 påstøp + 10 avretting" ("Betong avretting" 10., "Betong påstøp" 80., "Betong" 400.) | property sets: Pset_SlabCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Other
          1 x IFCROOF | object type "Basic Roof:Tak betong 320 + 170:305166" | names: "Basic Roof:Tak betong 320 + 170:4447733" | parts: 1 IFCSLAB | property sets: Pset_RoofCommon, Pset_TFM, Constraints, Construction, Dimensions, Identity Data
          1 x IFCSLAB | object type "Floor:Betongdekke 400 + 80 iso + 10 avretting" | FLOOR | names: "Floor:Betongdekke 400 + 80 iso + 10 avretting:4450355" | material: layers "Floor:Betongdekke 400 + 80 iso + 10 avretting" ("Betong avretting" 10., "NO_isolasjon" 80., "Betong" 400.) | property sets: Pset_SlabCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          2 x IFCROOF | object type "Basic Roof:Tak betong 200 + 150" | names: "Basic Roof:Tak betong 200 + 150:4637260", "Basic Roof:Tak betong 200 + 150:4637455" | parts: 2 IFCSLAB | property sets: Pset_RoofCommon, Pset_TFM, Constraints, Construction, Dimensions, Other
          5 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 7.1 121mm Skjørt" | object type "Basic Wall:IVA 7.1 121mm Skjørt:2853494" | names: "Basic Wall:IVA 7.1 121mm Skjørt:4769166", "Basic Wall:IVA 7.1 121mm Skjørt:4769254", "Basic Wall:IVA 7.1 121mm Skjørt:4769330" (+2 more) | material: layers "Basic Wall:IVA 7.1 121mm Skjørt" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 7.2 111mm Skjørt 2" | object type "Basic Wall:IVA 7.2 111mm Skjørt 2:6929591" | names: "Basic Wall:IVA 7.2 111mm Skjørt 2:4769704", "Basic Wall:IVA 7.2 111mm Skjørt 2:4769706" | material: layers "Basic Wall:IVA 7.2 111mm Skjørt 2" ("Gips" 13., "stender/isolasjon" 98.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          5 x IFCROOF | object type "Basic Roof:Tak isolasjon:4787841" | names: "Basic Roof:Tak isolasjon:4787839", "Basic Roof:Tak isolasjon:4788320", "Basic Roof:Tak isolasjon:4793624" (+2 more) | material: "Isolasjon tak" | property sets: Pset_RoofCommon, Pset_TFM, Constraints, Construction, Dimensions, Other
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:IVA 3.3 145mm 44dB (RN-95-NR)" | object type "Basic Wall:IVA 3.3 145mm 44dB (RN-95-NR):4816971" | names: "Basic Wall:IVA 3.3 145mm 44dB (RN-95-NR):4810616" | material: layers "Basic Wall:IVA 3.3 145mm 44dB (RN-95-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCWINDOW | type IFCWINDOWSTYLE "GF 1.3 12x21 38dB" | object type "GF 1.3 12x21 38dB" | names: "Vindu-Fast:GF 1.3 12x21 38dB:5046044" | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          10 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:YVL 1.1 250mm leca isoblokk" | object type "Basic Wall:YVL 1.1 250mm leca isoblokk:5103281" | names: "Basic Wall:YVL 1.1 250mm leca isoblokk:5092383", "Basic Wall:YVL 1.1 250mm leca isoblokk:5092472", "Basic Wall:YVL 1.1 250mm leca isoblokk:5093480" (+7 more) | material: layers "Basic Wall:YVL 1.1 250mm leca isoblokk" ("Mur" 82., "NO_Hard isolasjon" 86., "Mur" 82.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          7 x IFCWINDOW | type IFCWINDOWSTYLE "V6 24x22" | object type "V6 24x22" | names: "Vindu 3 felt:V6 24x22:5448868", "Vindu 3 felt:V6 24x22:5449148", "Vindu 3 felt:V6 24x22:5449245" (+4 more) | material: materials ("NCS S 0502-Y", "N_Windows - Glass") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          3 x IFCWINDOW | type IFCWINDOWSTYLE "V10 30x22" | object type "V10 30x22" | names: "Vindu 3 felt:V10 30x22:5449018", "Vindu 3 felt:V10 30x22:5450200", "Vindu 3 felt:V10 30x22:5450454" | material: materials ("NCS S 0502-Y", "N_Windows - Glass") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "V6 24x22" | object type "V6 24x22" | names: "Vindu 3 felt:V6 24x22:5449631" | material: materials ("NCS S 0502-Y", "N_Windows - Glass") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "V8 27x22" | object type "V8 27x22" | names: "Vindu 3 felt:V8 27x22:5449824" | material: materials ("NCS S 0502-Y", "N_Windows - Glass") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          2 x IFCWINDOW | type IFCWINDOWSTYLE "V12 35x22" | object type "V12 35x22" | names: "Vindu 3 felt:V12 35x22:5471862", "Vindu 3 felt:V12 35x22:5471944" | material: materials ("NO_Aluminium", "NCS S 0502-Y", "N_Windows - Glass") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWINDOW | type IFCWINDOWSTYLE "V12 35x22" | object type "V12 35x22" | names: "Vindu 3 felt:V12 35x22:5472149" | material: materials ("NO_Aluminium", "NCS S 0502-Y", "N_Windows - Glass") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          2 x IFCWINDOW | type IFCWINDOWSTYLE "V11 35x22" | object type "V11 35x22" | names: "Vindu 3 felt:V11 35x22:5472303", "Vindu 3 felt:V11 35x22:5472408" | material: materials ("NO_Aluminium", "NCS S 0502-Y", "N_Windows - Glass") | property sets: Pset_WindowCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:YV 5.1 233 Gesims Midtbygg" | object type "Basic Wall:YV 5.1 233 Gesims Midtbygg:2484317" | names: "Basic Wall:YV 5.1 233 Gesims Midtbygg:5750220" | material: layers "Basic Wall:YV 5.1 233 Gesims Midtbygg" ("Beslag" 5., "Vindsperre" 15., "<Unnamed>" 36., "<Unnamed>" 15., "Stender isolert vegg" 198., "Kryssfiner" 15.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:YV stolpe" | object type "Basic Wall:YV stolpe:5563726" | names: "Basic Wall:YV stolpe:5762759", "Basic Wall:YV stolpe:5763051", "Basic Wall:YV stolpe:5763182" (+1 more) | material: layers "Basic Wall:YV stolpe" ("Vindsperre" 9., "Stender isolert vegg" 98., "Gips" 13.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          37 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:YV 18.1 136 Takhatt" | object type "Basic Wall:YV 18.1 136 Takhatt:6190526" | names: "Basic Wall:YV 18.1 136 Takhatt:6146730", "Basic Wall:YV 18.1 136 Takhatt:6146731", "Basic Wall:YV 18.1 136 Takhatt:6146732" (+34 more) | material: layers "Basic Wall:YV 18.1 136 Takhatt" ("Kryssfiner" 15., "Stender isolert vegg" 98.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          1 x IFCROOF | object type "Basic Roof:Tak tre 198 - Takhatt:6224156" | names: "Basic Roof:Tak tre 198 - Takhatt:6146736" | material: "stender/isolasjon" | property sets: Pset_RoofCommon, Pset_TFM, Constraints, Construction, Dimensions, Identity Data
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:YV 18.1 136 Takhatt 3" | object type "Basic Wall:YV 18.1 136 Takhatt 3:6227222" | names: "Basic Wall:YV 18.1 136 Takhatt 3:6225359" | material: layers "Basic Wall:YV 18.1 136 Takhatt 3" ("Stender isolert vegg" 98.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCWALL | type IFCWALLTYPE "Basic Wall:YV 12.1 411 Ventilasjonsrom" | object type "Basic Wall:YV 12.1 411 Ventilasjonsrom:5093016" | names: "Basic Wall:YV 12.1 411 Ventilasjonsrom:6268428" | material: layers "Basic Wall:YV 12.1 411 Ventilasjonsrom" ("Spiler ute" 19., "Luftsjikt" 36., "Luftsjikt" 36., "Vindsperre" 9., "Stender isolert vegg" 250., "Stender isolert vegg" 48., "Habito" 12.5, "Habito" 12.5) | property sets: Constraints, Dimensions, Graphics, Identity Data, Other, Phasing
          1 x IFCWALL | type IFCWALLTYPE "Basic Wall:YV 12.1 411 Ventilasjonsrom EI 60" | object type "Basic Wall:YV 12.1 411 Ventilasjonsrom EI 60:5093156" | names: "Basic Wall:YV 12.1 411 Ventilasjonsrom EI 60:6268558" | material: layers "Basic Wall:YV 12.1 411 Ventilasjonsrom EI 60" ("Spiler ute" 19., "Luftsjikt" 36., "Luftsjikt" 36., "Vindsperre" 9., "Stender isolert vegg" 250., "Stender isolert vegg" 48., "Habito" 12.5, "Habito" 12.5) | property sets: Constraints, Dimensions, Graphics, Other, Phasing, Structural
          1 x IFCDOOR | type IFCDOORSTYLE "IDT 8.1 18x21M 33dB" | object type "IDT 8.1 18x21M 33dB" | names: "_Dør Dobbel_Ulike_Dørblader_Glassfelt2:IDT 8.1 18x21M 33dB:6481147" | material: materials ("Glass Klart", "Lys grå", "Terskel Tre", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          2 x IFCDOOR | type IFCDOORSTYLE "Luke 600" | object type "Luke 600" | names: "Luke600:Luke 600:6623636", "Luke600:Luke 600:6623637" | material: materials ("Light grey", "Karm Malt") | property sets: Pset_DoorCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:YVL 3.1 300mm leca isoblokk" | object type "Basic Wall:YVL 3.1 300mm leca isoblokk:7026949" | names: "Basic Wall:YVL 3.1 300mm leca isoblokk:7019401", "Basic Wall:YVL 3.1 300mm leca isoblokk:7028122" | material: layers "Basic Wall:YVL 3.1 300mm leca isoblokk" ("Mur" 82., "NO_Hard isolasjon" 186., "Mur" 82.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
        IFCSPACE "17" | long name "Area" | INTERNAL
        IFCSPACE "18" | long name "Area" | INTERNAL
        IFCSPACE "03129" | long name "gruppe" | INTERNAL
          contains 3 elements
            1 x IFCCOVERING | object type "Compound Ceiling:Himling System 600x1200" | CEILING | names: "Compound Ceiling:Himling System 600x1200:3047902" | material: layers "Compound Ceiling:Himling System 600x1200" ("Himling Metallprofil" 38., "Himling System 600x1200" 12.) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Other
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Tavle 2m" | object type "Tavle 2m" | names: "Tavle:Tavle 2m:4361302" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "TV-skjerm" | object type "TV-skjerm" | names: "TV-skjerm:TV-skjerm:4453855" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
        IFCSPACE "03127" | long name "klasse" | INTERNAL
          contains 3 elements
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "PC-skap" | object type "PC-skap" | names: "Spesialutstyr:PC-skap:3379955" | material: "hvit malt" | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Tavle 2m" | object type "Tavle 2m" | names: "Tavle:Tavle 2m:5299997" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Smartboard 2m" | object type "Smartboard 2m" | names: "Smartboard:Smartboard 2m:5299998" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
        IFCSPACE "03123" | long name "fellesområde" | INTERNAL
          contains 11 elements
            1 x IFCCOVERING | object type "Compound Ceiling:Himling System 600x1200" | CEILING | names: "Compound Ceiling:Himling System 600x1200:3047866" | material: layers "Compound Ceiling:Himling System 600x1200" ("Himling Metallprofil" 38., "Himling System 600x1200" 12.) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
            1 x IFCFLOWTERMINAL | object type "Vaskerenne 1200mm" | names: "intra_wash_throuh_wall_mounted_1200_mm:Vaskerenne 1200mm:3641143" | material: materials ("f26d4e4b_a025_4dbf_b085_30ed485788cf", "4b4a701a_e8ab_4354_ac15_234043769b9c") | property sets: Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data, Mechanical
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Tavle 2m" | object type "Tavle 2m" | names: "Tavle:Tavle 2m:4358316" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
            2 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Skap, resirkulering 400 x 400 x 825mm" | object type "Skap, resirkulering 400 x 400 x 825mm" | names: "Base Cabinet Single Door:Skap, resirkulering 400 x 400 x 825mm:7157824", "Base Cabinet Single Door:Skap, resirkulering 400 x 400 x 825mm:7157825" | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
            2 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Skap, resirkulering 300 x 400 x 825mm" | object type "Skap, resirkulering 300 x 400 x 825mm" | names: "Base Cabinet Single Door:Skap, resirkulering 300 x 400 x 825mm:7157826", "Base Cabinet Single Door:Skap, resirkulering 300 x 400 x 825mm:7157827" | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
            1 x IFCFLOWTERMINAL | object type "Delabie flaskefyller" | names: "M_Tap_2:Delabie flaskefyller:7580636" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            2 x IFCFLOWCONTROLLER | type IFCVALVETYPE "Blandebatteri berøringsfri 1724FT" | object type "Blandebatteri berøringsfri 1724FT" | names: "1724FT(2013):Blandebatteri berøringsfri 1724FT:7582033", "1724FT(2013):Blandebatteri berøringsfri 1724FT:7582128" | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Benkeplate kildesortering 2" | object type "Benkeplate kildesortering 2" | names: "N_CounterTop:Benkeplate kildesortering 2:7722159" | material: "hvit malt" | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
        IFCSPACE "03126" | long name "gruppe" | INTERNAL
          contains 2 elements
            1 x IFCCOVERING | object type "Compound Ceiling:Himling System 600x1200" | CEILING | names: "Compound Ceiling:Himling System 600x1200:3047918" | material: layers "Compound Ceiling:Himling System 600x1200" ("Himling Metallprofil" 38., "Himling System 600x1200" 12.) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Other
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Tavle 2m" | object type "Tavle 2m" | names: "Tavle:Tavle 2m:4361028" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
        IFCSPACE "03148" | long name "ventilasjon" | INTERNAL
          contains 2 elements
            1 x IFCFLOWTERMINAL | object type "Utslagsvask" | names: "intra_gub1_bucket_sink_wall_mounted:Utslagsvask:3640249" | material: "f26d4e4b_a025_4dbf_b085_30ed485788cf" | property sets: Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data, Mechanical
            1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "Blandebatteri 3970" | object type "Blandebatteri 3970" | names: "Oras Saga:Blandebatteri 3970:7601145" | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
        IFCSPACE "03107" | long name "klasse" | INTERNAL
          contains 3 elements
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "PC-skap" | object type "PC-skap" | names: "Spesialutstyr:PC-skap:3380265" | material: "hvit malt" | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Tavle 2m" | object type "Tavle 2m" | names: "Tavle:Tavle 2m:5300977" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Smartboard 2m" | object type "Smartboard 2m" | names: "Smartboard:Smartboard 2m:5300978" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
        IFCSPACE "03124" | long name "klasse" | INTERNAL
          contains 3 elements
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "PC-skap" | object type "PC-skap" | names: "Spesialutstyr:PC-skap:3379514" | material: "hvit malt" | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Tavle 2m" | object type "Tavle 2m" | names: "Tavle:Tavle 2m:5300158" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Smartboard 2m" | object type "Smartboard 2m" | names: "Smartboard:Smartboard 2m:5300159" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
        IFCSPACE "03110" | long name "klasse" | INTERNAL
          contains 3 elements
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "PC-skap" | object type "PC-skap" | names: "Spesialutstyr:PC-skap:3379513" | material: "hvit malt" | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Tavle 2m" | object type "Tavle 2m" | names: "Tavle:Tavle 2m:5301098" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Smartboard 2m" | object type "Smartboard 2m" | names: "Smartboard:Smartboard 2m:5301099" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
        IFCSPACE "03121" | long name "lærerarbeid" | INTERNAL
        IFCSPACE "03128" | long name "klasse" | INTERNAL
          contains 3 elements
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "PC-skap" | object type "PC-skap" | names: "Spesialutstyr:PC-skap:3379511" | material: "hvit malt" | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Tavle 2m" | object type "Tavle 2m" | names: "Tavle:Tavle 2m:5300279" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Smartboard 2m" | object type "Smartboard 2m" | names: "Smartboard:Smartboard 2m:5300280" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
        IFCSPACE "03140" | long name "trapp" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | object type "Compound Ceiling:Himling System 600x600" | CEILING | names: "Compound Ceiling:Himling System 600x600:3924501" | material: layers "Compound Ceiling:Himling System 600x600" ("Himling Metallprofil" 38., "Himling System 600x600" 12.) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Other
        IFCSPACE "03105" | long name "fellesområde" | INTERNAL
          contains 10 elements
            1 x IFCFLOWTERMINAL | object type "Vaskerenne 1200mm" | names: "intra_wash_throuh_wall_mounted_1200_mm:Vaskerenne 1200mm:3641326" | material: materials ("f26d4e4b_a025_4dbf_b085_30ed485788cf", "4b4a701a_e8ab_4354_ac15_234043769b9c") | property sets: Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data, Mechanical
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Tavle 2m" | object type "Tavle 2m" | names: "Tavle:Tavle 2m:4358317" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
            2 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Skap, resirkulering 400 x 400 x 825mm" | object type "Skap, resirkulering 400 x 400 x 825mm" | names: "Base Cabinet Single Door:Skap, resirkulering 400 x 400 x 825mm:7157937", "Base Cabinet Single Door:Skap, resirkulering 400 x 400 x 825mm:7157938" | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
            2 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Skap, resirkulering 300 x 400 x 825mm" | object type "Skap, resirkulering 300 x 400 x 825mm" | names: "Base Cabinet Single Door:Skap, resirkulering 300 x 400 x 825mm:7157939", "Base Cabinet Single Door:Skap, resirkulering 300 x 400 x 825mm:7157940" | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Other, Phasing
            1 x IFCFLOWTERMINAL | object type "Delabie flaskefyller" | names: "M_Tap_2:Delabie flaskefyller:7580259" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            2 x IFCFLOWCONTROLLER | type IFCVALVETYPE "Blandebatteri berøringsfri 1724FT" | object type "Blandebatteri berøringsfri 1724FT" | names: "1724FT(2013):Blandebatteri berøringsfri 1724FT:7582212", "1724FT(2013):Blandebatteri berøringsfri 1724FT:7582287" | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Benkeplate kildesortering 2" | object type "Benkeplate kildesortering 2" | names: "N_CounterTop:Benkeplate kildesortering 2:7722276" | material: "hvit malt" | property sets: Pset_TFM, Constraints, Dimensions, Other, Phasing, Text
        IFCSPACE "03111" | long name "klasse" | INTERNAL
          contains 3 elements
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "PC-skap" | object type "PC-skap" | names: "Spesialutstyr:PC-skap:3379512" | material: "hvit malt" | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Tavle 2m" | object type "Tavle 2m" | names: "Tavle:Tavle 2m:5300384" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Smartboard 2m" | object type "Smartboard 2m" | names: "Smartboard:Smartboard 2m:5300385" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
        IFCSPACE "03109" | long name "gruppe" | INTERNAL
          contains 1 element
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Tavle 2m" | object type "Tavle 2m" | names: "Tavle:Tavle 2m:4361923" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
        IFCSPACE "03106" | long name "gruppe" | INTERNAL
          contains 2 elements
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Tavle 2m" | object type "Tavle 2m" | names: "Tavle:Tavle 2m:4361963" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "TV-skjerm" | object type "TV-skjerm" | names: "TV-skjerm:TV-skjerm:4453983" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
        IFCSPACE "03108" | long name "gruppe" | INTERNAL
          contains 1 element
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Tavle 2m" | object type "Tavle 2m" | names: "Tavle:Tavle 2m:4361784" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
        IFCSPACE "03112" | long name "gruppe" | INTERNAL
          contains 1 element
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Tavle 2m" | object type "Tavle 2m" | names: "Tavle:Tavle 2m:4361670" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
        IFCSPACE "03030" | long name "ventilasjon" | INTERNAL
          contains 1 element
            1 x IFCFLOWTERMINAL | object type "Utslagsvask" | names: "intra_gub1_bucket_sink_wall_mounted:Utslagsvask:4628623" | material: "f26d4e4b_a025_4dbf_b085_30ed485788cf" | property sets: Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data, Mechanical
        IFCSPACE "03113" | long name "hcwc" | INTERNAL
          contains 5 elements
            1 x IFCFLOWTERMINAL | object type "Gulvstående toalett - Nautic 1546" | names: "WC-GBG-Nautic_1546-Floor_Standing:Gulvstående toalett - Nautic 1546:1919227" | material: materials ("Gustavsberg Chrome - Polished", "Gustavsberg Porcelain - White", "Gustavsberg Plastic - White") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWTERMINAL | object type "Servant HCWC - 7119" | names: "Washbasin-GBG-7119_Bolt_Mounting:Servant HCWC - 7119:3628930" | material: "Gustavsberg Porcelain - White" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "Blandebatteri berøringsfri 1724FT" | object type "Blandebatteri berøringsfri 1724FT" | names: "1724FT(2013):Blandebatteri berøringsfri 1724FT:7589088" | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Armstøtte veggmontert" | object type "Armstøtte veggmontert" | names: "WC_Armrest-GBG-1712_Wall_Mounted:Armstøtte veggmontert:7602540", "WC_Armrest-GBG-1712_Wall_Mounted:Armstøtte veggmontert:7602560" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_TFM, Constraints, Dimensions, Electrical - Loads
        IFCSPACE "03125" | long name "gruppe" | INTERNAL
          contains 2 elements
            1 x IFCCOVERING | object type "Compound Ceiling:Himling System 600x1200" | CEILING | names: "Compound Ceiling:Himling System 600x1200:3047843" | material: layers "Compound Ceiling:Himling System 600x1200" ("Himling Metallprofil" 38., "Himling System 600x1200" 12.) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Tavle 2m" | object type "Tavle 2m" | names: "Tavle:Tavle 2m:4361195" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Other
        IFCSPACE "03100" | long name "trapp" | INTERNAL
        IFCSPACE "03101" | long name "EL" | INTERNAL
        IFCSPACE "03114" | long name "wc" | INTERNAL
          contains 3 elements
            1 x IFCFLOWTERMINAL | object type "Vegghengt toalett" | names: "WC-GBG-Nautic_1522-Wall_Mounted:Vegghengt toalett:3625316" | material: materials ("Gustavsberg Chrome - Polished", "Gustavsberg Porcelain - White (with C+)", "Gustavsberg Plastic - White") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWTERMINAL | object type "Servant - Ecco 50x35" | names: "Ecco:Servant - Ecco 50x35:3629340" | material: materials ("Gustavsberg Chrome - Polished", "Gustavsberg Porcelain - White") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "Blandebatteri berøringsfri 1724FT" | object type "Blandebatteri berøringsfri 1724FT" | names: "1724FT(2013):Blandebatteri berøringsfri 1724FT:7575747" | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
        IFCSPACE "03120" | long name "stille" | INTERNAL
        IFCSPACE "03119" | long name "kopi" | INTERNAL
        IFCSPACE "03118" | long name "lærerarbeid" | INTERNAL
        IFCSPACE "03104" | long name "garderobe" | INTERNAL
          contains 45 elements
            9 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Elevskap" | object type "Elevskap" | names: "Lockers x 2:Elevskap:3375646", "Lockers x 2:Elevskap:3375647", "Lockers x 2:Elevskap:3375648" (+6 more) | material: materials ("Paint - Grey", "_White") | property sets: Pset_TFM, Constraints, Dimensions, Materials and Finishes, Other, Phasing
            36 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Elevskap" | object type "Elevskap" | names: "Lockers x 2:Elevskap:3375655", "Lockers x 2:Elevskap:3375656", "Lockers x 2:Elevskap:3375657" (+33 more) | material: materials ("Paint - Grey", "_White") | property sets: Pset_TFM, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
        IFCSPACE "03144" | long name "bk" | INTERNAL
          contains 2 elements
            1 x IFCFLOWTERMINAL | object type "Utslagsvask" | names: "intra_gub1_bucket_sink_wall_mounted:Utslagsvask:3640219" | material: "f26d4e4b_a025_4dbf_b085_30ed485788cf" | property sets: Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data, Mechanical
            1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "Blandebatteri 3970" | object type "Blandebatteri 3970" | names: "Oras Saga:Blandebatteri 3970:7601250" | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
        IFCSPACE "03122" | long name "garderobe" | INTERNAL
          contains 45 elements
            18 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Elevskap" | object type "Elevskap" | names: "Lockers x 2:Elevskap:3375601", "Lockers x 2:Elevskap:3375602", "Lockers x 2:Elevskap:3375603" (+15 more) | material: materials ("Paint - Grey", "_White") | property sets: Pset_TFM, Constraints, Dimensions, Materials and Finishes, Other, Phasing
            9 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Elevskap" | object type "Elevskap" | names: "Lockers x 2:Elevskap:3375619", "Lockers x 2:Elevskap:3375620", "Lockers x 2:Elevskap:3375621" (+6 more) | material: materials ("Paint - Grey", "Skapdør 2", "Gul avdeling") | property sets: Pset_TFM, Constraints, Dimensions, Materials and Finishes, Other, Phasing
            18 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Elevskap" | object type "Elevskap" | names: "Lockers x 2:Elevskap:3375628", "Lockers x 2:Elevskap:3375629", "Lockers x 2:Elevskap:3375630" (+15 more) | material: materials ("Paint - Grey", "Skapdør 2", "Gul avdeling") | property sets: Pset_TFM, Constraints, Dimensions, Materials and Finishes, Other, Phasing
        IFCSPACE "03102" | long name "IKT" | INTERNAL
        IFCSPACE "03142" | long name "disp" | INTERNAL
        IFCSPACE "03103" | long name "korridor" | INTERNAL
        IFCSPACE "03115" | long name "wc" | INTERNAL
          contains 4 elements
            1 x IFCCOVERING | object type "Compound Ceiling:Himling System 600x600" | CEILING | names: "Compound Ceiling:Himling System 600x600:3048405" | material: layers "Compound Ceiling:Himling System 600x600" ("Himling Metallprofil" 38., "Himling System 600x600" 12.) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Other
            1 x IFCFLOWTERMINAL | object type "Vegghengt toalett" | names: "WC-GBG-Nautic_1522-Wall_Mounted:Vegghengt toalett:3625342" | material: materials ("Gustavsberg Chrome - Polished", "Gustavsberg Porcelain - White (with C+)", "Gustavsberg Plastic - White") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWTERMINAL | object type "Servant - Ecco 50x35" | names: "Ecco:Servant - Ecco 50x35:3629444" | material: materials ("Gustavsberg Chrome - Polished", "Gustavsberg Porcelain - White") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "Blandebatteri berøringsfri 1724FT" | object type "Blandebatteri berøringsfri 1724FT" | names: "1724FT(2013):Blandebatteri berøringsfri 1724FT:7575630" | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
        IFCSPACE "03116" | long name "wc" | INTERNAL
          contains 4 elements
            1 x IFCCOVERING | object type "Compound Ceiling:Himling System 600x600" | CEILING | names: "Compound Ceiling:Himling System 600x600:3048412" | material: layers "Compound Ceiling:Himling System 600x600" ("Himling Metallprofil" 38., "Himling System 600x600" 12.) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Other
            1 x IFCFLOWTERMINAL | object type "Vegghengt toalett" | names: "WC-GBG-Nautic_1522-Wall_Mounted:Vegghengt toalett:3625445" | material: materials ("Gustavsberg Chrome - Polished", "Gustavsberg Porcelain - White (with C+)", "Gustavsberg Plastic - White") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWTERMINAL | object type "Servant - Ecco 50x35" | names: "Ecco:Servant - Ecco 50x35:3629665" | material: materials ("Gustavsberg Chrome - Polished", "Gustavsberg Porcelain - White") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "Blandebatteri berøringsfri 1724FT" | object type "Blandebatteri berøringsfri 1724FT" | names: "1724FT(2013):Blandebatteri berøringsfri 1724FT:7575838" | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
        IFCSPACE "03117" | long name "korridor" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | object type "Compound Ceiling:Himling System 600x1200" | CEILING | names: "Compound Ceiling:Himling System 600x1200:3047859" | material: layers "Compound Ceiling:Himling System 600x1200" ("Himling Metallprofil" 38., "Himling System 600x1200" 12.) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
        IFCSPACE "03141" | long name "EL" | INTERNAL
        IFCSPACE "03143" | long name "korridor" | INTERNAL
        IFCSPACE "03017" | long name "heis" | INTERNAL
        IFCSPACE "03145" | long name "wc" | INTERNAL
          contains 4 elements
            1 x IFCCOVERING | object type "Compound Ceiling:Himling System 600x600" | CEILING | names: "Compound Ceiling:Himling System 600x600:3048451" | material: layers "Compound Ceiling:Himling System 600x600" ("Himling Metallprofil" 38., "Himling System 600x600" 12.) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
            1 x IFCFLOWTERMINAL | object type "Vegghengt toalett" | names: "WC-GBG-Nautic_1522-Wall_Mounted:Vegghengt toalett:3625106" | material: materials ("Gustavsberg Chrome - Polished", "Gustavsberg Porcelain - White (with C+)", "Gustavsberg Plastic - White") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWTERMINAL | object type "Servant - Ecco 50x35" | names: "Ecco:Servant - Ecco 50x35:3629192" | material: materials ("Gustavsberg Chrome - Polished", "Gustavsberg Porcelain - White") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "Blandebatteri berøringsfri 1724FT" | object type "Blandebatteri berøringsfri 1724FT" | names: "1724FT(2013):Blandebatteri berøringsfri 1724FT:7576055" | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
        IFCSPACE "03147" | long name "wc" | INTERNAL
          contains 4 elements
            1 x IFCCOVERING | object type "Compound Ceiling:Himling System 600x600" | CEILING | names: "Compound Ceiling:Himling System 600x600:3048465" | material: layers "Compound Ceiling:Himling System 600x600" ("Himling Metallprofil" 38., "Himling System 600x600" 12.) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
            1 x IFCFLOWTERMINAL | object type "Vegghengt toalett" | names: "WC-GBG-Nautic_1522-Wall_Mounted:Vegghengt toalett:3625022" | material: materials ("Gustavsberg Chrome - Polished", "Gustavsberg Porcelain - White (with C+)", "Gustavsberg Plastic - White") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWTERMINAL | object type "Servant - Ecco 50x35" | names: "Ecco:Servant - Ecco 50x35:3629023" | material: materials ("Gustavsberg Chrome - Polished", "Gustavsberg Porcelain - White") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "Blandebatteri berøringsfri 1724FT" | object type "Blandebatteri berøringsfri 1724FT" | names: "1724FT(2013):Blandebatteri berøringsfri 1724FT:7576116" | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
        IFCSPACE "03146" | long name "wc" | INTERNAL
          contains 4 elements
            1 x IFCCOVERING | object type "Compound Ceiling:Himling System 600x600" | CEILING | names: "Compound Ceiling:Himling System 600x600:3048458" | material: layers "Compound Ceiling:Himling System 600x600" ("Himling Metallprofil" 38., "Himling System 600x600" 12.) | property sets: Pset_CoveringCommon, Pset_TFM, BaseQuantities, Constraints, Dimensions, Identity Data
            1 x IFCFLOWTERMINAL | object type "Vegghengt toalett" | names: "WC-GBG-Nautic_1522-Wall_Mounted:Vegghengt toalett:3625043" | material: materials ("Gustavsberg Chrome - Polished", "Gustavsberg Porcelain - White (with C+)", "Gustavsberg Plastic - White") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWTERMINAL | object type "Servant - Ecco 50x35" | names: "Ecco:Servant - Ecco 50x35:3629073" | material: materials ("Gustavsberg Chrome - Polished", "Gustavsberg Porcelain - White") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
            1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "Blandebatteri berøringsfri 1724FT" | object type "Blandebatteri berøringsfri 1724FT" | names: "1724FT(2013):Blandebatteri berøringsfri 1724FT:7575984" | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Pset_TFM, Constraints, Dimensions, Identity Data
        IFCSPACE "03152" | long name "sjakt" | INTERNAL
        IFCSPACE "03149" | long name "sjakt" | INTERNAL
        IFCSPACE "4" | long name "Area" | INTERNAL
        IFCSPACE "5" | long name "Area" | INTERNAL
        IFCSPACE "03153" | long name "møte" | INTERNAL
          contains 1 element
            1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Tavle 2m" | object type "Tavle 2m" | names: "Tavle:Tavle 2m:4361460" | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Pset_BuildingElementProxyCommon, Pset_TFM, Constraints, Dimensions, Electrical - Loads, Identity Data
      IFCBUILDINGSTOREY "Plan 04" | long name "Plan 04" | elevation 12030.
        contains 78 elements
          2 x IFCROOF | object type "Basic Roof:Tak betong 320 + 150" | names: "Basic Roof:Tak betong 320 + 150:1703344", "Basic Roof:Tak betong 320 + 150:4448200" | parts: 2 IFCSLAB | property sets: Pset_RoofCommon, Pset_TFM, Constraints, Construction, Dimensions, Identity Data
          1 x IFCROOF | object type "Basic Roof:Tak betong 320 + 150:4791515" | names: "Basic Roof:Tak betong 320 + 150:1704457" | parts: 1 IFCSLAB | property sets: Pset_RoofCommon, Pset_TFM, Constraints, Construction, Dimensions, Other
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:YV 4.1 373 Gesims" | object type "Basic Wall:YV 4.1 373 Gesims:2482013" | names: "Basic Wall:YV 4.1 373 Gesims:2483950", "Basic Wall:YV 4.1 373 Gesims:2483951", "Basic Wall:YV 4.1 373 Gesims:2483952" (+1 more) | material: layers "Basic Wall:YV 4.1 373 Gesims" ("Trekledning" 19., "Luftsjikt" 48., "Luftsjikt" 36., "Luftsjikt" 48., "Vindsperre" 9., "Stender isolert vegg" 198., "Kryssfiner" 15.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCROOF | object type "Basic Roof:Tak betong 400 + 80 + 70" | names: "Basic Roof:Tak betong 400 + 80 + 70:2558359" | parts: 1 IFCSLAB | property sets: Pset_RoofCommon, Pset_TFM, Constraints, Construction, Dimensions, Other
          1 x IFCROOF | object type "Basic Roof:Tak betong 400 +150" | names: "Basic Roof:Tak betong 400 +150:4447956" | parts: 1 IFCSLAB | property sets: Pset_RoofCommon, Pset_TFM, Constraints, Construction, Dimensions, Identity Data
          2 x IFCROOF | object type "Basic Roof:Tak betong 320 + påstøp 80 + 70" | names: "Basic Roof:Tak betong 320 + påstøp 80 + 70:4447987", "Basic Roof:Tak betong 320 + påstøp 80 + 70:4499067" | parts: 2 IFCSLAB | property sets: Pset_RoofCommon, Pset_TFM, Constraints, Construction, Dimensions, Other
          3 x IFCROOF | object type "Basic Roof:Tak betong 200 + 80 påstøp + 70:4865556" | names: "Basic Roof:Tak betong 200 + 80 påstøp + 70:4498860", "Basic Roof:Tak betong 200 + 80 påstøp + 70:4499006", "Basic Roof:Tak betong 200 + 80 påstøp + 70:4618009" | parts: 3 IFCSLAB | property sets: Pset_RoofCommon, Pset_TFM, Constraints, Construction, Dimensions, Identity Data
          4 x IFCROOF | object type "Basic Roof:Tak isolasjon:4787841" | names: "Basic Roof:Tak isolasjon:4791722", "Basic Roof:Tak isolasjon:4791729", "Basic Roof:Tak isolasjon:4792396" (+1 more) | material: "Isolasjon tak" | property sets: Pset_RoofCommon, Pset_TFM, Constraints, Construction, Dimensions, Other
          8 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:YV 13.1 313 Gesims Ventilasjonsrom" | object type "Basic Wall:YV 13.1 313 Gesims Ventilasjonsrom:5093077" | names: "Basic Wall:YV 13.1 313 Gesims Ventilasjonsrom:5403022", "Basic Wall:YV 13.1 313 Gesims Ventilasjonsrom:5405864", "Basic Wall:YV 13.1 313 Gesims Ventilasjonsrom:5406096" (+5 more) | material: layers "Basic Wall:YV 13.1 313 Gesims Ventilasjonsrom" ("Spiler ute" 19., "Luftsjikt" 36., "Luftsjikt" 36., "Vindsperre" 9., "Stender isolert vegg" 198., "Kryssfiner" 15.) | property sets: BaseQuantities, Constraints, Dimensions, Identity Data, Other, Phasing
          36 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:TGF" | object type "Basic Wall:TGF:6975599" | names: "Basic Wall:TGF:6195944", "Basic Wall:TGF:6195970", "Basic Wall:TGF:6195989" (+33 more) | material: layers "Basic Wall:TGF" ("<Unnamed>" 12., "Stender isolert vegg" 36.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          8 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:YV 23.1 136 Røykluke" | object type "Basic Wall:YV 23.1 136 Røykluke:6256065" | names: "Basic Wall:YV 23.1 136 Røykluke:6202059", "Basic Wall:YV 23.1 136 Røykluke:6202091", "Basic Wall:YV 23.1 136 Røykluke:6202118" (+5 more) | material: layers "Basic Wall:YV 23.1 136 Røykluke" ("Kryssfiner" 15., "Stender isolert vegg" 198., "Gips" 12.5) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          8 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:YV 18.1 136 Takhatt" | object type "Basic Wall:YV 18.1 136 Takhatt:6190526" | names: "Basic Wall:YV 18.1 136 Takhatt:6541859", "Basic Wall:YV 18.1 136 Takhatt:6541887", "Basic Wall:YV 18.1 136 Takhatt:6541915" (+5 more) | material: layers "Basic Wall:YV 18.1 136 Takhatt" ("Kryssfiner" 15., "Stender isolert vegg" 98.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural

Types
  IFCWALLTYPE "Basic Wall:IVL 5.1 100mm leca EI60" | STANDARD | 5 occurrences | material: layers "Basic Wall:IVL 5.1 100mm leca EI60" ("Mur" 100.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:IV 100" | STANDARD | 5 occurrences | material: layers "Basic Wall:IV 100" ("hvit malt" 100.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "IDS 1.1 10x21 EI60S" | 1 occurrence | material: materials ("Light grey", "Lys grå", "Karm Malt") | property sets: Dør Enkel:IDS 1.1 10x21 EI60S:2027286, Analytical Properties, Construction, Dimensions, Identity Data, Other
  IFCDOORSTYLE "IDS 2.1 13x21M EI60S" | 1 occurrence | material: materials ("Lys grå", "Terskel Tre", "Karm Malt") | property sets: Dør Dobbel_Ulike_Dørblader:IDS 2.1 13x21M EI60S:2027581, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCDOORSTYLE "IDS 1.2 10x21M EI120CS" | 1 occurrence | material: materials ("Light grey", "Lys grå", "Karm Malt") | property sets: Dør Enkel:IDS 1.2 10x21M EI120CS:2294117, Analytical Properties, Construction, Dimensions, Identity Data, Other
  IFCDOORSTYLE "IDS 2.1 13x21M EI60S" | 1 occurrence | material: materials ("Lys grå", "Terskel Tre", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:IVA 3.3 145mm EI60 (RN-95-NR)" | STANDARD | 38 occurrences | material: layers "Basic Wall:IVA 3.3 145mm EI60 (RN-95-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCWALLTYPE "Basic Wall:110mm Heisvegg" | STANDARD | 4 occurrences | material: layers "Basic Wall:110mm Heisvegg" ("hvit malt" 110.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "IDS 2.1 13x21M EI60S" | 1 occurrence | material: materials ("Lys grå", "Terskel Tre", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "IDS 6.1 8x21M" | 1 occurrence | material: materials ("_White", "Lys grå", "Karm Malt") | property sets: Dør Enkel:IDS 6.1 8x21M:4109271, Analytical Properties, Construction, Dimensions, Identity Data, Other
  IFCDOORSTYLE "IDS 5.1 13x21M EI60CS" | 1 occurrence | material: materials ("Light grey", "Karm Malt") | property sets: Dør Enkel:IDS 5.1 13x21M EI60CS:6509988, Analytical Properties, Construction, Dimensions, Identity Data, Other
  IFCDOORSTYLE "IDS 5.1 13x21M EI60CS" | 1 occurrence | material: materials ("Light grey", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Other, Text
  IFCDOORSTYLE "IDA 11 10x6" | 2 occurrences | material: materials ("Light grey", "Karm Malt") | property sets: Luke600:IDA 11 10x6:6972200, Analytical Properties, Construction, Dimensions, Identity Data, Other
  IFCBUILDINGELEMENTPROXYTYPE "Innvendig screen" | 1 occurrence | material: "hvit malt" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCBUILDINGELEMENTPROXYTYPE "Innvendig screen" | 1 occurrence | material: "hvit malt" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCBUILDINGELEMENTPROXYTYPE "Innvendig screen" | 1 occurrence | material: "hvit malt" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:IVA 7.2 108mm Skjørt" | STANDARD | 29 occurrences | material: layers "Basic Wall:IVA 7.2 108mm Skjørt" ("Gips" 13., "stender/isolasjon" 95.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCVALVETYPE "Blandebatteri 3970" | 9 occurrences | material: "Brass" | property sets: Dimensions, General, Green Building Properties, Identity Data, Materials and Finishes, Mechanical
  IFCBUILDINGELEMENTPROXYTYPE "Moppekjøleskap" | 1 occurrence | material: materials ("Metal - Chrome", "Metal - Paint Finish - Ivory,Matte") | property sets: Identity Data, Other
  IFCFURNITURETYPE "Skap, krogsæter 600 x 600 x 860mm" | element type "Skap, krogsæter 600 x 600 x 860mm" | 2 occurrences | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Skap, krogsæter 600 x 600 x 860mm" | element type "Skap, krogsæter 600 x 600 x 860mm" | 3 occurrences | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Stålhylle, Krogsæter 900 x 500mm" | element type "Stålhylle, Krogsæter 900 x 500mm" | 3 occurrences | property sets: Dimensions, Identity Data, Other
  IFCFURNITURETYPE "Stålhylle, Krogsæter 600 x 500mm" | element type "Stålhylle, Krogsæter 600 x 500mm" | 3 occurrences | property sets: Dimensions, Identity Data, Other
  IFCFURNITURETYPE "Stålhylle, Krogsæter 900 x 300mm" | element type "Stålhylle, Krogsæter 900 x 300mm" | 2 occurrences | property sets: Dimensions, Identity Data, Other
  IFCFURNITURETYPE "Stålhylle, Krogsæter 600 x 300mm" | element type "Stålhylle, Krogsæter 600 x 300mm" | 2 occurrences | property sets: Dimensions, Identity Data, Other
  IFCFURNITURETYPE "Benkeplate 625mm, krogsæter" | element type "Benkeplate 625mm, krogsæter" | 1 occurrence | material: "hvit malt" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCBUILDINGELEMENTPROXYTYPE "Miele moppevaskemaskin" | 1 occurrence | material: "hvit malt" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCBUILDINGELEMENTPROXYTYPE "Miele vaskemaskin" | 1 occurrence | material: "hvit malt" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCBUILDINGELEMENTPROXYTYPE "gard skap 30cm 3" | 1 occurrence | material: materials ("Gul avdeling", "Steel - Hadrian - Black") | property sets: Analytical Model, Constraints, Dimensions, Green Building Properties, Identity Data, Layers
  IFCBUILDINGELEMENTPROXYTYPE "gard skap 30cm 3" | 1 occurrence | material: materials ("Gul avdeling", "Steel - Hadrian - Black") | property sets: Analytical Model, Constraints, Dimensions, Green Building Properties, Identity Data, Layers
  IFCWALLTYPE "Basic Wall:YV 10.1 295mm Vindfang 2" | STANDARD | 1 occurrence | material: layers "Basic Wall:YV 10.1 295mm Vindfang 2" ("Cembrit Metro Copenhagen" 8., "Luftsjikt" 36., "Vindsperre" 9., "Stender isolert vegg" 198., "NO_Utlekting" 173., "<Unnamed>" 36., "Gips" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCCURTAINWALLTYPE "Curtain Wall:Glassfasade 7" | 1 occurrence | property sets: Construction, Horizontal Grid, Horizontal Mullions, Identity Data, Other, Vertical Grid
  IFCWALLTYPE "Basic Wall:YV 10.1 295mm Vindfang" | STANDARD | 3 occurrences | material: layers "Basic Wall:YV 10.1 295mm Vindfang" ("Cembrit Metro Copenhagen" 8., "Luftsjikt" 36., "Vindsperre" 9., "Stender isolert vegg" 198., "NO_Utlekting" 36., "Cembrit Metro Copenhagen" 8.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:YV 1.1 517mm" | STANDARD | 22 occurrences | material: layers "Basic Wall:YV 1.1 517mm" ("Trekledning" 19., "Luftsjikt" 48., "Luftsjikt" 36., "Luftsjikt" 48., "Vindsperre" 9., "Stender isolert vegg" 296., "NO_Utlekting" 48., "Robustgips" 12.5) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:YV 2.1 406M" | STANDARD | 2 occurrences | material: layers "Basic Wall:YV 2.1 406M" ("Trekledning" 19., "Luftsjikt" 48., "Luftsjikt" 36., "Luftsjikt" 48., "Vindsperre" 9., "Stender isolert vegg" 246.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:IVA 6.1 272mm 60dB EI60 (HN-95-30-95-NH)" | STANDARD | 2 occurrences | material: layers "Basic Wall:IVA 6.1 272mm 60dB EI60 (HN-95-30-95-NH)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 95., "Luftsjikt" 30., "stender/isolasjon" 95., "Gips" 13., "Habito" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCWALLTYPE "Basic Wall:IVA 3.3 145mm 48dB (RN-95-NR)" | STANDARD | 30 occurrences | material: layers "Basic Wall:IVA 3.3 145mm 48dB (RN-95-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCWALLTYPE "Basic Wall:IVA 2.3 134mm 34dB (R-95-NR)" | STANDARD | 13 occurrences | material: layers "Basic Wall:IVA 2.3 134mm 34dB (R-95-NR)" ("Robustgips" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCWALLTYPE "Basic Wall:IVA 3.3 145mm 37dB EI60 (RN-95-NR)" | STANDARD | 11 occurrences | material: layers "Basic Wall:IVA 3.3 145mm 37dB EI60 (RN-95-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCWALLTYPE "Basic Wall:IVA 3.3 145mm 44dB EI60 (RN-95-NR)" | STANDARD | 1 occurrence | material: layers "Basic Wall:IVA 3.3 145mm 44dB EI60 (RN-95-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCWALLTYPE "Basic Wall:IVA 3.3 145mm 34dB E30 (RN-95-NR)" | STANDARD | 1 occurrence | material: layers "Basic Wall:IVA 3.3 145mm 34dB E30 (RN-95-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:IVA 3.1 145mm EI60 (HN-95-NH)" | STANDARD | 1 occurrence | material: layers "Basic Wall:IVA 3.1 145mm EI60 (HN-95-NH)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCWALLTYPE "Basic Wall:IVA 3.2 145mm EI60 (HN-95-NR)" | STANDARD | 10 occurrences | material: layers "Basic Wall:IVA 3.2 145mm EI60 (HN-95-NR)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCWALLTYPE "Basic Wall:IVA 3.2 145mm 48dB EI60 (HN-95-NR)" | STANDARD | 7 occurrences | material: layers "Basic Wall:IVA 3.2 145mm 48dB EI60 (HN-95-NR)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCDOORSTYLE "IDT 2.6 10x21M 38dB" | 1 occurrence | material: materials ("Light grey", "Lys grå", "Karm Malt") | property sets: Dør Enkel:IDT 2.6 10x21M 38dB:1753119, Analytical Properties, Construction, Dimensions, Identity Data, Other
  IFCWALLTYPE "Basic Wall:IVA 6.2 272mm 60dB (HN-95-30-95-NR)" | STANDARD | 1 occurrence | material: layers "Basic Wall:IVA 6.2 272mm 60dB (HN-95-30-95-NR)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 95., "Luftsjikt" 30., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCWALLTYPE "Basic Wall:IVA 6.2 352mm 60dB (HN-95-110-95-NR)" | STANDARD | 1 occurrence | material: layers "Basic Wall:IVA 6.2 352mm 60dB (HN-95-110-95-NR)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 95., "Luftsjikt" 110., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCWALLTYPE "Basic Wall:IVA 3.3 145mm 34dB (RN-95-NR)" | STANDARD | 17 occurrences | material: layers "Basic Wall:IVA 3.3 145mm 34dB (RN-95-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCDOORSTYLE "IDT 2.3 10x21M 33dB" | 1 occurrence | material: materials ("Terskel Tre", "Lys grå", "Karm Malt") | property sets: Dør Enkel:IDT 2.3 10x21M 33dB:1753211, Analytical Properties, Construction, Dimensions, Identity Data, Other
  IFCWALLTYPE "Basic Wall:IVA 5.1 212mm EI60 (HN-160-NR)" | STANDARD | 1 occurrence | material: layers "Basic Wall:IVA 5.1 212mm EI60 (HN-160-NR)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 160., "Gips" 13., "Robustgips" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCWALLTYPE "Basic Wall:IVA 4.1 172mm (HN-120-NH)" | STANDARD | 2 occurrences | material: layers "Basic Wall:IVA 4.1 172mm (HN-120-NH)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 120., "Gips" 13., "Habito" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCWALLTYPE "Basic Wall:IVA 1.1 121mm (H-95-H)" | STANDARD | 12 occurrences | material: layers "Basic Wall:IVA 1.1 121mm (H-95-H)" ("Habito" 13., "stender/isolasjon" 95., "Habito" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:IVA 1.1 121mm 44dB (H-95-H)" | STANDARD | 44 occurrences | material: layers "Basic Wall:IVA 1.1 121mm 44dB (H-95-H)" ("Habito" 13., "stender/isolasjon" 95., "Habito" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCWALLTYPE "Basic Wall:IVA 3.1 145mm 48dB (HN-95-NH)" | STANDARD | 4 occurrences | material: layers "Basic Wall:IVA 3.1 145mm 48dB (HN-95-NH)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Habito" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCDOORSTYLE "IDT 2.1 10x21M" | 1 occurrence | material: materials ("_White", "NCS S 0500-N", "Karm Malt") | property sets: Dør Enkel:IDT 2.1 10x21M:1753234, Analytical Properties, Construction, Dimensions, Identity Data, Other
  IFCDOORSTYLE "IDT 2.1 10x21M" | 1 occurrence | material: materials ("_White", "NCS S 0500-N", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Other, Text
  IFCWALLTYPE "Basic Wall:IVA 3.3 145mm 34dB EI60 (RN-95-NR)" | STANDARD | 4 occurrences | material: layers "Basic Wall:IVA 3.3 145mm 34dB EI60 (RN-95-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCWALLTYPE "Basic Wall:IVA 3.3 145mm 48dB EI60 (RN-95-NR)" | STANDARD | 19 occurrences | material: layers "Basic Wall:IVA 3.3 145mm 48dB EI60 (RN-95-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCWALLTYPE "Basic Wall:IVA 3.3 145mm 44dB (RN-95-NR)" | STANDARD | 4 occurrences | material: layers "Basic Wall:IVA 3.3 145mm 44dB (RN-95-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCDOORSTYLE "IDT 2.4 10x21M 38dB EI30S" | 1 occurrence | material: materials ("Terskel Tre", "Vindsperre", "Karm Malt") | property sets: Dør Enkel:IDT 2.4 10x21M 38dB EI30S:1753266, Analytical Properties, Construction, Dimensions, Identity Data, Other
  IFCDOORSTYLE "IDT 3.4 10x21M 33dB E30CS" | 1 occurrence | material: materials ("Lys grå", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Dør Enkel_ Glassfelt:IDT 3.4 10x21M 33dB E30CS:1753271, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCDOORSTYLE "IDT 3.2 10x21M 28dB EI30S" | 1 occurrence | material: materials ("Lys grå", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Dør Enkel_ Glassfelt:IDT 3.2 10x21M 28dB EI30S:1753273, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCDOORSTYLE "IDT 2.1 10x21M" | 1 occurrence | material: materials ("_White", "NCS S 0500-N", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Other, Text
  IFCDOORSTYLE "IDT 3.8 10x21M 28dB E30CS" | 1 occurrence | material: materials ("Lys grå", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Dør Enkel_ Glassfelt:IDT 3.8 10x21M 28dB E30CS:1753280, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCWALLTYPE "Basic Wall:IVA 3.2 145mm 37dB EI60 (HN-95-NR)" | STANDARD | 4 occurrences | material: layers "Basic Wall:IVA 3.2 145mm 37dB EI60 (HN-95-NR)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCDOORSTYLE "IDT 2.3 10x21M 33dB" | 2 occurrences | material: materials ("Terskel Tre", "Lys grå", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Other, Text
  IFCWALLTYPE "Basic Wall:IVL 2.1 123mm (flis-leca) 34dB" | STANDARD | 6 occurrences | material: layers "Basic Wall:IVL 2.1 123mm (flis-leca) 34dB" ("Flis" 5., "Mur" 118.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "IDA 5.1 10x21M 33dB" | 1 occurrence | material: materials ("hvit", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Dør Enkel_ Glassfelt:IDA 5.1 10x21M 33dB:1755293, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCWALLTYPE "Basic Wall:IVL 1.1 118mm leca" | STANDARD | 7 occurrences | material: layers "Basic Wall:IVL 1.1 118mm leca" ("Mur" 118.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:YV 7.1 410mm grå platekledning" | STANDARD | 4 occurrences | material: layers "Basic Wall:YV 7.1 410mm grå platekledning" ("Cembrit Metro London" 8., "Luftsjikt" 36., "Vindsperre" 9., "Stender isolert vegg" 296., "NO_Utlekting" 48., "Gips" 12.5) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:YV 6.1 299mm rød platekledning basseng" | STANDARD | 6 occurrences | material: layers "Basic Wall:YV 6.1 299mm rød platekledning basseng" ("Cembrit Metro Copenhagen" 8., "Luftsjikt" 36., "Vindsperre" 9., "Stender isolert vegg" 246.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:IVA 2.4 134mm (R-95-NH)" | STANDARD | 2 occurrences | material: layers "Basic Wall:IVA 2.4 134mm (R-95-NH)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 95., "Robustgips" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCWALLTYPE "Basic Wall:IVA 3.1 145mm 34dB (HN-95-NH)" | STANDARD | 2 occurrences | material: layers "Basic Wall:IVA 3.1 145mm 34dB (HN-95-NH)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Habito" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCWALLTYPE "Basic Wall:IVA 2.2 134mm 34dB (H-95-NR)" | STANDARD | 3 occurrences | material: layers "Basic Wall:IVA 2.2 134mm 34dB (H-95-NR)" ("Habito" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCWALLTYPE "Basic Wall:IVA 1.2T 121mm 34dB (R-95-H)" | STANDARD | 3 occurrences | material: layers "Basic Wall:IVA 1.2T 121mm 34dB (R-95-H)" ("Habito" 13., "stender/isolasjon" 95., "Robustgips" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:IVA 3.3T 145mm EI60 (RN-95-NR)" | STANDARD | 12 occurrences | material: layers "Basic Wall:IVA 3.3T 145mm EI60 (RN-95-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCWALLTYPE "Basic Wall:IVA 4.2 172mm 52dB (HN-120-NR)" | STANDARD | 1 occurrence | material: layers "Basic Wall:IVA 4.2 172mm 52dB (HN-120-NR)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 120., "Gips" 13., "Robustgips" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCWALLTYPE "Basic Wall:IVA 3.3 145mm (RN-95-NR)" | STANDARD | 2 occurrences | material: layers "Basic Wall:IVA 3.3 145mm (RN-95-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCWALLTYPE "Basic Wall:IVA 6.3T 332mm 34dB EI60 (RN-95-90-95-NR)" | STANDARD | 1 occurrence | material: layers "Basic Wall:IVA 6.3T 332mm 34dB EI60 (RN-95-90-95-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95., "Luftsjikt" 90., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCDOORSTYLE "IDT 3.3 10x21M 33dB" | 2 occurrences | material: materials ("Lys grå", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Dør Enkel_ Glassfelt:IDT 3.3 10x21M 33dB:1785179, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCDOORSTYLE "IDT 2.9 10x21M EI60S" | 1 occurrence | material: materials ("Light grey", "Lys grå", "Karm Malt") | property sets: Dør Enkel:IDT 2.9 10x21M EI60S:1785182, Analytical Properties, Construction, Dimensions, Identity Data, Other
  IFCWALLTYPE "Basic Wall:IVA 3.3T 145mm 48dB EI60 (RN-95-NR)" | STANDARD | 5 occurrences | material: layers "Basic Wall:IVA 3.3T 145mm 48dB EI60 (RN-95-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCDOORSTYLE "IDT 3.6 10x21M 38dB" | 1 occurrence | material: materials ("NCS S 2500-N", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:IVA 2.1 134mm 48dB (H-95-NH)" | STANDARD | 12 occurrences | material: layers "Basic Wall:IVA 2.1 134mm 48dB (H-95-NH)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 95., "Habito" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCDOORSTYLE "IDT 2.6 10x21M 38dB" | 1 occurrence | material: materials ("Light grey", "Lys grå", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Other, Text
  IFCWALLTYPE "Basic Wall:IVA 3.2 145mm 48dB (HN-95-NR)" | STANDARD | 3 occurrences | material: layers "Basic Wall:IVA 3.2 145mm 48dB (HN-95-NR)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCDOORSTYLE "IDT 3.3 10x21M 33dB" | 2 occurrences | material: materials ("Lys grå", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:IVA 4.1 172mm 52dB (HN-120-NH)" | STANDARD | 2 occurrences | material: layers "Basic Wall:IVA 4.1 172mm 52dB (HN-120-NH)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 120., "Gips" 13., "Habito" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCDOORSTYLE "IDT 3.3 10x21M 33dB" | 1 occurrence | material: materials ("Lys grå", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "IDT 2.1 10x21M" | 1 occurrence | material: materials ("_White", "NCS S 0500-N", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Other, Text
  IFCWALLTYPE "Basic Wall:IVA 4.3 172mm 34dB (RN-120-NR)" | STANDARD | 4 occurrences | material: layers "Basic Wall:IVA 4.3 172mm 34dB (RN-120-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 120., "Gips" 13., "Robustgips" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCWALLTYPE "Basic Wall:IVA 1.2 121mm (R-95-H)" | STANDARD | 2 occurrences | material: layers "Basic Wall:IVA 1.2 121mm (R-95-H)" ("Habito" 13., "stender/isolasjon" 95., "Robustgips" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "IDT 1.1 8x21M" | 3 occurrences | material: materials ("Terskel Tre", "Lys grå", "Karm Malt") | property sets: Dør Enkel:IDT 1.1 8x21M:1785284, Analytical Properties, Construction, Dimensions, Identity Data, Other
  IFCWALLTYPE "Basic Wall:IVA 2.2 134mm (H-95-NR)" | STANDARD | 1 occurrence | material: layers "Basic Wall:IVA 2.2 134mm (H-95-NR)" ("Habito" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCWALLTYPE "Basic Wall:IVA 1.2 121mm 34dB (R-95-H)" | STANDARD | 4 occurrences | material: layers "Basic Wall:IVA 1.2 121mm 34dB (R-95-H)" ("Habito" 13., "stender/isolasjon" 95., "Robustgips" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:IVA 1.3 121mm (R-95-R)" | STANDARD | 9 occurrences | material: layers "Basic Wall:IVA 1.3 121mm (R-95-R)" ("Robustgips" 13., "stender/isolasjon" 95., "Robustgips" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "IDT 2.1 10x21M" | 1 occurrence | material: materials ("_White", "Light grey", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Other, Text
  IFCDOORSTYLE "IDT 5.1 15x21M" | 1 occurrence | material: materials ("Lys grå", "Terskel Tre", "Karm Malt") | property sets: Dør Dobbel:IDT 5.1 15x21M:1790017, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCWALLTYPE "Basic Wall:IVL 3.1 128mm (flis-leca-flis) 34dB" | STANDARD | 6 occurrences | material: layers "Basic Wall:IVL 3.1 128mm (flis-leca-flis) 34dB" ("Flis" 5., "Mur" 118., "Flis" 5.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:IVL 2.1 123mm (flis-leca)" | STANDARD | 5 occurrences | material: layers "Basic Wall:IVL 2.1 123mm (flis-leca)" ("Flis" 5., "Mur" 118.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "IDA 1.1 10x21M" | 1 occurrence | material: materials ("hvit", "Glassfiberfylling", "Terskel Tre", "Karm Malt") | property sets: Dør Enkel_ Glassfelt:IDA 1.1 10x21M:1795541, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCDOORSTYLE "YDA 1.2 16x21M EI 30S" | 1 occurrence | material: materials ("Glass Klart", "Lys grå", "Terskel Tre", "Karm Malt") | property sets: _Dør Dobbel_Ulike_Dørblader_Glassfelt2:YDA 1.2 16x21M EI 30S:1796394, Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data
  IFCDOORSTYLE "IDA 7.1 15x21M EI60CS" | 3 occurrences | material: materials ("Karm Malt", "Lys grå", "Terskel Tre") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "IDT 2.6 10x21M 38dB" | 6 occurrences | material: materials ("Terskel Tre", "Lys grå", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Other, Text
  IFCDOORSTYLE "IDT 2.6 10x21M 38dB" | 1 occurrence | material: materials ("Terskel Tre", "Lys grå", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Other, Text
  IFCWALLTYPE "Basic Wall:IVA 7.1 121mm (95-NR)" | STANDARD | 8 occurrences | material: layers "Basic Wall:IVA 7.1 121mm (95-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:IVL 1.1 118mm leca EI60" | STANDARD | 1 occurrence | material: layers "Basic Wall:IVL 1.1 118mm leca EI60" ("Mur" 118.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:IVL 3.1 128mm (flis-leca-flis)" | STANDARD | 2 occurrences | material: layers "Basic Wall:IVL 3.1 128mm (flis-leca-flis)" ("Flis" 5., "Mur" 118., "Flis" 5.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "IDT 3.5 10x21M 38dB EI30S" | 1 occurrence | material: materials ("Lys grå", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Dør Enkel_ Glassfelt:IDT 3.5 10x21M 38dB EI30S:1814193, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCWALLTYPE "Basic Wall:IVA 6.1 272mm 60dB (HN-95-30-95-NH)" | STANDARD | 1 occurrence | material: layers "Basic Wall:IVA 6.1 272mm 60dB (HN-95-30-95-NH)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 95., "Luftsjikt" 30., "stender/isolasjon" 95., "Gips" 13., "Habito" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCDOORSTYLE "IDT 3.3 10x21M 33dB" | 2 occurrences | material: materials ("Lys grå", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:IVA 7.1 121mm 37dB (95-NR)" | STANDARD | 3 occurrences | material: layers "Basic Wall:IVA 7.1 121mm 37dB (95-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:IVA 2.1 134mm 34dB (H-95-NH)" | STANDARD | 3 occurrences | material: layers "Basic Wall:IVA 2.1 134mm 34dB (H-95-NH)" ("Habito" 13., "stender/isolasjon" 95., "Gips" 13., "Habito" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCWALLTYPE "Basic Wall:IVA 2.4 134mm 34dB (R-95-NH)" | STANDARD | 6 occurrences | material: layers "Basic Wall:IVA 2.4 134mm 34dB (R-95-NH)" ("Robustgips" 13., "stender/isolasjon" 95., "Gips" 13., "Habito" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCDOORSTYLE "IDA 1.1 10x21M" | 1 occurrence | material: materials ("hvit", "Glassfiberfylling", "Terskel Tre", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:IVL 2.1 123mm (flis-leca) 34dB EI60" | STANDARD | 3 occurrences | material: layers "Basic Wall:IVL 2.1 123mm (flis-leca) 34dB EI60" ("Flis" 5., "Mur" 118.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "IDT 2.1 10x21M" | 1 occurrence | material: materials ("_White", "NCS S 0500-N", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Other, Text
  IFCDOORSTYLE "IDT 2.1 10x21M" | 1 occurrence | material: materials ("_White", "NCS S 0500-N", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Other, Text
  IFCDOORSTYLE "IDT 2.3 10x21M 33dB" | 1 occurrence | material: materials ("Terskel Tre", "Lys grå", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Other, Text
  IFCDOORSTYLE "IDT 3.3 10x21M 33dB" | 1 occurrence | material: materials ("Lys grå", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:IVA 1.3 121mm 34dB (R-95-R)" | STANDARD | 6 occurrences | material: layers "Basic Wall:IVA 1.3 121mm 34dB (R-95-R)" ("Robustgips" 13., "stender/isolasjon" 95., "Robustgips" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCDOORSTYLE "IDT 1.3 8x21M EI30S" | 1 occurrence | material: materials ("Terskel Tre", "Lys grå", "Karm Malt") | property sets: Dør Enkel:IDT 1.3 8x21M EI30S:1824685, Analytical Properties, Construction, Dimensions, Identity Data, Other
  IFCDOORSTYLE "IDT 1.1 8x21M" | 1 occurrence | material: materials ("Terskel Tre", "Lys grå", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Other, Text
  IFCDOORSTYLE "IDT 3.6 10x21M 38dB" | 1 occurrence | material: materials ("NCS S 2500-N", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:IVA 1.3 121mm 37dB (R-95-R)" | STANDARD | 2 occurrences | material: layers "Basic Wall:IVA 1.3 121mm 37dB (R-95-R)" ("Robustgips" 13., "stender/isolasjon" 95., "Robustgips" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCDOORSTYLE "IDT 3.2 10x21M 28dB EI30S" | 1 occurrence | material: materials ("Lys grå", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "IDT 3.6 10x21M 38dB" | 1 occurrence | material: materials ("NCS S 2500-N", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "IDA 3.3 18x21M 33dB EI60CS" | 1 occurrence | material: materials ("Glass Klart", "Lys grå", "Terskel Tre", "Karm Malt") | property sets: _Dør Dobbel_Ulike_Dørblader_Glassfelt:IDA 3.3 18x21M 33dB EI60CS:1851355, Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data
  IFCDOORSTYLE "IDA 3.4 18x21M EI30CS" | 1 occurrence | material: materials ("Glass Klart", "Lys grå", "Terskel Tre", "Karm Malt") | property sets: _Dør Dobbel_Ulike_Dørblader_Glassfelt:IDA 3.4 18x21M EI30CS:1851357, Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data
  IFCDOORSTYLE "IDT 3.3 10x21M 33dB" | 1 occurrence | material: materials ("Lys grå", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "IDT 3.3 10x21M 33dB" | 1 occurrence | material: materials ("Lys grå", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "IDT 3.3 10x21M 33dB" | 1 occurrence | material: materials ("Lys grå", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCWINDOWSTYLE "V13 12x16" | 3 occurrences | material: materials ("Glass Klart", "NCS S 0502-Y", "Karm Malt") | property sets: Vindu-Hengslet:V13 12x16:1852971, Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data
  IFCDOORSTYLE "IDT 2.9 10x21M EI60S" | 1 occurrence | material: materials ("Light grey", "Lys grå", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Other, Text
  IFCDOORSTYLE "IDA 1.1 10x21M" | 1 occurrence | material: materials ("hvit", "Glassfiberfylling", "Terskel Tre", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "IDT 5.2 15x21M EI60S" | 2 occurrences | material: materials ("NCS S 1000-N", "Terskel Tre", "Karm Malt") | property sets: Dør Dobbel:IDT 5.2 15x21M EI60S:1899943, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCDOORSTYLE "IDT 2.2 10x21M 28dB EI30S" | 1 occurrence | material: materials ("Light grey", "Lys grå", "Karm Malt") | property sets: Dør Enkel:IDT 2.2 10x21M 28dB EI30S:1924849, Analytical Properties, Construction, Dimensions, Identity Data, Other
  IFCDOORSTYLE "IDT 5.2 15x21M EI60S" | 4 occurrences | material: materials ("NCS S 1000-N", "Terskel Tre", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "IDT 1.2 8x21M 33dB" | 3 occurrences | material: materials ("Terskel Tre", "NCS S 0500-N", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Other, Text
  IFCDOORSTYLE "IDT 2.9 10x21M EI60S" | 1 occurrence | material: materials ("_White", "Lys grå", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Other, Text
  IFCDOORSTYLE "IDT 2.8 10x21M EI30S" | 1 occurrence | material: materials ("Terskel Tre", "Lys grå", "Karm Malt") | property sets: Dør Enkel:IDT 2.8 10x21M EI30S:2008423, Analytical Properties, Construction, Dimensions, Identity Data, Other
  IFCDOORSTYLE "IDT 3.6 10x21M 38dB" | 16 occurrences | material: materials ("NCS S 2500-N", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Dør Enkel_ Glassfelt:IDT 3.6 10x21M 38dB:1781401, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCWALLTYPE "Basic Wall:IVA 6.3 272mm 60dB (RN-95-30-95-NR)" | STANDARD | 4 occurrences | material: layers "Basic Wall:IVA 6.3 272mm 60dB (RN-95-30-95-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95., "Luftsjikt" 30., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCDOORSTYLE "IDT 2.6 10x21M 38dB" | 1 occurrence | material: materials ("Light grey", "Lys grå", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Other, Text
  IFCDOORSTYLE "IDT 2.6 10x21M 38dB" | 1 occurrence | material: materials ("Light grey", "Lys grå", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Other, Text
  IFCDOORSTYLE "IDT 2.3 10x21M 33dB" | 1 occurrence | material: materials ("_White", "Lys grå", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Other, Text
  IFCWALLTYPE "Basic Wall:IVA 14.1 126mm (R-100-R)" | STANDARD | 1 occurrence | material: layers "Basic Wall:IVA 14.1 126mm (R-100-R)" ("Gips" 15., "Massivtre" 100., "Gips" 15.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCWALLTYPE "Basic Wall:IVA 14.1 126mm EI60 (R-100-R)" | STANDARD | 5 occurrences | material: layers "Basic Wall:IVA 14.1 126mm EI60 (R-100-R)" ("Branngips" 15., "Massivtre" 100., "Branngips" 15.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCWALLTYPE "Basic Wall:IVA 13.1 344mm EI60 (HN-95-110-100-N)" | STANDARD | 1 occurrence | material: layers "Basic Wall:IVA 13.1 344mm EI60 (HN-95-110-100-N)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 95., "Luftsjikt" 110., "Massivtre" 100., "Branngips" 15.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "IDT 2.11 10x21M 33dB EI30S" | 1 occurrence | material: materials ("Terskel Tre", "Lys grå", "Karm Malt") | property sets: Dør Enkel:IDT 2.11 10x21M 33dB EI30S:2067575, Analytical Properties, Construction, Dimensions, Identity Data, Other
  IFCWALLTYPE "Basic Wall:IVA 13.1 272mm EI60 (HN-95-100-95-NR) 2" | STANDARD | 1 occurrence | material: layers "Basic Wall:IVA 13.1 272mm EI60 (HN-95-100-95-NR) 2" ("Habito" 13., "Gips" 13., "stender/isolasjon" 95., "Luftsjikt" 144., "Massivtre" 100., "Robustgips" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "IDT 2.3 10x21M 33dB" | 1 occurrence | material: materials ("_White", "Lys grå", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Other, Text
  IFCDOORSTYLE "IDT 1.2 8x21M 33dB" | 1 occurrence | material: materials ("Terskel Tre", "NCS S 0500-N", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Other, Text
  IFCWALLTYPE "Basic Wall:IVA 4.2T 172mm 34dB (HN-120-NR)" | STANDARD | 1 occurrence | material: layers "Basic Wall:IVA 4.2T 172mm 34dB (HN-120-NR)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 120., "Gips" 13., "Robustgips" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCDOORSTYLE "IDT 2.1 10x21M" | 1 occurrence | material: materials ("_White", "NCS S 0500-N", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Other, Text
  IFCDOORSTYLE "IDT 2.3 10x21M 33dB" | 1 occurrence | material: materials ("_White", "NCS S 0500-N", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Other, Text
  IFCDOORSTYLE "IDT 2.12 10x21M 24dB EI30S" | 1 occurrence | material: materials ("Terskel Tre", "Lys grå", "Karm Malt") | property sets: Dør Enkel:IDT 2.12 10x21M 24dB EI30S:2077177, Analytical Properties, Construction, Dimensions, Identity Data, Other
  IFCWALLTYPE "Basic Wall:IVA 1.1 121mm 34dB (H-95-H)" | STANDARD | 6 occurrences | material: layers "Basic Wall:IVA 1.1 121mm 34dB (H-95-H)" ("Habito" 13., "stender/isolasjon" 95., "Habito" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:IVA 1.4 121mm (B-95-B)" | STANDARD | 1 occurrence | material: layers "Basic Wall:IVA 1.4 121mm (B-95-B)" ("Baderomspanel" 13., "stender/isolasjon" 95., "Baderomspanel" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "IDT 3.4 10x21M 33dB E30CS" | 1 occurrence | material: materials ("Lys grå", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:IVL 1.1 118mm (leca) 34dB EI60" | STANDARD | 2 occurrences | material: layers "Basic Wall:IVL 1.1 118mm (leca) 34dB EI60" ("Mur" 118.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "IDT 2.1 10x21M" | 3 occurrences | material: materials ("_White", "NCS S 0500-N", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Other, Text
  IFCDOORSTYLE "IDA 1.1 10x21M" | 1 occurrence | material: materials ("hvit", "Glassfiberfylling", "Terskel Tre", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "IDT 2.3 10x21M 33dB" | 1 occurrence | material: materials ("Terskel Tre", "Lys grå", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Other, Text
  IFCDOORSTYLE "IDT 2.3 10x21M 33dB" | 1 occurrence | material: materials ("Terskel Tre", "Lys grå", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Other, Text
  IFCWALLTYPE "Basic Wall:IVA 1.1T 121mm (H-95-H)" | STANDARD | 1 occurrence | material: layers "Basic Wall:IVA 1.1T 121mm (H-95-H)" ("Habito" 13., "stender/isolasjon" 95., "Habito" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "IDT 1.2 8x21M 33dB" | 9 occurrences | material: materials ("Terskel Tre", "NCS S 0500-N", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Other, Text
  IFCDOORSTYLE "IDA 10.1 14x21M E30CS" | 1 occurrence | material: materials ("Light grey", "Karm Malt", "Lys grå") | property sets: Dør Enkel:IDA 10.1 14x21M E30CS:2114687, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCDOORSTYLE "IDT 2.4 10x21M 38dB EI30S" | 1 occurrence | material: materials ("Terskel Tre", "Lys grå", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Other, Text
  IFCDOORSTYLE "IDT 3.1 10x21M EI 30S" | 1 occurrence | material: materials ("Lys grå", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Dør Enkel_ Glassfelt:IDT 3.1 10x21M EI 30S:2118010, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCWALLTYPE "Basic Wall:IV 50 - skillevegg" | STANDARD | 7 occurrences | material: layers "Basic Wall:IV 50 - skillevegg" ("<Unnamed>" 50.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCDOORSTYLE "IDT 2.9 10x21M EI60S" | 1 occurrence | material: materials ("Light grey", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Other, Text
  IFCDOORSTYLE "IDT 2.10 10x21M 38dB EI60S" | 1 occurrence | material: materials ("Light grey", "Lys grå", "Karm Malt") | property sets: Dør Enkel:IDT 2.10 10x21M 38dB EI60S:2135168, Analytical Properties, Construction, Dimensions, Identity Data, Other
  IFCDOORSTYLE "IDT 3.6 10x21M 38dB" | 1 occurrence | material: materials ("NCS S 2500-N", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "IDT 4.2 13x21M EI 60S" | 1 occurrence | material: materials ("Trekledning", "Terskel Tre", "Karm Malt") | property sets: Dør Dobbel_Ulike_Dørblader:IDT 4.2 13x21M EI 60S:2137996, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCDOORSTYLE "IDT 3.6 10x21M 38dB" | 21 occurrences | material: materials ("NCS S 2500-N", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:IVA 6.3 272mm 48dB (RN-95-30-95-NR)" | STANDARD | 1 occurrence | material: layers "Basic Wall:IVA 6.3 272mm 48dB (RN-95-30-95-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95., "Luftsjikt" 30., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCWALLTYPE "Basic Wall:IVA 6.3 272mm 55dB EI60 (RN-95-30-95-NR)" | STANDARD | 5 occurrences | material: layers "Basic Wall:IVA 6.3 272mm 55dB EI60 (RN-95-30-95-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95., "Luftsjikt" 30., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCWALLTYPE "Basic Wall:IVA 4.2 172mm 34dB (HN-120-NR)" | STANDARD | 1 occurrence | material: layers "Basic Wall:IVA 4.2 172mm 34dB (HN-120-NR)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 120., "Gips" 13., "Robustgips" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCDOORSTYLE "IDT 2.7 10x21M 38dB EI60S" | 1 occurrence | material: materials ("Light grey", "Lys grå", "Karm Malt") | property sets: Dør Enkel:IDT 2.7 10x21M 38dB EI60S:2154214, Analytical Properties, Construction, Dimensions, Identity Data, Other
  IFCDOORSTYLE "IDF 1.1 Foldevegg 6500x2800" | 1 occurrence | material: materials ("Light grey", "Karm Malt") | property sets: Side_Stack_Operable_Wall_6500:IDF 1.1 Foldevegg 6500x2800:2154531, Analytical Properties, Constraints, Construction, Dimensions, Identity Data
  IFCWALLTYPE "Basic Wall:IVA 3.3 145mm E30 (RN-95-NR)" | STANDARD | 2 occurrences | material: layers "Basic Wall:IVA 3.3 145mm E30 (RN-95-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "IDA 6.2 12x21M EI 30CS" | 3 occurrences | material: materials ("Lys grå", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Dør Enkel_ Glassfelt:IDA 6.2 12x21M EI 30CS:1700926, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCDOORSTYLE "IDT 2.1 10x21M" | 2 occurrences | material: materials ("_White", "NCS S 0500-N", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Other, Text
  IFCDOORSTYLE "IDT 2.1 10x21M" | 1 occurrence | material: materials ("_White", "NCS S 0500-N", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Other, Text
  IFCBUILDINGELEMENTPROXYTYPE "NUS - 0,0 - Kake" | 1 occurrence | property sets: Dimensions, Identity Data, Other
  IFCDOORSTYLE "IDT 2.5 10x21M 33dB EI60S" | 1 occurrence | material: materials ("Light grey", "Lys grå", "Karm Malt") | property sets: Dør Enkel:IDT 2.5 10x21M 33dB EI60S:2235152, Analytical Properties, Construction, Dimensions, Identity Data, Other
  IFCDOORSTYLE "IDA 3.2 18x21M 33dB" | 1 occurrence | material: materials ("Glass Klart", "Lys grå", "Terskel Tre", "Karm Malt") | property sets: _Dør Dobbel_Ulike_Dørblader_Glassfelt2:IDA 3.2 18x21M 33dB:2235278, Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data
  IFCWALLTYPE "Basic Wall:IVA 8.1 125mm sjaktvegg EI60" | STANDARD | 5 occurrences | material: layers "Basic Wall:IVA 8.1 125mm sjaktvegg EI60" ("Branngips" 15., "Branngips" 15., "stender/isolasjon" 95.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:IVA 6.2 272mm 55dB EI60 (RN-95-30-95-NH)" | STANDARD | 3 occurrences | material: layers "Basic Wall:IVA 6.2 272mm 55dB EI60 (RN-95-30-95-NH)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 95., "Luftsjikt" 30., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCWALLTYPE "Basic Wall:IVL 2.1 123mm (flis-leca) EI60" | STANDARD | 5 occurrences | material: layers "Basic Wall:IVL 2.1 123mm (flis-leca) EI60" ("Flis" 5., "Mur" 118.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "IDT 2.9 10x21M EI60S" | 1 occurrence | material: materials ("Light grey", "Lys grå", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Other, Text
  IFCWINDOWSTYLE "V13 12x16" | 4 occurrences | material: materials ("Glass Klart", "NCS S 0502-Y", "Karm Malt") | property sets: Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCWINDOWSTYLE "V15 24x16" | 1 occurrence | material: materials ("NCS S 0502-Y", "Glass Klart") | property sets: Fast vindu+ åpningsvindu:V15 24x16:2427850, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCWINDOWSTYLE "V14 14x16" | 1 occurrence | material: materials ("Glass Klart", "NCS S 0502-Y") | property sets: Vindu-Fast:V14 14x16:2430034, Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data
  IFCWINDOWSTYLE "V14 14x16" | 1 occurrence | material: materials ("Glass Klart", "NCS S 0502-Y") | property sets: Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCWALLTYPE "Basic Wall:YV 8.2 458mm gul platekledning EI60" | STANDARD | 1 occurrence | material: layers "Basic Wall:YV 8.2 458mm gul platekledning EI60" ("Cembrit Metro Amsterdam" 8., "Luftsjikt" 36., "Luftsjikt" 48., "Vindsperre" 9., "Stender isolert vegg" 296., "NO_Utlekting" 48., "Branngips" 15.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "IDT 2.5 10x21M 33dB EI60S" | 1 occurrence | material: materials ("Light grey", "Lys grå", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Other, Text
  IFCDOORSTYLE "IDT 2.5 10x21M 33dB EI60S" | 1 occurrence | material: materials ("Light grey", "Lys grå", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Other, Text
  IFCWALLTYPE "Basic Wall:IVL 1.1 118mm (leca) 34dB" | STANDARD | 2 occurrences | material: layers "Basic Wall:IVL 1.1 118mm (leca) 34dB" ("Mur" 118.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:IVL 1.1 118mm (leca) 44dB" | STANDARD | 1 occurrence | material: layers "Basic Wall:IVL 1.1 118mm (leca) 44dB" ("Mur" 118.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "IDT 2.1 10x21M" | 1 occurrence | material: materials ("_White", "NCS S 0500-N", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Other, Text
  IFCDOORSTYLE "IDT 2.1 10x21M" | 2 occurrences | material: materials ("_White", "NCS S 0500-N", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Other, Text
  IFCDOORSTYLE "IDT 2.1 10x21M" | 1 occurrence | material: materials ("_White", "NCS S 0500-N", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Other, Text
  IFCDOORSTYLE "IDT 2.1 10x21M" | 1 occurrence | material: materials ("Light grey", "NCS S 0500-N", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Other, Text
  IFCWINDOWSTYLE "GF 3.6 6x21 33dB" | 2 occurrences | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCWINDOWSTYLE "GF 3.6 6x21 33dB" | 1 occurrence | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCWINDOWSTYLE "GF 6.1 8x21 33dB" | 1 occurrence | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCWINDOWSTYLE "GF 2.2 9x21 33dB" | 3 occurrences | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Vindu-Fast:GF 2.2 9x21 33dB:2504598, Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data
  IFCWINDOWSTYLE "GF 2.2 9x21 33dB" | 1 occurrence | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCWINDOWSTYLE "GF 2.2 9x21 33dB" | 1 occurrence | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCWINDOWSTYLE "GF 2.2 9x21 33dB" | 1 occurrence | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCWINDOWSTYLE "GF 2.2 9x21 33dB" | 1 occurrence | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCWINDOWSTYLE "GF 2.1 9x21 38dB" | 1 occurrence | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Vindu-Fast:GF 2.1 9x21 38dB:2527441, Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data
  IFCWINDOWSTYLE "GF 5.3 5x21 33dB" | 1 occurrence | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Vindu-Fast:GF 5.3 5x21 33dB:2527482, Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data
  IFCWINDOWSTYLE "GF 15.1 36x10 33dB" | 1 occurrence | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Vindu-Fast:GF 15.1 36x10 33dB:2529032, Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data
  IFCWINDOWSTYLE "GF 8.1 7x7 58dB" | 1 occurrence | material: materials ("Glass Klart", "NCS S 1002-Y") | property sets: Vindu-Fast:GF 8.1 7x7 58dB:2529523, Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data
  IFCWINDOWSTYLE "GF 2.4 9x21 25dB E30" | 1 occurrence | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Vindu-Fast:GF 2.4 9x21 25dB E30:2529908, Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data
  IFCWINDOWSTYLE "GF 2.3 9x21 25dB EI30" | 1 occurrence | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Vindu-Fast:GF 2.3 9x21 25dB EI30:2530890, Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data
  IFCWINDOWSTYLE "GF 3.1 6x21 25dB EI30" | 1 occurrence | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Vindu-Fast:GF 3.1 6x21 25dB EI30:2531956, Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data
  IFCWINDOWSTYLE "GF 4.3 33dB EI30" | 1 occurrence | material: materials ("Karm Malt", "Glass Klart", "NCS S 3502-Y") | property sets: Vindu_2felt:GF 4.3 33dB EI30:2532106, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCWINDOWSTYLE "GF 3.4 6x21 33dB E30" | 1 occurrence | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Vindu-Fast:GF 3.4 6x21 33dB E30:2532146, Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data
  IFCWINDOWSTYLE "GF 2.2 9x21 33dB" | 2 occurrences | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCWINDOWSTYLE "GF 2.2 9x21 33dB" | 4 occurrences | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCWINDOWSTYLE "GF 6.1 8x21 33dB" | 1 occurrence | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCWALLTYPE "Basic Wall:YV 7.3 410mm rød platekledning" | STANDARD | 27 occurrences | material: layers "Basic Wall:YV 7.3 410mm rød platekledning" ("Cembrit Metro Copenhagen" 8., "Luftsjikt" 36., "Vindsperre" 9., "Stender isolert vegg" 296., "NO_Utlekting" 48., "Robustgips" 12.5) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:YV 7.2 410mm grønn platekledning" | STANDARD | 20 occurrences | material: layers "Basic Wall:YV 7.2 410mm grønn platekledning" ("Cembrit Metro Hamburg" 8., "Luftsjikt" 36., "Vindsperre" 9., "Stender isolert vegg" 296., "NO_Utlekting" 48., "Robustgips" 12.5) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCWINDOWSTYLE "V25 12x30 36dB" | 2 occurrences | material: materials ("Glass Klart", "NCS S 0502-Y") | property sets: Analysis Results(Type), Analytical Properties(Type), Construction(Type), Dimensions(Type), Identity Data(Type), Materials and Finishes(Type)
  IFCWALLTYPE "Basic Wall:YV 7.4 410mm gul platekledning" | STANDARD | 20 occurrences | material: layers "Basic Wall:YV 7.4 410mm gul platekledning" ("Cembrit Metro Amsterdam" 8., "Luftsjikt" 36., "Vindsperre" 9., "Stender isolert vegg" 296., "NO_Utlekting" 48., "Robustgips" 12.5) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCWINDOWSTYLE "VA1 12x24" | 1 occurrence | material: materials ("Glass Klart", "NCS S 0502-Y") | property sets: Analysis Results(Type), Analytical Properties(Type), Construction(Type), Dimensions(Type), Identity Data(Type), Materials and Finishes(Type)
  IFCWINDOWSTYLE "GF 7.4 15x21 EI60" | 2 occurrences | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Vindu-Fast:GF 7.4 15x21 EI60:2552756, Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data
  IFCDOORSTYLE "IDT 3.9 10x21M 28dB" | 1 occurrence | material: materials ("Lys grå", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Dør Enkel_ Glassfelt:IDT 3.9 10x21M 28dB:2571576, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCWINDOWSTYLE "GF 7.1 15x21 25dB" | 1 occurrence | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Vindu-Fast:GF 7.1 15x21 25dB:2571640, Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data
  IFCWALLTYPE "Basic Wall:YV 20.1" | STANDARD | 5 occurrences | material: layers "Basic Wall:YV 20.1" ("Trekledning" 19., "Luftsjikt" 36., "Luftsjikt" 36., "Vindsperre" 9., "Stender isolert vegg" 148., "Kryssfiner" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:YV 20.3" | STANDARD | 3 occurrences | material: layers "Basic Wall:YV 20.3" ("Trekledning" 19., "Luftsjikt" 36., "Luftsjikt" 36., "Vindsperre" 9., "Stender isolert vegg" 148., "Baderomspanel" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:IV 20.1" | STANDARD | 1 occurrence | material: layers "Basic Wall:IV 20.1" ("Baderomspanel" 10.2, "stender" 98., "Robustgips" 12.5) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "YDT 1.2 10x21M Isolert" | 1 occurrence | material: materials ("_White", "Lys grå", "Beslag") | property sets: Dør Enkel:YDT 1.2 10x21M Isolert:2583745, Analytical Properties, Construction, Dimensions, Identity Data, Other
  IFCWINDOWSTYLE "VA1 12x24" | 2 occurrences | material: materials ("Glass Klart", "NCS S 0502-Y") | property sets: Analysis Results(Type), Analytical Properties(Type), Construction(Type), Dimensions(Type), Identity Data(Type), Materials and Finishes(Type)
  IFCWALLTYPE "Basic Wall:Sokkel pusset" | STANDARD | 19 occurrences | material: layers "Basic Wall:Sokkel pusset" ("Webertherm 260" 10., "NO_isolasjon" 100.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCWINDOWSTYLE "GF 3.2 6x21 38dB" | 9 occurrences | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Vindu-Fast:GF 3.2 6x21 38dB:2498596, Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data
  IFCDOORSTYLE "IDT 2.3 10x21M 33dB" | 1 occurrence | material: materials ("Terskel Tre", "Lys grå", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Other, Text
  IFCWALLTYPE "Basic Wall:IVA 3.2 145mm 34dB E30 (HN-95-NR)" | STANDARD | 1 occurrence | material: layers "Basic Wall:IVA 3.2 145mm 34dB E30 (HN-95-NR)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCWALLTYPE "Basic Wall:IVA 2.4 134mm 44dB (R-95-NH)" | STANDARD | 1 occurrence | material: layers "Basic Wall:IVA 2.4 134mm 44dB (R-95-NH)" ("Robustgips" 13., "stender/isolasjon" 95., "Gips" 13., "Habito" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCWALLTYPE "Basic Wall:IVA 13.1 126mm 48dB (HN-95+20+100-R)" | STANDARD | 1 occurrence | material: layers "Basic Wall:IVA 13.1 126mm 48dB (HN-95+20+100-R)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 95., "Luftsjikt" 20., "Massivtre" 100., "Branngips" 15.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:IVL 2.1 123mm (flis-leca) 44dB" | STANDARD | 2 occurrences | material: layers "Basic Wall:IVL 2.1 123mm (flis-leca) 44dB" ("Flis" 5., "Mur" 118.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:IVA 4.3T 172mm 34dB (RN-120-NR)" | STANDARD | 3 occurrences | material: layers "Basic Wall:IVA 4.3T 172mm 34dB (RN-120-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 120., "Gips" 13., "Robustgips" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCWALLTYPE "Basic Wall:IVA 2.3T 134mm 34dB (R-95-NR)" | STANDARD | 5 occurrences | material: layers "Basic Wall:IVA 2.3T 134mm 34dB (R-95-NR)" ("Robustgips" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCWALLTYPE "Basic Wall:IVA 3.2T 145mm 48dB EI60 (HN-95-NR)" | STANDARD | 5 occurrences | material: layers "Basic Wall:IVA 3.2T 145mm 48dB EI60 (HN-95-NR)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCWALLTYPE "Basic Wall:IVA 3.2T 145mm 44dB (HN-95-NR)" | STANDARD | 1 occurrence | material: layers "Basic Wall:IVA 3.2T 145mm 44dB (HN-95-NR)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCWALLTYPE "Basic Wall:IVA 3.2T 145mm EI60 (HN-95-NR)" | STANDARD | 3 occurrences | material: layers "Basic Wall:IVA 3.2T 145mm EI60 (HN-95-NR)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCWALLTYPE "Basic Wall:IVA 12.1 121mm (95-NR)" | STANDARD | 1 occurrence | material: layers "Basic Wall:IVA 12.1 121mm (95-NR)" ("Flis" 5., "Litex" 12., "Kryssfiner" 15., "stender/isolasjon" 95.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:YV 19.1 256mm EI60" | STANDARD | 1 occurrence | material: layers "Basic Wall:YV 19.1 256mm EI60" ("Trekledning" 19., "Luftsjikt" 48., "Luftsjikt" 36., "Vindsperre" 9., "Stender isolert vegg" 48., "Stender isolert vegg" 96.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCCURTAINWALLTYPE "Curtain Wall:YV 100 S" | 13 occurrences | property sets: Construction, Horizontal Grid, Horizontal Mullions, Identity Data, Other, Vertical Grid
  IFCWALLTYPE "Basic Wall:YV 3.1 306mm EI60" | STANDARD | 8 occurrences | material: layers "Basic Wall:YV 3.1 306mm EI60" ("Trekledning" 19., "Luftsjikt" 48., "Luftsjikt" 36., "Luftsjikt" 48., "Vindsperre" 9., "Stender isolert vegg" 146.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "YDA 1.2 16x21M EI 30S" | 1 occurrence | material: materials ("Glass Klart", "Lys grå", "Terskel Tre", "Karm Malt") | property sets: Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCDOORSTYLE "YDA 1.2 16x21M EI 30S" | 1 occurrence | material: materials ("Glass Klart", "Lys grå", "Terskel Tre", "Karm Malt") | property sets: Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCCURTAINWALLTYPE "Curtain Wall:Glassfasade 6" | 1 occurrence | property sets: Construction, Horizontal Grid, Horizontal Mullions, Identity Data, Other, Vertical Grid
  IFCWALLTYPE "Basic Wall:IVA 7.1 121mm Skjørt" | STANDARD | 15 occurrences | material: layers "Basic Wall:IVA 7.1 121mm Skjørt" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCCURTAINWALLTYPE "Curtain Wall:GFA 2 38dB" | 1 occurrence | property sets: Construction, Horizontal Grid, Identity Data, Other, Vertical Grid
  IFCCURTAINWALLTYPE "Curtain Wall:GFA 1 38dB EI30S" | 1 occurrence | property sets: Construction, Horizontal Grid, Identity Data, Other, Vertical Grid
  IFCDOORSTYLE "IDT 9.1 10x21M" | 1 occurrence | material: materials ("_White", "Light grey", "Karm Malt") | property sets: Dør Enkel:IDT 9.1 10x21M:3427527, Analytical Properties, Construction, Dimensions, Identity Data, Other
  IFCDOORSTYLE "IDT 3.5 10x21M 38dB EI30S" | 1 occurrence | material: materials ("Lys grå", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:IVA 2.3 134mm 37dB (R-95-NR)" | STANDARD | 1 occurrence | material: layers "Basic Wall:IVA 2.3 134mm 37dB (R-95-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95., "Robustgips" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCWINDOWSTYLE "GF 8.2 58dB" | 1 occurrence | material: materials ("Glass Klart", "NCS S 1002-Y", "Karm Malt") | property sets: Vindu-Hengslet:GF 8.2 58dB:3566352, Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data
  IFCWALLTYPE "Basic Wall:Flis" | STANDARD | 32 occurrences | material: layers "Basic Wall:Flis" ("Flis" 5.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCWALLTYPE "Basic Wall:IVA 6.2 272mm 34dB (HN-95-60-95-NR)" | STANDARD | 1 occurrence | material: layers "Basic Wall:IVA 6.2 272mm 34dB (HN-95-60-95-NR)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 95., "Luftsjikt" 30., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCWALLTYPE "Basic Wall:IVA 6.3 332mm 44dB (RN-95-90-95-NR)" | STANDARD | 1 occurrence | material: layers "Basic Wall:IVA 6.3 332mm 44dB (RN-95-90-95-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95., "Luftsjikt" 90., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCWALLTYPE "Basic Wall:IVL 4.1 173mm leca + litex EI60" | STANDARD | 1 occurrence | material: layers "Basic Wall:IVL 4.1 173mm leca + litex EI60" ("<Unnamed>" 5., "Litex" 12., "Mur" 118.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:IVA 7.1 121mm 37dB EI30 (95-NR)" | STANDARD | 22 occurrences | material: layers "Basic Wall:IVA 7.1 121mm 37dB EI30 (95-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "IDA 9.1 12x21M EI60CS" | 1 occurrence | material: materials ("Light grey", "Karm Malt", "Lys grå") | property sets: Dør Enkel:IDA 9.1 12x21M EI60CS:3676346, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCDOORSTYLE "IDA 7.1 15x21M EI60CS" | 2 occurrences | material: materials ("Karm Malt", "Lys grå", "Terskel Tre") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "IDA 3.5 18x21M 33dB EI30S" | 1 occurrence | material: materials ("Lys grå", "Terskel Tre", "Karm Malt") | property sets: Dør Dobbel_Ulike_Dørblader:IDA 3.5 18x21M 33dB EI30S:3705902, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCBEAMTYPE "IPE-Beams:IPE 200" | BEAM | 1 occurrence | property sets: Dimensions, Identity Data, Other, Structural
  IFCBEAMTYPE "IPE330" | element type "IPE330" | BEAM | 1 occurrence | property sets: Dimensions, Identity Data, Materials and Finishes, Other, Structural
  IFCWALLTYPE "Basic Wall:IVA 3.2T 145mm 34dB EI60 (HN-95-NR)" | STANDARD | 1 occurrence | material: layers "Basic Wall:IVA 3.2T 145mm 34dB EI60 (HN-95-NR)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCWINDOWSTYLE "V22 14x14" | 4 occurrences | material: materials ("Glass Klart", "NCS S 0502-Y") | property sets: Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCDOORSTYLE "YDS 2.1 13x21M" | 1 occurrence | material: materials ("Terskel Tre", "Dørblad Tre", "Karm Malt") | property sets: Dør Enkel:YDS 2.1 13x21M:3971723, Analytical Properties, Construction, Dimensions, Identity Data, Other
  IFCDOORSTYLE "YDA 2.1 12x30 36dB" | 1 occurrence | material: materials ("N_Windows - Glass", "RAL 9004", "Terskel Tre") | property sets: Analytical Properties(Type), Construction(Type), Dimensions(Type), Identity Data(Type), Materials and Finishes(Type), Other(Type)
  IFCDOORSTYLE "IDT 2.8 10x21M EI30S" | 1 occurrence | material: materials ("Terskel Tre", "Lys grå", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Other, Text
  IFCWALLTYPE "Basic Wall:250mm" | STANDARD | 2 occurrences | material: layers "Basic Wall:250mm" ("hvit malt" 250.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:IVA 6.2T 272mm 48dB EI60 (HN-95-30-95-NR)" | STANDARD | 3 occurrences | material: layers "Basic Wall:IVA 6.2T 272mm 48dB EI60 (HN-95-30-95-NR)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 95., "Luftsjikt" 30., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCWALLTYPE "Basic Wall:IVA 3.1 145mm 48dB EI60 (HN-95-NH)" | STANDARD | 1 occurrence | material: layers "Basic Wall:IVA 3.1 145mm 48dB EI60 (HN-95-NH)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Habito" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCWALLTYPE "Basic Wall:IVA 6.2 342mm 48dB EI 60 (HN-95-100-95-NR)" | STANDARD | 1 occurrence | material: layers "Basic Wall:IVA 6.2 342mm 48dB EI 60 (HN-95-100-95-NR)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 95., "Luftsjikt" 100., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCWALLTYPE "Basic Wall:IVA 3.2 145mm 44dB EI60 (HN-95-NR)" | STANDARD | 1 occurrence | material: layers "Basic Wall:IVA 3.2 145mm 44dB EI60 (HN-95-NR)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCWALLTYPE "Basic Wall:YV 11.1 266 Gesims Vindfang" | STANDARD | 2 occurrences | material: layers "Basic Wall:YV 11.1 266 Gesims Vindfang" ("Cembrit Metro Copenhagen" 8., "Luftsjikt" 36., "Vindsperre" 9., "Stender isolert vegg" 198., "Kryssfiner" 15.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:YV 11.1 266 Gesims Vindfang 2" | STANDARD | 1 occurrence | material: layers "Basic Wall:YV 11.1 266 Gesims Vindfang 2" ("Cembrit Metro Copenhagen" 8., "Stender isolert vegg" 198.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:IVA 4.3 172mm 48dB (RN-120-NR)" | STANDARD | 2 occurrences | material: layers "Basic Wall:IVA 4.3 172mm 48dB (RN-120-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 120., "Gips" 13., "Robustgips" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCWALLTYPE "Basic Wall:YV 21.1" | STANDARD | 4 occurrences | material: layers "Basic Wall:YV 21.1" ("Trekledning" 19., "stender" 148.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "YDA 6.1 Skyvedører" | 1 occurrence | material: materials ("Aluminio Manusa", "Glass") | property sets: Analytical Properties(Type), Construction(Type), Dimensions(Type), General(Type), Graphics(Type), Identity Data(Type)
  IFCDOORSTYLE "YDT 1.1 10x21M" | 1 occurrence | material: materials ("Terskel Tre", "Lys grå", "Karm Malt", "Trekledning") | property sets: Dør Enkel:YDT 1.1 10x21M:4118873, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCWALLTYPE "Basic Wall:YV 15.1 150 EI60" | STANDARD | 1 occurrence | material: layers "Basic Wall:YV 15.1 150 EI60" ("<Unnamed>" 8., "<Unnamed>" 36., "Vindsperre" 9., "Vindsperre" 9., "stender" 98., "Vindsperre" 9., "<Unnamed>" 9., "<Unnamed>" 36., "<Unnamed>" 8., "<Unnamed>" 36., "<Unnamed>" 48.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:30mm" | STANDARD | 4 occurrences | material: layers "Basic Wall:30mm" ("hvit malt" 30.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "IDT 3.6 10x21M 38dB" | 3 occurrences | material: materials ("NCS S 2500-N", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "IDT 3.2 10x21M 28dB EI30S" | 1 occurrence | material: materials ("Lys grå", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "YDT 1.2 10x21M Isolert" | 1 occurrence | material: materials ("_White", "Lys grå", "Beslag") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Other, Text
  IFCWALLTYPE "Basic Wall:Bassabsorbent" | STANDARD | 2 occurrences | material: layers "Basic Wall:Bassabsorbent" ("stender/isolasjon" 98.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:IV 21.1" | STANDARD | 1 occurrence | material: layers "Basic Wall:IV 21.1" ("Kryssfiner" 12., "Stender isolert vegg" 148., "Kryssfiner" 12.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "YDP 1.1 2400 x 2100mm" | 1 occurrence | material: "Metal - Paint Finish - Ivory, Matte" | property sets: M_Overhead-Sectional:YDP 1.1 2400 x 2100mm:4214299, Analytical Properties, Construction, Dimensions, Identity Data, Other
  IFCDOORSTYLE "IDA 1.1 10x21M" | 1 occurrence | material: materials ("hvit", "Glassfiberfylling", "Terskel Tre", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "IDA 1.1 10x21M" | 1 occurrence | material: materials ("hvit", "Glassfiberfylling", "Terskel Tre", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "IDT 6.1 15x21M 33dB" | 1 occurrence | material: materials ("Glass Klart", "Lys grå", "Terskel Tre", "Karm Malt") | property sets: Analysis Results(Type), Analytical Properties(Type), Construction(Type), Dimensions(Type), Identity Data(Type), Materials and Finishes(Type)
  IFCBUILDINGELEMENTPROXYTYPE "TV-skjerm" | 14 occurrences | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "1700 x 2100mm" | 1 occurrence | material: "Metal - Paint Finish - Ivory, Matte" | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:IVSP 84mm SPILEVEGG" | 42 occurrences | material: layers "Basic Wall:IVSP 84mm SPILEVEGG" ("NO_isolasjon" 48., "<Unnamed>" 16., "Spiler" 34.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCDOORSTYLE "IDT 6.2 15x21M 38dB" | 1 occurrence | material: materials ("Glass Klart", "Lys grå", "Terskel Tre", "Karm Malt") | property sets: _Dør Dobbel_Ulike_Dørblader_Glassfelt2:IDT 6.2 15x21M 38dB:4452497, Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data
  IFCWINDOWSTYLE "GF 2.2 9x21 33dB" | 2 occurrences | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCDOORSTYLE "YDA 5.1 16x21M" | 1 occurrence | material: materials ("Glass Klart", "Lys grå", "Terskel Tre", "Karm Malt") | property sets: _Dør Dobbel_Ulike_Dørblader_Glassfelt:YDA 5.1 16x21M:4543202, Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 2" | 1 occurrence | material: "Lys grå" | property sets: Identity Data, Other
  IFCCURTAINWALLTYPE "Sloped Glazing:Tak glass - Baldakintak" | 2 occurrences | property sets: Construction, Grid 1, Grid 2, Identity Data, Other
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 2" | 1 occurrence | material: "Lys grå" | property sets: Identity Data, Other
  IFCWALLTYPE "Basic Wall:IVA 8.1T 125mm sjaktvegg EI60" | STANDARD | 3 occurrences | material: layers "Basic Wall:IVA 8.1T 125mm sjaktvegg EI60" ("Branngips" 15., "Branngips" 15., "stender/isolasjon" 95.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCCURTAINWALLTYPE "Curtain Wall:Glassfasade 5e" | 1 occurrence | property sets: Construction, Horizontal Grid, Identity Data, Other, Vertical Grid
  IFCCURTAINWALLTYPE "Curtain Wall:Glassfasade 4c" | 1 occurrence | property sets: Construction, Horizontal Grid, Identity Data, Other, Vertical Grid
  IFCCURTAINWALLTYPE "Curtain Wall:Glassfasade 3a" | 1 occurrence | property sets: Construction, Horizontal Grid, Identity Data, Other, Vertical Grid
  IFCCURTAINWALLTYPE "Curtain Wall:Glassfasade 2a" | 1 occurrence | property sets: Construction, Horizontal Grid, Identity Data, Other, Vertical Grid
  IFCCURTAINWALLTYPE "Curtain Wall:Glassfasade 1c" | 1 occurrence | property sets: Construction, Horizontal Grid, Identity Data, Other, Vertical Grid
  IFCWALLTYPE "Basic Wall:IVA 6.1 342mm (HN-95-100-95-NH)" | STANDARD | 1 occurrence | material: layers "Basic Wall:IVA 6.1 342mm (HN-95-100-95-NH)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 95., "Luftsjikt" 100., "stender/isolasjon" 95., "Gips" 13., "Habito" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCWALLTYPE "Basic Wall:YV 14.1 371mm u/kledning" | STANDARD | 2 occurrences | material: layers "Basic Wall:YV 14.1 371mm u/kledning" ("RAL 9004" 5., "Vindsperre" 9., "Stender isolert vegg" 296., "NO_Utlekting" 48., "Gips" 12.5) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:IVA 6.3 252mm EI60 (RN-95-40-95-NR)" | STANDARD | 2 occurrences | material: layers "Basic Wall:IVA 6.3 252mm EI60 (RN-95-40-95-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95., "Luftsjikt" 20., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCWALLTYPE "Basic Wall:YV 14.2 371mm u/kledning EI60" | STANDARD | 1 occurrence | material: layers "Basic Wall:YV 14.2 371mm u/kledning EI60" ("RAL 9004" 5., "Vindsperre" 9., "Stender isolert vegg" 296., "NO_Utlekting" 48., "Branngips" 15.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 3" | 1 occurrence | material: "Lys grå" | property sets: Identity Data, Other
  IFCWINDOWSTYLE "GF 13.1 36x21 38dB" | 1 occurrence | material: materials ("Karm Malt", "Glass Klart", "NCS S 3502-Y") | property sets: Vindu_3felt:GF 13.1 36x21 38dB:5149291, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCWINDOWSTYLE "GF 14.1" | 1 occurrence | material: materials ("Karm Malt", "Glass Klart", "NCS S 3502-Y") | property sets: Vindu_2felt:GF 14.1:5156029, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCWALLTYPE "Basic Wall:YV 6.2 299mm grå platekledning basseng" | STANDARD | 3 occurrences | material: layers "Basic Wall:YV 6.2 299mm grå platekledning basseng" ("Cembrit Metro London" 8., "Luftsjikt" 36., "Vindsperre" 9., "Stender isolert vegg" 246.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCWINDOWSTYLE "V16 21x16" | 1 occurrence | material: materials ("NCS S 0502-Y", "Glass Klart") | property sets: Analytical Properties(Type), Construction(Type), Dimensions(Type), Identity Data(Type), Materials and Finishes(Type), Other(Type)
  IFCWINDOWSTYLE "V17 21x16" | 2 occurrences | material: materials ("NCS S 0502-Y", "Glass Klart") | property sets: Analytical Properties(Type), Construction(Type), Dimensions(Type), Identity Data(Type), Materials and Finishes(Type), Other(Type)
  IFCWINDOWSTYLE "V18 21x16" | 2 occurrences | material: materials ("NCS S 0502-Y", "Glass Klart") | property sets: Analytical Properties(Type), Construction(Type), Dimensions(Type), Identity Data(Type), Materials and Finishes(Type), Other(Type)
  IFCWINDOWSTYLE "V19 21x16" | 1 occurrence | material: materials ("NCS S 0502-Y", "Glass Klart") | property sets: Analytical Properties(Type), Construction(Type), Dimensions(Type), Identity Data(Type), Materials and Finishes(Type), Other(Type)
  IFCWINDOWSTYLE "V19 21x16" | 1 occurrence | material: materials ("NCS S 0502-Y", "Glass Klart") | property sets: Analytical Properties(Type), Construction(Type), Dimensions(Type), Identity Data(Type), Materials and Finishes(Type), Other(Type)
  IFCWINDOWSTYLE "V20 19x16" | 1 occurrence | material: materials ("NCS S 0502-Y", "Glass Klart") | property sets: Analytical Properties(Type), Construction(Type), Dimensions(Type), Identity Data(Type), Materials and Finishes(Type), Other(Type)
  IFCWINDOWSTYLE "V15 24x16" | 1 occurrence | material: materials ("NCS S 0502-Y", "Glass Klart") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCWINDOWSTYLE "V21 35x16" | 2 occurrences | material: materials ("NCS S 0502-Y", "Glass Klart") | property sets: Analytical Properties(Type), Construction(Type), Dimensions(Type), Identity Data(Type), Materials and Finishes(Type), Other(Type)
  IFCCOLUMNTYPE "115x115mm" | element type "115x115mm" | COLUMN | 1 occurrence | property sets: Dimensions, Graphics, Identity Data, Materials and Finishes, Other
  IFCCOLUMNTYPE "115x115mm" | element type "115x115mm" | COLUMN | 1 occurrence | property sets: Dimensions, Graphics, Identity Data, Materials and Finishes, Other
  IFCCOLUMNTYPE "115x115mm" | element type "115x115mm" | COLUMN | 1 occurrence | property sets: Dimensions, Graphics, Identity Data, Materials and Finishes, Other
  IFCCOLUMNTYPE "115x115mm" | element type "115x115mm" | COLUMN | 1 occurrence | property sets: Dimensions, Graphics, Identity Data, Materials and Finishes, Other
  IFCCOLUMNTYPE "115x115mm" | element type "115x115mm" | COLUMN | 1 occurrence | property sets: Dimensions, Graphics, Identity Data, Materials and Finishes, Other
  IFCCOLUMNTYPE "115x115mm" | element type "115x115mm" | COLUMN | 1 occurrence | property sets: Dimensions, Graphics, Identity Data, Materials and Finishes, Other
  IFCCOLUMNTYPE "115x115mm" | element type "115x115mm" | COLUMN | 1 occurrence | property sets: Dimensions, Graphics, Identity Data, Materials and Finishes, Other
  IFCCOLUMNTYPE "115x115mm" | element type "115x115mm" | COLUMN | 1 occurrence | property sets: Dimensions, Graphics, Identity Data, Materials and Finishes, Other
  IFCCOLUMNTYPE "115x115mm" | element type "115x115mm" | COLUMN | 1 occurrence | property sets: Dimensions, Graphics, Identity Data, Materials and Finishes, Other
  IFCCOLUMNTYPE "115x115mm" | element type "115x115mm" | COLUMN | 1 occurrence | property sets: Dimensions, Graphics, Identity Data, Materials and Finishes, Other
  IFCCOLUMNTYPE "115x115mm" | element type "115x115mm" | COLUMN | 1 occurrence | property sets: Dimensions, Graphics, Identity Data, Materials and Finishes, Other
  IFCCOLUMNTYPE "115x115mm" | element type "115x115mm" | COLUMN | 1 occurrence | property sets: Dimensions, Graphics, Identity Data, Materials and Finishes, Other
  IFCCOLUMNTYPE "115x115mm" | element type "115x115mm" | COLUMN | 1 occurrence | property sets: Dimensions, Graphics, Identity Data, Materials and Finishes, Other
  IFCCOLUMNTYPE "115x115mm" | element type "115x115mm" | COLUMN | 1 occurrence | property sets: Dimensions, Graphics, Identity Data, Materials and Finishes, Other
  IFCCOLUMNTYPE "115x115mm" | element type "115x115mm" | COLUMN | 1 occurrence | property sets: Dimensions, Graphics, Identity Data, Materials and Finishes, Other
  IFCCOLUMNTYPE "96x130mm" | element type "96x130mm" | COLUMN | 1 occurrence | property sets: Dimensions, Graphics, Identity Data, Materials and Finishes, Other
  IFCCOLUMNTYPE "96x130mm" | element type "96x130mm" | COLUMN | 1 occurrence | property sets: Dimensions, Graphics, Identity Data, Materials and Finishes, Other
  IFCCOLUMNTYPE "96x130mm" | element type "96x130mm" | COLUMN | 1 occurrence | property sets: Dimensions, Graphics, Identity Data, Materials and Finishes, Other
  IFCCOLUMNTYPE "96x130mm" | element type "96x130mm" | COLUMN | 1 occurrence | property sets: Dimensions, Graphics, Identity Data, Materials and Finishes, Other
  IFCCOLUMNTYPE "96x130mm" | element type "96x130mm" | COLUMN | 1 occurrence | property sets: Dimensions, Graphics, Identity Data, Materials and Finishes, Other
  IFCCOLUMNTYPE "96x130mm" | element type "96x130mm" | COLUMN | 1 occurrence | property sets: Dimensions, Graphics, Identity Data, Materials and Finishes, Other
  IFCCOLUMNTYPE "96x130mm" | element type "96x130mm" | COLUMN | 1 occurrence | property sets: Dimensions, Graphics, Identity Data, Materials and Finishes, Other
  IFCCOLUMNTYPE "96x130mm" | element type "96x130mm" | COLUMN | 1 occurrence | property sets: Dimensions, Graphics, Identity Data, Materials and Finishes, Other
  IFCCOLUMNTYPE "96x130mm" | element type "96x130mm" | COLUMN | 1 occurrence | property sets: Dimensions, Graphics, Identity Data, Materials and Finishes, Other
  IFCCOLUMNTYPE "96x130mm" | element type "96x130mm" | COLUMN | 1 occurrence | property sets: Dimensions, Graphics, Identity Data, Materials and Finishes, Other
  IFCCOLUMNTYPE "96x130mm" | element type "96x130mm" | COLUMN | 1 occurrence | property sets: Dimensions, Graphics, Identity Data, Materials and Finishes, Other
  IFCBUILDINGELEMENTPROXYTYPE "Lysrigg" | 3 occurrences | material: "hvit malt" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCBEAMTYPE "NOR-Bjelke-Tre-Stiplet:bjelke bod 2" | BEAM | 1 occurrence | property sets: Identity Data, Materials and Finishes, Other, Structural
  IFCBEAMTYPE "NOR-Bjelke-Tre-Stiplet:50x50" | BEAM | 35 occurrences | property sets: Identity Data, Materials and Finishes, Other, Structural
  IFCWALLTYPE "Basic Wall:YV 16.2 437mm grå platekledning" | STANDARD | 1 occurrence | material: layers "Basic Wall:YV 16.2 437mm grå platekledning" ("Cembrit Metro London" 8., "Luftsjikt" 36., "Vindsperre" 9., "Stender isolert vegg" 246., "Luftsjikt" 15., "stender/isolasjon" 98., "<Unnamed>" 12.5, "Robustgips" 12.5) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCWINDOWSTYLE "GF 14.2 12x21 33dB E30" | 2 occurrences | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Vindu-Fast:GF 14.2 12x21 33dB E30:5676778, Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data
  IFCWALLTYPE "Basic Wall:YV 16.1 437mm gul platekledning" | 1 occurrence | material: layers "Basic Wall:YV 16.1 437mm gul platekledning" ("Cembrit Metro Amsterdam" 8., "Luftsjikt" 36., "Vindsperre" 9., "Stender isolert vegg" 246., "Luftsjikt" 15., "Stender isolert vegg" 98., "<Unnamed>" 12.5, "Robustgips" 12.5) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:YV 17.1 279 Vegg glassfelt" | 2 occurrences | material: layers "Basic Wall:YV 17.1 279 Vegg glassfelt" ("Vindsperre" 15., "Stender isolert vegg" 198., "Stender isolert vegg" 48., "Robustgips" 12.5) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:YV 5.1 233 Gesims Midtbygg" | STANDARD | 2 occurrences | material: layers "Basic Wall:YV 5.1 233 Gesims Midtbygg" ("Beslag" 5., "Vindsperre" 15., "<Unnamed>" 36., "<Unnamed>" 15., "Stender isolert vegg" 198., "Kryssfiner" 15.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "YDA 6.1 Skyvedører" | 1 occurrence | material: materials ("Aluminio Manusa", "Glass") | property sets: Analytical Properties(Type), Construction(Type), Dimensions(Type), General(Type), Graphics(Type), Identity Data(Type)
  IFCWALLTYPE "Basic Wall:YV kle søyle" | STANDARD | 2 occurrences | material: layers "Basic Wall:YV kle søyle" ("Beslag" 5., "Vindsperre" 9., "Stender isolert vegg" 136.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCPIPESEGMENTTYPE "Gutter:Takrenne:5043645" | element type "Gutter:Takrenne:5043645" | GUTTER | 1 occurrence
  IFCDOORSTYLE "IDA 2.2 15x21M EI60SC" | 1 occurrence | material: materials ("Lys grå", "Terskel Tre", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "IDA 6.1 12x21M EI60 CS" | 1 occurrence | material: materials ("Lys grå", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Dør Enkel_ Glassfelt:IDA 6.1 12x21M EI60 CS:5876404, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCDOORSTYLE "2680 x 1275mm" | 1 occurrence | material: "Metal - Paint Finish - Ivory, Matte" | property sets: M_Overhead-Rolling:2680 x 1275mm:5883834, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCDOORSTYLE "IDA 7.1 15x21M EI60CS" | 1 occurrence | material: materials ("Karm Malt", "Lys grå", "Terskel Tre") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "YDA 4.1 14x21M" | 1 occurrence | material: materials ("Lys grå", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Dør Enkel_ Glassfelt:YDA 4.1 14x21M:5953506, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCDOORSTYLE "YDA 4.1 14x21M" | 1 occurrence | material: materials ("Lys grå", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:YV 24.1 mellom glassvegger" | STANDARD | 12 occurrences | material: layers "Basic Wall:YV 24.1 mellom glassvegger" ("Beslag" 5., "Vindsperre" 9., "Stender isolert vegg" 123., "Stender isolert vegg" 48., "Gips" 12.5, "Robustgips" 12.5) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCCURTAINWALLTYPE "Curtain Wall:Glassfasade 3c" | 1 occurrence | property sets: Construction, Horizontal Grid, Identity Data, Other, Vertical Grid
  IFCCURTAINWALLTYPE "Curtain Wall:Glassfasade 3b" | 1 occurrence | property sets: Construction, Horizontal Grid, Identity Data, Other, Vertical Grid
  IFCCURTAINWALLTYPE "Curtain Wall:Glassfasade 4a" | 1 occurrence | property sets: Construction, Horizontal Grid, Identity Data, Other, Vertical Grid
  IFCCURTAINWALLTYPE "Curtain Wall:Glassfasade 4b" | 1 occurrence | property sets: Construction, Horizontal Grid, Identity Data, Other, Vertical Grid
  IFCCURTAINWALLTYPE "Curtain Wall:Glassfasade 5a" | 1 occurrence | property sets: Construction, Horizontal Grid, Identity Data, Other, Vertical Grid
  IFCCURTAINWALLTYPE "Curtain Wall:Glassfasade 5b" | 1 occurrence | property sets: Construction, Horizontal Grid, Identity Data, Other, Vertical Grid
  IFCCURTAINWALLTYPE "Curtain Wall:Glassfasade 5c" | 1 occurrence | property sets: Construction, Horizontal Grid, Identity Data, Other, Vertical Grid
  IFCCURTAINWALLTYPE "Curtain Wall:Glassfasade 5d" | 1 occurrence | property sets: Construction, Horizontal Grid, Identity Data, Other, Vertical Grid
  IFCCURTAINWALLTYPE "Curtain Wall:Glassfasade 2b" | 1 occurrence | property sets: Construction, Horizontal Grid, Identity Data, Other, Vertical Grid
  IFCCURTAINWALLTYPE "Curtain Wall:Glassfasade 1b" | 1 occurrence | property sets: Construction, Horizontal Grid, Identity Data, Other, Vertical Grid
  IFCCURTAINWALLTYPE "Curtain Wall:Glassfasade 1a" | 1 occurrence | property sets: Construction, Horizontal Grid, Identity Data, Other, Vertical Grid
  IFCCURTAINWALLTYPE "Curtain Wall:Glassfasade 3d" | 1 occurrence | property sets: Construction, Horizontal Grid, Identity Data, Other, Vertical Grid
  IFCWALLTYPE "Basic Wall:YVL 2.1 150mm lecablokk" | STANDARD | 4 occurrences | material: layers "Basic Wall:YVL 2.1 150mm lecablokk" ("Mur" 150.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCWALLTYPE "Basic Wall:IVL 4.1 173mm leca + litex" | STANDARD | 3 occurrences | material: layers "Basic Wall:IVL 4.1 173mm leca + litex" ("Flis" 5., "Litex" 12., "Mur" 118.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCPIPESEGMENTTYPE "Gutter:Takrenne 2:5819303" | element type "Gutter:Takrenne 2:5819303" | GUTTER | 1 occurrence
  IFCCOLUMNTYPE "115x115mm" | element type "115x115mm" | COLUMN | 1 occurrence | property sets: Dimensions, Graphics, Identity Data, Materials and Finishes, Other
  IFCCOLUMNTYPE "115x115mm" | element type "115x115mm" | COLUMN | 1 occurrence | property sets: Dimensions, Graphics, Identity Data, Materials and Finishes, Other
  IFCCOLUMNTYPE "115x115mm" | element type "115x115mm" | COLUMN | 1 occurrence | property sets: Dimensions, Graphics, Identity Data, Materials and Finishes, Other
  IFCCOLUMNTYPE "115x115mm" | element type "115x115mm" | COLUMN | 1 occurrence | property sets: Dimensions, Graphics, Identity Data, Materials and Finishes, Other
  IFCCOLUMNTYPE "115x115mm" | element type "115x115mm" | COLUMN | 1 occurrence | property sets: Dimensions, Graphics, Identity Data, Materials and Finishes, Other
  IFCCOLUMNTYPE "115x115mm" | element type "115x115mm" | COLUMN | 1 occurrence | property sets: Dimensions, Graphics, Identity Data, Materials and Finishes, Other
  IFCCOLUMNTYPE "115x115mm" | element type "115x115mm" | COLUMN | 1 occurrence | property sets: Dimensions, Graphics, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:YVL 4.1 118mm lecablokk + puss" | STANDARD | 1 occurrence | material: layers "Basic Wall:YVL 4.1 118mm lecablokk + puss" ("<Unnamed>" 8., "Mur" 118., "<Unnamed>" 8.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCWALLTYPE "Basic Wall:YVB 1.1 220 Betong" | STANDARD | 3 occurrences | material: layers "Basic Wall:YVB 1.1 220 Betong" ("Betong walls" 220.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCBEAMTYPE "NOR-Bjelke-Tre-Stiplet:bjelke bod" | BEAM | 2 occurrences | property sets: Identity Data, Materials and Finishes, Other, Structural
  IFCWALLTYPE "Basic Wall:Skranke" | STANDARD | 5 occurrences | material: layers "Basic Wall:Skranke" ("Baderomsinnredning Benkeplate" 100.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:Brannmursplate" | STANDARD | 2 occurrences | material: layers "Basic Wall:Brannmursplate" ("Branngips" 50.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCBUILDINGELEMENTPROXYTYPE "Lerret" | 1 occurrence | material: "hvit malt" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:YV 17.1 279 Vegg glassfelt 2" | STANDARD | 1 occurrence | material: layers "Basic Wall:YV 17.1 279 Vegg glassfelt 2" ("<Unnamed>" 5., "<Unnamed>" 15., "<Unnamed>" 36., "Vindsperre" 15., "Stender isolert vegg" 198., "Stender isolert vegg" 48., "Robustgips" 12.5) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCBUILDINGELEMENTPROXYTYPE "Innvendig screen" | 2 occurrences | material: "hvit malt" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "2680 x 1275mm" | 1 occurrence | material: "Metal - Paint Finish - Ivory, Matte" | property sets: Rullegitter:2680 x 1275mm:7267956, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCBUILDINGELEMENTPROXYTYPE "Innvendig screen" | 1 occurrence | material: "hvit malt" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCBUILDINGELEMENTPROXYTYPE "Innvendig screen" | 1 occurrence | material: "hvit malt" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "Luke 10M" | 1 occurrence | material: materials ("Light grey", "Karm Malt") | property sets: Luke600:Luke 10M:7318563, Analytical Properties, Construction, Dimensions, Identity Data, Other
  IFCWALLTYPE "Basic Wall:IVA 13.1 126mm 48dB EI60 (HN-95+20+100-R)" | STANDARD | 1 occurrence | material: layers "Basic Wall:IVA 13.1 126mm 48dB EI60 (HN-95+20+100-R)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 95., "Luftsjikt" 20., "Massivtre" 100., "Branngips" 15.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCPIPESEGMENTTYPE "Gutter:Takrenne 3:6462446" | element type "Gutter:Takrenne 3:6462446" | GUTTER | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 3" | 1 occurrence | material: "Lys grå" | property sets: Identity Data, Other
  IFCWALLTYPE "Basic Wall:Bassabsorbent 2" | STANDARD | 2 occurrences | material: layers "Basic Wall:Bassabsorbent 2" ("Metal - Steel" 10.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:Veggabsorbent" | STANDARD | 3 occurrences | material: layers "Basic Wall:Veggabsorbent" ("stender/isolasjon" 40.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:Litex" | STANDARD | 3 occurrences | material: layers "Basic Wall:Litex" ("Litex" 12., "Flis" 5.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCWALLTYPE "Basic Wall:Baderomspanel" | STANDARD | 15 occurrences | material: layers "Basic Wall:Baderomspanel" ("Baderomspanel" 10.2) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCBUILDINGELEMENTPROXYTYPE "Høytaler" | 2 occurrences | material: "hvit malt" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "IDT 10.1 7x21M" | 1 occurrence | material: materials ("_White", "Light grey", "Karm Malt", "Trekledning") | property sets: Dør Enkel:IDT 10.1 7x21M:7828245, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCBUILDINGELEMENTPROXYTYPE "Tavle 2m" | 21 occurrences | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCBUILDINGELEMENTPROXYTYPE "Smartboard 2m" | 17 occurrences | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Skap, resirkulering 450 x 450 x 692mm" | element type "Skap, resirkulering 450 x 450 x 692mm" | 3 occurrences | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Skap, resirkulering 450 x 450 x 692mm" | element type "Skap, resirkulering 450 x 450 x 692mm" | 1 occurrence | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Demobenk, naturfag" | element type "Demobenk, naturfag" | 1 occurrence | material: "hvit malt" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Skap, demobenk naturfag 1200 x 600 x 860mm" | element type "Skap, demobenk naturfag 1200 x 600 x 860mm" | 1 occurrence | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCBUILDINGELEMENTPROXYTYPE "Naturfagsbord" | 2 occurrences | property sets: Identity Data, Other
  IFCBUILDINGELEMENTPROXYTYPE "Naturfagsbord" | 2 occurrences | property sets: Identity Data, Other
  IFCBUILDINGELEMENTPROXYTYPE "Gasskap" | 1 occurrence | material: "hvit malt" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCBUILDINGELEMENTPROXYTYPE "Tavle 2m" | 35 occurrences | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCBUILDINGELEMENTPROXYTYPE "Smartboard 2m" | 13 occurrences | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Underskap gasskap" | element type "Underskap gasskap" | 1 occurrence | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCBUILDINGELEMENTPROXYTYPE "Siemens induksjon" | 3 occurrences | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Benkeplate 625mm, Sigdal" | element type "Benkeplate 625mm, Sigdal" | 1 occurrence | material: "hvit malt" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Benkeplate 625mm" | element type "Benkeplate 625mm" | 4 occurrences | material: "hvit malt" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCBUILDINGELEMENTPROXYTYPE "Siemens induksjon" | 7 occurrences | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Skap, kjøkken 800 x 600 x 860mm" | element type "Skap, kjøkken 800 x 600 x 860mm" | 5 occurrences | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Skap, kjøkken 600 x 600 x 860mm" | element type "Skap, kjøkken 600 x 600 x 860mm" | 6 occurrences | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Skap, kjøkken 600 x 600 x 860mm" | element type "Skap, kjøkken 600 x 600 x 860mm" | 8 occurrences | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Skap, kjøkken 400 x 600 x 860mm" | element type "Skap, kjøkken 400 x 600 x 860mm" | 4 occurrences | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Skap, kjøkken, hjørne 900 x 600 x 860mm" | element type "Skap, kjøkken, hjørne 900 x 600 x 860mm" | 4 occurrences | material: "N_Cabinets" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Overskap 800 x 300 x 720mm" | element type "Overskap 800 x 300 x 720mm" | 5 occurrences | material: "N_Cabinets" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Overskap 300 x 300 x 700mm" | element type "Overskap 300 x 300 x 700mm" | 5 occurrences | material: "N_Cabinets" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Overskap 600 x 300 x 700mm" | element type "Overskap 600 x 300 x 700mm" | 12 occurrences | material: "N_Cabinets" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Benkeplate 625mm" | element type "Benkeplate 625mm" | 3 occurrences | material: "hvit malt" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Skap, kjøkken 800 x 600 x 860mm" | element type "Skap, kjøkken 800 x 600 x 860mm" | 6 occurrences | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Skap, kjøkken 600 x 600 x 860mm" | element type "Skap, kjøkken 600 x 600 x 860mm" | 6 occurrences | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Skap, kjøkken 600 x 600 x 860mm" | element type "Skap, kjøkken 600 x 600 x 860mm" | 9 occurrences | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Skap, kjøkken 400 x 600 x 860mm" | element type "Skap, kjøkken 400 x 600 x 860mm" | 3 occurrences | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Skap, kjøkken, hjørne 900 x 600 x 860mm" | element type "Skap, kjøkken, hjørne 900 x 600 x 860mm" | 4 occurrences | material: "N_Cabinets" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Overskap 800 x 300 x 720mm" | element type "Overskap 800 x 300 x 720mm" | 3 occurrences | material: "N_Cabinets" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Overskap 300 x 300 x 700mm" | element type "Overskap 300 x 300 x 700mm" | 4 occurrences | material: "N_Cabinets" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Overskap 600 x 300 x 700mm" | element type "Overskap 600 x 300 x 700mm" | 8 occurrences | material: "N_Cabinets" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCBUILDINGELEMENTPROXYTYPE "Asko oppvaskmaskin" | 2 occurrences | material: materials ("N_Cabinets", "EQ-Cozinha-Maquinas", "EQ-Cozinha-Maquinas-Porta", "Default Light Source", "N_Cabinets - Handles") | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Skap, resirkulering, sigdal" | element type "Skap, resirkulering, sigdal" | 2 occurrences | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Skap, resirkulering, sigdal" | element type "Skap, resirkulering, sigdal" | 2 occurrences | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Skap, kjøkken 600 x 500 x 860mm" | element type "Skap, kjøkken 600 x 500 x 860mm" | 1 occurrence | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCBUILDINGELEMENTPROXYTYPE "Høyskap med ovn 600 x 600 x 2105mm" | 1 occurrence | material: "Glass" | property sets: Dimensions, Identity Data, Other
  IFCBUILDINGELEMENTPROXYTYPE "Siemens frittstående kjøleskap" | 1 occurrence | material: materials ("Metal - Chrome", "Metal - Paint Finish - Ivory,Matte") | property sets: Identity Data, Other
  IFCBUILDINGELEMENTPROXYTYPE "Siemens Frittstående fryseskap" | 2 occurrences | material: materials ("Metal - Chrome", "Metal - Paint Finish - Ivory,Matte") | property sets: Identity Data, Other
  IFCBUILDINGELEMENTPROXYTYPE "Siemens innebygget ovn" | 7 occurrences | material: materials ("Glass", "EQ-Cozinha-Maquinas", "EQ-Cozinha-Maquinas-Porta") | property sets: Identity Data, Materials and Finishes, Other
  IFCBUILDINGELEMENTPROXYTYPE "Siemens innebygget ovn" | 3 occurrences | material: materials ("Glass", "EQ-Cozinha-Maquinas", "EQ-Cozinha-Maquinas-Porta") | property sets: Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Benkeplate 625mm, Sigdal" | element type "Benkeplate 625mm, Sigdal" | 1 occurrence | material: "hvit malt" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Høyskap, kjøkken 600 x 600 x 2100mm" | element type "Høyskap, kjøkken 600 x 600 x 2100mm" | 1 occurrence | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Skap, kjøkken 300 x 600 x 860mm" | element type "Skap, kjøkken 300 x 600 x 860mm" | 1 occurrence | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Benkeplate 625mm, Sigdal" | element type "Benkeplate 625mm, Sigdal" | 1 occurrence | material: "hvit malt" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCVALVETYPE "Blandebatteri berøringsfri 1724FT" | FAUCET | 20 occurrences | material: "Brass" | property sets: Dimensions, Electrical, Electrical Engineering, General, Green Building Properties, Identity Data
  IFCVALVETYPE "Blandebatteri - Oras Saphira 1039F" | FAUCET | 1 occurrence | material: "Brass" | property sets: Dimensions, General, Green Building Properties, Identity Data, Materials and Finishes, Mechanical
  IFCFURNITURETYPE "Benkeplate" | element type "Benkeplate" | 1 occurrence | material: "hvit malt" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Benkeplate 625mm, krogsæter" | element type "Benkeplate 625mm, krogsæter" | 1 occurrence | material: "hvit malt" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Hylle 300mm" | element type "Hylle 300mm" | 6 occurrences | material: "hvit malt" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Hylle 300mm" | element type "Hylle 300mm" | 6 occurrences | material: "hvit malt" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Skap, krogsæter 1000 x 600 x 860mm" | element type "Skap, krogsæter 1000 x 600 x 860mm" | 2 occurrences | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Skap, krogsæter 1000 x 600 x 860mm" | element type "Skap, krogsæter 1000 x 600 x 860mm" | 1 occurrence | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Benkeplate 625mm, krogsæter" | element type "Benkeplate 625mm, krogsæter" | 1 occurrence | material: "hvit malt" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCBUILDINGELEMENTPROXYTYPE "Miele oppvaskmaskin" | 1 occurrence | material: materials ("N_Cabinets", "EQ-Cozinha-Maquinas", "EQ-Cozinha-Maquinas-Porta", "Default Light Source", "N_Cabinets - Handles") | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Overskap, krogsæter 600 x 300 x 720mm" | element type "Overskap, krogsæter 600 x 300 x 720mm" | 1 occurrence | material: "N_Cabinets" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCBUILDINGELEMENTPROXYTYPE "Kjemikalieskap" | 1 occurrence | material: "hvit malt" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Overskap, krogsæter 600 x 300 x 720mm" | element type "Overskap, krogsæter 600 x 300 x 720mm" | 1 occurrence | material: "N_Cabinets" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Skuff, krogsæter 600 x 600 x 860mm" | element type "Skuff, krogsæter 600 x 600 x 860mm" | 1 occurrence | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Høyskap 500 x 600 x 2100mm" | element type "Høyskap 500 x 600 x 2100mm" | 1 occurrence | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Høyskap 500 x 600 x 2100mm" | element type "Høyskap 500 x 600 x 2100mm" | 1 occurrence | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCVALVETYPE "Blandebatteri - Oras Saphira 1039F" | FAUCET | 6 occurrences | material: "Brass" | property sets: Dimensions, General, Green Building Properties, Identity Data, Materials and Finishes, Mechanical
  IFCFURNITURETYPE "Benkeplate 625mm, Sigdal" | element type "Benkeplate 625mm, Sigdal" | 1 occurrence | material: "hvit malt" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Benkeplate" | element type "Benkeplate" | 1 occurrence | material: "hvit malt" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCBUILDINGELEMENTPROXYTYPE "Asko oppvaskmaskin" | 1 occurrence | material: materials ("N_Cabinets", "EQ-Cozinha-Maquinas", "EQ-Cozinha-Maquinas-Porta", "Default Light Source", "N_Cabinets - Handles") | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Skap, kjøkken 600 x 500 x 860mm" | element type "Skap, kjøkken 600 x 500 x 860mm" | 2 occurrences | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCBUILDINGELEMENTPROXYTYPE "Høyskap med ovn 600 x 600 x 2105mm" | 1 occurrence | material: "Glass" | property sets: Dimensions, Identity Data, Other
  IFCBUILDINGELEMENTPROXYTYPE "Siemens Vaskemaskin, Sigdal" | 2 occurrences | material: materials ("Glass", "EQ-Cozinha-Maquinas-Porta", "N_Cabinets", "EQ-Cozinha-Maquinas", "Default Light Source", "N_Cabinets - Handles") | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCBUILDINGELEMENTPROXYTYPE "Siemens Varmep.trommel Sigdal" | 2 occurrences | material: materials ("Glass", "EQ-Cozinha-Maquinas-Porta", "N_Cabinets", "EQ-Cozinha-Maquinas", "Default Light Source", "N_Cabinets - Handles") | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCBUILDINGELEMENTPROXYTYPE "Siemens frittstående kjøleskap" | 2 occurrences | material: materials ("Metal - Chrome", "Metal - Paint Finish - Ivory,Matte") | property sets: Identity Data, Other
  IFCBUILDINGELEMENTPROXYTYPE "Siemens Frittstående fryseskap" | 1 occurrence | material: materials ("Metal - Chrome", "Metal - Paint Finish - Ivory,Matte") | property sets: Identity Data, Other
  IFCFURNITURETYPE "Høyskap, kjøkken 600 x 600 x 2100mm" | element type "Høyskap, kjøkken 600 x 600 x 2100mm" | 1 occurrence | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Skap, kjøkken 900 x 600 x 860mm" | element type "Skap, kjøkken 900 x 600 x 860mm" | 1 occurrence | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Skap, resirkulering 300 x 450 x 690mm" | element type "Skap, resirkulering 300 x 450 x 690mm" | 12 occurrences | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Skap, resirkulering 450 x 450 x 860mm" | element type "Skap, resirkulering 450 x 450 x 860mm" | 4 occurrences | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Demobenk, naturfag" | element type "Demobenk, naturfag" | 1 occurrence | material: "hvit malt" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Skap, demobenk naturfag 1200 x 600 x 860mm" | element type "Skap, demobenk naturfag 1200 x 600 x 860mm" | 1 occurrence | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCBUILDINGELEMENTPROXYTYPE "Naturfagsbord" | 2 occurrences | property sets: Identity Data, Other
  IFCBUILDINGELEMENTPROXYTYPE "Naturfagsbord" | 2 occurrences | property sets: Identity Data, Other
  IFCBUILDINGELEMENTPROXYTYPE "dreieskive560x720x540" | 1 occurrence | material: "hvit malt" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCBUILDINGELEMENTPROXYTYPE "Gipsutskiller" | 1 occurrence | material: "hvit malt" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCVALVETYPE "Blandebatteri berøringsfri 1724FT" | FAUCET | 2 occurrences | material: "Brass" | property sets: Dimensions, Electrical, Electrical Engineering, General, Green Building Properties, Identity Data
  IFCBUILDINGELEMENTPROXYTYPE "Whiteboard 2,5m" | 2 occurrences | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCBUILDINGELEMENTPROXYTYPE "Sybord" | 5 occurrences | material: materials ("Farge sort", "Paint Hvit(1)") | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Skap, resirkulering 300 x 450 x 860mm" | element type "Skap, resirkulering 300 x 450 x 860mm" | 4 occurrences | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Benkeplate 625mm, Sigdal" | element type "Benkeplate 625mm, Sigdal" | 1 occurrence | material: "hvit malt" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Skap, kjøkken 500 x 600 x 860mm" | element type "Skap, kjøkken 500 x 600 x 860mm" | 1 occurrence | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Overskap 1000 x 300 x 720mm" | element type "Overskap 1000 x 300 x 720mm" | 1 occurrence | material: "N_Cabinets" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCBUILDINGELEMENTPROXYTYPE "Siemens Kjøleskap under benk" | 1 occurrence | material: materials ("Metal - Chrome", "Metal - Paint Finish - Ivory,Matte") | property sets: Identity Data, Other
  IFCBUILDINGELEMENTPROXYTYPE "Armstøtte veggmontert" | 24 occurrences | property sets: Constraints, Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Vegghengt benk" | element type "Vegghengt benk" | 7 occurrences | material: "hvit malt" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Vegghengt benk" | element type "Vegghengt benk" | 2 occurrences | material: "hvit malt" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCBUILDINGELEMENTPROXYTYPE "gard skap 5rom 30cm" | 2 occurrences | material: materials ("Gul avdeling", "Steel - Hadrian - Black") | property sets: Analytical Model, Constraints, Dimensions, Green Building Properties, Identity Data, Layers
  IFCBUILDINGELEMENTPROXYTYPE "gard skap 5rom 30cm" | 1 occurrence | material: materials ("Gul avdeling", "Steel - Hadrian - Black") | property sets: Analytical Model, Constraints, Dimensions, Green Building Properties, Identity Data, Layers
  IFCVALVETYPE "Blandebatteri dusj 7267" | 3 occurrences | material: "Brass" | property sets: Dimensions, General, Green Building Properties, Identity Data, Materials and Finishes, Mechanical
  IFCBUILDINGELEMENTPROXYTYPE "Armstøtte veggmontert" | 2 occurrences | property sets: Constraints, Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Hylle 350mm" | element type "Hylle 350mm" | 1 occurrence | material: "hvit malt" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Skap, resirkulering 300 x 460 x 825mm" | element type "Skap, resirkulering 300 x 460 x 825mm" | 1 occurrence | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCBUILDINGELEMENTPROXYTYPE "Siemens mikro, 20L" | 3 occurrences | material: materials ("Glass - black", "Metal - Aluminium", "Metal - Firring") | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Skap, resirkulering 400 x 460 x 825mm" | element type "Skap, resirkulering 400 x 460 x 825mm" | 6 occurrences | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Skap, resirkulering 300 x 460 x 825mm" | element type "Skap, resirkulering 300 x 460 x 825mm" | 5 occurrences | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Benkeplate kildesortering" | element type "Benkeplate kildesortering" | 3 occurrences | material: "hvit malt" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Benkeplate 625mm, Sigdal" | element type "Benkeplate 625mm, Sigdal" | 1 occurrence | material: "hvit malt" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCBUILDINGELEMENTPROXYTYPE "Siemens Kombiskap, hvit,186 cm" | 1 occurrence | material: "N_Cabinets" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCBUILDINGELEMENTPROXYTYPE "OPPV.MASK, FRITTSTÅENDE, 60 CM" | 2 occurrences | material: materials ("N_Cabinets", "EQ-Cozinha-Maquinas", "EQ-Cozinha-Maquinas-Porta", "Default Light Source", "N_Cabinets - Handles") | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Overskap 800 x 300 x 600mm" | element type "Overskap 800 x 300 x 600mm" | 1 occurrence | material: "N_Cabinets" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Overskap 600 x 300 x 600mm" | element type "Overskap 600 x 300 x 600mm" | 4 occurrences | material: "N_Cabinets" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCBUILDINGELEMENTPROXYTYPE "Siemens mikro, 60skap" | 3 occurrences | material: materials ("Glass - black", "Metal - Aluminium", "Metal - Firring") | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Overskap 600 x 300 x 600mm" | element type "Overskap 600 x 300 x 600mm" | 1 occurrence | material: "N_Cabinets" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCBUILDINGELEMENTPROXYTYPE "Båsgarderobe 400 x 350 x 2000mm" | 10 occurrences | material: "N_Cabinets" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCBUILDINGELEMENTPROXYTYPE "Båsgarderobe 400 x 350 x 2000mm" | 10 occurrences | material: "N_Cabinets" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCBUILDINGELEMENTPROXYTYPE "gard skap 5rom 30cm" | 2 occurrences | material: materials ("Gul avdeling", "hvit malt") | property sets: Analytical Model, Constraints, Dimensions, Green Building Properties, Identity Data, Layers
  IFCFURNITURETYPE "Hattehylle360mm" | element type "Hattehylle360mm" | 1 occurrence | material: "Wood - Birch, Natural" | property sets: Identity Data, Other
  IFCFURNITURETYPE "Skohylle" | element type "Skohylle" | 1 occurrence | material: "hvit malt" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCBUILDINGELEMENTPROXYTYPE "Rullestol-ikon" | 2 occurrences | material: "Paint - White" | property sets: Identity Data, Other
  IFCBUILDINGELEMENTPROXYTYPE "gard skap 5rom 30cm" | 2 occurrences | material: materials ("Gul avdeling", "hvit malt") | property sets: Analytical Model, Constraints, Dimensions, Green Building Properties, Identity Data, Layers
  IFCFURNITURETYPE "Vegghengt benk" | element type "Vegghengt benk" | 1 occurrence | material: "hvit malt" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCVALVETYPE "Blandebatteri dusj 7264" | FAUCET | 4 occurrences | material: "Brass" | property sets: Dimensions, General, Green Building Properties, Identity Data, Materials and Finishes, Mechanical
  IFCBUILDINGELEMENTPROXYTYPE "gard skap 5rom 30cm" | 2 occurrences | material: materials ("Gul avdeling", "hvit malt") | property sets: Analytical Model, Constraints, Dimensions, Green Building Properties, Identity Data, Layers
  IFCFURNITURETYPE "Vegghengt benk" | element type "Vegghengt benk" | 1 occurrence | material: "hvit malt" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCBUILDINGELEMENTPROXYTYPE "Båndsag" | 1 occurrence | material: "hvit malt" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCBUILDINGELEMENTPROXYTYPE "Avretter" | 1 occurrence | material: "hvit malt" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCBUILDINGELEMENTPROXYTYPE "Sponavsug" | 1 occurrence | material: "hvit malt" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCBUILDINGELEMENTPROXYTYPE "Keramikkovn" | 1 occurrence | material: "hvit malt" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Eskoleia småvarereol 1000 x 400mm" | element type "Eskoleia småvarereol 1000 x 400mm" | 10 occurrences | property sets: Dimensions, Identity Data, Other
  IFCFURNITURETYPE "Eskoleia småvarereol 1000 x 400mm" | element type "Eskoleia småvarereol 1000 x 400mm" | 5 occurrences | property sets: Dimensions, Identity Data, Other
  IFCBUILDINGELEMENTPROXYTYPE "AV rack" | 1 occurrence | material: materials ("Cabinets", "Cabinets - Handles", "Cabinets - Panel") | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Benkeplate 625mm, Sigdal" | element type "Benkeplate 625mm, Sigdal" | 1 occurrence | material: "hvit malt" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Benkeplate 625mm, Sigdal" | element type "Benkeplate 625mm, Sigdal" | 1 occurrence | material: "hvit malt" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Benkeplate 625mm, Sigdal" | element type "Benkeplate 625mm, Sigdal" | 1 occurrence | material: "hvit malt" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Overskap, hjørne 600 x 300 x 720mm" | element type "Overskap, hjørne 600 x 300 x 720mm" | 1 occurrence | material: "N_Cabinets" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Overskap 400 x 300 x 700mm" | element type "Overskap 400 x 300 x 700mm" | 2 occurrences | material: "N_Cabinets" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Skap, kjøken 400 x 600 x 860mm" | element type "Skap, kjøken 400 x 600 x 860mm" | 3 occurrences | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Overskap 400 x 300 x 700mm" | element type "Overskap 400 x 300 x 700mm" | 1 occurrence | material: "N_Cabinets" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Benkeplate, sigdal" | element type "Benkeplate, sigdal" | 1 occurrence | material: "hvit malt" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Skap, kjøkken 600 x 350 x 860mm" | element type "Skap, kjøkken 600 x 350 x 860mm" | 1 occurrence | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Skap, kjøkken 600 x 350 x 860mm" | element type "Skap, kjøkken 600 x 350 x 860mm" | 1 occurrence | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCBUILDINGELEMENTPROXYTYPE "Kjøleskap_plass for" | 1 occurrence | material: "N_Cabinets" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Overskap 500 x 300 x 700mm" | element type "Overskap 500 x 300 x 700mm" | 1 occurrence | material: "N_Cabinets" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCBUILDINGELEMENTPROXYTYPE "Kjøleskap_plass for" | 1 occurrence | material: "N_Cabinets" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Eskoleia småvarereol 800 x 400mm" | element type "Eskoleia småvarereol 800 x 400mm" | 8 occurrences | property sets: Dimensions, Identity Data, Other
  IFCFURNITURETYPE "Eskoleia småvarereol 800 x 400mm" | element type "Eskoleia småvarereol 800 x 400mm" | 8 occurrences | property sets: Dimensions, Identity Data, Other
  IFCVALVETYPE "Blandebatteri berøringsfri 1724FT" | FAUCET | 43 occurrences | material: "Brass" | property sets: Dimensions, Electrical, Electrical Engineering, General, Green Building Properties, Identity Data
  IFCFURNITURETYPE "Vegghengt benk" | element type "Vegghengt benk" | 7 occurrences | material: "hvit malt" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Vegghengt benk" | element type "Vegghengt benk" | 3 occurrences | material: "hvit malt" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCBUILDINGELEMENTPROXYTYPE "gard skap 5rom 30cm" | 2 occurrences | material: materials ("Gul avdeling", "Steel - Hadrian - Black") | property sets: Analytical Model, Constraints, Dimensions, Green Building Properties, Identity Data, Layers
  IFCBUILDINGELEMENTPROXYTYPE "gard skap 5rom 30cm" | 1 occurrence | material: materials ("Gul avdeling", "Steel - Hadrian - Black") | property sets: Analytical Model, Constraints, Dimensions, Green Building Properties, Identity Data, Layers
  IFCFURNITURETYPE "Stålhylle, krogsæter 900 x 400mm" | element type "Stålhylle, krogsæter 900 x 400mm" | 15 occurrences | property sets: Dimensions, Identity Data, Other
  IFCFURNITURETYPE "høyskap 800" | element type "høyskap 800" | 2 occurrences | material: "Elevreol 2" | property sets: Dimensions, Graphics, Identity Data, Materials and Finishes, Other
  IFCBUILDINGELEMENTPROXYTYPE "Kjemikalieskap maling" | 1 occurrence | material: "hvit malt" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Benkeplate 265mm, krogsæter" | element type "Benkeplate 265mm, krogsæter" | 1 occurrence | material: "hvit malt" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Benkeplate 265mm, krogsæter" | element type "Benkeplate 265mm, krogsæter" | 2 occurrences | material: "hvit malt" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Benkeplate 265mm, krogsæter" | element type "Benkeplate 265mm, krogsæter" | 1 occurrence | material: "hvit malt" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCBUILDINGELEMENTPROXYTYPE "Inkubator" | 1 occurrence | material: "hvit malt" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:IVA 1.1T 121mm 44dB (H-95-H)" | STANDARD | 10 occurrences | material: layers "Basic Wall:IVA 1.1T 121mm 44dB (H-95-H)" ("Habito" 13., "stender/isolasjon" 95., "Habito" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCWALLTYPE "Basic Wall:IVA 3.3T 145mm 48dB (RN-95-NR)" | STANDARD | 3 occurrences | material: layers "Basic Wall:IVA 3.3T 145mm 48dB (RN-95-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCDOORSTYLE "IDT 1.2 8x21M 33dB" | 4 occurrences | material: materials ("Terskel Tre", "NCS S 0500-N", "Karm Malt") | property sets: Dør Enkel:IDT 1.2 8x21M 33dB:1725481, Analytical Properties, Construction, Dimensions, Identity Data, Other
  IFCDOORSTYLE "IDA 2.2 15x21M EI60SC" | 1 occurrence | material: materials ("Lys grå", "Terskel Tre", "Karm Malt") | property sets: Dør Dobbel_Ulike_Dørblader:IDA 2.2 15x21M EI60SC:1728746, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCWINDOWSTYLE "V23 14x14" | 3 occurrences | material: materials ("Glass Klart", "NCS S 0502-Y", "Karm Malt") | property sets: Vindu-Hengslet:V23 14x14:1761672, Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data
  IFCWALLTYPE "Basic Wall:IVA 2.1 134mm 44dB (H-95-NH)" | STANDARD | 4 occurrences | material: layers "Basic Wall:IVA 2.1 134mm 44dB (H-95-NH)" ("Habito" 13., "stender/isolasjon" 95., "Gips" 13., "Habito" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCDOORSTYLE "IDT 2.3 10x21M 33dB" | 1 occurrence | material: materials ("Terskel Tre", "Lys grå", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Other, Text
  IFCWALLTYPE "Basic Wall:IVA 11.1 193mm 48dB (RN-95-NR)" | STANDARD | 2 occurrences | material: layers "Basic Wall:IVA 11.1 193mm 48dB (RN-95-NR)" ("Robustgips" 13., "<Unnamed>" 13., "<Unnamed>" 10., "stender/isolasjon" 98., "<Unnamed>" 20., "<Unnamed>" 48., "Gips" 13., "Robustgips" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCDOORSTYLE "IDF 2.1 Foldevegg 8000x2800" | 2 occurrences | material: materials ("Light grey", "Karm Malt") | property sets: Side_Stack_Operable_Wall_8000:IDF 2.1 Foldevegg 8000x2800:1780830, Analytical Properties, Constraints, Construction, Dimensions, Identity Data
  IFCWALLTYPE "Basic Wall:IVA 3.3 145mm 48dB EI30 (RN-95-NR) 2" | STANDARD | 1 occurrence | material: layers "Basic Wall:IVA 3.3 145mm 48dB EI30 (RN-95-NR) 2" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCWALLTYPE "Basic Wall:YV 9.1 500mm uisolert" | STANDARD | 1 occurrence | material: layers "Basic Wall:YV 9.1 500mm uisolert" ("Trekledning" 19., "Luftsjikt" 48., "Luftsjikt" 36., "Luftsjikt" 48., "Vindsperre" 9., "stender" 296., "Luftsjikt" 36., "Cembrit Metro Amsterdam" 8.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:IVA 4.3 172mm 48dB EI60 (RN-120-NR)" | STANDARD | 1 occurrence | material: layers "Basic Wall:IVA 4.3 172mm 48dB EI60 (RN-120-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 120., "Gips" 13., "Robustgips" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCWALLTYPE "Basic Wall:YV 8.3 458mm gul platekledning EI60" | STANDARD | 1 occurrence | material: layers "Basic Wall:YV 8.3 458mm gul platekledning EI60" ("Cembrit Metro Amsterdam" 8., "Luftsjikt" 36., "Luftsjikt" 48., "Vindsperre" 9., "Stender isolert vegg" 296., "NO_Utlekting" 48., "Gips" 12.5, "Gips" 12.5) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:YV 7.5 410mm gul platekledning EI60" | STANDARD | 1 occurrence | material: layers "Basic Wall:YV 7.5 410mm gul platekledning EI60" ("Cembrit Metro Amsterdam" 8., "Luftsjikt" 36., "Vindsperre" 9., "Stender isolert vegg" 296., "NO_Utlekting" 48., "Branngips" 15.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "YDA 5.2 16x21M EI 30S" | 1 occurrence | material: materials ("Glass Klart", "Lys grå", "Terskel Tre", "Karm Malt") | property sets: _Dør Dobbel_Ulike_Dørblader_Glassfelt:YDA 5.2 16x21M EI 30S:1835036, Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data
  IFCWALLTYPE "Basic Wall:IVA 4.1 172mm 34dB (HN-120-NH)" | STANDARD | 1 occurrence | material: layers "Basic Wall:IVA 4.1 172mm 34dB (HN-120-NH)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 120., "Gips" 13., "Habito" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCWALLTYPE "Basic Wall:IVA 6.1 302mm 34dB (HN-95-60-95-NH)" | STANDARD | 2 occurrences | material: layers "Basic Wall:IVA 6.1 302mm 34dB (HN-95-60-95-NH)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 95., "Luftsjikt" 60., "stender/isolasjon" 95., "Gips" 13., "Habito" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCDOORSTYLE "IDT 6.1 15x21M 33dB" | 1 occurrence | material: materials ("Glass Klart", "Lys grå", "Terskel Tre", "Karm Malt") | property sets: Analysis Results(Type), Analytical Properties(Type), Construction(Type), Dimensions(Type), Identity Data(Type), Materials and Finishes(Type)
  IFCWALLTYPE "Basic Wall:IVA 1.1T 121mm 34dB (H-95-H)" | STANDARD | 5 occurrences | material: layers "Basic Wall:IVA 1.1T 121mm 34dB (H-95-H)" ("Habito" 13., "stender/isolasjon" 95., "Habito" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "IDT 3.3 10x21M 33dB" | 1 occurrence | material: materials ("Lys grå", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "IDA 6.2 12x21M EI 30CS" | 1 occurrence | material: materials ("Lys grå", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "IDA 3.1 18x21M 33db EI30S" | 3 occurrences | material: materials ("Glass Klart", "Lys grå", "Terskel Tre", "Karm Malt") | property sets: _Dør Dobbel_Ulike_Dørblader_Glassfelt:IDA 3.1 18x21M 33db EI30S:1852022, Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data
  IFCDOORSTYLE "IDT 2.3 10x21M 33dB" | 1 occurrence | material: materials ("Terskel Tre", "Lys grå", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Other, Text
  IFCDOORSTYLE "IDT 3.3 10x21M 33dB" | 4 occurrences | material: materials ("Lys grå", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "IDT 2.1 10x21M" | 1 occurrence | material: materials ("_White", "NCS S 0500-N", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Other, Text
  IFCDOORSTYLE "IDA 3.1 18x21M 33db EI30S" | 1 occurrence | material: materials ("Glass Klart", "Lys grå", "Terskel Tre", "Karm Malt") | property sets: Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCWALLTYPE "Basic Wall:IVA 8.1T 125mm sjaktvegg 48dB EI60" | STANDARD | 1 occurrence | material: layers "Basic Wall:IVA 8.1T 125mm sjaktvegg 48dB EI60" ("Branngips" 15., "Branngips" 15., "stender/isolasjon" 95.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCDOORSTYLE "IDT 1.2 8x21M 33dB" | 2 occurrences | material: materials ("Terskel Tre", "NCS S 0500-N", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Other, Text
  IFCDOORSTYLE "IDT 1.1 8x21M" | 1 occurrence | material: materials ("Terskel Tre", "Lys grå", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Other, Text
  IFCWALLTYPE "Basic Wall:IVA 2.1T 134mm 44dB (H-95-NH)" | STANDARD | 1 occurrence | material: layers "Basic Wall:IVA 2.1T 134mm 44dB (H-95-NH)" ("Habito" 13., "stender/isolasjon" 95., "Gips" 13., "Habito" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCDOORSTYLE "IDT 3.6 10x21M 38dB" | 1 occurrence | material: materials ("NCS S 2500-N", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCWINDOWSTYLE "V3 18x22" | 5 occurrences | material: materials ("N_Windows - Glass", "NCS S 0502-Y") | property sets: Vindu-Fast:V3 18x22:1892833, Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data
  IFCWINDOWSTYLE "V4 23x22" | 10 occurrences | material: materials ("Glass Klart", "NCS S 0502-Y") | property sets: Vindu-Fast:V4 23x22:1896885, Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data
  IFCWINDOWSTYLE "V22 14x14" | 2 occurrences | material: materials ("Glass Klart", "NCS S 0502-Y") | property sets: Vindu-Fast:V22 14x14:1897688, Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data
  IFCWINDOWSTYLE "V1 12x22" | 4 occurrences | material: materials ("NCS S 0502-Y", "Glass Klart") | property sets: Vindu-Hengslet_1200 opening:V1 12x22:1898390, Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data
  IFCWINDOWSTYLE "V1 12x22" | 6 occurrences | material: materials ("NCS S 0502-Y", "Glass Klart") | property sets: Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCWINDOWSTYLE "V3 18x22" | 4 occurrences | material: materials ("N_Windows - Glass", "NCS S 0502-Y") | property sets: Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCWINDOWSTYLE "V4 23x22" | 4 occurrences | material: materials ("Glass Klart", "NCS S 0502-Y") | property sets: Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCWINDOWSTYLE "V22 14x14" | 2 occurrences | material: materials ("Glass Klart", "NCS S 0502-Y") | property sets: Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCDOORSTYLE "IDA 3.1 18x21M 33db EI30S" | 1 occurrence | material: materials ("Glass Klart", "Lys grå", "Terskel Tre", "Karm Malt") | property sets: Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCWALLTYPE "Basic Wall:IVA 2.1T 134mm 48dB (H-95-NH)" | STANDARD | 6 occurrences | material: layers "Basic Wall:IVA 2.1T 134mm 48dB (H-95-NH)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 95., "Habito" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCDOORSTYLE "IDT 3.6 10x21M 38dB" | 8 occurrences | material: materials ("NCS S 2500-N", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "IDT 3.6 10x21M 38dB" | 2 occurrences | material: materials ("NCS S 2500-N", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "IDT 3.6 10x21M 38dB" | 1 occurrence | material: materials ("NCS S 2500-N", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:IVA 3.1 F 145mm 48dB (HN-95-NH)" | STANDARD | 1 occurrence | material: layers "Basic Wall:IVA 3.1 F 145mm 48dB (HN-95-NH)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Habito" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCWALLTYPE "Basic Wall:IVA 1.1 F 121mm 44dB (H-95-H)" | STANDARD | 1 occurrence | material: layers "Basic Wall:IVA 1.1 F 121mm 44dB (H-95-H)" ("Habito" 13., "stender/isolasjon" 95., "Habito" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCDOORSTYLE "IDT 3.6 10x21M 38dB" | 1 occurrence | material: materials ("NCS S 2500-N", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "IDT 5.2 15x21M EI60S" | 4 occurrences | material: materials ("NCS S 1000-N", "Terskel Tre", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "IDT 3.3 10x21M 33dB" | 1 occurrence | material: materials ("Lys grå", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:IVA 10.1 193mm 48dB (RN-95-NR)" | STANDARD | 1 occurrence | material: layers "Basic Wall:IVA 10.1 193mm 48dB (RN-95-NR)" ("Robustgips" 13., "<Unnamed>" 13., "Gips" 13., "<Unnamed>" 10., "stender/isolasjon" 98., "<Unnamed>" 10., "<Unnamed>" 13., "Gips" 13., "Robustgips" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCDOORSTYLE "IDF 3.1 Foldevegg 9700x2500" | 1 occurrence | material: materials ("Light grey", "Karm Malt") | property sets: Side_Stack_Operable_Wall_h2500_w9700:IDF 3.1 Foldevegg 9700x2500:2031491, Analytical Properties, Constraints, Construction, Dimensions, Identity Data
  IFCWINDOWSTYLE "GFA 3 8x27 38dB" | 1 occurrence | material: materials ("Glass Klart", "RAL 9004") | property sets: Vindu-Fast:GFA 3 8x27 38dB:2067745, Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data
  IFCWALLTYPE "Basic Wall:IVA 6.3T 302mm EI 30 (RN-95-60-95-NR)" | STANDARD | 1 occurrence | material: layers "Basic Wall:IVA 6.3T 302mm EI 30 (RN-95-60-95-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95., "Luftsjikt" 60., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCDOORSTYLE "IDT 1.2 8x21M 33dB" | 6 occurrences | material: materials ("Terskel Tre", "NCS S 0500-N", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Other, Text
  IFCWALLTYPE "Basic Wall:IVA 1.3T 121mm 34dB (R-95-R)" | STANDARD | 2 occurrences | material: layers "Basic Wall:IVA 1.3T 121mm 34dB (R-95-R)" ("Robustgips" 13., "stender/isolasjon" 95., "Robustgips" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCWALLTYPE "Basic Wall:IVA 6.3T 272mm 48dB EI60 (RN-95-30-95-NR)" | STANDARD | 1 occurrence | material: layers "Basic Wall:IVA 6.3T 272mm 48dB EI60 (RN-95-30-95-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95., "Luftsjikt" 30., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCWALLTYPE "Basic Wall:IVA 6.1 302mm (HN-95-60-95-NH)" | STANDARD | 2 occurrences | material: layers "Basic Wall:IVA 6.1 302mm (HN-95-60-95-NH)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 95., "Luftsjikt" 60., "stender/isolasjon" 95., "Gips" 13., "Habito" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCDOORSTYLE "IDT 3.3 10x21M 33dB" | 1 occurrence | material: materials ("Lys grå", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "IDT 3.3 10x21M 33dB" | 1 occurrence | material: materials ("Lys grå", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "IDT 1.1 8x21M" | 1 occurrence | material: materials ("Terskel Tre", "Lys grå", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Other, Text
  IFCDOORSTYLE "IDT 1.1 8x21M" | 2 occurrences | material: materials ("Terskel Tre", "Lys grå", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Other, Text
  IFCWALLTYPE "Basic Wall:IVA 7.3 121mm 37dB EI30 (95-NH)" | STANDARD | 4 occurrences | material: layers "Basic Wall:IVA 7.3 121mm 37dB EI30 (95-NH)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:IVA 6.3 302mm 48dB (RN-95-60-95-NR)" | STANDARD | 1 occurrence | material: layers "Basic Wall:IVA 6.3 302mm 48dB (RN-95-60-95-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95., "Luftsjikt" 60., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCDOORSTYLE "IDT 5.2 15x21M EI60S" | 2 occurrences | material: materials ("NCS S 1000-N", "Terskel Tre", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "IDT 5.2 15x21M EI60S" | 2 occurrences | material: materials ("NCS S 1000-N", "Terskel Tre", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "IDT 3.6 10x21M 38dB" | 2 occurrences | material: materials ("NCS S 2500-N", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "IDT 3.3 10x21M 33dB" | 1 occurrence | material: materials ("Lys grå", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "IDT 2.1 10x21M" | 1 occurrence | material: materials ("_White", "NCS S 0500-N", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Other, Text
  IFCWALLTYPE "Basic Wall:IVA 8.1 125mm sjaktvegg 37dB EI60" | STANDARD | 2 occurrences | material: layers "Basic Wall:IVA 8.1 125mm sjaktvegg 37dB EI60" ("Branngips" 15., "Branngips" 15., "stender/isolasjon" 95.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCWINDOWSTYLE "V2 12x22" | 2 occurrences | material: materials ("Glass Klart", "NCS S 0502-Y") | property sets: Vindu-Fast:V2 12x22:2275275, Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data
  IFCDOORSTYLE "IDT 1.1 8x21M" | 1 occurrence | material: materials ("Terskel Tre", "Lys grå", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Other, Text
  IFCWINDOWSTYLE "V5 8x22" | 1 occurrence | material: materials ("Glass Klart", "NCS S 0502-Y") | property sets: Vindu-Fast:V5 8x22:2399390, Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data
  IFCWINDOWSTYLE "V1 12x22" | 1 occurrence | material: materials ("NCS S 0502-Y", "Glass Klart") | property sets: Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCWINDOWSTYLE "V23 14x14" | 2 occurrences | material: materials ("Glass Klart", "NCS S 0502-Y", "Karm Malt") | property sets: Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCWINDOWSTYLE "GF 1.3 12x21 38dB" | 6 occurrences | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Vindu-Fast:GF 1.3 12x21 38dB:2493195, Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data
  IFCWINDOWSTYLE "GF 3.3 6x21 44dB" | 1 occurrence | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Vindu-Fast:GF 3.3 6x21 44dB:2493355, Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data
  IFCWINDOWSTYLE "GF 1.1 12x21 33dB" | 11 occurrences | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Vindu-Fast:GF 1.1 12x21 33dB:2493862, Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data
  IFCWINDOWSTYLE "GF 4.2 18x21 33dB" | 2 occurrences | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Vindu-Fast:GF 4.2 18x21 33dB:2498708, Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data
  IFCWINDOWSTYLE "GF 4.2 18x21 33dB" | 2 occurrences | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCWINDOWSTYLE "GF 1.1 12x21 33dB" | 1 occurrence | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCWINDOWSTYLE "GF 1.3 12x21 38dB" | 9 occurrences | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCWINDOWSTYLE "GF 4.1 18x21 38dB" | 1 occurrence | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Vindu-Fast:GF 4.1 18x21 38dB:2500740, Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data
  IFCWINDOWSTYLE "GF 10.2 8x27 38dB" | 1 occurrence | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Vindu-Fast:GF 10.2 8x27 38dB:2500909, Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data
  IFCWINDOWSTYLE "GF 4.2 18x21 33dB" | 1 occurrence | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCWINDOWSTYLE "GF 10.2 8x27 38dB" | 1 occurrence | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCWINDOWSTYLE "GF 1.1 12x21 33dB" | 1 occurrence | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCWINDOWSTYLE "GF 3.3 6x21 44dB" | 2 occurrences | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCWINDOWSTYLE "GF 11.1 12x27 33dB" | 2 occurrences | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Vindu-Fast:GF 11.1 12x27 33dB:2505892, Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data
  IFCWINDOWSTYLE "GF 2.2 9x21 33dB" | 1 occurrence | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCWINDOWSTYLE "GF 6.1 8x21 33dB" | 1 occurrence | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Vindu-Fast:GF 6.1 8x21 33dB:2506671, Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data
  IFCWINDOWSTYLE "GF 1.1 12x21 33dB" | 1 occurrence | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCWINDOWSTYLE "GF 7.2 15x21 38dB" | 1 occurrence | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Vindu-Fast:GF 7.2 15x21 38dB:2506998, Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data
  IFCWINDOWSTYLE "GF 3.6 6x21 33dB" | 1 occurrence | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Vindu-Fast:GF 3.6 6x21 33dB:2507587, Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data
  IFCWINDOWSTYLE "GF 7.2 15x21 38dB" | 1 occurrence | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCWINDOWSTYLE "GF 1.3 12x21 38dB" | 1 occurrence | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCWINDOWSTYLE "GF 4.1 18x21 38dB" | 1 occurrence | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCWINDOWSTYLE "GF 2.2 9x21 33dB" | 1 occurrence | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCWINDOWSTYLE "GF 1.1 12x21 33dB" | 1 occurrence | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCWINDOWSTYLE "GF 1.3 12x21 38dB" | 1 occurrence | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCWINDOWSTYLE "GF 3.2 6x21 38dB" | 1 occurrence | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCWALLTYPE "Basic Wall:IVA 5.1 212mm 34 dB (HN-160-NR)" | STANDARD | 1 occurrence | material: layers "Basic Wall:IVA 5.1 212mm 34 dB (HN-160-NR)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 160., "Gips" 13., "Robustgips" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:IVA 4.1T 172mm 34dB (HN-120-NH)" | STANDARD | 2 occurrences | material: layers "Basic Wall:IVA 4.1T 172mm 34dB (HN-120-NH)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 120., "Gips" 13., "Habito" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCWALLTYPE "Basic Wall:IVA 6.3 376mm 34dB (RN-95-134-95-NR)" | STANDARD | 1 occurrence | material: layers "Basic Wall:IVA 6.3 376mm 34dB (RN-95-134-95-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95., "Luftsjikt" 198., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCWALLTYPE "Basic Wall:IVA 3.3 F 145mm 48dB (RN-95-NR)" | STANDARD | 1 occurrence | material: layers "Basic Wall:IVA 3.3 F 145mm 48dB (RN-95-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCWINDOWSTYLE "GF 1.4 12x21 44dB" | 2 occurrences | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Vindu-Fast:GF 1.4 12x21 44dB:2992305, Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data
  IFCWINDOWSTYLE "GF 1.1 12x21 33dB" | 2 occurrences | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCWINDOWSTYLE "GF 2.1 9x21 38dB" | 1 occurrence | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCWALLTYPE "Basic Wall:IVA 6.1 302mm 44dB (HN-95-30-95-NH)" | STANDARD | 2 occurrences | material: layers "Basic Wall:IVA 6.1 302mm 44dB (HN-95-30-95-NH)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 95., "Luftsjikt" 60., "stender/isolasjon" 95., "Gips" 13., "Habito" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCDOORSTYLE "IDT 3.6 10x21M 38dB" | 2 occurrences | material: materials ("NCS S 2500-N", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCWINDOWSTYLE "GF 1.1 12x21 33dB" | 2 occurrences | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCWINDOWSTYLE "GF 9.1 11x26.5 33dB" | 2 occurrences | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Analysis Results(Type), Analytical Properties(Type), Construction(Type), Dimensions(Type), Identity Data(Type), Materials and Finishes(Type)
  IFCWINDOWSTYLE "GF 16.1 5x31 38dB" | 2 occurrences | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Vindu-Fast:GF 16.1 5x31 38dB:2997461, Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data
  IFCWINDOWSTYLE "GF 1.1 12x21 33dB" | 2 occurrences | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCWINDOWSTYLE "GF 12.1 6x31 38dB" | 5 occurrences | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Vindu-Fast:GF 12.1 6x31 38dB:2998710, Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data
  IFCDOORSTYLE "1700 x 2100mm" | 1 occurrence | material: "Metal - Paint Finish - Ivory, Matte" | property sets: M_Overhead-Rolling:1700 x 2100mm:3038740, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCDOORSTYLE "IDT 2.3 10x21M 33dB" | 2 occurrences | material: materials ("Terskel Tre", "Lys grå", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Other, Text
  IFCDOORSTYLE "IDT 2.3 10x21M 33dB" | 2 occurrences | material: materials ("Terskel Tre", "Lys grå", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Other, Text
  IFCWINDOWSTYLE "GF 12.1 6x31 38dB" | 2 occurrences | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCWINDOWSTYLE "GF 12.1 6x31 38dB" | 2 occurrences | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCWINDOWSTYLE "GF 10.1 8x27 33dB" | 1 occurrence | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Vindu-Fast:GF 10.1 8x27 33dB:3382692, Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data
  IFCDOORSTYLE "IDT 2.1 10x21M" | 1 occurrence | material: materials ("_White", "NCS S 0500-N", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Other, Text
  IFCWINDOWSTYLE "V3 18x22" | 2 occurrences | material: materials ("N_Windows - Glass", "NCS S 0502-Y") | property sets: Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCWALLTYPE "Basic Wall:IVA 6.2 272mm 48dB EI60 (HN-95-30-95-NR)" | STANDARD | 1 occurrence | material: layers "Basic Wall:IVA 6.2 272mm 48dB EI60 (HN-95-30-95-NR)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 95., "Luftsjikt" 30., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCDOORSTYLE "IDA 10.1 14x21M E30CS" | 1 occurrence | material: materials ("Light grey", "Karm Malt", "Lys grå") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "IDT 3.3 10x21M 33dB" | 1 occurrence | material: materials ("Lys grå", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:IVA 7.1T 121mm (95-NR)" | STANDARD | 2 occurrences | material: layers "Basic Wall:IVA 7.1T 121mm (95-NR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "IDT 3.3 10x21M 33dB" | 1 occurrence | material: materials ("Lys grå", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCWINDOWSTYLE "V5 8x22" | 1 occurrence | material: materials ("Glass Klart", "NCS S 0502-Y") | property sets: Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCWALLTYPE "Basic Wall:YV 9.2 536mm uisolert" | STANDARD | 1 occurrence | material: layers "Basic Wall:YV 9.2 536mm uisolert" ("Trekledning" 19., "Luftsjikt" 48., "Luftsjikt" 36., "Luftsjikt" 48., "Vindsperre" 9., "stender" 296., "<Unnamed>" 36., "Luftsjikt" 36., "Cembrit Metro Amsterdam" 8.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "IDT 7.1 13x21M 38dB" | 1 occurrence | material: materials ("Lys grå", "Terskel Tre", "Karm Malt") | property sets: Dør Dobbel_Ulike_Dørblader:IDT 7.1 13x21M 38dB:4801842, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCWINDOWSTYLE "GFA 3 8x27 38dB" | 1 occurrence | material: materials ("Glass Klart", "RAL 9004") | property sets: Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCWINDOWSTYLE "GF 1.3 12x21 38dB" | 2 occurrences | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCWINDOWSTYLE "GF 13.1 36x21 38dB" | 1 occurrence | material: materials ("Karm Malt", "Glass Klart", "NCS S 3502-Y") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCWINDOWSTYLE "V7 24x22" | 4 occurrences | material: materials ("NCS S 0502-Y", "N_Windows - Glass") | property sets: Analytical Properties(Type), Construction(Type), Dimensions(Type), Identity Data(Type), Materials and Finishes(Type), Other(Type)
  IFCWINDOWSTYLE "V11 35x22" | 2 occurrences | material: materials ("NO_Aluminium", "NCS S 0502-Y", "N_Windows - Glass") | property sets: Analytical Properties(Type), Construction(Type), Dimensions(Type), Identity Data(Type), Materials and Finishes(Type), Other(Type)
  IFCWINDOWSTYLE "V9 30x22" | 3 occurrences | material: materials ("NCS S 0502-Y", "N_Windows - Glass") | property sets: Analytical Properties(Type), Construction(Type), Dimensions(Type), Identity Data(Type), Materials and Finishes(Type), Other(Type)
  IFCWINDOWSTYLE "V10 30x22" | 1 occurrence | material: materials ("NCS S 0502-Y", "N_Windows - Glass") | property sets: Analytical Properties(Type), Construction(Type), Dimensions(Type), Identity Data(Type), Materials and Finishes(Type), Other(Type)
  IFCWINDOWSTYLE "V9 30x22" | 2 occurrences | material: materials ("NCS S 0502-Y", "N_Windows - Glass") | property sets: Analytical Properties(Type), Construction(Type), Dimensions(Type), Identity Data(Type), Materials and Finishes(Type), Other(Type)
  IFCWINDOWSTYLE "V8 27x22" | 3 occurrences | material: materials ("NCS S 0502-Y", "N_Windows - Glass") | property sets: Analytical Properties(Type), Construction(Type), Dimensions(Type), Identity Data(Type), Materials and Finishes(Type), Other(Type)
  IFCWINDOWSTYLE "V6 24x22" | 11 occurrences | material: materials ("NCS S 0502-Y", "N_Windows - Glass") | property sets: Analytical Properties(Type), Construction(Type), Dimensions(Type), Identity Data(Type), Materials and Finishes(Type), Other(Type)
  IFCWINDOWSTYLE "V7 24x22" | 6 occurrences | material: materials ("NCS S 0502-Y", "N_Windows - Glass") | property sets: Analytical Properties(Type), Construction(Type), Dimensions(Type), Identity Data(Type), Materials and Finishes(Type), Other(Type)
  IFCWINDOWSTYLE "V10 30x22" | 4 occurrences | material: materials ("NCS S 0502-Y", "N_Windows - Glass") | property sets: Analytical Properties(Type), Construction(Type), Dimensions(Type), Identity Data(Type), Materials and Finishes(Type), Other(Type)
  IFCWINDOWSTYLE "V12 35x22" | 4 occurrences | material: materials ("NO_Aluminium", "NCS S 0502-Y", "N_Windows - Glass") | property sets: Analytical Properties(Type), Construction(Type), Dimensions(Type), Identity Data(Type), Materials and Finishes(Type), Other(Type)
  IFCWINDOWSTYLE "V11 35x22" | 7 occurrences | material: materials ("NO_Aluminium", "NCS S 0502-Y", "N_Windows - Glass") | property sets: Analytical Properties(Type), Construction(Type), Dimensions(Type), Identity Data(Type), Materials and Finishes(Type), Other(Type)
  IFCWINDOWSTYLE "V12 35x22" | 3 occurrences | material: materials ("NO_Aluminium", "NCS S 0502-Y", "N_Windows - Glass") | property sets: Analytical Properties(Type), Construction(Type), Dimensions(Type), Identity Data(Type), Materials and Finishes(Type), Other(Type)
  IFCWINDOWSTYLE "V6 24x22" | 1 occurrence | material: materials ("NCS S 0502-Y", "N_Windows - Glass") | property sets: Analytical Properties(Type), Construction(Type), Dimensions(Type), Identity Data(Type), Materials and Finishes(Type), Other(Type)
  IFCWALLTYPE "Basic Wall:Rekkverksvegg" | STANDARD | 2 occurrences | material: layers "Basic Wall:Rekkverksvegg" ("Farge sort" 6.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCWALLTYPE "Basic Wall:YV stolpe" | STANDARD | 13 occurrences | material: layers "Basic Wall:YV stolpe" ("Vindsperre" 9., "Stender isolert vegg" 98., "Gips" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "IDT 8.1 18x21M 33dB" | 1 occurrence | material: materials ("Glass Klart", "Lys grå", "Terskel Tre", "Karm Malt") | property sets: _Dør Dobbel_Ulike_Dørblader_Glassfelt2:IDT 8.1 18x21M 33dB:6481045, Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data
  IFCDOORSTYLE "Luke 600" | 2 occurrences | material: materials ("Light grey", "Karm Malt") | property sets: Analytical Properties(Type), Construction(Type), Dimensions(Type), Identity Data(Type), Other(Type), Text(Type)
  IFCDOORSTYLE "Luke 600" | 4 occurrences | material: materials ("Light grey", "Karm Malt") | property sets: Analytical Properties(Type), Construction(Type), Dimensions(Type), Identity Data(Type), Other(Type), Text(Type)
  IFCWALLTYPE "Basic Wall:YV 1.2 517mm EI60" | 1 occurrence | material: layers "Basic Wall:YV 1.2 517mm EI60" ("Trekledning" 19., "Luftsjikt" 48., "Luftsjikt" 36., "Luftsjikt" 48., "Vindsperre" 9., "Stender isolert vegg" 296., "NO_Utlekting" 48., "Branngips" 15.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:IVA 3.1T 145mm 48dB EI60 (HN-95-NH)" | STANDARD | 3 occurrences | material: layers "Basic Wall:IVA 3.1T 145mm 48dB EI60 (HN-95-NH)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Habito" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCWALLTYPE "Basic Wall:18mm 2" | STANDARD | 2 occurrences | material: layers "Basic Wall:18mm 2" ("Laminate, Ivory, Matte" 18.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCBUILDINGELEMENTPROXYTYPE "Projector" | 1 occurrence | material: "hvit malt" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:IVA 3.3T 145mm 48dB EI60 (RN-95-NNNR)" | STANDARD | 1 occurrence | material: layers "Basic Wall:IVA 3.3T 145mm 48dB EI60 (RN-95-NNNR)" ("Robustgips" 13., "Gips" 13., "stender/isolasjon" 95., "Gips" 13., "Gips" 13., "Gips" 13., "Robustgips" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCFURNITURETYPE "Skap, resirkulering 400 x 400 x 825mm" | element type "Skap, resirkulering 400 x 400 x 825mm" | 14 occurrences | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Skap, resirkulering 300 x 400 x 825mm" | element type "Skap, resirkulering 300 x 400 x 825mm" | 14 occurrences | material: materials ("N_Cabinets", "N_Cabinets - Handles") | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Benkeplate kildesortering 2" | element type "Benkeplate kildesortering 2" | 7 occurrences | material: "hvit malt" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCBUILDINGELEMENTPROXYTYPE "PC-skap" | 12 occurrences | material: "hvit malt" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Hattehylle360mm" | element type "Hattehylle360mm" | 1 occurrence | material: "Wood - Birch, Natural" | property sets: Identity Data, Other
  IFCFURNITURETYPE "Skohylle" | element type "Skohylle" | 1 occurrence | material: "hvit malt" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCBUILDINGELEMENTPROXYTYPE "Tørkeskap" | 2 occurrences | material: "hvit malt" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCBUILDINGELEMENTPROXYTYPE "Tørkeskap" | 2 occurrences | material: "hvit malt" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCBUILDINGELEMENTPROXYTYPE "gard skap 30cm 3" | 7 occurrences | material: materials ("Gul avdeling", "Steel - Hadrian - Black") | property sets: Analytical Model, Constraints, Dimensions, Green Building Properties, Identity Data, Layers
  IFCBUILDINGELEMENTPROXYTYPE "Siemens frittstående kombiskap" | 1 occurrence | material: "N_Cabinets" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCBUILDINGELEMENTPROXYTYPE "Siemens frittstående kombiskap" | 1 occurrence | material: "N_Cabinets" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Benkeplate 625mm, Sigdal" | element type "Benkeplate 625mm, Sigdal" | 1 occurrence | material: "hvit malt" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCBUILDINGELEMENTPROXYTYPE "PC-skap" | 7 occurrences | material: "hvit malt" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Benkeplate 265mm, krogsæter" | element type "Benkeplate 265mm, krogsæter" | 1 occurrence | material: "hvit malt" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Benkeplate 265mm, krogsæter" | element type "Benkeplate 265mm, krogsæter" | 1 occurrence | material: "hvit malt" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCBUILDINGELEMENTPROXYTYPE "Tavle 2,5m" | 1 occurrence | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Mixebord" | element type "Mixebord" | 1 occurrence | material: materials ("Default", "hvit malt") | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCBUILDINGELEMENTPROXYTYPE "Tavle 1,5m" | 1 occurrence | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Skohylle" | element type "Skohylle" | 1 occurrence | material: "hvit malt" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Hattehylle360mm" | element type "Hattehylle360mm" | 1 occurrence | material: "Wood - Birch, Natural" | property sets: Identity Data, Other
  IFCFURNITURETYPE "Elevskap" | element type "Elevskap" | 18 occurrences | material: materials ("Paint - Grey", "Skapdør 2", "Gul avdeling") | property sets: Graphics, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Elevskap" | element type "Elevskap" | 9 occurrences | material: materials ("Paint - Grey", "Skapdør 3", "Skapdør 2") | property sets: Graphics, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Elevskap" | element type "Elevskap" | 9 occurrences | material: materials ("Paint - Grey", "Gul avdeling", "Skapdør 3") | property sets: Graphics, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Elevskap" | element type "Elevskap" | 6 occurrences | material: materials ("Paint - Grey", "Gul avdeling", "Skapdør 3") | property sets: Graphics, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Elevskap" | element type "Elevskap" | 24 occurrences | material: materials ("Paint - Grey", "Skapdør 2", "Gul avdeling") | property sets: Graphics, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Elevskap" | element type "Elevskap" | 6 occurrences | material: materials ("Paint - Grey", "Skapdør 3", "Skapdør 2") | property sets: Graphics, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Elevskap" | element type "Elevskap" | 79 occurrences | material: materials ("Paint - Grey", "_White") | property sets: Graphics, Identity Data, Materials and Finishes, Other
  IFCFURNITURETYPE "Elevskap" | element type "Elevskap" | 135 occurrences | material: materials ("Paint - Grey", "_White") | property sets: Graphics, Identity Data, Materials and Finishes, Other
  IFCBUILDINGELEMENTPROXYTYPE "Ladeskap - sykkel" | 1 occurrence | material: "hvit malt" | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCBUILDINGELEMENTPROXYTYPE "Corpus 800" | 3 occurrences | material: materials ("Gul avdeling", "Steel - Hadrian - Black") | property sets: Analytical Model, Constraints, Dimensions, Green Building Properties, Identity Data, Layers
  IFCBUILDINGELEMENTPROXYTYPE "Corpus 800" | 2 occurrences | material: materials ("Gul avdeling", "Steel - Hadrian - Black") | property sets: Analytical Model, Constraints, Dimensions, Green Building Properties, Identity Data, Layers
  IFCBUILDINGELEMENTPROXYTYPE "Whiteboard 3m" | 1 occurrence | material: materials ("Focus - Dør - Håndtak", "Default tavle") | property sets: Dimensions, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "IDA 7.1 15x21M EI60CS" | 1 occurrence | material: materials ("Karm Malt", "Lys grå", "Terskel Tre") | property sets: Enfløyet_aludør:IDA 7.1 15x21M EI60CS:1700918, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCDOORSTYLE "IDA 7.1 15x21M EI60CS" | 1 occurrence | material: materials ("Karm Malt", "Lys grå", "Terskel Tre") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "IDA 3.1 18x21M 33db EI30S" | 1 occurrence | material: materials ("Glass Klart", "Lys grå", "Terskel Tre", "Karm Malt") | property sets: Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCWALLTYPE "Basic Wall:IVA 6.2T 272mm 55dB EI60 (HN-95-30-95-NR)" | STANDARD | 1 occurrence | material: layers "Basic Wall:IVA 6.2T 272mm 55dB EI60 (HN-95-30-95-NR)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 95., "Luftsjikt" 30., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCWALLTYPE "Basic Wall:IVA 6.2T 272mm 48dB EI60 (HN-95-60-95-NR)" | STANDARD | 1 occurrence | material: layers "Basic Wall:IVA 6.2T 272mm 48dB EI60 (HN-95-60-95-NR)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 95., "Luftsjikt" 60., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCWALLTYPE "Basic Wall:IVA 6.1T 272mm 55dB EI60 (HN-95-30-95-NH)" | STANDARD | 1 occurrence | material: layers "Basic Wall:IVA 6.1T 272mm 55dB EI60 (HN-95-30-95-NH)" ("Habito" 13., "Gips" 13., "stender/isolasjon" 95., "Luftsjikt" 30., "stender/isolasjon" 95., "Gips" 13., "Habito" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCWINDOWSTYLE "V24 20x20" | 1 occurrence | material: materials ("Glass Klart", "NCS S 0502-Y") | property sets: Vindu-Fast:V24 20x20:2217007, Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data
  IFCWINDOWSTYLE "V24 20x20" | 1 occurrence | material: materials ("Glass Klart", "NCS S 0502-Y") | property sets: Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCWALLTYPE "Basic Wall:YV 12.1 411 Ventilasjonsrom" | STANDARD | 5 occurrences | material: layers "Basic Wall:YV 12.1 411 Ventilasjonsrom" ("Spiler ute" 19., "Luftsjikt" 36., "Luftsjikt" 36., "Vindsperre" 9., "Stender isolert vegg" 250., "Stender isolert vegg" 48., "Habito" 12.5, "Habito" 12.5) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:YV 12.1 411 Ventilasjonsrom EI 60" | STANDARD | 3 occurrences | material: layers "Basic Wall:YV 12.1 411 Ventilasjonsrom EI 60" ("Spiler ute" 19., "Luftsjikt" 36., "Luftsjikt" 36., "Vindsperre" 9., "Stender isolert vegg" 250., "Stender isolert vegg" 48., "Habito" 12.5, "Habito" 12.5) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "YDS 1.2 15x21M EI 60S" | 1 occurrence | material: materials ("Lys grå", "Terskel Tre", "Karm Malt") | property sets: _Dør Dobbel_Ulike_Dørblader:YDS 1.2 15x21M EI 60S:2389213, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCDOORSTYLE "YDS 1.1 15x21M" | 1 occurrence | material: materials ("Lys grå", "Terskel Tre", "Karm Malt") | property sets: _Dør Dobbel_Ulike_Dørblader:YDS 1.1 15x21M:2389269, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCWINDOWSTYLE "V3 18x22" | 1 occurrence | material: materials ("N_Windows - Glass", "NCS S 0502-Y") | property sets: Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCWINDOWSTYLE "V2 12x22" | 1 occurrence | material: materials ("Glass Klart", "NCS S 0502-Y") | property sets: Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCWALLTYPE "Basic Wall:YV 4.1 373 Gesims" | STANDARD | 9 occurrences | material: layers "Basic Wall:YV 4.1 373 Gesims" ("Trekledning" 19., "Luftsjikt" 48., "Luftsjikt" 36., "Luftsjikt" 48., "Vindsperre" 9., "Stender isolert vegg" 198., "Kryssfiner" 15.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCWINDOWSTYLE "GF 3.3 6x21 44dB" | 1 occurrence | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCDOORSTYLE "IDT 2.1 10x21M" | 1 occurrence | material: materials ("_White", "NCS S 0500-N", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Other, Text
  IFCDOORSTYLE "IDS 3.1 18x21M 38dB EI60S" | 1 occurrence | material: materials ("Lys grå", "Terskel Tre", "Karm Malt") | property sets: Dør Dobbel:IDS 3.1 18x21M 38dB EI60S:2551141, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCDOORSTYLE "IDS 3.1 18x21M 38dB EI60S" | 1 occurrence | material: materials ("Lys grå", "Terskel Tre", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:IVA 2.2T 134mm 34dB (H-95-NR)" | STANDARD | 1 occurrence | material: layers "Basic Wall:IVA 2.2T 134mm 34dB (H-95-NR)" ("Habito" 13., "stender/isolasjon" 95., "Gips" 13., "Robustgips" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCWALLTYPE "Basic Wall:YV 22.1" | STANDARD | 1 occurrence | material: layers "Basic Wall:YV 22.1" ("Trekledning" 19., "Luftsjikt" 48., "Luftsjikt" 36., "Luftsjikt" 48., "Vindsperre" 9., "Stender isolert vegg" 296., "NO_Utlekting" 48., "Habito" 12.5, "Habito" 12.5) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "IDT 2.3 10x21M 33dB" | 1 occurrence | material: materials ("Terskel Tre", "Lys grå", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Other, Text
  IFCDOORSTYLE "IDT 3.6 10x21M 38dB" | 1 occurrence | material: materials ("NCS S 2500-N", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCWINDOWSTYLE "GF 10.1 8x27 33dB" | 1 occurrence | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCDOORSTYLE "IDT 3.6 10x21M 38dB" | 1 occurrence | material: materials ("NCS S 2500-N", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "IDT 3.6 10x21M 38dB" | 1 occurrence | material: materials ("NCS S 2500-N", "Glass Klart", "Terskel Tre", "Karm Malt") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCWINDOWSTYLE "GF 2.1 9x21 38dB" | 1 occurrence | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCWINDOWSTYLE "GF 2.1 9x21 38dB" | 1 occurrence | material: materials ("Glass Klart", "NCS S 3502-Y") | property sets: Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCWALLTYPE "Basic Wall:IVA 7.2 111mm Skjørt 2" | STANDARD | 2 occurrences | material: layers "Basic Wall:IVA 7.2 111mm Skjørt 2" ("Gips" 13., "stender/isolasjon" 98.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:YVL 1.1 250mm leca isoblokk" | STANDARD | 10 occurrences | material: layers "Basic Wall:YVL 1.1 250mm leca isoblokk" ("Mur" 82., "NO_Hard isolasjon" 86., "Mur" 82.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCWINDOWSTYLE "V6 24x22" | 1 occurrence | material: materials ("NCS S 0502-Y", "N_Windows - Glass") | property sets: Analytical Properties(Type), Construction(Type), Dimensions(Type), Identity Data(Type), Materials and Finishes(Type), Other(Type)
  IFCWALLTYPE "Basic Wall:YV 18.1 136 Takhatt" | STANDARD | 45 occurrences | material: layers "Basic Wall:YV 18.1 136 Takhatt" ("Kryssfiner" 15., "Stender isolert vegg" 98.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:YV 18.1 136 Takhatt 3" | STANDARD | 1 occurrence | material: layers "Basic Wall:YV 18.1 136 Takhatt 3" ("Stender isolert vegg" 98.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "IDT 8.1 18x21M 33dB" | 1 occurrence | material: materials ("Glass Klart", "Lys grå", "Terskel Tre", "Karm Malt") | property sets: Analysis Results, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCWALLTYPE "Basic Wall:YVL 3.1 300mm leca isoblokk" | STANDARD | 2 occurrences | material: layers "Basic Wall:YVL 3.1 300mm leca isoblokk" ("Mur" 82., "NO_Hard isolasjon" 186., "Mur" 82.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:YV 13.1 313 Gesims Ventilasjonsrom" | STANDARD | 8 occurrences | material: layers "Basic Wall:YV 13.1 313 Gesims Ventilasjonsrom" ("Spiler ute" 19., "Luftsjikt" 36., "Luftsjikt" 36., "Vindsperre" 9., "Stender isolert vegg" 198., "Kryssfiner" 15.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:TGF" | STANDARD | 36 occurrences | material: layers "Basic Wall:TGF" ("<Unnamed>" 12., "Stender isolert vegg" 36.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:YV 23.1 136 Røykluke" | STANDARD | 8 occurrences | material: layers "Basic Wall:YV 23.1 136 Røykluke" ("Kryssfiner" 15., "Stender isolert vegg" 198., "Gips" 12.5) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other

Property sets
  Text | properties | on 846 objects (661 IFCMEMBER, 176 IFCPLATE, 9 IFCBUILDINGELEMENTPROXY)
    TFM11FkSys = "" (IFCTEXT)
  Text | properties | on 496 objects (496 IFCWALLSTANDARDCASE)
    TFM Samlet = "+135.01=242.001" (IFCTEXT)
    TFM Systemløpenummer = "001" (IFCTEXT)
    TFM11FkSys = "242" (IFCTEXT)
  Text | properties | on 286 objects (286 IFCFURNISHINGELEMENT)
    TFM Komponentkode = "FS" (IFCTEXT)
    TFM Komponentløpenummer = "014" (IFCTEXT)
    TFM Samlet = "+135.01=275.001-FS014T" (IFCTEXT)
    TFM Systemløpenummer = "001" (IFCTEXT)
    TFM Typeunik = "T" (IFCTEXT)
    TFM11FkSys = "275" (IFCTEXT)
  Text | properties | on 181 objects (173 IFCWALLSTANDARDCASE, 8 IFCWALL)
    TFM Samlet = "+135.01=232.001" (IFCTEXT)
    TFM Systemløpenummer = "001" (IFCTEXT)
    TFM11FkSys = "232" (IFCTEXT)
  Text | properties | on 111 objects (111 IFCCOVERING)
    NOBB = "710033" (IFCTEXT)
    TFM Samlet = "+135.01=257.007" (IFCTEXT)
    TFM Systemløpenummer = "007" (IFCTEXT)
    TFM11FkSys = "257" (IFCTEXT)
  Text | properties | on 94 objects (94 IFCCOVERING)
    NOBB = "49058172" (IFCTEXT)
    TFM Samlet = "+135.01=257.002" (IFCTEXT)
    TFM Systemløpenummer = "002" (IFCTEXT)
    TFM11FkSys = "257" (IFCTEXT)
  Text | properties | on 88 objects (88 IFCWALLSTANDARDCASE)
    TFM Samlet = "+135.01=242." (IFCTEXT)
    TFM11FkSys = "242" (IFCTEXT)
  Text | properties | on 84 objects (84 IFCSPACE)
    NOBB = "47194957" (IFCTEXT)
    TFM Komponentkode = "EB" (IFCTEXT)
    TFM Komponentløpenummer = "001" (IFCTEXT)
    TFM Samlet = "+135.01=255.001-EB001T" (IFCTEXT)
    TFM Systemløpenummer = "001" (IFCTEXT)
    TFM Typeunik = "T" (IFCTEXT)
    TFM11FkSys = "255" (IFCTEXT)
  Text: 344 more contents on 2469 objects not shown
  Other | properties | on 286 objects (286 IFCFURNISHINGELEMENT)
    Category = "Casework" (IFCLABEL)
    Family = "Lockers x 2: Elevskap" (IFCLABEL)
    Family and Type = "Lockers x 2: Elevskap" (IFCLABEL)
    Type = "Lockers x 2: Elevskap" (IFCLABEL)
    Type Id = "Lockers x 2: Elevskap" (IFCLABEL)
  Other | properties | on 282 objects (282 IFCSPACE)
    Category = "Rooms" (IFCLABEL)
    Phase Id = "New Construction" (IFCLABEL)
  Other | properties | on 160 objects (160 IFCMEMBER)
    Category = "Curtain Wall Mullions" (IFCLABEL)
    Family = "Rectangular Mullion: 50x125 Skjermtak" (IFCLABEL)
    Family and Type = "Rectangular Mullion: 50x125 Skjermtak" (IFCLABEL)
    Host Id = "Sloped Glazing: Tak glass - Baldakintak" (IFCLABEL)
    Type = "Rectangular Mullion: 50x125 Skjermtak" (IFCLABEL)
    Type Id = "Rectangular Mullion: 50x125 Skjermtak" (IFCLABEL)
  Other | properties | on 111 objects (111 IFCCOVERING)
    Category = "Ceilings" (IFCLABEL)
    Family = "Compound Ceiling: Himling System 600x1200" (IFCLABEL)
    Family and Type = "Compound Ceiling: Himling System 600x1200" (IFCLABEL)
    Type = "Compound Ceiling: Himling System 600x1200" (IFCLABEL)
    Type Id = "Compound Ceiling: Himling System 600x1200" (IFCLABEL)
  Other | properties | on 94 objects (94 IFCCOVERING)
    Category = "Ceilings" (IFCLABEL)
    Family = "Compound Ceiling: Himling System 600x600" (IFCLABEL)
    Family and Type = "Compound Ceiling: Himling System 600x600" (IFCLABEL)
    Type = "Compound Ceiling: Himling System 600x600" (IFCLABEL)
    Type Id = "Compound Ceiling: Himling System 600x600" (IFCLABEL)
  Other | properties | on 87 objects (87 IFCOPENINGELEMENT)
    Category = "<Sketch>" (IFCLABEL)
  Other | properties | on 74 objects (74 IFCMEMBER)
    Category = "Curtain Wall Mullions" (IFCLABEL)
    Family = "Rectangular Mullion: 50x180 Glassfasade 6-7" (IFCLABEL)
    Family and Type = "Rectangular Mullion: 50x180 Glassfasade 6-7" (IFCLABEL)
    Host Id = "Curtain Wall: Glassfasade 6" (IFCLABEL)
    Type = "Rectangular Mullion: 50x180 Glassfasade 6-7" (IFCLABEL)
    Type Id = "Rectangular Mullion: 50x180 Glassfasade 6-7" (IFCLABEL)
  Other | properties | on 65 objects (65 IFCFLOWCONTROLLER)
    AssetIdentifier = "n/a" (IFCTEXT)
    Barcode = "n/a" (IFCTEXT)
    Category = "Plumbing Fixtures" (IFCLABEL)
    Family = "1724FT(2013): Blandebatteri berøringsfri 1724FT" (IFCLABEL)
    Family and Type = "1724FT(2013): Blandebatteri berøringsfri 1724FT" (IFCLABEL)
    InstallationDate = "n/a" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    Type = "1724FT(2013): Blandebatteri berøringsfri 1724FT" (IFCLABEL)
    Type Id = "1724FT(2013): Blandebatteri berøringsfri 1724FT" (IFCLABEL)
    WarrantyStartDate = "n/a" (IFCTEXT)
  Other: 906 more contents on 3908 objects not shown
  Pset_SpaceCommon | properties | on 3 objects (3 IFCSPACE)
    Category = "Areas" (IFCLABEL)
    Reference = "Area 4" (IFCIDENTIFIER)
  Pset_SpaceCommon | properties | on 2 objects (2 IFCSPACE)
    Category = "Areas" (IFCLABEL)
    Reference = "Area 14" (IFCIDENTIFIER)
  Pset_SpaceCommon | properties | on 2 objects (2 IFCSPACE)
    Category = "Areas" (IFCLABEL)
    Reference = "Area 3" (IFCIDENTIFIER)
  Pset_SpaceCommon | properties | on 2 objects (2 IFCSPACE)
    Category = "Rooms" (IFCLABEL)
    CeilingCovering = "Støvbundet" (IFCLABEL)
    FloorCovering = "-" (IFCLABEL)
    Reference = "sjakt 02055" (IFCIDENTIFIER)
  Pset_SpaceCommon | properties | on 2 objects (2 IFCSPACE)
    Category = "Areas" (IFCLABEL)
    Reference = "Area 6" (IFCIDENTIFIER)
  Pset_SpaceCommon | properties | on 2 objects (2 IFCSPACE)
    Category = "Areas" (IFCLABEL)
    Reference = "Area 7" (IFCIDENTIFIER)
  Pset_SpaceCommon | properties | on 1 object (1 IFCSPACE)
    Category = "Areas" (IFCLABEL)
    Reference = "Area 15" (IFCIDENTIFIER)
  Pset_SpaceCommon | properties | on 1 object (1 IFCSPACE)
    Category = "Areas" (IFCLABEL)
    Reference = "Area 17" (IFCIDENTIFIER)
  Pset_SpaceCommon: 292 more contents on 292 objects not shown
  BaseQuantities | quantities | on 99 objects (99 IFCDOOR)
    Area = 2.85073200000162 [SQUARE_METRE]
    Height = 2090. [MILLI METRE]
    Width = 990. [MILLI METRE]
  BaseQuantities | quantities | on 74 objects (74 IFCMEMBER)
    CrossSectionArea = 150.699051233016 [SQUARE_METRE]
    Length = 20858.0001706681 [MILLI METRE]
  BaseQuantities | quantities | on 69 objects (69 IFCDOOR)
    Area = 2.74290800000015 [SQUARE_METRE]
    Height = 2090. [MILLI METRE]
    Width = 990. [MILLI METRE]
  BaseQuantities | quantities | on 59 objects (59 IFCMEMBER)
    CrossSectionArea = 138.422511233018 [SQUARE_METRE]
    Length = 20858.000170668 [MILLI METRE]
  BaseQuantities | quantities | on 51 objects (51 IFCOPENINGELEMENT)
    Depth = 121. [MILLI METRE]
    Height = 1009.99999999998 [MILLI METRE]
    Width = 2100. [MILLI METRE]
  BaseQuantities | quantities | on 44 objects (44 IFCWINDOW)
    Area = 3.10628399999968 [SQUARE_METRE]
    Height = 2090. [MILLI METRE]
    Width = 1190. [MILLI METRE]
  BaseQuantities | quantities | on 40 objects (40 IFCMEMBER)
    CrossSectionArea = 29.1208499999765 [SQUARE_METRE]
    Length = 9804.99999999995 [MILLI METRE]
  BaseQuantities | quantities | on 36 objects (36 IFCDOOR)
    Area = 2.28010800000015 [SQUARE_METRE]
    Height = 2090. [MILLI METRE]
    Width = 790. [MILLI METRE]
  BaseQuantities: 2142 more contents on 3467 objects not shown
  Constraints | properties | on 1073 objects (829 IFCMEMBER, 230 IFCPLATE, 8 IFCDOOR, 6 IFCSPACE)
    Level = "Level: Plan 01" (IFCLABEL)
  Constraints | properties | on 258 objects (172 IFCFURNISHINGELEMENT, 68 IFCBUILDINGELEMENTPROXY, 18 IFCFLOWTERMINAL)
    Host = "Level : Plan 01" (IFCTEXT)
    Level = "Level: Plan 01" (IFCLABEL)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 219 objects (172 IFCFURNISHINGELEMENT, 45 IFCBUILDINGELEMENTPROXY, 2 IFCFLOWTERMINAL)
    Host = "Level : Plan 02" (IFCTEXT)
    Level = "Level: Plan 02" (IFCLABEL)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 178 objects (134 IFCDOOR, 34 IFCWINDOW, 10 IFCOPENINGELEMENT)
    Level = "Level: Plan 01" (IFCLABEL)
    Sill Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 172 objects (101 IFCDOOR, 68 IFCWINDOW, 3 IFCOPENINGELEMENT)
    Level = "Level: Plan 02" (IFCLABEL)
    Sill Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 135 objects (69 IFCOPENINGELEMENT, 66 IFCWINDOW)
    Level = "Level: Plan 02" (IFCLABEL)
    Sill Height = 800. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 94 objects (94 IFCWALLSTANDARDCASE)
    Base Constraint = "Level: Plan 01" (IFCLABEL)
    Base Extension Distance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Base Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Base is Attached = FALSE (IFCBOOLEAN)
    Location Line = "Wall Centerline" (IFCIDENTIFIER)
    Related to Mass = FALSE (IFCBOOLEAN)
    Room Bounding = TRUE (IFCBOOLEAN)
    Top Constraint = "Level: Plan 02" (IFCLABEL)
    Top Extension Distance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top is Attached = TRUE (IFCBOOLEAN)
    Unconnected Height = 3999.99999999761 (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 84 objects (62 IFCFURNISHINGELEMENT, 22 IFCBUILDINGELEMENTPROXY)
    Host = "Level : Plan 03" (IFCTEXT)
    Level = "Level: Plan 03" (IFCLABEL)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints: 740 more contents on 2761 objects not shown
  Dimensions | properties | on 286 objects (286 IFCFURNISHINGELEMENT)
    Area = 3.01332291335339 (IFCAREAMEASURE) [SQUARE_METRE]
    Depth = 450. (IFCLENGTHMEASURE) [MILLI METRE]
    Locker Height = 1700. (IFCLENGTHMEASURE) [MILLI METRE]
    Plinth Height = 100. (IFCLENGTHMEASURE) [MILLI METRE]
    Plinth Setback = 50. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 0.0553555851033449 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Width = 300. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 98 objects (98 IFCMEMBER)
    Area = 0.129506000000017 (IFCAREAMEASURE) [SQUARE_METRE]
    Length = 578.600000000082 (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 0.00462880000000066 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 89 objects (89 IFCDOOR)
    Area = 2.85073200000162 (IFCAREAMEASURE) [SQUARE_METRE]
    Joint = 10. (IFCLENGTHMEASURE) [MILLI METRE]
    Joint Bottom = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Placement = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 0.0550243920000606 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 73 objects (73 IFCMEMBER)
    Area = 0.34445 (IFCAREAMEASURE) [SQUARE_METRE]
    Length = 1300. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 0.013455 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 57 objects (57 IFCMEMBER)
    Area = 0.151700000000001 (IFCAREAMEASURE) [SQUARE_METRE]
    Length = 550.000000000002 (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 0.00569250000000002 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 56 objects (56 IFCBUILDINGELEMENTPROXY)
    Area = 2.69119999999998 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.0916479999999994 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 54 objects (54 IFCMEMBER)
    Area = 0.559566601583655 (IFCAREAMEASURE) [SQUARE_METRE]
    Length = 2626.50762658883 (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 0.0210120610127107 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 53 objects (53 IFCMEMBER)
    Area = 0.24165 (IFCAREAMEASURE) [SQUARE_METRE]
    Length = 900. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 0.009315 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions: 2566 more contents on 4263 objects not shown
  Identity Data | properties | on 1727 objects (435 IFCMEMBER, 416 IFCWALLSTANDARDCASE, 297 IFCFURNISHINGELEMENT, 136 IFCBUILDINGELEMENTPROXY)
    Design Option = "Main Model" (IFCTEXT)
  Identity Data | properties | on 63 objects (56 IFCWALLSTANDARDCASE, 7 IFCCURTAINWALL)
    Comments = "x" (IFCTEXT)
  Identity Data | properties | on 61 objects (47 IFCWALLSTANDARDCASE, 13 IFCCURTAINWALL, 1 IFCPLATE)
    Comments = "x" (IFCTEXT)
    Design Option = "Main Model" (IFCTEXT)
  Identity Data | properties | on 23 objects (22 IFCWALLSTANDARDCASE, 1 IFCPLATE)
    Comments = "" (IFCTEXT)
    Design Option = "Main Model" (IFCTEXT)
  Identity Data | properties | on 22 objects (21 IFCWALLSTANDARDCASE, 1 IFCWALL)
    Comments = "" (IFCTEXT)
  Identity Data | properties | on 4 objects (3 IFCOPENINGELEMENT, 1 IFCDOOR)
    Comments = "Se XX A 200 61 537 for skjema" (IFCTEXT)
    Design Option = "Main Model" (IFCTEXT)
    Mark = "01002.2" (IFCTEXT)
    NTI_DoorSwing = "-" (IFCTEXT)
    NTI_DoorType = "DU" (IFCTEXT)
    NTI_ExteriorDoorDirection = "INN" (IFCTEXT)
    NTI_HostWallWidth = "279" (IFCTEXT)
    NTI_RoomAssociation = "01002" (IFCTEXT)
  Identity Data | properties | on 3 objects (2 IFCOPENINGELEMENT, 1 IFCDOOR)
    Comments = "Se XX A 200 61 537 for skjema" (IFCTEXT)
    Mark = "01001.1" (IFCTEXT)
    NTI_DoorSwing = "-" (IFCTEXT)
    NTI_DoorType = "DU" (IFCTEXT)
    NTI_ExteriorDoorDirection = "UT" (IFCTEXT)
    NTI_HostWallWidth = "312" (IFCTEXT)
    NTI_RoomAssociation = "01001" (IFCTEXT)
    Veggtykkelse = "" (IFCTEXT)
  Identity Data | properties | on 3 objects (2 IFCOPENINGELEMENT, 1 IFCDOOR)
    Comments = "Glass i dørblad" (IFCTEXT)
    Mark = "01061.2" (IFCTEXT)
    NTI_DoorSwing = "H" (IFCTEXT)
    NTI_DoorType = "DI" (IFCTEXT)
    NTI_HostWallWidth = "134" (IFCTEXT)
    NTI_RoomAssociation = "01061" (IFCTEXT)
  Identity Data: 1657 more contents on 1313 objects not shown
  Energy Analysis | properties | on 282 objects (282 IFCSPACE)
    Actual Lighting Load = 0. (IFCPOWERMEASURE) [WATT]
    Actual Lighting Load per area = 0. (IFCREAL)
    Actual Power Load = 0. (IFCPOWERMEASURE) [WATT]
    Actual Power Load per area = 0. (IFCREAL)
    Area per Person = 28.5714285714286 (IFCAREAMEASURE) [SQUARE_METRE]
    Base Lighting Load on = "By Space Type" (IFCIDENTIFIER)
    Base Power Load on = "By Space Type" (IFCIDENTIFIER)
    Heat Load Values = "By Space Type" (IFCIDENTIFIER)
    Latent Heat Gain per person = 630.91814901261 (IFCREAL)
    Lighting Load Units = "Power Density" (IFCIDENTIFIER)
    Number of People = 0. (IFCREAL)
    Plenum Lighting Contribution = 0.2 (IFCREAL)
    Power Load Units = "Power Density" (IFCIDENTIFIER)
    Sensible Heat Gain per person = 788.647686265762 (IFCREAL)
    Specified Lighting Load = 0. (IFCPOWERMEASURE) [WATT]
    Specified Lighting Load per area = 10.7639104167097 (IFCREAL)
    Specified Power Load = 0. (IFCPOWERMEASURE) [WATT]
    Specified Power Load per area = 13.9930835417226 (IFCREAL)
    Total Heat Gain per person = 1419.56583527837 (IFCREAL)
  Phasing | properties | on 4655 objects (1041 IFCWALLSTANDARDCASE, 852 IFCMEMBER, 627 IFCFURNISHINGELEMENT, 310 IFCDOOR)
    Phase Created = "New Construction" (IFCLABEL)
  Phasing | properties | on 282 objects (282 IFCSPACE)
    Phase = "New Construction" (IFCLABEL)
  Phasing | properties | on 12 type objects
    Expected Lifespan (Years) = 0 (IFCINTEGER)
    Installation Phase = "" (IFCTEXT)
    Maintenance Schedule (Months) = 0 (IFCINTEGER)
    Warranty Duration (Years) = 0 (IFCINTEGER)
  Structural | properties | on 1069 objects (1019 IFCWALLSTANDARDCASE, 34 IFCCURTAINWALL, 16 IFCWALL)
    Enable Analytical Model = FALSE (IFCBOOLEAN)
    Structural = FALSE (IFCBOOLEAN)
    Structural Usage = "Non-bearing" (IFCIDENTIFIER)
  Structural | properties | on 83 objects (83 IFCSLAB)
    Enable Analytical Model = FALSE (IFCBOOLEAN)
    Structural = FALSE (IFCBOOLEAN)
  Structural | properties | on 22 objects (22 IFCWALLSTANDARDCASE)
    Enable Analytical Model = TRUE (IFCBOOLEAN)
    Rebar Cover - Exterior Face = "Rebar Cover Settings: Rebar Cover 1" (IFCLABEL)
    Rebar Cover - Interior Face = "Rebar Cover Settings: Rebar Cover 1" (IFCLABEL)
    Rebar Cover - Other Faces = "Rebar Cover Settings: Rebar Cover 1" (IFCLABEL)
    Structural = TRUE (IFCBOOLEAN)
    Structural Usage = "Bearing" (IFCIDENTIFIER)
  Structural | properties | on 9 objects (9 IFCSTAIR)
    Rebar Cover = "Rebar Cover Settings: Rebar Cover 1" (IFCLABEL)
  Structural | properties | on 6 objects (6 IFCBEAM)
    Cut Length = 2099.99999999999 (IFCLENGTHMEASURE) [MILLI METRE]
    Enable Analytical Model = TRUE (IFCBOOLEAN)
    Rebar Cover - Bottom Face = "Rebar Cover Settings: Rebar Cover 1" (IFCLABEL)
    Rebar Cover - Other Faces = "Rebar Cover Settings: Rebar Cover 1" (IFCLABEL)
    Rebar Cover - Top Face = "Rebar Cover Settings: Rebar Cover 1" (IFCLABEL)
    Structural Usage = "Other" (IFCIDENTIFIER)
  Structural | properties | on 5 objects (5 IFCBEAM)
    Cut Length = 2701.00000000003 (IFCLENGTHMEASURE) [MILLI METRE]
    Enable Analytical Model = TRUE (IFCBOOLEAN)
    Rebar Cover - Bottom Face = "Rebar Cover Settings: Rebar Cover 1" (IFCLABEL)
    Rebar Cover - Other Faces = "Rebar Cover Settings: Rebar Cover 1" (IFCLABEL)
    Rebar Cover - Top Face = "Rebar Cover Settings: Rebar Cover 1" (IFCLABEL)
    Structural Usage = "Other" (IFCIDENTIFIER)
  Structural | properties | on 3 objects (3 IFCBEAM)
    Cut Length = 2999.99999999999 (IFCLENGTHMEASURE) [MILLI METRE]
    Enable Analytical Model = TRUE (IFCBOOLEAN)
    Rebar Cover - Bottom Face = "Rebar Cover Settings: Rebar Cover 1" (IFCLABEL)
    Rebar Cover - Other Faces = "Rebar Cover Settings: Rebar Cover 1" (IFCLABEL)
    Rebar Cover - Top Face = "Rebar Cover Settings: Rebar Cover 1" (IFCLABEL)
    Structural Usage = "Other" (IFCIDENTIFIER)
  Structural | properties | on 3 objects (3 IFCBEAM)
    Cut Length = 11086.5808776411 (IFCLENGTHMEASURE) [MILLI METRE]
    Enable Analytical Model = TRUE (IFCBOOLEAN)
    Rebar Cover - Bottom Face = "Rebar Cover Settings: Rebar Cover 1" (IFCLABEL)
    Rebar Cover - Other Faces = "Rebar Cover Settings: Rebar Cover 1" (IFCLABEL)
    Rebar Cover - Top Face = "Rebar Cover Settings: Rebar Cover 1" (IFCLABEL)
    Structural Usage = "Other" (IFCIDENTIFIER)
  Structural: 19 more contents on 23 objects not shown
  Materials and Finishes | properties | on 214 objects (214 IFCFURNISHINGELEMENT)
    Locker 1 = "_White" (IFCLABEL)
    Locker 2 = "_White" (IFCLABEL)
  Materials and Finishes | properties | on 165 objects (83 IFCWINDOW, 82 IFCOPENINGELEMENT)
    Farge karm = "NCS S 0502-Y" (IFCTEXT)
  Materials and Finishes | properties | on 121 objects (120 IFCWINDOW, 1 IFCOPENINGELEMENT)
    Farge karm = "NCS S 3502-Y" (IFCTEXT)
  Materials and Finishes | properties | on 104 objects (100 IFCDOOR, 4 IFCOPENINGELEMENT)
    Finish = "F7902 Iron" (IFCTEXT)
    Frame Material = "NCS S 3502-Y" (IFCTEXT)
    Kantlist = "NCS S 2500-N" (IFCTEXT)
  Materials and Finishes | properties | on 104 objects (52 IFCOPENINGELEMENT, 52 IFCWINDOW)
    Farge karm = "NCS S 0502-Y" (IFCTEXT)
    Sidefelt = "N_Windows - Vinduspanel" (IFCLABEL)
  Materials and Finishes | properties | on 42 objects (42 IFCFURNISHINGELEMENT)
    Locker 1 = "Skapdør 2" (IFCLABEL)
    Locker 2 = "Gul avdeling" (IFCLABEL)
  Materials and Finishes | properties | on 27 objects (27 IFCDOOR)
    Finish = "F7934 Pearl" (IFCTEXT)
    Frame Material = "NCS S 1002-Y" (IFCTEXT)
    Kantlist = "NCS S 0502-G50Y" (IFCTEXT)
    Material Panel = "Lys grå" (IFCLABEL)
  Materials and Finishes | properties | on 25 objects (25 IFCDOOR)
    Finish = "RAL 7044" (IFCTEXT)
    Frame Material = "RAL 7044" (IFCTEXT)
  Materials and Finishes: 87 more contents on 231 objects not shown
  Pset_WallCommon | properties | on 42 objects (35 IFCWALLSTANDARDCASE, 7 IFCWALL)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    FireRating = "" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "IVSP 84mm SPILEVEGG" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 41 objects (41 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    FireRating = "" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "YV 18.1 136 Takhatt" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 36 objects (36 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    FireRating = "" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "TGF" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 32 objects (32 IFCWALLSTANDARDCASE)
    AcousticRating = "" (IFCLABEL)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    FireRating = "" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Flis" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 28 objects (28 IFCWALLSTANDARDCASE)
    AcousticRating = "44dB" (IFCLABEL)
    ExtendToStructure = TRUE (IFCBOOLEAN)
    FireRating = "" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "IVA 1.1 121mm 44dB (H-95-H)" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 28 objects (28 IFCWALLSTANDARDCASE)
    AcousticRating = "48dB" (IFCLABEL)
    ExtendToStructure = TRUE (IFCBOOLEAN)
    FireRating = "" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "IVA 3.3 145mm 48dB (RN-95-NR)" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 27 objects (27 IFCWALLSTANDARDCASE)
    ExtendToStructure = TRUE (IFCBOOLEAN)
    FireRating = "EI 60" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "IVA 3.3 145mm EI60 (RN-95-NR)" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 27 objects (27 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    FireRating = "" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "YV 7.3 410mm rød platekledning" (IFCIDENTIFIER)
  Pset_WallCommon: 252 more contents on 796 objects not shown
  Pset_TFM | properties | on 846 objects (661 IFCMEMBER, 176 IFCPLATE, 9 IFCBUILDINGELEMENTPROXY)
    TFM11FkSys = "" (IFCTEXT)
  Pset_TFM | properties | on 506 objects (496 IFCWALLSTANDARDCASE, 10 IFCOPENINGELEMENT)
    TFM Samlet = "+135.01=242.001" (IFCTEXT)
    TFM Systemløpenummer = "001" (IFCTEXT)
    TFM11FkSys = "242" (IFCTEXT)
  Pset_TFM | properties | on 371 objects (190 IFCOPENINGELEMENT, 173 IFCWALLSTANDARDCASE, 8 IFCWALL)
    TFM Samlet = "+135.01=232.001" (IFCTEXT)
    TFM Systemløpenummer = "001" (IFCTEXT)
    TFM11FkSys = "232" (IFCTEXT)
  Pset_TFM | properties | on 286 objects (286 IFCFURNISHINGELEMENT)
    TFM Komponentkode = "FS" (IFCTEXT)
    TFM Komponentløpenummer = "014" (IFCTEXT)
    TFM Samlet = "+135.01=275.001-FS014T" (IFCTEXT)
    TFM Systemløpenummer = "001" (IFCTEXT)
    TFM Typeunik = "T" (IFCTEXT)
    TFM11FkSys = "275" (IFCTEXT)
  Pset_TFM | properties | on 111 objects (111 IFCCOVERING)
    TFM Samlet = "+135.01=257.007" (IFCTEXT)
    TFM Systemløpenummer = "007" (IFCTEXT)
    TFM11FkSys = "257" (IFCTEXT)
  Pset_TFM | properties | on 106 objects (88 IFCWALLSTANDARDCASE, 18 IFCOPENINGELEMENT)
    TFM Samlet = "+135.01=242." (IFCTEXT)
    TFM11FkSys = "242" (IFCTEXT)
  Pset_TFM | properties | on 94 objects (94 IFCCOVERING)
    TFM Samlet = "+135.01=257.002" (IFCTEXT)
    TFM Systemløpenummer = "002" (IFCTEXT)
    TFM11FkSys = "257" (IFCTEXT)
  Pset_TFM | properties | on 84 objects (81 IFCWALLSTANDARDCASE, 3 IFCOPENINGELEMENT)
    TFM Samlet = "+135.01=245.001" (IFCTEXT)
    TFM Systemløpenummer = "001" (IFCTEXT)
    TFM11FkSys = "245" (IFCTEXT)
  Pset_TFM: 286 more contents on 2115 objects not shown
  Pset_SlabCommon | properties | on 25 objects (25 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Flis - trapp" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 7 objects (7 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Betong 200mm" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 7 objects (7 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Betong 200mm" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 4 objects (4 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Betongdekke 320 + 80 påstøp + 10 avretting" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 4 objects (4 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Fotskraperist" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 4 objects (4 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Repo som trappeløp" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 3 objects (3 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Betongdekke 320 + 80 påstøp + 10 avretting" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 3 objects (3 IFCSLAB)
    IsExternal = TRUE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Tak betong 320 + 150" (IFCIDENTIFIER)
  Pset_SlabCommon: 45 more contents on 69 objects not shown
  Pset_CurtainWallCommon | properties | on 13 objects (13 IFCCURTAINWALL)
    FireRating = "" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "YV 100 S" (IFCIDENTIFIER)
  Pset_CurtainWallCommon | properties | on 1 object (1 IFCCURTAINWALL)
    FireRating = "" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Glassfasade 7" (IFCIDENTIFIER)
  Pset_CurtainWallCommon | properties | on 1 object (1 IFCCURTAINWALL)
    FireRating = "" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Glassfasade 6" (IFCIDENTIFIER)
  Pset_CurtainWallCommon | properties | on 1 object (1 IFCCURTAINWALL)
    AcousticRating = "38 dB" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "GFA 2 38dB" (IFCIDENTIFIER)
  Pset_CurtainWallCommon | properties | on 1 object (1 IFCCURTAINWALL)
    AcousticRating = "38 dB" (IFCLABEL)
    FireRating = "EI 30" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "GFA 1 38dB EI30S" (IFCIDENTIFIER)
  Pset_CurtainWallCommon | properties | on 1 object (1 IFCCURTAINWALL)
    FireRating = "" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Glassfasade 5e" (IFCIDENTIFIER)
  Pset_CurtainWallCommon | properties | on 1 object (1 IFCCURTAINWALL)
    FireRating = "" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Glassfasade 4c" (IFCIDENTIFIER)
  Pset_CurtainWallCommon | properties | on 1 object (1 IFCCURTAINWALL)
    FireRating = "" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Glassfasade 3a" (IFCIDENTIFIER)
  Pset_CurtainWallCommon: 14 more contents on 14 objects not shown
  Pset_PlateCommon | properties | on 100 objects (100 IFCPLATE)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Glass - profilstørrelse 120" (IFCIDENTIFIER)
  Pset_PlateCommon | properties | on 53 objects (53 IFCPLATE)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Glass - 13mm" (IFCIDENTIFIER)
  Pset_PlateCommon | properties | on 43 objects (43 IFCPLATE)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Glass - CW300" (IFCIDENTIFIER)
  Pset_PlateCommon | properties | on 17 objects (17 IFCPLATE)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Tett felt - CW100" (IFCIDENTIFIER)
  Pset_PlateCommon | properties | on 12 objects (12 IFCPLATE)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Glass - aula" (IFCIDENTIFIER)
  Pset_PlateCommon | properties | on 2 objects (2 IFCPLATE)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Tett felt - 180profiler" (IFCIDENTIFIER)
  Pset_PlateCommon | properties | on 2 objects (2 IFCPLATE)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Tett felt - aula" (IFCIDENTIFIER)
  Pset_PlateCommon | properties | on 1 object (1 IFCPLATE)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Glass - profilstørrelse 120" (IFCIDENTIFIER)
  Pset_MemberCommon | properties | on 98 objects (98 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "50x125 Skjermtak" (IFCIDENTIFIER)
    Span = 578.600000000082 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_MemberCommon | properties | on 73 objects (73 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "50x120 Glassfasade 1-5" (IFCIDENTIFIER)
    Span = 1300. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_MemberCommon | properties | on 57 objects (57 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "50x120 Glassfasade 1-5" (IFCIDENTIFIER)
    Span = 550.000000000002 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_MemberCommon | properties | on 55 objects (55 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "50x120 Glassfasade 1-5" (IFCIDENTIFIER)
    Span = 900. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_MemberCommon | properties | on 54 objects (54 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "50x125 Skjermtak" (IFCIDENTIFIER)
    Span = 2626.50762658883 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_MemberCommon | properties | on 49 objects (49 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "50x120 Glassfasade 1-5" (IFCIDENTIFIER)
    Span = 769.999999997085 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_MemberCommon | properties | on 31 objects (31 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "50x120 Glassfasade 1-5" (IFCIDENTIFIER)
    Span = 719.999999997085 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_MemberCommon | properties | on 27 objects (27 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "50x120 Glassfasade 1-5" (IFCIDENTIFIER)
    Span = 449.999999999979 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_MemberCommon: 141 more contents on 408 objects not shown
  Horizontal Grid | properties | on 34 objects (34 IFCCURTAINWALL)
    Angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Justification = "Beginning" (IFCIDENTIFIER)
    Number = 4 (IFCINTEGER)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Horizontal Grid | properties | on 22 type objects
    Adjust for Mullion Size = FALSE (IFCBOOLEAN)
    Layout = "None" (IFCIDENTIFIER)
    Spacing = 2500. (IFCLENGTHMEASURE) [MILLI METRE]
  Vertical Grid | properties | on 15 objects (15 IFCCURTAINWALL)
    Angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Justification = "Beginning" (IFCIDENTIFIER)
    Number = 4 (IFCINTEGER)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Vertical Grid | properties | on 5 objects (5 IFCCURTAINWALL)
    Angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Justification = "Beginning" (IFCIDENTIFIER)
    Number = 20 (IFCINTEGER)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Vertical Grid | properties | on 4 objects (4 IFCCURTAINWALL)
    Angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Justification = "Beginning" (IFCIDENTIFIER)
    Number = 15 (IFCINTEGER)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Vertical Grid | properties | on 3 objects (3 IFCCURTAINWALL)
    Angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Justification = "Beginning" (IFCIDENTIFIER)
    Number = 10 (IFCINTEGER)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Vertical Grid | properties | on 3 objects (3 IFCCURTAINWALL)
    Angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Justification = "Beginning" (IFCIDENTIFIER)
    Number = 7 (IFCINTEGER)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Vertical Grid | properties | on 2 objects (2 IFCCURTAINWALL)
    Angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Justification = "Beginning" (IFCIDENTIFIER)
    Number = 11 (IFCINTEGER)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Vertical Grid | properties | on 2 objects (2 IFCCURTAINWALL)
    Angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Justification = "Beginning" (IFCIDENTIFIER)
    Number = 9 (IFCINTEGER)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Vertical Grid | properties | on 19 type objects
    Adjust for Mullion Size = FALSE (IFCBOOLEAN)
    Layout = "None" (IFCIDENTIFIER)
    Spacing = 1500. (IFCLENGTHMEASURE) [MILLI METRE]
  Vertical Grid: 2 more contents on 0 objects not shown
  Construction | properties | on 26 objects (26 IFCBUILDINGELEMENTPROXY)
    Available Options = "as Specified" (IFCTEXT)
  Construction | properties | on 20 objects (20 IFCCOLUMN)
    Attachment Justification At Top = "Minimum Intersection" (IFCIDENTIFIER)
    Offset From Attachment At Top = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Construction | properties | on 9 objects (9 IFCSTAIRFLIGHT)
    Begin with Riser = TRUE (IFCBOOLEAN)
    End with Riser = FALSE (IFCBOOLEAN)
  Construction | properties | on 7 objects (5 IFCOPENINGELEMENT, 2 IFCDOOR)
    Automatic Lock = FALSE (IFCBOOLEAN)
    Lateral pillar = FALSE (IFCBOOLEAN)
    Lock NO = TRUE (IFCBOOLEAN)
    Manual Lock = FALSE (IFCBOOLEAN)
    Normal Guide = FALSE (IFCBOOLEAN)
    Safety Control Guide = FALSE (IFCBOOLEAN)
    Safety Guide (optional on A20-2 and A20-2R) = FALSE (IFCBOOLEAN)
  Construction | properties | on 7 objects (7 IFCSTAIRFLIGHT)
    Begin with Riser = TRUE (IFCBOOLEAN)
    End with Riser = TRUE (IFCBOOLEAN)
    Extend Below Riser Base = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Construction | properties | on 5 objects (5 IFCROOF)
    Fascia Depth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Maximum Ridge Height = 8349.99999999973 (IFCLENGTHMEASURE) [MILLI METRE]
    Rafter Cut = "Plumb Cut" (IFCIDENTIFIER)
  Construction | properties | on 4 objects (4 IFCROOF)
    Fascia Depth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Maximum Ridge Height = 12180. (IFCLENGTHMEASURE) [MILLI METRE]
    Rafter Cut = "Plumb Cut" (IFCIDENTIFIER)
  Construction | properties | on 4 objects (4 IFCROOF)
    Fascia Depth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Maximum Ridge Height = 8199.99999999973 (IFCLENGTHMEASURE) [MILLI METRE]
    Rafter Cut = "Plumb Cut" (IFCIDENTIFIER)
  Construction: 118 more contents on 30 objects not shown
  Electrical - Loads | properties | on 292 objects (292 IFCBUILDINGELEMENTPROXY)
    Circuit Number = "" (IFCTEXT)
    Panel = "" (IFCTEXT)
  Electrical - Loads | properties | on 7 objects (5 IFCOPENINGELEMENT, 2 IFCDOOR)
    Power supply = 220. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
    Power supply on request 120V = FALSE (IFCBOOLEAN)
    Standard Power Supply 220V = TRUE (IFCBOOLEAN)
  Graphics | properties | on 12 objects (10 IFCWALLSTANDARDCASE, 2 IFCWALL)
    Center Mark Visible = FALSE (IFCBOOLEAN)
  Graphics | properties | on 7 objects (5 IFCOPENINGELEMENT, 2 IFCDOOR)
    Closed = TRUE (IFCBOOLEAN)
    Open = FALSE (IFCBOOLEAN)
    Opening % Control = 0 (IFCINTEGER)
  Graphics | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Horizontal Align = "Left" (IFCIDENTIFIER)
    Text = "NITTEDAL UNGDOMSSKOLE" (IFCTEXT)
  Graphics | properties | on 1 object (1 IFCSTAIR)
    Down arrow = FALSE (IFCBOOLEAN)
    Down label = FALSE (IFCBOOLEAN)
    Down text = "DN" (IFCTEXT)
    Show Up arrow in all views = FALSE (IFCBOOLEAN)
    Up arrow = FALSE (IFCBOOLEAN)
    Up label = FALSE (IFCBOOLEAN)
    Up text = "UP" (IFCTEXT)
  Graphics | properties | on 1 object (1 IFCSTAIR)
    Down arrow = FALSE (IFCBOOLEAN)
    Down label = FALSE (IFCBOOLEAN)
    Down text = "DN" (IFCTEXT)
    Show Up arrow in all views = FALSE (IFCBOOLEAN)
    Up arrow = TRUE (IFCBOOLEAN)
    Up label = FALSE (IFCBOOLEAN)
    Up text = "UP" (IFCTEXT)
  Graphics | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Horizontal Align = "Left" (IFCIDENTIFIER)
    Text = "bibliotek" (IFCTEXT)
  Graphics | properties | on 96 type objects
    Coarse Scale Fill Color = 8421504 (IFCINTEGER)
    Coarse Scale Fill Pattern = "<Solid fill>" (IFCLABEL)
  Graphics | properties | on 89 type objects
    Coarse Scale Fill Color = 0 (IFCINTEGER)
  Graphics: 9 more contents on 0 objects not shown
  Pset_DoorCommon | properties | on 64 objects (64 IFCDOOR)
    AcousticRating = "38dB" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "IDT 3.6 10x21M 38dB" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 25 objects (25 IFCDOOR)
    AcousticRating = "33dB" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "IDT 1.2 8x21M 33dB" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 23 objects (23 IFCDOOR)
    FireRating = "" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "IDT 2.1 10x21M" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 22 objects (22 IFCDOOR)
    AcousticRating = "33dB" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "IDT 3.3 10x21M 33dB" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 17 objects (17 IFCDOOR)
    AcousticRating = "33dB" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "IDT 2.3 10x21M 33dB" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 14 objects (14 IFCDOOR)
    AcousticRating = "" (IFCLABEL)
    FireRating = "EI 60S" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "IDT 5.2 15x21M EI60S" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 11 objects (11 IFCDOOR)
    AcousticRating = "38dB" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "IDT 2.6 10x21M 38dB" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 9 objects (9 IFCDOOR)
    FireRating = "" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "IDT 1.1 8x21M" (IFCIDENTIFIER)
  Pset_DoorCommon: 69 more contents on 125 objects not shown
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 478.918715747521 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "Tak betong 320 + 150" (IFCIDENTIFIER)
    TotalArea = 478.91871574752 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 273.429641403696 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "Tak betong 320 + påstøp 80 + 150" (IFCIDENTIFIER)
    TotalArea = 273.469859846584 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 240.356764315186 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "Tak betong 320 + 150" (IFCIDENTIFIER)
    TotalArea = 233.761518072121 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 9.81309999999982 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "Tak tre 223 - vindfang" (IFCIDENTIFIER)
    TotalArea = 9.81619659307669 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 286.056571847368 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "Tak betong 320 + påstøp 80 + 150" (IFCIDENTIFIER)
    TotalArea = 286.355193492095 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 8.65755274669471 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "Tak tre 246" (IFCIDENTIFIER)
    TotalArea = 8.65755274669477 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 46.3027000000013 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "Tak tre 246 + spiler" (IFCIDENTIFIER)
    TotalArea = 46.3027000000015 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 45.3896237769021 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "Tak betong 400 + 80 + 70" (IFCIDENTIFIER)
    TotalArea = 45.3896237769022 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_RoofCommon: 31 more contents on 31 objects not shown
  Pset_ManufacturerTypeInformation | properties | on 65 objects (65 IFCFLOWCONTROLLER)
    Manufacturer = "Oras" (IFCLABEL)
    ModelReference = "1724FT" (IFCLABEL)
  Pset_ManufacturerTypeInformation | properties | on 31 objects (31 IFCFLOWTERMINAL)
    ArticleNumber = "GB111522201211" (IFCIDENTIFIER)
    Manufacturer = "Villeroy & Boch Gustavsberg AB" (IFCLABEL)
  Pset_ManufacturerTypeInformation | properties | on 31 objects (31 IFCFLOWTERMINAL)
    ArticleNumber = "41005001" (IFCIDENTIFIER)
    Manufacturer = "Villeroy & Boch Gustavsberg AB" (IFCLABEL)
  Pset_ManufacturerTypeInformation | properties | on 27 objects (20 IFCFLOWTERMINAL, 7 IFCFLOWCONTROLLER)
    Manufacturer = "Oras" (IFCLABEL)
    ModelReference = "1038F" (IFCLABEL)
  Pset_ManufacturerTypeInformation | properties | on 26 objects (26 IFCBUILDINGELEMENTPROXY)
    Manufacturer = "Hadrian Inc." (IFCLABEL)
  Pset_ManufacturerTypeInformation | properties | on 26 objects (26 IFCBUILDINGELEMENTPROXY)
    ArticleNumber = "GB88171201" (IFCIDENTIFIER)
    Manufacturer = "Villeroy & Boch Gustavsberg AB" (IFCLABEL)
  Pset_ManufacturerTypeInformation | properties | on 17 objects (9 IFCFLOWTERMINAL, 8 IFCBUILDINGELEMENTPROXY)
    Manufacturer = "Revit" (IFCLABEL)
  Pset_ManufacturerTypeInformation | properties | on 13 objects (13 IFCFLOWTERMINAL)
    ArticleNumber = "GB111546201211" (IFCIDENTIFIER)
    Manufacturer = "Villeroy & Boch Gustavsberg AB" (IFCLABEL)
  Pset_ManufacturerTypeInformation: 5 more contents on 35 objects not shown
  Pset_DistributionFlowElementCommon | properties | on 65 objects (65 IFCFLOWCONTROLLER)
    Reference = "Blandebatteri berøringsfri 1724FT" (IFCIDENTIFIER)
  Pset_DistributionFlowElementCommon | properties | on 31 objects (31 IFCFLOWTERMINAL)
    Reference = "Vegghengt toalett" (IFCIDENTIFIER)
  Pset_DistributionFlowElementCommon | properties | on 31 objects (31 IFCFLOWTERMINAL)
    Reference = "Servant - Ecco 50x35" (IFCIDENTIFIER)
  Pset_DistributionFlowElementCommon | properties | on 20 objects (20 IFCFLOWTERMINAL)
    Reference = "Blandebatteri - Oras Saphira 1038F" (IFCIDENTIFIER)
  Pset_DistributionFlowElementCommon | properties | on 11 objects (11 IFCFLOWTERMINAL)
    Reference = "Gulvstående toalett - Nautic 1546" (IFCIDENTIFIER)
  Pset_DistributionFlowElementCommon | properties | on 11 objects (11 IFCFLOWTERMINAL)
    Reference = "Servant HCWC - 7119" (IFCIDENTIFIER)
  Pset_DistributionFlowElementCommon | properties | on 10 objects (10 IFCFLOWTERMINAL)
    Reference = "Kum kjøkken" (IFCIDENTIFIER)
  Pset_DistributionFlowElementCommon | properties | on 10 objects (10 IFCFLOWTERMINAL)
    Reference = "Utslagsvask" (IFCIDENTIFIER)
  Pset_DistributionFlowElementCommon: 28 more contents on 90 objects not shown
  Mechanical | properties | on 70 objects (70 IFCFLOWTERMINAL)
    System Abbreviation = "" (IFCTEXT)
    System Classification = "Sanitary" (IFCTEXT)
    System Name = "" (IFCTEXT)
  Mechanical | properties | on 65 objects (65 IFCFLOWCONTROLLER)
    System Abbreviation = "" (IFCTEXT)
    System Classification = "Domestic Hot Water,Domestic Cold Water,Power" (IFCTEXT)
    System Name = "" (IFCTEXT)
  Mechanical | properties | on 34 objects (20 IFCFLOWTERMINAL, 14 IFCFLOWCONTROLLER)
    System Abbreviation = "" (IFCTEXT)
    System Classification = "Domestic Hot Water,Domestic Cold Water" (IFCTEXT)
    System Name = "" (IFCTEXT)
  Mechanical | properties | on 31 objects (31 IFCFLOWTERMINAL)
    System Abbreviation = "" (IFCTEXT)
    System Classification = "Sanitary,Domestic Cold Water" (IFCTEXT)
    System Name = "" (IFCTEXT)
  Mechanical | properties | on 13 objects (13 IFCFLOWTERMINAL)
    System Abbreviation = "" (IFCTEXT)
    System Classification = "Domestic Cold Water,Sanitary" (IFCTEXT)
    System Name = "" (IFCTEXT)
  Mechanical | properties | on 9 objects (9 IFCFLOWCONTROLLER)
    System Abbreviation = "" (IFCTEXT)
    System Classification = "Domestic Cold Water" (IFCTEXT)
    System Name = "" (IFCTEXT)
  Mechanical | properties | on 3 type objects
    Connection Size = "G3/8" (IFCTEXT)
    DN Size = "DN15" (IFCTEXT)
    Flow = "Limitation option for maximum flow-rate" (IFCTEXT)
    Flow Rate At 300kPa With Flow Controller = 0.0282517333771909 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Installation Type = "Deck mounted" (IFCTEXT)
    Installation and Maintenance = "http://static.oras.com/manual/1724FT" (IFCTEXT)
    Intelligent After Flow Period = "2 s ±1 s" (IFCTEXT)
    Lever Handle = "Temperature control handle" (IFCTEXT)
    Max Flow Period = 120. (IFCREAL)
    Max. Hot Water Supply = 70. (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
    Mechanical Parts = "Non-return valve(s);Litter filter(s)" (IFCTEXT)
    Noise Class = "I (ISO 3822)" (IFCTEXT)
    Pipes = "Flexible inlet pipe(s)" (IFCTEXT)
    Pressure Loss With Flow 01ls = 200000. (IFCPRESSUREMEASURE) [PASCAL]
    Protection Class = "IP 55 / transformer IP 40" (IFCTEXT)
    Recognition Range = "Optimally preset" (IFCTEXT)
    Spare Parts = "http://static.oras.com/sp/1724FT" (IFCTEXT)
    Spout Type = "Fixed spout" (IFCTEXT)
  Mechanical | properties | on 2 type objects
    Advanced Features = "3S-Installation" (IFCTEXT)
    Connection Size = "G1/2" (IFCTEXT)
    Flow = "Limitation option for maximum flowrate" (IFCTEXT)
    Flow Rate At 300kPa = 0.0074160800115126 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Installation Type = "Deck mounted" (IFCTEXT)
    Installation and Maintenance = "http://static.oras.com/manual/1038F" (IFCTEXT)
    Max. Hot Water Supply = 80. (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
    Mounting Holes = "1 mounting hole" (IFCTEXT)
    Noise Class = "I (ISO 3822)" (IFCTEXT)
    Pipes = "Flexible inlet pipes" (IFCTEXT)
    Pressure Loss With Flow 02ls = 270000. (IFCPRESSUREMEASURE) [PASCAL]
    Spare Parts = "http://static.oras.com/sp/1038F" (IFCTEXT)
    Spout Swivel Range = "120° (60° / 0°)" (IFCTEXT)
    Spout Type = "Swivel spout" (IFCTEXT)
  Mechanical: 2 more contents on 0 objects not shown
  Pset_WindowCommon | properties | on 18 objects (18 IFCWINDOW)
    AcousticRating = "38 dB" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "GF 1.3 12x21 38dB" (IFCIDENTIFIER)
  Pset_WindowCommon | properties | on 17 objects (17 IFCWINDOW)
    AcousticRating = "33 dB" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "GF 1.1 12x21 33dB" (IFCIDENTIFIER)
  Pset_WindowCommon | properties | on 14 objects (14 IFCWINDOW)
    AcousticRating = "28 dB" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "V4 23x22" (IFCIDENTIFIER)
  Pset_WindowCommon | properties | on 13 objects (13 IFCWINDOW)
    AcousticRating = "28 dB" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "V6 24x22" (IFCIDENTIFIER)
  Pset_WindowCommon | properties | on 12 objects (12 IFCWINDOW)
    AcousticRating = "28 dB" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "V3 18x22" (IFCIDENTIFIER)
  Pset_WindowCommon | properties | on 11 objects (11 IFCWINDOW)
    AcousticRating = "28 dB" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "V1 12x22" (IFCIDENTIFIER)
  Pset_WindowCommon | properties | on 10 objects (10 IFCWINDOW)
    AcousticRating = "28 dB" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "V7 24x22" (IFCIDENTIFIER)
  Pset_WindowCommon | properties | on 9 objects (9 IFCWINDOW)
    AcousticRating = "38 dB" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "GF 3.2 6x21 38dB" (IFCIDENTIFIER)
  Pset_WindowCommon: 59 more contents on 162 objects not shown
  Slab Shape Edit | properties | on 28 objects (15 IFCROOF, 13 IFCSLAB)
    Curved Edge Condition = 0 (IFCINTEGER)
  Pset_BuildingElementProxyCommon | properties | on 56 objects (56 IFCBUILDINGELEMENTPROXY)
    Reference = "Tavle 2m" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 30 objects (30 IFCBUILDINGELEMENTPROXY)
    Reference = "Smartboard 2m" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 26 objects (26 IFCBUILDINGELEMENTPROXY)
    Reference = "Armstøtte veggmontert" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 20 objects (20 IFCBUILDINGELEMENTPROXY)
    Reference = "Båsgarderobe 400 x 350 x 2000mm" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 19 objects (19 IFCBUILDINGELEMENTPROXY)
    Reference = "PC-skap" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 14 objects (14 IFCBUILDINGELEMENTPROXY)
    Reference = "TV-skjerm" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 12 objects (12 IFCBUILDINGELEMENTPROXY)
    Reference = "gard skap 5rom 30cm" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 10 objects (10 IFCBUILDINGELEMENTPROXY)
    Reference = "Siemens induksjon" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon: 50 more contents on 114 objects not shown
  Pset_CoveringCommon | properties | on 111 objects (111 IFCCOVERING)
    Finish = "Himling System 600x1200;" (IFCTEXT)
    Reference = "Himling System 600x1200" (IFCIDENTIFIER)
    TotalThickness = 50. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_CoveringCommon | properties | on 94 objects (94 IFCCOVERING)
    Finish = "Himling System 600x600;" (IFCTEXT)
    Reference = "Himling System 600x600" (IFCIDENTIFIER)
    TotalThickness = 50. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_CoveringCommon | properties | on 13 objects (13 IFCCOVERING)
    Finish = "Himling System 600x600;" (IFCTEXT)
    Reference = "Himling System 600x600 hygiene korrosjonsklasse" (IFCIDENTIFIER)
    TotalThickness = 50. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_CoveringCommon | properties | on 11 objects (11 IFCCOVERING)
    Reference = "Lydhimling gips" (IFCIDENTIFIER)
    TotalThickness = 73. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_CoveringCommon | properties | on 11 objects (11 IFCCOVERING)
    Finish = "Himling System 600x600;" (IFCTEXT)
    Reference = "Himling System 600x600 hygiene" (IFCIDENTIFIER)
    TotalThickness = 50. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_CoveringCommon | properties | on 4 objects (4 IFCCOVERING)
    Reference = "Himling spiler" (IFCIDENTIFIER)
    TotalThickness = 82. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_CoveringCommon | properties | on 4 objects (4 IFCCOVERING)
    Finish = "Himling System 600x600;" (IFCTEXT)
    Reference = "Himling System 600x600 Venus Kant A 42dB" (IFCIDENTIFIER)
    TotalThickness = 50. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_CoveringCommon | properties | on 4 objects (4 IFCCOVERING)
    Finish = "Himling System 600x600;" (IFCTEXT)
    Reference = "Himling System 600x600 Master Gamma" (IFCIDENTIFIER)
    TotalThickness = 48. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_CoveringCommon: 5 more contents on 7 objects not shown
  Pset_StairCommon | properties | on 5 objects (5 IFCSTAIR)
    IsExternal = FALSE (IFCBOOLEAN)
    NumberOfRiser = 24. (IFCCOUNTMEASURE)
    NumberOfTreads = 23. (IFCCOUNTMEASURE)
    Reference = "Betongtrapp t=150 repo=200" (IFCIDENTIFIER)
    RiserHeight = 166.666666666567 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    TreadLength = 272.2 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_StairCommon | properties | on 2 objects (2 IFCSTAIR)
    IsExternal = FALSE (IFCBOOLEAN)
    NumberOfRiser = 24. (IFCCOUNTMEASURE)
    NumberOfTreads = 23. (IFCCOUNTMEASURE)
    Reference = "Betongtrapp t=150 repo=200" (IFCIDENTIFIER)
    RiserHeight = 169.166666666777 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    TreadLength = 272.2 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_StairCommon | properties | on 1 object (1 IFCSTAIR)
    IsExternal = FALSE (IFCBOOLEAN)
    NumberOfRiser = 12. (IFCCOUNTMEASURE)
    NumberOfTreads = 12. (IFCCOUNTMEASURE)
    Reference = "amfi" (IFCIDENTIFIER)
    RiserHeight = 333.333333332938 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    TreadLength = 1173.33333333412 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_StairCommon | properties | on 1 object (1 IFCSTAIR)
    IsExternal = TRUE (IFCBOOLEAN)
    NumberOfRiser = 24. (IFCCOUNTMEASURE)
    NumberOfTreads = 24. (IFCCOUNTMEASURE)
    Reference = "Trapp amfi" (IFCIDENTIFIER)
    RiserHeight = 166.666666666463 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    TreadLength = 286.666666667074 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_StairCommon | properties | on 1 object (1 IFCSTAIR)
    IsExternal = FALSE (IFCBOOLEAN)
    NumberOfRiser = 24. (IFCCOUNTMEASURE)
    NumberOfTreads = 24. (IFCCOUNTMEASURE)
    Reference = "Gitterrist" (IFCIDENTIFIER)
    RiserHeight = 168.749999999901 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    TreadLength = 272.2 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_StairCommon | properties | on 1 object (1 IFCSTAIR)
    IsExternal = FALSE (IFCBOOLEAN)
    NumberOfRiser = 24. (IFCCOUNTMEASURE)
    NumberOfTreads = 24. (IFCCOUNTMEASURE)
    Reference = "Ståltrapp" (IFCIDENTIFIER)
    RiserHeight = 166.666666666567 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    TreadLength = 274.2 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_BeamCommon | properties | on 27 objects (27 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "50x50" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_BeamCommon | properties | on 2 objects (2 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "bjelke bod" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_BeamCommon | properties | on 2 objects (2 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "50x50" (IFCIDENTIFIER)
    Slope = 36.1755746511457 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_BeamCommon | properties | on 2 objects (2 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "50x50" (IFCIDENTIFIER)
    Slope = 35.7289617254847 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_BeamCommon | properties | on 2 objects (2 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "50x50" (IFCIDENTIFIER)
    Slope = 34.2939237081215 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_BeamCommon | properties | on 2 objects (2 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "50x50" (IFCIDENTIFIER)
    Slope = 35.2643896827548 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_BeamCommon | properties | on 1 object (1 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "IPE 200" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_BeamCommon | properties | on 1 object (1 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "IPE330" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_BeamCommon: 1 more content on 1 objects not shown
  Geometric Position | properties | on 10 objects (10 IFCBEAM)
    End Extension = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Join Status = "Both joins enabled" (IFCIDENTIFIER)
    Start Extension = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    y Justification = "Origin" (IFCIDENTIFIER)
    y Offset Value = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    yz Justification = "Uniform" (IFCIDENTIFIER)
    z Justification = "Top" (IFCIDENTIFIER)
    z Offset Value = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Geometric Position | properties | on 6 objects (6 IFCBEAM)
    End Extension = -1837.99342391824 (IFCLENGTHMEASURE) [MILLI METRE]
    Join Status = "Both joins enabled" (IFCIDENTIFIER)
    Start Extension = -762.00657608178 (IFCLENGTHMEASURE) [MILLI METRE]
    y Justification = "Origin" (IFCIDENTIFIER)
    y Offset Value = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    yz Justification = "Uniform" (IFCIDENTIFIER)
    z Justification = "Top" (IFCIDENTIFIER)
    z Offset Value = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Geometric Position | properties | on 5 objects (5 IFCBEAM)
    End Extension = -3753.01885684339 (IFCLENGTHMEASURE) [MILLI METRE]
    Join Status = "Both joins enabled" (IFCIDENTIFIER)
    Start Extension = 1754.01885684343 (IFCLENGTHMEASURE) [MILLI METRE]
    y Justification = "Origin" (IFCIDENTIFIER)
    y Offset Value = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    yz Justification = "Uniform" (IFCIDENTIFIER)
    z Justification = "Top" (IFCIDENTIFIER)
    z Offset Value = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Geometric Position | properties | on 3 objects (3 IFCBEAM)
    End Extension = -937.993423918232 (IFCLENGTHMEASURE) [MILLI METRE]
    Join Status = "Both joins enabled" (IFCIDENTIFIER)
    Start Extension = -762.00657608178 (IFCLENGTHMEASURE) [MILLI METRE]
    y Justification = "Origin" (IFCIDENTIFIER)
    y Offset Value = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    yz Justification = "Uniform" (IFCIDENTIFIER)
    z Justification = "Top" (IFCIDENTIFIER)
    z Offset Value = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Geometric Position | properties | on 3 objects (3 IFCBEAM)
    End Extension = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    End Join Cutback = 12.7 (IFCLENGTHMEASURE) [MILLI METRE]
    Join Status = "Both joins enabled" (IFCIDENTIFIER)
    Start Extension = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    y Justification = "Origin" (IFCIDENTIFIER)
    y Offset Value = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    yz Justification = "Uniform" (IFCIDENTIFIER)
    z Justification = "Top" (IFCIDENTIFIER)
    z Offset Value = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Geometric Position | properties | on 2 objects (2 IFCBEAM)
    End Extension = -1922.99342391809 (IFCLENGTHMEASURE) [MILLI METRE]
    Join Status = "Both joins enabled" (IFCIDENTIFIER)
    Start Extension = 1237.99342391815 (IFCLENGTHMEASURE) [MILLI METRE]
    y Justification = "Origin" (IFCIDENTIFIER)
    y Offset Value = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    yz Justification = "Uniform" (IFCIDENTIFIER)
    z Justification = "Top" (IFCIDENTIFIER)
    z Offset Value = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Geometric Position | properties | on 2 objects (2 IFCBEAM)
    End Extension = -16.9179500481122 (IFCLENGTHMEASURE) [MILLI METRE]
    Join Status = "Both joins enabled" (IFCIDENTIFIER)
    Start Extension = -35.8720411310767 (IFCLENGTHMEASURE) [MILLI METRE]
    y Justification = "Origin" (IFCIDENTIFIER)
    y Offset Value = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    yz Justification = "Uniform" (IFCIDENTIFIER)
    z Justification = "Top" (IFCIDENTIFIER)
    z Offset Value = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Geometric Position | properties | on 1 object (1 IFCBEAM)
    End Extension = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Join Status = "Both joins enabled" (IFCIDENTIFIER)
    Start Extension = 159.49999999999 (IFCLENGTHMEASURE) [MILLI METRE]
    y Justification = "Origin" (IFCIDENTIFIER)
    y Offset Value = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    yz Justification = "Uniform" (IFCIDENTIFIER)
    z Justification = "Top" (IFCIDENTIFIER)
    z Offset Value = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Geometric Position: 8 more contents on 8 objects not shown
  Pset_StairFlightCommon | properties | on 10 objects (10 IFCSTAIRFLIGHT)
    NosingLength = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NumberOfRiser = 24. (IFCCOUNTMEASURE)
    NumberOfTreads = 23. (IFCCOUNTMEASURE)
    Reference = "Betong 150mm" (IFCIDENTIFIER)
    RiserHeight = 166.666666666567 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    TreadLength = 272.2 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    TreadLengthAtOffset = 272.2 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    WaistThickness = 1500. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    WalkingLineOffset = 750. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_StairFlightCommon | properties | on 4 objects (4 IFCSTAIRFLIGHT)
    NosingLength = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NumberOfRiser = 24. (IFCCOUNTMEASURE)
    NumberOfTreads = 23. (IFCCOUNTMEASURE)
    Reference = "Betong 150mm" (IFCIDENTIFIER)
    RiserHeight = 169.166666666777 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    TreadLength = 272.2 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    TreadLengthAtOffset = 272.2 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    WaistThickness = 1500. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    WalkingLineOffset = 750. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_StairFlightCommon | properties | on 2 objects (2 IFCSTAIRFLIGHT)
    NosingLength = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NumberOfRiser = 24. (IFCCOUNTMEASURE)
    NumberOfTreads = 24. (IFCCOUNTMEASURE)
    Reference = "Inntrinn 50mm Opptrinn 13mm" (IFCIDENTIFIER)
    RiserHeight = 168.749999999901 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    TreadLength = 272.2 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    TreadLengthAtOffset = 272.2 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    WaistThickness = 1200. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    WalkingLineOffset = 600. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_StairFlightCommon | properties | on 2 objects (2 IFCSTAIRFLIGHT)
    NosingLength = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NumberOfRiser = 24. (IFCCOUNTMEASURE)
    NumberOfTreads = 24. (IFCCOUNTMEASURE)
    Reference = "Inntrinn 50mm Opptrinn 13mm" (IFCIDENTIFIER)
    RiserHeight = 166.666666666567 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    TreadLength = 274.2 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    TreadLengthAtOffset = 274.2 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    WaistThickness = 1800. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    WalkingLineOffset = 900. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Grid 1 | properties | on 2 objects (2 IFCROOF)
    Angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Justification = "Beginning" (IFCIDENTIFIER)
    Number = 4 (IFCINTEGER)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Grid 1 | properties | on 1 type object
    Adjust for Mullion Size = FALSE (IFCBOOLEAN)
    Layout = "None" (IFCIDENTIFIER)
  Grid 2 | properties | on 2 objects (2 IFCROOF)
    Angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Justification = "Beginning" (IFCIDENTIFIER)
    Number = 4 (IFCINTEGER)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Grid 2 | properties | on 1 type object
    Adjust for Mullion Size = FALSE (IFCBOOLEAN)
    Layout = "None" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 22 objects (22 IFCCOLUMN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "115x115mm" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_ColumnCommon | properties | on 11 objects (11 IFCCOLUMN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "96x130mm" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Profile | properties | on 3 objects (3 IFCFLOWSEGMENT)
    Angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_RailingCommon | properties | on 8 objects (8 IFCRAILING)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Handrail - elevtrapper" (IFCIDENTIFIER)
  Pset_RailingCommon | properties | on 7 objects (7 IFCRAILING)
    Height = 1219.2 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Rekkverk rømningstrapp" (IFCIDENTIFIER)
  Pset_RailingCommon | properties | on 6 objects (6 IFCRAILING)
    Height = 1079. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Glassfelt - h=1000 bro" (IFCIDENTIFIER)
  Pset_RailingCommon | properties | on 6 objects (6 IFCRAILING)
    Height = 1219.2 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Spiler bod" (IFCIDENTIFIER)
  Pset_RailingCommon | properties | on 6 objects (6 IFCRAILING)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Handrail - h=1000" (IFCIDENTIFIER)
  Pset_RailingCommon | properties | on 6 objects (6 IFCRAILING)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Handrail - vestibyle" (IFCIDENTIFIER)
  Pset_RailingCommon | properties | on 3 objects (3 IFCRAILING)
    Height = 1219.2 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Spiler1" (IFCIDENTIFIER)
  Pset_RailingCommon | properties | on 2 objects (2 IFCRAILING)
    Height = 1219.2 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Rekkverk elevtrapper" (IFCIDENTIFIER)
  Pset_RailingCommon: 1 more content on 2 objects not shown
  Pset_BuildingStoreyCommon | properties | on 3 objects (3 IFCBUILDINGSTOREY)
    AboveGround = TRUE (IFCLOGICAL)
  Pset_BuildingStoreyCommon | properties | on 2 objects (2 IFCBUILDINGSTOREY)
    AboveGround = TRUE (IFCLOGICAL)
    EntranceLevel = TRUE (IFCBOOLEAN)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 5 (IFCINTEGER)
  Analytical Properties(Type) | properties | on 379 objects (259 IFCCOVERING, 83 IFCSLAB, 37 IFCROOF)
    Absorptance = 0.1 (IFCREAL)
    Roughness = 1 (IFCINTEGER)
  Analytical Properties(Type) | properties | on 32 type objects
    Analytic Construction = "<None>" (IFCTEXT)
  Construction(Type) | properties | on 234 objects (234 IFCCOVERING)
    Thickness = 50. (IFCLENGTHMEASURE) [MILLI METRE]
  Construction(Type) | properties | on 25 objects (25 IFCSLAB)
    Default Thickness = 5. (IFCLENGTHMEASURE) [MILLI METRE]
    Function = "Interior" (IFCIDENTIFIER)
  Construction(Type) | properties | on 14 objects (14 IFCSTAIRFLIGHT)
    Structural Depth = 150. (IFCLENGTHMEASURE) [MILLI METRE]
    Underside Surface = "Smooth" (IFCIDENTIFIER)
  Construction(Type) | properties | on 14 objects (14 IFCSLAB)
    Monolithic Thickness = 230. (IFCLENGTHMEASURE) [MILLI METRE]
  Construction(Type) | properties | on 11 objects (11 IFCCOVERING)
    Thickness = 73. (IFCLENGTHMEASURE) [MILLI METRE]
  Construction(Type) | properties | on 9 objects (9 IFCROOF)
    Default Thickness = 150. (IFCLENGTHMEASURE) [MILLI METRE]
  Construction(Type) | properties | on 9 objects (9 IFCRAILING)
    Angled Joins = "Add Vertical/Horizontal Segments" (IFCIDENTIFIER)
    Baluster Offset = 50. (IFCLENGTHMEASURE) [MILLI METRE]
    Landing Height Adjustment = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Rail Connections = "Trim" (IFCIDENTIFIER)
    Railing Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tangent Joins = "Extend Rails to Meet" (IFCIDENTIFIER)
    Use Landing Height Adjustment = FALSE (IFCBOOLEAN)
  Construction(Type) | properties | on 9 objects (9 IFCRAILING)
    Angled Joins = "Add Vertical/Horizontal Segments" (IFCIDENTIFIER)
    Baluster Offset = -25. (IFCLENGTHMEASURE) [MILLI METRE]
    Landing Height Adjustment = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Rail Connections = "Trim" (IFCIDENTIFIER)
    Railing Height = 1000. (IFCLENGTHMEASURE) [MILLI METRE]
    Tangent Joins = "Extend Rails to Meet" (IFCIDENTIFIER)
    Use Landing Height Adjustment = FALSE (IFCBOOLEAN)
  Construction(Type): 54 more contents on 142 objects not shown
  Graphics(Type) | properties | on 373 objects (253 IFCCOVERING, 83 IFCSLAB, 37 IFCROOF)
    Coarse Scale Fill Color = 0 (IFCINTEGER)
  Graphics(Type) | properties | on 9 objects (9 IFCSTAIR)
    Cut Mark Type = "Stair Cut Mark: Enkel" (IFCLABEL)
  Graphics(Type) | properties | on 6 objects (6 IFCCOVERING)
    Coarse Scale Fill Color = 0 (IFCINTEGER)
    Coarse Scale Fill Pattern = "Horisontal 3.0mm" (IFCLABEL)
  Graphics(Type) | properties | on 5 objects (5 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Centre" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "Symbol - Level Head - Trekant: Trekant" (IFCLABEL)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Graphics(Type) | properties | on 2 objects (2 IFCSTAIR)
    Break Symbol in Plan = TRUE (IFCBOOLEAN)
    Text Font = "Arial" (IFCTEXT)
    Text Size = 2.5 (IFCLENGTHMEASURE) [MILLI METRE]
  Graphics(Type) | properties | on 2 type objects
    Bottom frame = FALSE (IFCBOOLEAN)
    Opening % = 0 (IFCINTEGER)
    Reduced top frame = FALSE (IFCBOOLEAN)
    Top frame = TRUE (IFCBOOLEAN)
  Identity Data(Type) | properties | on 111 objects (111 IFCCOVERING)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Type Mark = "" (IFCTEXT)
    Type Name = "Himling System 600x1200" (IFCTEXT)
  Identity Data(Type) | properties | on 94 objects (94 IFCCOVERING)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Type Mark = "" (IFCTEXT)
    Type Name = "Himling System 600x600" (IFCTEXT)
  Identity Data(Type) | properties | on 31 objects (31 IFCFLOWTERMINAL)
    Article Number = "GB111522201211" (IFCTEXT)
    Assembly Code = "D2010100" (IFCTEXT)
    Assembly Description = "Water Closets" (IFCTEXT)
    Care Instruction URL = "http://www.gustavsberg.com/fileadmin/uploads/Citat/G-berg_Mounting/GUST_productcare_instructions_uk.pdf" (IFCTEXT)
    Code EAN = "7391530067384" (IFCTEXT)
    Code LVI FIN = "-" (IFCTEXT)
    Code NRF NOR = "-" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Code RSK SWE = "7819929" (IFCTEXT)
    Code VVS DNK = "-" (IFCTEXT)
    Description = "1522 Nautic WC for wall installation with cistern" (IFCTEXT)
    Flush Rate = "4/2L" (IFCTEXT)
    Installation Instruction URL = "http://www.gustavsberg.com/fileadmin/uploads/Citat/G-berg_Mounting/Nautic.Wc.Bidet.pdf" (IFCTEXT)
    Manufacturer = "Villeroy & Boch Gustavsberg AB" (IFCTEXT)
    Model = "1522" (IFCTEXT)
    OmniClass Number = "23.45.05.21.11" (IFCTEXT)
    OmniClass Title = "Water Closets" (IFCTEXT)
    Product Family = "Nautic" (IFCTEXT)
    Product Page URL = "https://www.gustavsberg.com/en/products/toilet/wall-hung-toilets/product/GB111522201211/wall-hung-toilet-nautic-1522-with-cistern-hygienic-flush-double-flush-24l-standard-seat/" (IFCTEXT)
    Type Comments = "1522 standard seat, Duo flush" (IFCTEXT)
    Type Name = "Vegghengt toalett" (IFCTEXT)
    URL = "http://www.gustavsberg.com/" (IFCTEXT)
  Identity Data(Type) | properties | on 31 objects (31 IFCFLOWTERMINAL)
    Article Number = "41005001" (IFCTEXT)
    Assembly Code = "D2010400" (IFCTEXT)
    Assembly Description = "Sinks" (IFCTEXT)
    Care Instruction URL = "http://www.gustavsberg.com/fileadmin/uploads/Citat/G-berg_Mounting/GUST_productcare_instructions_uk.pdf" (IFCTEXT)
    Code EAN = "4051202323424" (IFCTEXT)
    Code LVI FIN = "5613145" (IFCTEXT)
    Code NRF NOR = "-" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Code RSK SWE = "-" (IFCTEXT)
    Code VVS DNK = "626172000" (IFCTEXT)
    Description = "410050 Nordic3 washbasin for bolt/bracket mounting" (IFCTEXT)
    Installation Instruction URL = "http://www.gustavsberg.com/fileadmin/uploads/Citat/G-berg_Mounting/GB1921100248_Washbasin_Complete.pdf" (IFCTEXT)
    Manufacturer = "Villeroy & Boch Gustavsberg AB" (IFCTEXT)
    Model = "410050" (IFCTEXT)
    OmniClass Number = "23.45.05.14.14" (IFCTEXT)
    OmniClass Title = "Sinks/Lavatories" (IFCTEXT)
    Product Family = "Nordic3" (IFCTEXT)
    Product Page URL = "http://www.gustavsberg.com/en/private-consumers/products/washbasins.html?tx_mmpdb_pi1%5Barticle_number%5D=410050&tx_mmpdb_pi1%5Bvia%5D=3b&tx_mmpdb_pi1%5Baction%5D=show&tx_mmpdb_pi1%5Bcontroller%5D=SolrProduct&cHash=1890ca88f4488d7355f69c2c83c154e5" (IFCTEXT)
    Type Comments = "410050" (IFCTEXT)
    Type Name = "Servant - Ecco 50x35" (IFCTEXT)
    URL = "http://www.gustavsberg.com/" (IFCTEXT)
  Identity Data(Type) | properties | on 25 objects (25 IFCSLAB)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Type Name = "Flis - trapp" (IFCTEXT)
    URL = "" (IFCTEXT)
  Identity Data(Type) | properties | on 23 objects (23 IFCMEMBER)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Type Name = "Side t=10 h=300" (IFCTEXT)
  Identity Data(Type) | properties | on 20 objects (20 IFCFLOWTERMINAL)
    2D/3D/BIM Files URL = "http://static.oras.com/bim/1038F" (IFCTEXT)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Catalog Drawing URL = "http://static.oras.com/catdrw/1038F" (IFCTEXT)
    Class = "Single lever" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Description = "" (IFCTEXT)
    Dimension Drawing URL = "http://static.oras.com/dimdrw/1038F" (IFCTEXT)
    FDV Document URL = "http://www.oras.com/datasheet/1038F/en/fdv" (IFCTEXT)
    Flow Drawing URL = "http://static.oras.com/flowchart/1038F" (IFCTEXT)
    Group = "Kitchen faucets" (IFCTEXT)
    Long Marketing = "Kitchen faucet with high spout. Swivel spout and aerator. Spout’s swing angle is factory preset at 120° (can be limited to 0° or 60° ). There are also in-built limitation options for water temperature and maximum flow-rate. F = with flexible pipes" (IFCTEXT)
    Manufacturer = "Oras" (IFCTEXT)
    Market = "INT;NOR;SWE;DNK;POL;RUS;EST;LTU;LVA;UKR" (IFCTEXT)
    Model = "1038F Kitchen faucet" (IFCTEXT)
    Name_en = "1038F Kitchen faucet" (IFCTEXT)
    OmniClass Number = "23.45.55.00" (IFCTEXT)
    OmniClass Title = "Sanitary Faucets, Wastes" (IFCTEXT)
    Package Weight = "2.07 kg" (IFCTEXT)
    Package external Dimensions = "754 x 334 x 63" (IFCTEXT)
    Product Code = "1038F" (IFCTEXT)
    Product Datasheet = "http://www.oras.com/datasheet/1038F/en" (IFCTEXT)
    Product Family = "Oras Safira" (IFCTEXT)
    Product Image URL = "http://static.oras.com/image/1038F" (IFCTEXT)
    Product URL = "http://static.oras.com/1038F" (IFCTEXT)
    Type Name = "Blandebatteri - Oras Saphira 1038F" (IFCTEXT)
    URL = "" (IFCTEXT)
  Identity Data(Type) | properties | on 14 objects (14 IFCSTAIRFLIGHT)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Type Name = "Betong 150mm" (IFCTEXT)
  Identity Data(Type): 130 more contents on 351 objects not shown
  Materials and Finishes(Type) | properties | on 61 objects (61 IFCFLOWTERMINAL)
    Material = "Gustavsberg Porcelain - White" (IFCLABEL)
  Materials and Finishes(Type) | properties | on 50 objects (50 IFCSLAB)
    Structural Material = "Betong" (IFCLABEL)
  Materials and Finishes(Type) | properties | on 31 objects (31 IFCFLOWTERMINAL)
    Material = "Gustavsberg Porcelain - White (with C+)" (IFCLABEL)
  Materials and Finishes(Type) | properties | on 28 objects (14 IFCSLAB, 14 IFCSTAIRFLIGHT)
    Monolithic Material = "Betong" (IFCLABEL)
  Materials and Finishes(Type) | properties | on 25 objects (25 IFCSLAB)
    Structural Material = "Flis 300x600" (IFCLABEL)
  Materials and Finishes(Type) | properties | on 23 objects (23 IFCMEMBER)
    Material = "Trapp Vange" (IFCLABEL)
  Materials and Finishes(Type) | properties | on 22 objects (22 IFCFLOWTERMINAL)
    Material main = "Stainless steel" (IFCTEXT)
    Material secondary = "" (IFCTEXT)
  Materials and Finishes(Type) | properties | on 22 objects (22 IFCFLOWTERMINAL)
    Material Hardware = "Aluminum" (IFCLABEL)
  Materials and Finishes(Type): 15 more contents on 56 objects not shown
  Other(Type) | properties | on 259 objects (259 IFCCOVERING)
    Category = "Ceilings" (IFCLABEL)
    Family Name = "Compound Ceiling" (IFCTEXT)
  Other(Type) | properties | on 83 objects (83 IFCSLAB)
    Category = "Floors" (IFCLABEL)
    Family Name = "Floor" (IFCTEXT)
  Other(Type) | properties | on 46 objects (46 IFCRAILING)
    Category = "Railings" (IFCLABEL)
    Family Name = "Railing" (IFCTEXT)
  Other(Type) | properties | on 37 objects (37 IFCROOF)
    Category = "Roofs" (IFCLABEL)
    Family Name = "Basic Roof" (IFCTEXT)
  Other(Type) | properties | on 31 objects (31 IFCFLOWTERMINAL)
    Category = "Plumbing Fixtures" (IFCLABEL)
    Duo = TRUE (IFCBOOLEAN)
    Duo Flush = TRUE (IFCBOOLEAN)
    Family Name = "WC-GBG-Nautic_1522-Wall_Mounted" (IFCTEXT)
    Low Duo Flush = FALSE (IFCBOOLEAN)
    Low Single Flush = FALSE (IFCBOOLEAN)
    Raised Button = TRUE (IFCBOOLEAN)
    SCQR Seat = FALSE (IFCBOOLEAN)
    Single Flush = FALSE (IFCBOOLEAN)
    Standard Seat = TRUE (IFCBOOLEAN)
  Other(Type) | properties | on 31 objects (31 IFCFLOWTERMINAL)
    Category = "Plumbing Fixtures" (IFCLABEL)
    Family Name = "Ecco" (IFCTEXT)
  Other(Type) | properties | on 23 objects (23 IFCMEMBER)
    Category = "Supports" (IFCLABEL)
    Family Name = "Stringer" (IFCTEXT)
  Other(Type) | properties | on 21 objects (21 IFCFLOWTERMINAL)
    Category = "Plumbing Fixtures" (IFCLABEL)
    Family Name = "Dusj" (IFCTEXT)
  Other(Type): 33 more contents on 169 objects not shown
  Dimensions(Type) | properties | on 31 objects (31 IFCFLOWTERMINAL)
    Cold Water Connection Diameter = 15. (IFCLENGTHMEASURE) [MILLI METRE]
    Cold Water Connection Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Cold Water Connection Radius = 7.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Height = 800. (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 700. (IFCLENGTHMEASURE) [MILLI METRE]
    Seat Height = 400. (IFCLENGTHMEASURE) [MILLI METRE]
    Waste Connection Diameter = 110. (IFCLENGTHMEASURE) [MILLI METRE]
    Waste Connection Radius = 55. (IFCLENGTHMEASURE) [MILLI METRE]
    Waste Connection Rough In = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Width = 345. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions(Type) | properties | on 31 objects (31 IFCFLOWTERMINAL)
    Height = 170. (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 370. (IFCLENGTHMEASURE) [MILLI METRE]
    Mounting Height = 850. (IFCLENGTHMEASURE) [MILLI METRE]
    Waste Connection Diameter = 50. (IFCLENGTHMEASURE) [MILLI METRE]
    Waste Connection Radius = 25. (IFCLENGTHMEASURE) [MILLI METRE]
    Width = 500. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions(Type) | properties | on 23 objects (23 IFCMEMBER)
    Flip Section Profile = FALSE (IFCBOOLEAN)
    Structural Depth On Landing = 225. (IFCLENGTHMEASURE) [MILLI METRE]
    Structural Depth On Run = 90. (IFCLENGTHMEASURE) [MILLI METRE]
    Total Depth = 300. (IFCLENGTHMEASURE) [MILLI METRE]
    Width = 10. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions(Type) | properties | on 20 objects (20 IFCFLOWTERMINAL)
    InletConnectionSize = 10. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalDepth = 261.5 (IFCLENGTHMEASURE) [MILLI METRE]
    NominalHeight = 338. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 54. (IFCLENGTHMEASURE) [MILLI METRE]
    Projection = 178. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions(Type) | properties | on 13 objects (13 IFCFLOWTERMINAL)
    Cold Water Connection Diameter = 15. (IFCLENGTHMEASURE) [MILLI METRE]
    Cold Water Connection Height = 400. (IFCLENGTHMEASURE) [MILLI METRE]
    Cold Water Connection Radius = 7.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Height = 900. (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 650. (IFCLENGTHMEASURE) [MILLI METRE]
    Seat Height = 460. (IFCLENGTHMEASURE) [MILLI METRE]
    Waste Connection Diameter = 110. (IFCLENGTHMEASURE) [MILLI METRE]
    Waste Connection Radius = 55. (IFCLENGTHMEASURE) [MILLI METRE]
    Waste Connection Rough In = 75. (IFCLENGTHMEASURE) [MILLI METRE]
    Width = 345. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions(Type) | properties | on 13 objects (13 IFCFLOWTERMINAL)
    Height = 190. (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 490. (IFCLENGTHMEASURE) [MILLI METRE]
    Mounting Height = 850. (IFCLENGTHMEASURE) [MILLI METRE]
    Waste Connection Diameter = 50. (IFCLENGTHMEASURE) [MILLI METRE]
    Waste Connection Radius = 25. (IFCLENGTHMEASURE) [MILLI METRE]
    Width = 600. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions(Type) | properties | on 11 objects (11 IFCFLOWTERMINAL)
    Depth = 600. (IFCLENGTHMEASURE) [MILLI METRE]
    Width = 800. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions(Type) | properties | on 6 objects (6 IFCFLOWTERMINAL)
    Depth = 535. (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Height = 900. (IFCLENGTHMEASURE) [MILLI METRE]
    Width = 760. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions(Type): 18 more contents on 6 objects not shown
  Plumbing(Type) | properties | on 31 objects (31 IFCFLOWTERMINAL)
    Nominal Flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Pressure Drop = 0. (IFCPRESSUREMEASURE) [PASCAL]
  Plumbing(Type) | properties | on 13 objects (13 IFCFLOWTERMINAL)
    Nominal Flow = 0.00353146667214886 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Pressure Drop = 0. (IFCPRESSUREMEASURE) [PASCAL]
  Text(Type) | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Bold = FALSE (IFCBOOLEAN)
    Italic = FALSE (IFCBOOLEAN)
    Text Font = "Arial" (IFCTEXT)
    Text Size = 350. (IFCLENGTHMEASURE) [MILLI METRE]
  Text(Type) | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Bold = FALSE (IFCBOOLEAN)
    Italic = FALSE (IFCBOOLEAN)
    Text Font = "Arial" (IFCTEXT)
    Text Size = 400. (IFCLENGTHMEASURE) [MILLI METRE]
  Text(Type) | properties | on 5 type objects
    Type Size = "21x16M" (IFCTEXT)
  Text(Type) | properties | on 5 type objects
    Type Size = "24x22M" (IFCTEXT)
  Text(Type) | properties | on 4 type objects
    Type Size = "35x22M" (IFCTEXT)
  Text(Type) | properties | on 4 type objects
    Type Size = "30x22M" (IFCTEXT)
  Text(Type) | properties | on 2 type objects
    Type Size = "12x30M" (IFCTEXT)
  Text(Type) | properties | on 2 type objects
    Type Size = "12x24M" (IFCTEXT)
  Text(Type): 7 more contents on 0 objects not shown
  Calculation Rules(Type) | properties | on 7 objects (7 IFCSTAIR)
    Maximum Riser Height = 180. (IFCLENGTHMEASURE) [MILLI METRE]
    Minimum Run Width = 1000. (IFCLENGTHMEASURE) [MILLI METRE]
    Minimum Tread Depth = 250. (IFCLENGTHMEASURE) [MILLI METRE]
  Calculation Rules(Type) | properties | on 2 objects (2 IFCSTAIR)
    Maximum Riser Height = 180. (IFCLENGTHMEASURE) [MILLI METRE]
    Minimum Run Width = 900. (IFCLENGTHMEASURE) [MILLI METRE]
    Minimum Tread Depth = 250. (IFCLENGTHMEASURE) [MILLI METRE]
  Calculation Rules(Type) | properties | on 1 object (1 IFCSTAIR)
    Maximum Riser Height = 700. (IFCLENGTHMEASURE) [MILLI METRE]
    Minimum Tread Depth = 900. (IFCLENGTHMEASURE) [MILLI METRE]
  Calculation Rules(Type) | properties | on 1 object (1 IFCSTAIR)
    Maximum Riser Height = 180. (IFCLENGTHMEASURE) [MILLI METRE]
    Minimum Tread Depth = 300. (IFCLENGTHMEASURE) [MILLI METRE]
  Risers(Type) | properties | on 18 objects (18 IFCSTAIRFLIGHT)
    Riser = FALSE (IFCBOOLEAN)
    Riser Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Riser To Tread Connection = "Extend Riser Behind Tread" (IFCIDENTIFIER)
    Slanted = FALSE (IFCBOOLEAN)
  Risers(Type) | properties | on 2 objects (2 IFCSTAIR)
    Begin with Riser = TRUE (IFCBOOLEAN)
    End with Riser = FALSE (IFCBOOLEAN)
    Riser Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Riser Type = "Straight" (IFCIDENTIFIER)
    Riser to Tread Connection = "Extend Riser Behind Tread" (IFCIDENTIFIER)
  Stringers(Type) | properties | on 1 object (1 IFCSTAIR)
    Landing Carriage Height = 200. (IFCLENGTHMEASURE) [MILLI METRE]
    Left Stringer = "Closed" (IFCIDENTIFIER)
    Middle Stringers = 0 (IFCINTEGER)
    Open Stringer Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Right Stringer = "Closed" (IFCIDENTIFIER)
    Stringer Carriage Height = 200. (IFCLENGTHMEASURE) [MILLI METRE]
    Stringer Height = 400. (IFCLENGTHMEASURE) [MILLI METRE]
    Stringer Thickness = 50. (IFCLENGTHMEASURE) [MILLI METRE]
    Trim Stringers at Top = "Do not trim" (IFCIDENTIFIER)
  Stringers(Type) | properties | on 1 object (1 IFCSTAIR)
    Landing Carriage Height = 230. (IFCLENGTHMEASURE) [MILLI METRE]
    Left Stringer = "Closed" (IFCIDENTIFIER)
    Middle Stringers = 0 (IFCINTEGER)
    Open Stringer Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Right Stringer = "Closed" (IFCIDENTIFIER)
    Stringer Carriage Height = 150. (IFCLENGTHMEASURE) [MILLI METRE]
    Stringer Height = 400. (IFCLENGTHMEASURE) [MILLI METRE]
    Stringer Thickness = 50. (IFCLENGTHMEASURE) [MILLI METRE]
    Trim Stringers at Top = "Do not trim" (IFCIDENTIFIER)
  Treads(Type) | properties | on 18 objects (18 IFCSLAB)
    Same as Run = TRUE (IFCBOOLEAN)
  Treads(Type) | properties | on 14 objects (14 IFCSTAIRFLIGHT)
    Apply Nosing Profile = "Front Only" (IFCIDENTIFIER)
    Nosing Length = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tread = FALSE (IFCBOOLEAN)
    Tread Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Treads(Type) | properties | on 4 objects (4 IFCSTAIRFLIGHT)
    Apply Nosing Profile = "Front Only" (IFCIDENTIFIER)
    Nosing Length = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tread = TRUE (IFCBOOLEAN)
    Tread Thickness = 75. (IFCLENGTHMEASURE) [MILLI METRE]
  Treads(Type) | properties | on 2 objects (2 IFCSTAIR)
    Apply Nosing Profile = "Front Only" (IFCIDENTIFIER)
    Nosing Length = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tread Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints(Type) | properties | on 48 objects (48 IFCFLOWTERMINAL)
    Default Elevation = 850. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints(Type) | properties | on 31 objects (31 IFCFLOWTERMINAL)
    Default Elevation = 400. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints(Type) | properties | on 22 objects (22 IFCFLOWTERMINAL)
    Default Elevation = 1219.2 (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints(Type) | properties | on 5 objects (5 IFCBUILDINGSTOREY)
    Elevation Base = "Survey Point" (IFCIDENTIFIER)
  General(Type) | properties | on 20 objects (20 IFCFLOWTERMINAL)
    Author = "Convergo AB" (IFCTEXT)
    BIMObjectName = "1038F(2017)" (IFCTEXT)
    ConvergoRefNr = "0087-1804-0024-FI" (IFCTEXT)
    ManufacterURL = "http://www.oras.com/" (IFCTEXT)
    ManufacturerName = "Oras" (IFCTEXT)
    NBSDescription = "Water supply fittings for wash basins and troughs" (IFCTEXT)
    NBSReference = "45-35-70/371" (IFCTEXT)
    ProductInformation = "Kitchen faucet with high spout" (IFCTEXT)
    Revision = "2" (IFCTEXT)
    Uniclass2 = "Pr_40_30_96_45" (IFCTEXT)
    Uniclass2015Description = "Sink manual water supply sets" (IFCTEXT)
    Uniclass2015Reference = "Pr_40_20_87_82" (IFCTEXT)
    Version = "2" (IFCTEXT)
    VersionDate = "01/01/2019" (IFCTEXT)
  General(Type) | properties | on 10 objects (10 IFCFLOWTERMINAL)
    Brand url = "http://www.intra-teka.com/svenska" (IFCTEXT)
    Date of publishing = "" (IFCTEXT)
    Design country = "Norway" (IFCTEXT)
    Edition number = 1 (IFCINTEGER)
    Manufacturer country = "Norway" (IFCTEXT)
    Manufacturer name = "Intra" (IFCTEXT)
    Nominal height = 10464.8 (IFCLENGTHMEASURE) [MILLI METRE]
    Nominal width = 11557. (IFCLENGTHMEASURE) [MILLI METRE]
    Product SKU = "GUB1" (IFCTEXT)
    Product family = "Bucket Sinks" (IFCTEXT)
    Product group = "310" (IFCTEXT)
    QR code = "http://bimobject.com/intra/product/GUB1" (IFCTEXT)
    Region Africa = "AO, BF, BI, BJ, BW, CD, CF, CG, CI, CM, CV, DJ, DZ, EH, ER, ET, GA, GH, GM, GN, GQ, GW, KE, KM, LR, LS, LY, MA, MG, ML, MR, MU, MW, MZ, NA, NE, NG, RE, RW, SC, SD, SH, SL, SN, SO, SS, ST, SZ, TD, TG, TN, TZ, UG, YT, ZA, ZM, ZW" (IFCTEXT)
    Region Antarctica = "None" (IFCTEXT)
    Region Asia = "AM, AZ, BD, BN, BT, CC, CN, CX, GE, HK, ID, IN, IO, JP, KG, KH, KP, KR, KZ, LA, LK, MM, MN, MO, MV, MY, NP, PH, PK, SG, TH, TJ, TM, TW, UZ, VN" (IFCTEXT)
    Region Europe = "AD, AL, AT, AX, BA, BE, BG, BY, CH, CY, CZ, DE, DK, EE, ES, FI, FO, FR, GB, GG, GI, GR, HR, HU, IE, IM, IS, IT, JE, LI, LT, LU, LV, MC, MD, ME, MK, MT, NL, NO, PL, PT, RO, RS, RU, SE, SI, SJ, SK, SM, UA, VA" (IFCTEXT)
    Region Middle East = "AE, AF, BH, EG, IL, IQ, IR, JO, KW, LB, OM, PS, QA, SA, SY, TR, YE" (IFCTEXT)
    Region North America = "AG, AI, AW, BB, BL, BM, BQ, BS, BZ, CA, CR, CU, CW, DM, DO, GD, GL, GP, GT, HN, HT, JM, KN, KY, LC, MF, MQ, MS, MX, NI, PA, PM, PR, SV, SX, TC, TT, US, VC, VG, VI" (IFCTEXT)
    Region Oceania = "AS, AU, CK, FJ, FM, GU, KI, MH, MP, NC, NF, NR, NU, NZ, PF, PG, PN, PW, SB, TK, TL, TO, TV, UM, WF, WS, VU" (IFCTEXT)
    Region South America = "AR, BO, BR, CL, CO, EC, FK, GF, GY, PE, PY, SR, UY, VE" (IFCTEXT)
    Weight Net (Kg) = "3.6" (IFCTEXT)
  General(Type) | properties | on 9 objects (9 IFCFLOWTERMINAL)
    Brand url = "http://www.intra-teka.com/svenska" (IFCTEXT)
    Date of publishing = "" (IFCTEXT)
    Design country = "Norway" (IFCTEXT)
    Edition number = 1 (IFCINTEGER)
    Manufacturer country = "Sweden" (IFCTEXT)
    Manufacturer name = "Intra" (IFCTEXT)
    Nominal height = 42672. (IFCLENGTHMEASURE) [MILLI METRE]
    Nominal width = 365760. (IFCLENGTHMEASURE) [MILLI METRE]
    Product SKU = "P121" (IFCTEXT)
    Product family = "Washtroughs" (IFCTEXT)
    Product group = "320" (IFCTEXT)
    QR code = "http://bimobject.com/intra/product/P121" (IFCTEXT)
    Region Africa = "AO, BF, BI, BJ, BW, CD, CF, CG, CI, CM, CV, DJ, DZ, EH, ER, ET, GA, GH, GM, GN, GQ, GW, KE, KM, LR, LS, LY, MA, MG, ML, MR, MU, MW, MZ, NA, NE, NG, RE, RW, SC, SD, SH, SL, SN, SO, SS, ST, SZ, TD, TG, TN, TZ, UG, YT, ZA, ZM, ZW" (IFCTEXT)
    Region Antarctica = "None" (IFCTEXT)
    Region Asia = "AM, AZ, BD, BN, BT, CC, CN, CX, GE, HK, ID, IN, IO, JP, KG, KH, KP, KR, KZ, LA, LK, MM, MN, MO, MV, MY, NP, PH, PK, SG, TH, TJ, TM, TW, UZ, VN" (IFCTEXT)
    Region Europe = "AD, AL, AT, AX, BA, BE, BG, BY, CH, CY, CZ, DE, DK, EE, ES, FI, FO, FR, GB, GG, GI, GR, HR, HU, IE, IM, IS, IT, JE, LI, LT, LU, LV, MC, MD, ME, MK, MT, NL, NO, PL, PT, RO, RS, RU, SE, SI, SJ, SK, SM, UA, VA" (IFCTEXT)
    Region Middle East = "AE, AF, BH, EG, IL, IQ, IR, JO, KW, LB, OM, PS, QA, SA, SY, TR, YE" (IFCTEXT)
    Region North America = "AG, AI, AW, BB, BL, BM, BQ, BS, BZ, CA, CR, CU, CW, DM, DO, GD, GL, GP, GT, HN, HT, JM, KN, KY, LC, MF, MQ, MS, MX, NI, PA, PM, PR, SV, SX, TC, TT, US, VC, VG, VI" (IFCTEXT)
    Region Oceania = "AS, AU, CK, FJ, FM, GU, KI, MH, MP, NC, NF, NR, NU, NZ, PF, PG, PN, PW, SB, TK, TL, TO, TV, UM, WF, WS, VU" (IFCTEXT)
    Region South America = "AR, BO, BR, CL, CO, EC, FK, GF, GY, PE, PY, SR, UY, VE" (IFCTEXT)
    Weight Net (Kg) = "9.6" (IFCTEXT)
  General(Type) | properties | on 3 objects (3 IFCFLOWTERMINAL)
    Brand url = "http://www.intra-teka.com/svenska" (IFCTEXT)
    Date of publishing = "" (IFCTEXT)
    Design country = "Norway" (IFCTEXT)
    Edition number = 1 (IFCINTEGER)
    Manufacturer country = "Sweden" (IFCTEXT)
    Manufacturer name = "Intra" (IFCTEXT)
    Nominal height = 42672. (IFCLENGTHMEASURE) [MILLI METRE]
    Nominal width = 548640. (IFCLENGTHMEASURE) [MILLI METRE]
    Product SKU = "P181" (IFCTEXT)
    Product family = "Washtroughs" (IFCTEXT)
    Product group = "320" (IFCTEXT)
    QR code = "http://bimobject.com/intra/product/P181" (IFCTEXT)
    Region Africa = "AO, BF, BI, BJ, BW, CD, CF, CG, CI, CM, CV, DJ, DZ, EH, ER, ET, GA, GH, GM, GN, GQ, GW, KE, KM, LR, LS, LY, MA, MG, ML, MR, MU, MW, MZ, NA, NE, NG, RE, RW, SC, SD, SH, SL, SN, SO, SS, ST, SZ, TD, TG, TN, TZ, UG, YT, ZA, ZM, ZW" (IFCTEXT)
    Region Antarctica = "None" (IFCTEXT)
    Region Asia = "AM, AZ, BD, BN, BT, CC, CN, CX, GE, HK, ID, IN, IO, JP, KG, KH, KP, KR, KZ, LA, LK, MM, MN, MO, MV, MY, NP, PH, PK, SG, TH, TJ, TM, TW, UZ, VN" (IFCTEXT)
    Region Europe = "AD, AL, AT, AX, BA, BE, BG, BY, CH, CY, CZ, DE, DK, EE, ES, FI, FO, FR, GB, GG, GI, GR, HR, HU, IE, IM, IS, IT, JE, LI, LT, LU, LV, MC, MD, ME, MK, MT, NL, NO, PL, PT, RO, RS, RU, SE, SI, SJ, SK, SM, UA, VA" (IFCTEXT)
    Region Middle East = "AE, AF, BH, EG, IL, IQ, IR, JO, KW, LB, OM, PS, QA, SA, SY, TR, YE" (IFCTEXT)
    Region North America = "AG, AI, AW, BB, BL, BM, BQ, BS, BZ, CA, CR, CU, CW, DM, DO, GD, GL, GP, GT, HN, HT, JM, KN, KY, LC, MF, MQ, MS, MX, NI, PA, PM, PR, SV, SX, TC, TT, US, VC, VG, VI" (IFCTEXT)
    Region Oceania = "AS, AU, CK, FJ, FM, GU, KI, MH, MP, NC, NF, NR, NU, NZ, PF, PG, PN, PW, SB, TK, TL, TO, TV, UM, WF, WS, VU" (IFCTEXT)
    Region South America = "AR, BO, BR, CL, CO, EC, FK, GF, GY, PE, PY, SR, UY, VE" (IFCTEXT)
    Weight Net (Kg) = "13.1" (IFCTEXT)
  General(Type) | properties | on 2 type objects
    Brand url = "http://www.manusa.com/en/" (IFCTEXT)
    Date of publishing = "" (IFCTEXT)
    Design country = "Spain" (IFCTEXT)
    Edition number = 1 (IFCINTEGER)
    Manufacturer country = "Spain" (IFCTEXT)
    Manufacturer name = "Manusa" (IFCTEXT)
    Nominal height = 3000. (IFCREAL)
    Nominal width = 2852. (IFCREAL)
    Product SKU = "bps_a20_1_wf" (IFCTEXT)
    Product family = "AUTOMATIC DOORS" (IFCTEXT)
    Product group = "Sliding doors" (IFCTEXT)
    QR code = "http://bimobject.com/manusa/product/bps_a20_1_wf" (IFCTEXT)
    Region Africa = "AO, BF, BI, BJ, BW, CD, CF, CG, CI, CM, CV, DJ, DZ, EH, ER, ET, GA, GH, GM, GN, GQ, GW, KE, KM, LR, LS, LY, MA, MG, ML, MR, MU, MW, MZ, NA, NE, NG, RE, RW, SC, SD, SH, SL, SN, SO, SS, ST, SZ, TD, TG, TN, TZ, UG, YT, ZA, ZM, ZW" (IFCTEXT)
    Region Antarctica = "AQ, BV, GS, HM, TF" (IFCTEXT)
    Region Asia = "AM, AZ, BD, BN, BT, CC, CN, CX, GE, HK, ID, IN, IO, JP, KG, KH, KP, KR, KZ, LA, LK, MM, MN, MO, MV, MY, NP, PH, PK, SG, TH, TJ, TM, TW, UZ, VN" (IFCTEXT)
    Region Europe = "AD, AL, AT, AX, BA, BE, BG, BY, CH, CY, CZ, DE, DK, EE, ES, FI, FO, FR, GB, GG, GI, GR, HR, HU, IE, IM, IS, IT, JE, LI, LT, LU, LV, MC, MD, ME, MK, MT, NL, NO, PL, PT, RO, RS, RU, SE, SI, SJ, SK, SM, UA, VA" (IFCTEXT)
    Region Middle East = "AE, AF, BH, EG, IL, IQ, IR, JO, KW, LB, OM, PS, QA, SA, SY, TR, YE" (IFCTEXT)
    Region North America = "AG, AI, AW, BB, BL, BM, BQ, BS, BZ, CA, CR, CU, CW, DM, DO, GD, GP, GT, HN, HT, JM, KN, KY, LC, MF, MQ, MS, MX, NI, PA, PM, PR, SV, SX, TC, TT, US, VC, VG, VI" (IFCTEXT)
    Region Oceania = "AS, AU, CK, FJ, FM, GU, KI, MH, MP, NC, NF, NR, NU, NZ, PF, PG, PN, PW, SB, TK, TL, TO, TV, UM, WF, WS, VU" (IFCTEXT)
    Region South America = "AR, BO, BR, CL, CO, EC, FK, GF, GY, PE, PY, SR, UY, VE" (IFCTEXT)
    Weight Net (Kg) = 0. (IFCREAL)
  Supports(Type) | properties | on 7 objects (7 IFCSTAIR)
    Left Lateral Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Left Support = "None" (IFCIDENTIFIER)
    Middle Support = FALSE (IFCBOOLEAN)
    Middle Support Number = 0 (IFCINTEGER)
    Right Lateral Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Right Support = "None" (IFCIDENTIFIER)
  Supports(Type) | properties | on 2 objects (2 IFCSTAIR)
    Left Lateral Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Left Support = "Stringer (Closed)" (IFCIDENTIFIER)
    Left Support Type = "Stringer: Side t=10 h=300" (IFCLABEL)
    Middle Support = FALSE (IFCBOOLEAN)
    Middle Support Number = 0 (IFCINTEGER)
    Right Lateral Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Right Support = "Stringer (Closed)" (IFCIDENTIFIER)
    Right Support Type = "Stringer: Side t=10 h=300" (IFCLABEL)
  Green Building Properties(Type) | properties | on 20 objects (20 IFCFLOWTERMINAL)
    Customs Code = "84818011" (IFCTEXT)
    EAN Number = "6414150078927" (IFCTEXT)
    EN Standard = "EN 817" (IFCTEXT)
    NRF Number = "4200415" (IFCTEXT)
    RSK Number = "8310573" (IFCTEXT)
    URL KIWA SE Type Approval = "http://static.oras.com/SETypeApproval/1038F" (IFCTEXT)
    VVS Number = "705897604" (IFCTEXT)
  Mechanical(Type) | properties | on 20 objects (20 IFCFLOWTERMINAL)
    Advanced Features = "3S-Installation" (IFCTEXT)
    Connection Size = "G1/2" (IFCTEXT)
    Flow = "Limitation option for maximum flowrate" (IFCTEXT)
    Flow Rate At 300kPa = 0.0074160800115126 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Installation Type = "Deck mounted" (IFCTEXT)
    Installation and Maintenance = "http://static.oras.com/manual/1038F" (IFCTEXT)
    Max. Hot Water Supply = 80. (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
    Mounting Holes = "1 mounting hole" (IFCTEXT)
    Noise Class = "I (ISO 3822)" (IFCTEXT)
    Pipes = "Flexible inlet pipes" (IFCTEXT)
    Pressure Loss With Flow 02ls = 270000. (IFCPRESSUREMEASURE) [PASCAL]
    Spare Parts = "http://static.oras.com/sp/1038F" (IFCTEXT)
    Spout Swivel Range = "120° (60° / 0°)" (IFCTEXT)
    Spout Type = "Swivel spout" (IFCTEXT)
  Handrail 1(Type) | properties | on 31 objects (31 IFCRAILING)
    Position = "None" (IFCIDENTIFIER)
  Handrail 1(Type) | properties | on 15 objects (15 IFCRAILING)
    Height = 900. (IFCLENGTHMEASURE) [MILLI METRE]
    Lateral Offset = 55. (IFCLENGTHMEASURE) [MILLI METRE]
    Position = "None" (IFCIDENTIFIER)
    Type = "Handrail Type: Sirkulær - veggmontert" (IFCLABEL)
  Handrail 2(Type) | properties | on 46 objects (46 IFCRAILING)
    Position = "None" (IFCIDENTIFIER)
  Top Rail(Type) | properties | on 22 objects (22 IFCRAILING)
    Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Use Top Rail = FALSE (IFCBOOLEAN)
  Top Rail(Type) | properties | on 18 objects (18 IFCRAILING)
    Height = 1219.2 (IFCLENGTHMEASURE) [MILLI METRE]
    Use Top Rail = FALSE (IFCBOOLEAN)
  Top Rail(Type) | properties | on 6 objects (6 IFCRAILING)
    Height = 1079. (IFCLENGTHMEASURE) [MILLI METRE]
    Type = "Top Rail Type: Ellipse - 40x30mm" (IFCLABEL)
    Use Top Rail = TRUE (IFCBOOLEAN)
  Analytical Properties | properties | on 279 type objects
    Analytic Construction = "<None>" (IFCTEXT)
  Analytical Properties | properties | on 203 type objects
    Absorptance = 0.1 (IFCREAL)
    Roughness = 1 (IFCINTEGER)
  Analytical Properties | properties | on 5 type objects
    Analytic Construction = "Metal" (IFCTEXT)
    Heat Transfer Coefficient (U) = 3.7021 (IFCREAL)
    Solar Heat Gain Coefficient = 0. (IFCREAL)
    Thermal Resistance (R) = 0.270116960643959 (IFCREAL)
    Visual Light Transmittance = 0. (IFCREAL)
  Analytical Properties | properties | on 1 type object
    Absorptance = 0.1 (IFCREAL)
    Heat Transfer Coefficient (U) = 11.6111111111111 (IFCREAL)
    Roughness = 1 (IFCINTEGER)
    Thermal Resistance (R) = 0.0861244019138756 (IFCREAL)
    Thermal mass = 40662. (IFCREAL)
  Dør Enkel:IDS 1.1 10x21 EI60S:2027286 | predefined | on 2 type objects
  Dør Dobbel_Ulike_Dørblader:IDS 2.1 13x21M EI60S:2027581 | predefined | on 2 type objects
  Visibility | properties | on 25 type objects
    Door Handle Left On = TRUE (IFCBOOLEAN)
    Door Handle Right On = TRUE (IFCBOOLEAN)
  Visibility | properties | on 4 type objects
    T-BH = TRUE (IFCBOOLEAN)
    T-HH = FALSE (IFCBOOLEAN)
    T-TH = FALSE (IFCBOOLEAN)
    T-VH = TRUE (IFCBOOLEAN)
  Visibility | properties | on 3 type objects
    B-BH = TRUE (IFCBOOLEAN)
    B-HH = FALSE (IFCBOOLEAN)
    B-TH = FALSE (IFCBOOLEAN)
    B-VH = TRUE (IFCBOOLEAN)
  Visibility | properties | on 1 type object
    T-BH = FALSE (IFCBOOLEAN)
    T-HH = FALSE (IFCBOOLEAN)
    T-TH = FALSE (IFCBOOLEAN)
    T-VH = TRUE (IFCBOOLEAN)
  Dør Enkel:IDS 1.2 10x21M EI120CS:2294117 | predefined | on 2 type objects
  Dør Dobbel_Ulike_Dørblader:IDS 2.1 13x21M EI60S:2294242 | predefined | on 2 type objects
  Dør Dobbel_Ulike_Dørblader:IDS 2.1 13x21M EI60S:4093959 | predefined | on 2 type objects
  Dør Enkel:IDS 6.1 8x21M:4109271 | predefined | on 2 type objects
  Dør Enkel:IDS 5.1 13x21M EI60CS:6509988 | predefined | on 2 type objects
  Dør Enkel:IDS 5.1 13x21M EI60CS:6510584 | predefined | on 2 type objects
  Luke600:IDA 11 10x6:6972200 | predefined | on 2 type objects
  General | properties | on 3 type objects
    Author = "Convergo AB" (IFCTEXT)
    BIMObjectName = "1724FT(2013)" (IFCTEXT)
    ConvergoRefNr = "0087-1710-0035-FI" (IFCTEXT)
    ManufacterURL = "http://www.oras.com/" (IFCTEXT)
    ManufacturerName = "Oras" (IFCTEXT)
    NBSDescription = "Water supply fittings for baths" (IFCTEXT)
    NBSReference = "45-35-70/315" (IFCTEXT)
    ProductInformation = "Touchless washbasin faucet with a temperature adjustment handle" (IFCTEXT)
    Revision = "2" (IFCTEXT)
    Uniclass2 = "Pr_40_30_96_78" (IFCTEXT)
    Uniclass2015Description = "Shower manual water supply sets" (IFCTEXT)
    Uniclass2015Reference = "Pr_40_20_87_78" (IFCTEXT)
    Version = "2" (IFCTEXT)
    VersionDate = "01/01/2019" (IFCTEXT)
  General | properties | on 2 type objects
    Author = "Convergo AB" (IFCTEXT)
    BIMObjectName = "1038F(2017)" (IFCTEXT)
    ConvergoRefNr = "0087-1804-0024-FI" (IFCTEXT)
    ManufacterURL = "http://www.oras.com/" (IFCTEXT)
    ManufacturerName = "Oras" (IFCTEXT)
    NBSDescription = "Water supply fittings for wash basins and troughs" (IFCTEXT)
    NBSReference = "45-35-70/371" (IFCTEXT)
    ProductInformation = "Kitchen faucet with high spout" (IFCTEXT)
    Revision = "2" (IFCTEXT)
    Uniclass2 = "Pr_40_30_96_45" (IFCTEXT)
    Uniclass2015Description = "Sink manual water supply sets" (IFCTEXT)
    Uniclass2015Reference = "Pr_40_20_87_82" (IFCTEXT)
    Version = "2" (IFCTEXT)
    VersionDate = "01/01/2019" (IFCTEXT)
  General | properties | on 2 type objects
    Author = "Convergo AB" (IFCTEXT)
    BIMObjectName = "7267(2013)" (IFCTEXT)
    ConvergoRefNr = "0087-1809-0065-FI" (IFCTEXT)
    ManufacterURL = "http://www.oras.com/" (IFCTEXT)
    ManufacturerName = "Oras" (IFCTEXT)
    NBSDescription = "Water supply fittings for baths" (IFCTEXT)
    NBSReference = "45-35-70/315" (IFCTEXT)
    ProductInformation = "n/a" (IFCTEXT)
    Revision = "2" (IFCTEXT)
    Uniclass2 = "Pr_40_30_96_07" (IFCTEXT)
    Uniclass2015Description = "Bath manual water supply sets" (IFCTEXT)
    Uniclass2015Reference = "Pr_40_20_87_07" (IFCTEXT)
    Version = "2" (IFCTEXT)
    VersionDate = "01/01/2019" (IFCTEXT)
  General | properties | on 1 type object
    Author = "Convergo AB" (IFCTEXT)
    BIMObjectName = "3970(2016)" (IFCTEXT)
    ConvergoRefNr = "0087-1803-0065-FI" (IFCTEXT)
    ManufacterURL = "http://www.oras.com/" (IFCTEXT)
    ManufacturerName = "Oras" (IFCTEXT)
    NBSDescription = "Water supply fittings for baths" (IFCTEXT)
    NBSReference = "45-35-70/315" (IFCTEXT)
    ProductInformation = "n/a" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2 = "Pr_40_30_96_78" (IFCTEXT)
    Uniclass2015Description = "Shower manual water supply sets" (IFCTEXT)
    Uniclass2015Reference = "Pr_40_20_87_78" (IFCTEXT)
    Version = "1" (IFCTEXT)
    VersionDate = "20/03/2019" (IFCTEXT)
  Green Building Properties | properties | on 12 type objects
    Recycled Content = "as Specified" (IFCTEXT)
  Green Building Properties | properties | on 3 type objects
    Approval KIWA SE Type Approval = "1462" (IFCTEXT)
    Backflow Prevention EN1717 = "EB" (IFCTEXT)
    Customs Code = "84818011" (IFCTEXT)
    EAN Number = "6414150073755" (IFCTEXT)
    EMC Directive = "2004/108/EY" (IFCTEXT)
    EN Standard = "EN 15091" (IFCTEXT)
    LVI Number = "6110158" (IFCTEXT)
    NRF Number = "4200118" (IFCTEXT)
    RSK Number = "8348038" (IFCTEXT)
    STF Certificate = "STF VTT-RTH-00024-12" (IFCTEXT)
    Sintef Certificate = "Sintef Nr. 3080" (IFCTEXT)
    URL KIWA SE Type Approval = "http://static.oras.com/SETypeApproval/1724FT" (IFCTEXT)
    URL STF = "http://static.oras.com/STF/1724FT" (IFCTEXT)
    VA Certificate = "VA 1.42/20137" (IFCTEXT)
  Green Building Properties | properties | on 2 type objects
    Customs Code = "84818011" (IFCTEXT)
    EAN Number = "6414150078927" (IFCTEXT)
    EN Standard = "EN 817" (IFCTEXT)
    NRF Number = "4200415" (IFCTEXT)
    RSK Number = "8310573" (IFCTEXT)
    URL KIWA SE Type Approval = "http://static.oras.com/SETypeApproval/1038F" (IFCTEXT)
    VVS Number = "705897604" (IFCTEXT)
  Green Building Properties | properties | on 2 type objects
    Backflow Prevention EN1717 = "EB" (IFCTEXT)
    Customs Code = "84818011" (IFCTEXT)
    EAN Number = "6414150072543" (IFCTEXT)
    EN Standard = "EN 1111" (IFCTEXT)
    LVI Number = "6310786" (IFCTEXT)
    NRF Number = "4200519" (IFCTEXT)
    STF Certificate = "STF VTT-RTH-00028-11" (IFCTEXT)
    Sintef Certificate = "Sintef Nr. 0280" (IFCTEXT)
    URL SINTEF = "http://static.oras.com/Sintef/7267" (IFCTEXT)
    URL STF = "http://static.oras.com/STF/7267" (IFCTEXT)
  Green Building Properties | properties | on 1 type object
    Backflow Prevention EN1717 = "EB" (IFCTEXT)
    Customs Code = "84818011" (IFCTEXT)
    EAN Number = "6414150078118" (IFCTEXT)
    EN Standard = "EN 817" (IFCTEXT)
    NRF Number = "4200538" (IFCTEXT)
    RSK Number = "8296204" (IFCTEXT)
    VVS Number = "727259004" (IFCTEXT)
  Analytical Model | properties | on 12 type objects
    Fire Performance = "as Specified" (IFCTEXT)
  Layers | properties | on 10 type objects
    doubletier = TRUE (IFCBOOLEAN)
    doubletierheight = 866.3 (IFCLENGTHMEASURE) [MILLI METRE]
    singletier = TRUE (IFCBOOLEAN)
    singletierheight = 1732.6 (IFCLENGTHMEASURE) [MILLI METRE]
  Layers | properties | on 2 type objects
    doubletier = TRUE (IFCBOOLEAN)
    doubletierheight = 923.8 (IFCLENGTHMEASURE) [MILLI METRE]
    singletier = TRUE (IFCBOOLEAN)
    singletierheight = 1847.6 (IFCLENGTHMEASURE) [MILLI METRE]
  Horizontal Mullions | properties | on 3 type objects
    Border 1 Type = "Rectangular Mullion: 50x100" (IFCLABEL)
    Border 2 Type = "Rectangular Mullion: 50x100" (IFCLABEL)
    Interior Type = "Rectangular Mullion: 50x100" (IFCLABEL)
  Vertical Mullions | properties | on 3 type objects
    Border 1 Type = "Rectangular Mullion: 50x100" (IFCLABEL)
    Border 2 Type = "Rectangular Mullion: 50x100" (IFCLABEL)
    Interior Type = "Rectangular Mullion: 50x100" (IFCLABEL)
  Dør Enkel:IDT 2.6 10x21M 38dB:1753119 | predefined | on 2 type objects
  Dør Enkel:IDT 2.3 10x21M 33dB:1753211 | predefined | on 2 type objects
  Dør Enkel:IDT 2.1 10x21M:1753234 | predefined | on 2 type objects
  Dør Enkel:IDT 2.1 10x21M:1753235 | predefined | on 2 type objects
  Dør Enkel:IDT 2.4 10x21M 38dB EI30S:1753266 | predefined | on 2 type objects
  Dør Enkel_ Glassfelt:IDT 3.4 10x21M 33dB E30CS:1753271 | predefined | on 2 type objects
  Dør Enkel_ Glassfelt:IDT 3.2 10x21M 28dB EI30S:1753273 | predefined | on 2 type objects
  Dør Enkel:IDT 2.1 10x21M:1753276 | predefined | on 2 type objects
  Dør Enkel_ Glassfelt:IDT 3.8 10x21M 28dB E30CS:1753280 | predefined | on 2 type objects
  Dør Enkel:IDT 2.3 10x21M 33dB:1753282 | predefined | on 2 type objects
  Dør Enkel_ Glassfelt:IDA 5.1 10x21M 33dB:1755293 | predefined | on 2 type objects
  Dør Enkel_ Glassfelt:IDT 3.3 10x21M 33dB:1785179 | predefined | on 2 type objects
  Dør Enkel:IDT 2.9 10x21M EI60S:1785182 | predefined | on 2 type objects
  Dør Enkel_ Glassfelt:IDT 3.6 10x21M 38dB:1785264 | predefined | on 2 type objects
  Dør Enkel:IDT 2.6 10x21M 38dB:1785269 | predefined | on 2 type objects
  Dør Enkel_ Glassfelt:IDT 3.3 10x21M 33dB:1785271 | predefined | on 2 type objects
  Dør Enkel_ Glassfelt:IDT 3.3 10x21M 33dB:1785275 | predefined | on 2 type objects
  Dør Enkel:IDT 2.1 10x21M:1785281 | predefined | on 2 type objects
  Dør Enkel:IDT 1.1 8x21M:1785284 | predefined | on 2 type objects
  Dør Enkel:IDT 2.1 10x21M:1789941 | predefined | on 2 type objects
  Dør Dobbel:IDT 5.1 15x21M:1790017 | predefined | on 2 type objects
  Dør Enkel_ Glassfelt:IDA 1.1 10x21M:1795541 | predefined | on 2 type objects
  _Dør Dobbel_Ulike_Dørblader_Glassfelt2:YDA 1.2 16x21M EI 30S:1796394 | predefined | on 2 type objects
  Analysis Results | properties | on 16 type objects
    Glass Area = 1.616836 (IFCAREAMEASURE) [SQUARE_METRE]
  Analysis Results | properties | on 15 type objects
    Glass Area = 2.218636 (IFCAREAMEASURE) [SQUARE_METRE]
  Analysis Results | properties | on 10 type objects
    Glass Area = 1.015036 (IFCAREAMEASURE) [SQUARE_METRE]
  Analysis Results | properties | on 5 type objects
    Glass Area = 2.277128 (IFCAREAMEASURE) [SQUARE_METRE]
  Analysis Results | properties | on 5 type objects
    Glass Area = 3.422236 (IFCAREAMEASURE) [SQUARE_METRE]
  Analysis Results | properties | on 4 type objects
    Glass Area = 1.914528 (IFCAREAMEASURE) [SQUARE_METRE]
  Analysis Results | properties | on 4 type objects
    Glass Area = 3.592836 (IFCAREAMEASURE) [SQUARE_METRE]
  Analysis Results | properties | on 4 type objects
    Glass Area = 1.839836 (IFCAREAMEASURE) [SQUARE_METRE]
  Analysis Results: 24 more contents on 0 objects not shown
  Enfløyet_aludør:IDA 7.1 15x21M EI60CS:1700924 | predefined | on 2 type objects
  Dør Enkel:IDT 2.6 10x21M 38dB:1799472 | predefined | on 2 type objects
  Dør Enkel:IDT 2.6 10x21M 38dB:1799883 | predefined | on 2 type objects
  Dør Enkel_ Glassfelt:IDT 3.5 10x21M 38dB EI30S:1814193 | predefined | on 2 type objects
  Dør Enkel_ Glassfelt:IDT 3.3 10x21M 33dB:1814533 | predefined | on 2 type objects
  Dør Enkel_ Glassfelt:IDA 1.1 10x21M:1816112 | predefined | on 2 type objects
  Dør Enkel:IDT 2.1 10x21M:1818637 | predefined | on 2 type objects
  Dør Enkel:IDT 2.1 10x21M:1819618 | predefined | on 2 type objects
  Dør Enkel:IDT 2.3 10x21M 33dB:1819877 | predefined | on 2 type objects
  Dør Enkel_ Glassfelt:IDT 3.3 10x21M 33dB:1824007 | predefined | on 2 type objects
  Dør Enkel:IDT 1.3 8x21M EI30S:1824685 | predefined | on 2 type objects
  Dør Enkel:IDT 1.1 8x21M:1824708 | predefined | on 2 type objects
  Dør Enkel_ Glassfelt:IDT 3.6 10x21M 38dB:1829818 | predefined | on 2 type objects
  Dør Enkel_ Glassfelt:IDT 3.2 10x21M 28dB EI30S:1830486 | predefined | on 2 type objects
  Dør Enkel_ Glassfelt:IDT 3.6 10x21M 38dB:1830683 | predefined | on 2 type objects
  _Dør Dobbel_Ulike_Dørblader_Glassfelt:IDA 3.3 18x21M 33dB EI60CS:1851355 | predefined | on 2 type objects
  _Dør Dobbel_Ulike_Dørblader_Glassfelt:IDA 3.4 18x21M EI30CS:1851357 | predefined | on 2 type objects
  Dør Enkel_ Glassfelt:IDT 3.3 10x21M 33dB:1851361 | predefined | on 2 type objects
  Dør Enkel_ Glassfelt:IDT 3.3 10x21M 33dB:1851362 | predefined | on 2 type objects
  Dør Enkel_ Glassfelt:IDT 3.3 10x21M 33dB:1851363 | predefined | on 2 type objects
  Vindu-Hengslet:V13 12x16:1852971 | predefined | on 1 type object
  Dør Enkel:IDT 2.9 10x21M EI60S:1865778 | predefined | on 2 type objects
  Dør Enkel_ Glassfelt:IDA 1.1 10x21M:1899884 | predefined | on 2 type objects
  Dør Dobbel:IDT 5.2 15x21M EI60S:1899943 | predefined | on 2 type objects
  Dør Enkel:IDT 2.2 10x21M 28dB EI30S:1924849 | predefined | on 2 type objects
  Dør Dobbel:IDT 5.2 15x21M EI60S:1937235 | predefined | on 2 type objects
  Dør Enkel:IDT 1.2 8x21M 33dB:1963500 | predefined | on 2 type objects
  Dør Enkel:IDT 2.9 10x21M EI60S:1968215 | predefined | on 2 type objects
  Dør Enkel:IDT 2.8 10x21M EI30S:2008423 | predefined | on 2 type objects
  Dør Enkel_ Glassfelt:IDT 3.6 10x21M 38dB:1781401 | predefined | on 2 type objects
  Dør Enkel:IDT 2.6 10x21M 38dB:2017473 | predefined | on 2 type objects
  Dør Enkel:IDT 2.6 10x21M 38dB:2017476 | predefined | on 2 type objects
  Dør Enkel:IDT 2.3 10x21M 33dB:2017571 | predefined | on 2 type objects
  Dør Enkel:IDT 2.11 10x21M 33dB EI30S:2067575 | predefined | on 2 type objects
  Dør Enkel:IDT 2.3 10x21M 33dB:2072049 | predefined | on 2 type objects
  Dør Enkel:IDT 1.2 8x21M 33dB:2072563 | predefined | on 2 type objects
  Dør Enkel:IDT 2.1 10x21M:2073002 | predefined | on 2 type objects
  Dør Enkel:IDT 2.3 10x21M 33dB:2074784 | predefined | on 2 type objects
  Dør Enkel:IDT 2.12 10x21M 24dB EI30S:2077177 | predefined | on 2 type objects
  Dør Enkel_ Glassfelt:IDT 3.4 10x21M 33dB E30CS:2080687 | predefined | on 2 type objects
  Dør Enkel:IDT 2.1 10x21M:2109495 | predefined | on 2 type objects
  Dør Enkel_ Glassfelt:IDA 1.1 10x21M:2110693 | predefined | on 2 type objects
  Dør Enkel:IDT 2.3 10x21M 33dB:2111466 | predefined | on 2 type objects
  Dør Enkel:IDT 2.3 10x21M 33dB:2111527 | predefined | on 2 type objects
  Dør Enkel:IDT 1.2 8x21M 33dB:2083379 | predefined | on 2 type objects
  Dør Enkel:IDA 10.1 14x21M E30CS:2114687 | predefined | on 2 type objects
  Dør Enkel:IDT 2.4 10x21M 38dB EI30S:2115769 | predefined | on 2 type objects
  Dør Enkel_ Glassfelt:IDT 3.1 10x21M EI 30S:2118010 | predefined | on 2 type objects
  Dør Enkel:IDT 2.9 10x21M EI60S:2134991 | predefined | on 2 type objects
  Dør Enkel:IDT 2.10 10x21M 38dB EI60S:2135168 | predefined | on 2 type objects
  Dør Enkel_ Glassfelt:IDT 3.6 10x21M 38dB:2135766 | predefined | on 2 type objects
  Dør Dobbel_Ulike_Dørblader:IDT 4.2 13x21M EI 60S:2137996 | predefined | on 2 type objects
  Dør Enkel_ Glassfelt:IDT 3.6 10x21M 38dB:1825698 | predefined | on 2 type objects
  Dør Enkel:IDT 2.7 10x21M 38dB EI60S:2154214 | predefined | on 2 type objects
  Side_Stack_Operable_Wall_6500:IDF 1.1 Foldevegg 6500x2800:2154531 | predefined | on 2 type objects
  Dør Enkel_ Glassfelt:IDA 6.2 12x21M EI 30CS:1700926 | predefined | on 2 type objects
  Dør Enkel:IDT 2.1 10x21M:2187712 | predefined | on 2 type objects
  Dør Enkel:IDT 2.1 10x21M:2223619 | predefined | on 2 type objects
  Dør Enkel:IDT 2.5 10x21M 33dB EI60S:2235152 | predefined | on 2 type objects
  _Dør Dobbel_Ulike_Dørblader_Glassfelt2:IDA 3.2 18x21M 33dB:2235278 | predefined | on 2 type objects
  Dør Enkel:IDT 2.9 10x21M EI60S:2379978 | predefined | on 2 type objects
  Vindu-Hengslet:V13 12x16:2425648 | predefined | on 1 type object
  Fast vindu+ åpningsvindu:V15 24x16:2427850 | predefined | on 1 type object
  Vindu-Fast:V14 14x16:2430034 | predefined | on 1 type object
  Vindu-Fast:V14 14x16:2431102 | predefined | on 1 type object
  Dør Enkel:IDT 2.5 10x21M 33dB EI60S:2467851 | predefined | on 2 type objects
  Dør Enkel:IDT 2.5 10x21M 33dB EI60S:2467890 | predefined | on 2 type objects
  Dør Enkel:IDT 2.1 10x21M:2486526 | predefined | on 2 type objects
  Dør Enkel:IDT 2.1 10x21M:2486579 | predefined | on 2 type objects
  Dør Enkel:IDT 2.1 10x21M:2487384 | predefined | on 2 type objects
  Dør Enkel:IDT 2.1 10x21M:2488521 | predefined | on 2 type objects
  Vindu-Fast:GF 3.6 6x21 33dB:2525684 | predefined | on 1 type object
  Vindu-Fast:GF 3.6 6x21 33dB:2525792 | predefined | on 1 type object
  Vindu-Fast:GF 6.1 8x21 33dB:2527002 | predefined | on 1 type object
  Vindu-Fast:GF 2.2 9x21 33dB:2504598 | predefined | on 1 type object
  Vindu-Fast:GF 2.2 9x21 33dB:2527134 | predefined | on 1 type object
  Vindu-Fast:GF 2.2 9x21 33dB:2527173 | predefined | on 1 type object
  Vindu-Fast:GF 2.2 9x21 33dB:2527217 | predefined | on 1 type object
  Vindu-Fast:GF 2.2 9x21 33dB:2527241 | predefined | on 1 type object
  Vindu-Fast:GF 2.1 9x21 38dB:2527441 | predefined | on 1 type object
  Vindu-Fast:GF 5.3 5x21 33dB:2527482 | predefined | on 1 type object
  Vindu-Fast:GF 15.1 36x10 33dB:2529032 | predefined | on 1 type object
  Vindu-Fast:GF 8.1 7x7 58dB:2529523 | predefined | on 1 type object
  Vindu-Fast:GF 2.4 9x21 25dB E30:2529908 | predefined | on 1 type object
  Vindu-Fast:GF 2.3 9x21 25dB EI30:2530890 | predefined | on 1 type object
  Vindu-Fast:GF 3.1 6x21 25dB EI30:2531956 | predefined | on 1 type object
  Vindu_2felt:GF 4.3 33dB EI30:2532106 | predefined | on 1 type object
  Vindu-Fast:GF 3.4 6x21 33dB E30:2532146 | predefined | on 1 type object
  Vindu-Fast:GF 2.2 9x21 33dB:2532505 | predefined | on 1 type object
  Vindu-Fast:GF 2.2 9x21 33dB:2532609 | predefined | on 1 type object
  Vindu-Fast:GF 6.1 8x21 33dB:2532752 | predefined | on 1 type object
  Analysis Results(Type) | properties | on 2 type objects
    Glass Area = 2.550436 (IFCAREAMEASURE) [SQUARE_METRE]
  Analysis Results(Type) | properties | on 2 type objects
    Glass Area = 1.647828 (IFCAREAMEASURE) [SQUARE_METRE]
  Analysis Results(Type) | properties | on 1 type object
    Glass Area = 3.214036 (IFCAREAMEASURE) [SQUARE_METRE]
  Analysis Results(Type) | properties | on 1 type object
    Glass Area = 2.571336 (IFCAREAMEASURE) [SQUARE_METRE]
  Vindu-Fast:V25 12x30 36dB:2535368 | predefined | on 1 type object
  Vindu-Fast:VA1 12x24:2537605 | predefined | on 1 type object
  Vindu-Fast:GF 7.4 15x21 EI60:2552756 | predefined | on 1 type object
  Dør Enkel_ Glassfelt:IDT 3.9 10x21M 28dB:2571576 | predefined | on 2 type objects
  Vindu-Fast:GF 7.1 15x21 25dB:2571640 | predefined | on 1 type object
  Dør Enkel:YDT 1.2 10x21M Isolert:2583745 | predefined | on 2 type objects
  Vindu-Fast:VA1 12x24:2601155 | predefined | on 1 type object
  Vindu-Fast:GF 3.2 6x21 38dB:2498596 | predefined | on 1 type object
  Dør Enkel:IDT 2.3 10x21M 33dB:2834668 | predefined | on 2 type objects
  _Dør Dobbel_Ulike_Dørblader_Glassfelt2:YDA 1.2 16x21M EI 30S:2980271 | predefined | on 2 type objects
  _Dør Dobbel_Ulike_Dørblader_Glassfelt2:YDA 1.2 16x21M EI 30S:2980522 | predefined | on 2 type objects
  Dør Enkel:IDT 9.1 10x21M:3427527 | predefined | on 2 type objects
  Dør Enkel_ Glassfelt:IDT 3.5 10x21M 38dB EI30S:3433322 | predefined | on 2 type objects
  Vindu-Hengslet:GF 8.2 58dB:3566352 | predefined | on 1 type object
  Dør Enkel:IDA 9.1 12x21M EI60CS:3676346 | predefined | on 2 type objects
  Enfløyet_aludør:IDA 7.1 15x21M EI60CS:1700923 | predefined | on 2 type objects
  Dør Dobbel_Ulike_Dørblader:IDA 3.5 18x21M 33dB EI30S:3705902 | predefined | on 2 type objects
  Vindu-Fast:V22 14x14:2393061 | predefined | on 1 type object
  Dør Enkel:YDS 2.1 13x21M:3971723 | predefined | on 2 type objects
  Dør Enkel_ Glassfelt_glassfelt over:YDA 2.1 12x30 36dB:3974002 | predefined | on 2 type objects
  Dør Enkel:IDT 2.8 10x21M EI30S:3988230 | predefined | on 2 type objects
  Doors-Sliding_Manusa_Biparting_sliding_fixed_INT:YDA 6.1 Skyvedører:4108057 | predefined | on 2 type objects
  Dør Enkel:YDT 1.1 10x21M:4118873 | predefined | on 2 type objects
  Dør Enkel_ Glassfelt:IDT 3.6 10x21M 38dB:2097868 | predefined | on 2 type objects
  Dør Enkel_ Glassfelt:IDT 3.2 10x21M 28dB EI30S:4195576 | predefined | on 2 type objects
  Dør Enkel:YDT 1.2 10x21M Isolert:4202873 | predefined | on 2 type objects
  M_Overhead-Sectional:YDP 1.1 2400 x 2100mm:4214299 | predefined | on 2 type objects
  Dør Enkel_ Glassfelt:IDA 1.1 10x21M:4270404 | predefined | on 2 type objects
  Dør Enkel_ Glassfelt:IDA 1.1 10x21M:4270571 | predefined | on 2 type objects
  Visibility(Type) | properties | on 2 type objects
    Door Handle Left On = TRUE (IFCBOOLEAN)
    Door Handle Right On = TRUE (IFCBOOLEAN)
  _Dør Dobbel_Ulike_Dørblader_Glassfelt2:IDT 6.1 15x21M 33dB:4433797 | predefined | on 2 type objects
  M_Overhead-Rolling:1700 x 2100mm:4451019 | predefined | on 2 type objects
  _Dør Dobbel_Ulike_Dørblader_Glassfelt2:IDT 6.2 15x21M 38dB:4452497 | predefined | on 2 type objects
  Vindu-Fast:GF 2.2 9x21 33dB:3088169 | predefined | on 1 type object
  _Dør Dobbel_Ulike_Dørblader_Glassfelt:YDA 5.1 16x21M:4543202 | predefined | on 2 type objects
  Vindu_3felt:GF 13.1 36x21 38dB:5149291 | predefined | on 1 type object
  Vindu_2felt:GF 14.1:5156029 | predefined | on 1 type object
  Fast vindu+ åpningsvindu:V16 21x16:5422930 | predefined | on 1 type object
  Fast vindu+ åpningsvindu:V17 21x16:5423978 | predefined | on 1 type object
  Fast vindu+ åpningsvindu:V18 21x16:5427464 | predefined | on 1 type object
  Fast vindu+ åpningsvindu:V19 21x16:5427952 | predefined | on 1 type object
  Fast vindu+ åpningsvindu:V19 21x16:5428378 | predefined | on 1 type object
  Fast vindu+ åpningsvindu:V20 19x16:5428885 | predefined | on 1 type object
  Fast vindu+ åpningsvindu:V15 24x16:5429707 | predefined | on 1 type object
  Fast vindu+ åpningsvindu:V21 35x16:5430404 | predefined | on 1 type object
  Vindu-Fast:GF 14.2 12x21 33dB E30:5676778 | predefined | on 1 type object
  Doors-Sliding_Manusa_Biparting_sliding_fixed_INT:YDA 6.1 Skyvedører:5720315 | predefined | on 2 type objects
  Dør Dobbel_Ulike_Dørblader:IDA 2.2 15x21M EI60SC:5866724 | predefined | on 2 type objects
  Dør Enkel_ Glassfelt:IDA 6.1 12x21M EI60 CS:5876404 | predefined | on 2 type objects
  M_Overhead-Rolling:2680 x 1275mm:5883834 | predefined | on 2 type objects
  Enfløyet_aludør:IDA 7.1 15x21M EI60CS:5924061 | predefined | on 2 type objects
  Dør Enkel_ Glassfelt:YDA 4.1 14x21M:5953506 | predefined | on 2 type objects
  Dør Enkel_ Glassfelt:YDA 4.1 14x21M:5953837 | predefined | on 2 type objects
  Rullegitter:2680 x 1275mm:7267956 | predefined | on 2 type objects
  Luke600:Luke 10M:7318563 | predefined | on 2 type objects
  Dør Enkel:IDT 10.1 7x21M:7828245 | predefined | on 2 type objects
  Electrical | properties | on 3 type objects
    Electrical Connection = "230 / 12 V" (IFCTEXT)
    Electronic Parts = "Autofocus sensor" (IFCTEXT)
  Electrical Engineering | properties | on 3 type objects
    Operating Voltage = 12. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
  Dør Enkel:IDT 1.2 8x21M 33dB:1725481 | predefined | on 2 type objects
  Dør Dobbel_Ulike_Dørblader:IDA 2.2 15x21M EI60SC:1728746 | predefined | on 2 type objects
  Vindu-Hengslet:V23 14x14:1761672 | predefined | on 1 type object
  Dør Enkel:IDT 2.3 10x21M 33dB:1779794 | predefined | on 2 type objects
  Side_Stack_Operable_Wall_8000:IDF 2.1 Foldevegg 8000x2800:1780830 | predefined | on 2 type objects
  _Dør Dobbel_Ulike_Dørblader_Glassfelt:YDA 5.2 16x21M EI 30S:1835036 | predefined | on 2 type objects
  _Dør Dobbel_Ulike_Dørblader_Glassfelt2:IDT 6.1 15x21M 33dB:1837647 | predefined | on 2 type objects
  Dør Enkel_ Glassfelt:IDT 3.3 10x21M 33dB:1841845 | predefined | on 2 type objects
  Dør Enkel_ Glassfelt:IDA 6.2 12x21M EI 30CS:1848683 | predefined | on 2 type objects
  _Dør Dobbel_Ulike_Dørblader_Glassfelt:IDA 3.1 18x21M 33db EI30S:1852022 | predefined | on 2 type objects
  Dør Enkel:IDT 2.3 10x21M 33dB:1857757 | predefined | on 2 type objects
  Dør Enkel_ Glassfelt:IDT 3.3 10x21M 33dB:1863225 | predefined | on 2 type objects
  Dør Enkel:IDT 2.1 10x21M:1866280 | predefined | on 2 type objects
  _Dør Dobbel_Ulike_Dørblader_Glassfelt:IDA 3.1 18x21M 33db EI30S:1870405 | predefined | on 2 type objects
  Dør Enkel:IDT 1.2 8x21M 33dB:1881849 | predefined | on 2 type objects
  Dør Enkel:IDT 1.1 8x21M:1881980 | predefined | on 2 type objects
  Dør Enkel_ Glassfelt:IDT 3.6 10x21M 38dB:1886980 | predefined | on 2 type objects
  Vindu-Fast:V3 18x22:1892833 | predefined | on 1 type object
  Vindu-Fast:V4 23x22:1896885 | predefined | on 1 type object
  Vindu-Fast:V22 14x14:1897688 | predefined | on 1 type object
  Vindu-Hengslet_1200 opening:V1 12x22:1898390 | predefined | on 1 type object
  Vindu-Hengslet_1200 opening:V1 12x22:1898690 | predefined | on 1 type object
  Vindu-Fast:V3 18x22:1899683 | predefined | on 1 type object
  Vindu-Fast:V4 23x22:1899685 | predefined | on 1 type object
  Vindu-Fast:V22 14x14:1901278 | predefined | on 1 type object
  _Dør Dobbel_Ulike_Dørblader_Glassfelt:IDA 3.1 18x21M 33db EI30S:1904044 | predefined | on 2 type objects
  Dør Enkel_ Glassfelt:IDT 3.6 10x21M 38dB:1904138 | predefined | on 2 type objects
  Dør Enkel_ Glassfelt:IDT 3.6 10x21M 38dB:1904144 | predefined | on 2 type objects
  Dør Enkel_ Glassfelt:IDT 3.6 10x21M 38dB:1904145 | predefined | on 2 type objects
  Dør Enkel_ Glassfelt:IDT 3.6 10x21M 38dB:1904154 | predefined | on 2 type objects
  Dør Dobbel:IDT 5.2 15x21M EI60S:1937292 | predefined | on 2 type objects
  Dør Enkel_ Glassfelt:IDT 3.3 10x21M 33dB:1941435 | predefined | on 2 type objects
  Side_Stack_Operable_Wall_h2500_w9700:IDF 3.1 Foldevegg 9700x2500:2031491 | predefined | on 2 type objects
  Vindu-Fast:GFA 3 8x27 38dB:2067745 | predefined | on 1 type object
  Dør Enkel:IDT 1.2 8x21M 33dB:2083373 | predefined | on 2 type objects
  Dør Enkel_ Glassfelt:IDT 3.3 10x21M 33dB:2099229 | predefined | on 2 type objects
  Dør Enkel_ Glassfelt:IDT 3.3 10x21M 33dB:2105557 | predefined | on 2 type objects
  Dør Enkel:IDT 1.1 8x21M:2147861 | predefined | on 2 type objects
  Dør Enkel:IDT 1.1 8x21M:2147862 | predefined | on 2 type objects
  Dør Dobbel:IDT 5.2 15x21M EI60S:2179297 | predefined | on 2 type objects
  Dør Dobbel:IDT 5.2 15x21M EI60S:2179356 | predefined | on 2 type objects
  Dør Enkel_ Glassfelt:IDT 3.6 10x21M 38dB:2186885 | predefined | on 2 type objects
  Dør Enkel_ Glassfelt:IDT 3.3 10x21M 33dB:2187413 | predefined | on 2 type objects
  Dør Enkel:IDT 2.1 10x21M:2187786 | predefined | on 2 type objects
  Vindu-Fast:V2 12x22:2275275 | predefined | on 1 type object
  Dør Enkel:IDT 1.1 8x21M:2275999 | predefined | on 2 type objects
  Vindu-Fast:V5 8x22:2399390 | predefined | on 1 type object
  Vindu-Hengslet_1200 opening:V1 12x22:2416707 | predefined | on 1 type object
  Vindu-Hengslet:V23 14x14:2424325 | predefined | on 1 type object
  Vindu-Fast:GF 1.3 12x21 38dB:2493195 | predefined | on 1 type object
  Vindu-Fast:GF 3.3 6x21 44dB:2493355 | predefined | on 1 type object
  Vindu-Fast:GF 1.1 12x21 33dB:2493862 | predefined | on 1 type object
  Vindu-Fast:GF 4.2 18x21 33dB:2498708 | predefined | on 1 type object
  Vindu-Fast:GF 4.2 18x21 33dB:2499363 | predefined | on 1 type object
  Vindu-Fast:GF 1.1 12x21 33dB:2500259 | predefined | on 1 type object
  Vindu-Fast:GF 1.3 12x21 38dB:2500325 | predefined | on 1 type object
  Vindu-Fast:GF 4.1 18x21 38dB:2500740 | predefined | on 1 type object
  Vindu-Fast:GF 10.2 8x27 38dB:2500909 | predefined | on 1 type object
  Vindu-Fast:GF 4.2 18x21 33dB:2501801 | predefined | on 1 type object
  Vindu-Fast:GF 10.2 8x27 38dB:2504695 | predefined | on 1 type object
  Vindu-Fast:GF 1.1 12x21 33dB:2504942 | predefined | on 1 type object
  Vindu-Fast:GF 3.3 6x21 44dB:2505781 | predefined | on 1 type object
  Vindu-Fast:GF 11.1 12x27 33dB:2505892 | predefined | on 1 type object
  Vindu-Fast:GF 2.2 9x21 33dB:2506361 | predefined | on 1 type object
  Vindu-Fast:GF 6.1 8x21 33dB:2506671 | predefined | on 1 type object
  Vindu-Fast:GF 1.1 12x21 33dB:2506898 | predefined | on 1 type object
  Vindu-Fast:GF 7.2 15x21 38dB:2506998 | predefined | on 1 type object
  Vindu-Fast:GF 3.6 6x21 33dB:2507587 | predefined | on 1 type object
  Vindu-Fast:GF 7.2 15x21 38dB:2507681 | predefined | on 1 type object
  Vindu-Fast:GF 1.3 12x21 38dB:2507723 | predefined | on 1 type object
  Vindu-Fast:GF 4.1 18x21 38dB:2508145 | predefined | on 1 type object
  Vindu-Fast:GF 2.2 9x21 33dB:2508462 | predefined | on 1 type object
  Vindu-Fast:GF 1.1 12x21 33dB:2569729 | predefined | on 1 type object
  Vindu-Fast:GF 1.3 12x21 38dB:2836552 | predefined | on 1 type object
  Vindu-Fast:GF 3.2 6x21 38dB:2846481 | predefined | on 1 type object
  Vindu-Fast:GF 1.4 12x21 44dB:2992305 | predefined | on 1 type object
  Vindu-Fast:GF 1.1 12x21 33dB:2994099 | predefined | on 1 type object
  Vindu-Fast:GF 2.1 9x21 38dB:2995137 | predefined | on 1 type object
  Dør Enkel_ Glassfelt:IDT 3.6 10x21M 38dB:2988444 | predefined | on 2 type objects
  Vindu-Fast:GF 1.1 12x21 33dB:2988448 | predefined | on 1 type object
  Vindu-Fast:GF 9.1 11x26.5 33dB:2988449 | predefined | on 1 type object
  Vindu-Fast:GF 16.1 5x31 38dB:2997461 | predefined | on 1 type object
  Vindu-Fast:GF 1.1 12x21 33dB:2987832 | predefined | on 1 type object
  Vindu-Fast:GF 12.1 6x31 38dB:2998710 | predefined | on 1 type object
  M_Overhead-Rolling:1700 x 2100mm:3038740 | predefined | on 2 type objects
  Dør Enkel:IDT 2.3 10x21M 33dB:2997375 | predefined | on 2 type objects
  Dør Enkel:IDT 2.3 10x21M 33dB:2997376 | predefined | on 2 type objects
  Vindu-Fast:GF 12.1 6x31 38dB:3212641 | predefined | on 1 type object
  Vindu-Fast:GF 12.1 6x31 38dB:3217776 | predefined | on 1 type object
  Vindu-Fast:GF 10.1 8x27 33dB:3382692 | predefined | on 1 type object
  Dør Enkel:IDT 2.1 10x21M:3443650 | predefined | on 2 type objects
  Vindu-Fast:V3 18x22:3466359 | predefined | on 1 type object
  Dør Enkel:IDA 10.1 14x21M E30CS:3697547 | predefined | on 2 type objects
  Dør Enkel_ Glassfelt:IDT 3.3 10x21M 33dB:4000707 | predefined | on 2 type objects
  Dør Enkel_ Glassfelt:IDT 3.3 10x21M 33dB:4202122 | predefined | on 2 type objects
  Vindu-Fast:V5 8x22:4272094 | predefined | on 1 type object
  Dør Dobbel_Ulike_Dørblader:IDT 7.1 13x21M 38dB:4801842 | predefined | on 2 type objects
  Vindu-Fast:GFA 3 8x27 38dB:4804571 | predefined | on 1 type object
  Vindu-Fast:GF 1.3 12x21 38dB:5046044 | predefined | on 1 type object
  Vindu_3felt:GF 13.1 36x21 38dB:5153882 | predefined | on 1 type object
  Vindu 3 felt:V7 24x22:5436093 | predefined | on 1 type object
  Vindu 3 felt:V11 35x22:5444204 | predefined | on 1 type object
  Vindu 3 felt:V9 30x22:5444681 | predefined | on 1 type object
  Vindu 3 felt:V10 30x22:5444956 | predefined | on 1 type object
  Vindu 3 felt:V9 30x22:5445253 | predefined | on 1 type object
  Vindu 3 felt:V8 27x22:5445842 | predefined | on 1 type object
  Vindu 3 felt:V6 24x22:5446097 | predefined | on 1 type object
  Vindu 3 felt:V7 24x22:5446726 | predefined | on 1 type object
  Vindu 3 felt:V10 30x22:5447393 | predefined | on 1 type object
  Vindu 3 felt:V12 35x22:5463949 | predefined | on 1 type object
  Vindu 3 felt:V11 35x22:5464245 | predefined | on 1 type object
  Vindu 3 felt:V12 35x22:5464550 | predefined | on 1 type object
  Vindu 3 felt:V6 24x22:5472792 | predefined | on 1 type object
  _Dør Dobbel_Ulike_Dørblader_Glassfelt2:IDT 8.1 18x21M 33dB:6481045 | predefined | on 2 type objects
  Luke600:Luke 600:6609756 | predefined | on 2 type objects
  Luke600:Luke 600:6623186 | predefined | on 2 type objects
  Enfløyet_aludør:IDA 7.1 15x21M EI60CS:1700918 | predefined | on 2 type objects
  Enfløyet_aludør:IDA 7.1 15x21M EI60CS:1700920 | predefined | on 2 type objects
  _Dør Dobbel_Ulike_Dørblader_Glassfelt:IDA 3.1 18x21M 33db EI30S:1915951 | predefined | on 2 type objects
  Vindu-Fast:V24 20x20:2217007 | predefined | on 1 type object
  Vindu-Fast:V24 20x20:2217110 | predefined | on 1 type object
  _Dør Dobbel_Ulike_Dørblader:YDS 1.2 15x21M EI 60S:2389213 | predefined | on 2 type objects
  _Dør Dobbel_Ulike_Dørblader:YDS 1.1 15x21M:2389269 | predefined | on 2 type objects
  Vindu-Fast:V3 18x22:2424976 | predefined | on 1 type object
  Vindu-Fast:V2 12x22:2424980 | predefined | on 1 type object
  Vindu-Fast:GF 3.3 6x21 44dB:2523913 | predefined | on 1 type object
  Dør Enkel:IDT 2.1 10x21M:2550978 | predefined | on 2 type objects
  Dør Dobbel:IDS 3.1 18x21M 38dB EI60S:2551141 | predefined | on 2 type objects
  Dør Dobbel:IDS 3.1 18x21M 38dB EI60S:2551181 | predefined | on 2 type objects
  Dør Enkel:IDT 2.3 10x21M 33dB:2997367 | predefined | on 2 type objects
  Dør Enkel_ Glassfelt:IDT 3.6 10x21M 38dB:2998549 | predefined | on 2 type objects
  Vindu-Fast:GF 10.1 8x27 33dB:3382939 | predefined | on 1 type object
  Dør Enkel_ Glassfelt:IDT 3.6 10x21M 38dB:4003185 | predefined | on 2 type objects
  Dør Enkel_ Glassfelt:IDT 3.6 10x21M 38dB:4003197 | predefined | on 2 type objects
  Vindu-Fast:GF 2.1 9x21 38dB:4003198 | predefined | on 1 type object
  Vindu-Fast:GF 2.1 9x21 38dB:4003205 | predefined | on 1 type object
  Vindu 3 felt:V6 24x22:5449631 | predefined | on 1 type object
  _Dør Dobbel_Ulike_Dørblader_Glassfelt2:IDT 8.1 18x21M 33dB:6481147 | predefined | on 2 type objects