IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition[CoordinationView_V2.0, QuantityTakeOffAddOnView]"
Description: "ExchangeRequirement[Structural, SurfaceGeometry]"
Description: "Option [BaseQuantities:On]"
Description: "Option [GridExport:On]"
Description: "Option [Assemblies:Off]"
Description: "Option [Bolts:On]"
Description: "Option [Rebars:On]"
Description: "Option [PourObjects:Off]"
Description: "Option [Welds:Off]"
Description: "Option [SurfaceTreatments:Off]"
Description: "Option [LocationBy:-2147483648]"
Description: "Option [ViewColors:On]"
Description: "Option [SectionedSpine:On]"
Description: "Option [PropertySets:On]"
Description: "Option [Export all:Off]"
File name: "M3D-CON-CD.ifc"
Time stamp: "2021-11-05T12:12:50"
Author: "DESKTOP-TK2EL9U\QC-PC-JAMES"
Organization: "Structural Designer"
Preprocessor: "IFC Database Version: Work"
Originating system: "Tekla Structures 2020 Service Pack 9, IFC Export Version: 4.0.0.0 Jun 21 2021"
Application: "Tekla Structures" version "2020 Service Pack 9" identifier "Multi material modeling" by Organization "Trimble Solutions Corporation"

People and organizations
  Person "Undefined" id "DESKTOP-TK2EL9U\QC-PC-JAMES" of Organization "Trimble Solutions Corporation"
  Owner history of Person "Undefined" id "DESKTOP-TK2EL9U\QC-PC-JAMES" of Organization "Trimble Solutions Corporation" | application "Tekla Structures" version "2020 Service Pack 9" identifier "Multi material modeling" by Organization "Trimble Solutions Corporation" | change NOCHANGE | created 1636132318 (2021-11-05T17:11:58Z)
  Owner history of Person "Undefined" id "DESKTOP-TK2EL9U\QC-PC-JAMES" of Organization "Trimble Solutions Corporation" | application "Tekla Structures" version "2020 Service Pack 9" identifier "Multi material modeling" by Organization "Trimble Solutions Corporation" | change NOCHANGE | created 1636063200 (2021-11-04T22:00:00Z)
  Owner history of Person "Undefined" id "DESKTOP-TK2EL9U\QC-PC-JAMES" of Organization "Trimble Solutions Corporation" | application "Tekla Structures" version "2020 Service Pack 9" identifier "Multi material modeling" by Organization "Trimble Solutions Corporation" | change NOCHANGE | created 1635462000 (2021-10-28T23:00:00Z)
  Owner history of Person "Undefined" id "DESKTOP-TK2EL9U\QC-PC-JAMES" of Organization "Trimble Solutions Corporation" | application "Tekla Structures" version "2020 Service Pack 9" identifier "Multi material modeling" by Organization "Trimble Solutions Corporation" | change NOCHANGE | created 1633039200 (2021-09-30T22:00:00Z)
  Owner history of Person "Undefined" id "DESKTOP-TK2EL9U\QC-PC-JAMES" of Organization "Trimble Solutions Corporation" | application "Tekla Structures" version "2020 Service Pack 9" identifier "Multi material modeling" by Organization "Trimble Solutions Corporation" | change NOCHANGE | created 1633363200 (2021-10-04T16:00:00Z)
  Owner history of Person "Undefined" id "DESKTOP-TK2EL9U\QC-PC-JAMES" of Organization "Trimble Solutions Corporation" | application "Tekla Structures" version "2020 Service Pack 9" identifier "Multi material modeling" by Organization "Trimble Solutions Corporation" | change NOCHANGE | created 1634662800 (2021-10-19T17:00:00Z)
  Owner history of Person "Undefined" id "DESKTOP-TK2EL9U\QC-PC-JAMES" of Organization "Trimble Solutions Corporation" | application "Tekla Structures" version "2020 Service Pack 9" identifier "Multi material modeling" by Organization "Trimble Solutions Corporation" | change NOCHANGE | created 1635980400 (2021-11-03T23:00:00Z)
  Owner history of Person "Undefined" id "DESKTOP-TK2EL9U\QC-PC-JAMES" of Organization "Trimble Solutions Corporation" | application "Tekla Structures" version "2020 Service Pack 9" identifier "Multi material modeling" by Organization "Trimble Solutions Corporation" | change NOCHANGE | created 1634835600 (2021-10-21T17:00:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  MASSUNIT: KILO GRAM
  TIMEUNIT: SECOND
  PLANEANGLEUNIT: RADIAN
  SOLIDANGLEUNIT: STERADIAN
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  LUMINOUSINTENSITYUNIT: LUMEN

Spatial structure
IFCPROJECT "VIA DE EVITAMIENTO DE CHIMBOTE"
  IFCSITE "VIA EXPRESA CHIMBOTE"
    IFCBUILDING "PUENTE SANTA" | postal address: "CHIMBOTE", "ANCASH", "PERU"
      contains 13 elements
        13 x IFCGRID | names: "+27.508", "+27.290", "+24.908" (+10 more)
    IFCBUILDING "Calzada Derecha"
      IFCBUILDINGSTOREY "Aislador" | elevation 0.
        contains 61 elements
          2 x IFCPLATE | type IFCPLATETYPE "PL10*600" | object type "PL10*600" | names: "PLATE" | descriptions: "PL10*600" | material: "STEEL/S235JR" | property sets: QC_Standard, Tekla Quantity, Pset_PlateCommon, BaseQuantities, Tekla Common
          2 x IFCPLATE | type IFCPLATETYPE "PL10*552" | object type "PL10*552" | names: "Base Plate" | descriptions: "PL10*552" | material: "STEEL/S235JR" | property sets: QC_Standard, Tekla Quantity, Pset_PlateCommon, Tekla Common, BaseQuantities
          1 x IFCPLATE | type IFCPLATETYPE "PL160*499" | object type "PL160*499" | names: "Base Plate" | descriptions: "PL160*499" | material: "STEEL/S235JR" | property sets: QC_Standard, Tekla Common, Tekla Quantity, Pset_PlateCommon, BaseQuantities
          4 x IFCCOLUMN | type IFCCOLUMNTYPE "D41.28" | object type "D41.28" | names: "BOTTOM_PART" | descriptions: "D41.28" | material: "STEEL/S235JR" | property sets: QC_Standard, Tekla Quantity, BaseQuantities, Tekla Common, Pset_ColumnCommon
          12 x IFCCOLUMN | type IFCCOLUMNTYPE "D25.96" | object type "D25.96" | names: "BOTTOM_PART" | descriptions: "D25.96" | material: "STEEL/S235JR" | property sets: QC_Standard, Tekla Quantity, BaseQuantities, Tekla Common, Pset_ColumnCommon
          4 x IFCCOLUMN | type IFCCOLUMNTYPE "EPD57*15.52" | object type "EPD57*15.52" | names: "BOTTOM_PART" | descriptions: "EPD57*15.52" | material: "STEEL/S235JR" | property sets: QC_Standard, Tekla Quantity, BaseQuantities, Tekla Common, Pset_ColumnCommon
          4 x IFCCOLUMN | type IFCCOLUMNTYPE "EPD52.4*13.22" | object type "EPD52.4*13.22" | names: "BOTTOM_PART" | descriptions: "EPD52.4*13.22" | material: "STEEL/S235JR" | property sets: QC_Standard, Tekla Quantity, BaseQuantities, Tekla Common, Pset_ColumnCommon
          8 x IFCCOLUMN | type IFCCOLUMNTYPE "EPD50.8*12.42" | object type "EPD50.8*12.42" | names: "BOTTOM_PART" | descriptions: "EPD50.8*12.42" | material: "STEEL/S235JR" | property sets: QC_Standard, Tekla Quantity, BaseQuantities, Tekla Common, Pset_ColumnCommon
          4 x IFCBEAM | type IFCBEAMTYPE "D41.28" | object type "D41.28" | names: "BOTTOM_PART" | descriptions: "D41.28" | material: "STEEL/S235JR" | property sets: QC_Standard, Tekla Common, Tekla Quantity, Pset_BeamCommon, BaseQuantities
          8 x IFCBEAM | type IFCBEAMTYPE "D25.96" | object type "D25.96" | names: "BOTTOM_PART" | descriptions: "D25.96" | material: "STEEL/S235JR" | property sets: QC_Standard, Tekla Common, Tekla Quantity, Pset_BeamCommon, BaseQuantities
          4 x IFCBEAM | type IFCBEAMTYPE "EPD57*15.52" | object type "EPD57*15.52" | names: "BOTTOM_PART" | descriptions: "EPD57*15.52" | material: "STEEL/S235JR" | property sets: QC_Standard, Tekla Common, Tekla Quantity, Pset_BeamCommon, BaseQuantities
          4 x IFCBEAM | type IFCBEAMTYPE "EPD52.4*13.22" | object type "EPD52.4*13.22" | names: "BOTTOM_PART" | descriptions: "EPD52.4*13.22" | material: "STEEL/S235JR" | property sets: QC_Standard, Tekla Common, Tekla Quantity, Pset_BeamCommon, BaseQuantities
          4 x IFCBEAM | type IFCBEAMTYPE "EPD50.8*12.42" | object type "EPD50.8*12.42" | names: "BOTTOM_PART" | descriptions: "EPD50.8*12.42" | material: "STEEL/S235JR" | property sets: QC_Standard, Tekla Common, Tekla Quantity, Pset_BeamCommon, BaseQuantities
      IFCBUILDINGSTOREY "SubEstructura" | elevation 0.
        contains 201 elements
          54 x IFCPILE | object type "D1500" | names: "PLT-E1", "PLT-P1", "PLT-P4" (+36 more) | descriptions: "D1500" | material: "CONCRETE/fc 280" | property sets: Tekla Common, QC_Standard, Tekla Quantity, BaseQuantities
          2 x IFCFOOTING | object type "14000*11000" | names: "ENC-E1", "ENC-E2" | descriptions: "14000*11000" | material: "CONCRETE/fc 280" | property sets: Tekla Quantity, BaseQuantities, QC_Standard, Tekla Common
          6 x IFCFOOTING | object type "12000*8100" | names: "ENC-P1", "ENC-P2", "ENC-P3" (+3 more) | descriptions: "12000*8100" | material: "CONCRETE/fc 280" | property sets: Tekla Common, Tekla Quantity, BaseQuantities, QC_Standard
          12 x IFCPILE | object type "D1800" | names: "F1A-P1", "F1B-P1", "F1A-P2" (+9 more) | descriptions: "D1800" | material: "CONCRETE/fc 280" | property sets: Tekla Common, Tekla Quantity, QC_Standard, BaseQuantities
          6 x IFCFOOTING | object type "2000*3924" | names: "DIN-P1", "DIN-P2", "DIN-P3" (+3 more) | descriptions: "2000*3924" | material: "CONCRETE/fc 280" | property sets: Tekla Common, Tekla Quantity, BaseQuantities, QC_Standard
          50 x IFCFOOTING | object type "780*780" | names: "DIN-P1", "DIN-P4", "EST-E1" (+30 more) | descriptions: "780*780" | material: "CONCRETE/fc 280" | property sets: Tekla Quantity, BaseQuantities, Tekla Common, QC_Standard
          1 x IFCFOOTING | object type "13000*10000" | names: "ENC-P4" | descriptions: "13000*10000" | material: "CONCRETE/fc 280" | property sets: QC_Standard, Tekla Common, Tekla Quantity, BaseQuantities
          2 x IFCPILE | object type "D2200" | names: "F1A-P4", "F1B-P4" | descriptions: "D2200" | material: "CONCRETE/fc 280" | property sets: QC_Standard, Tekla Common, Tekla Quantity, BaseQuantities
          1 x IFCFOOTING | object type "3800*3824" | names: "DIN-P4" | descriptions: "3800*3824" | material: "CONCRETE/fc 280" | property sets: QC_Standard, Tekla Common, Tekla Quantity, BaseQuantities
          24 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "TUBE76.2*10" | object type "TUBE76.2*10" | names: "TE2-3"" | descriptions: "TUBE76.2*10" | material: "STEEL/Tubo Metalico" | property sets: Tekla Common, QC_Standard, Tekla Quantity, Pours
          12 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "TUBE50.8*10" | object type "TUBE50.8*10" | names: "TP1-3"" | descriptions: "TUBE50.8*10" | material: "STEEL/Tubo Metalico" | property sets: QC_Standard, Tekla Quantity, Tekla Common, Pours
          12 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "TUBE101.6*10" | object type "TUBE101.6*10" | names: "TP1-3"" | descriptions: "TUBE101.6*10" | material: "STEEL/Tubo Metalico" | property sets: QC_Standard, Tekla Quantity, Tekla Common, Pours
          4 x IFCFOOTING | object type "500*250" | names: "EST-E1", "EST-E2" | descriptions: "500*250" | material: "CONCRETE/fc 280" | property sets: Tekla Quantity, QC_Standard, Tekla Common, BaseQuantities
          4 x IFCFOOTING | object type "400*2867" | names: "EST-E1", "EST-E2" | descriptions: "400*2867" | material: "CONCRETE/fc 280" | property sets: Tekla Quantity, BaseQuantities, QC_Standard, Tekla Common
          4 x IFCFOOTING | object type "2150*1000" | names: "EST-E1", "EST-E2" | descriptions: "2150*1000" | material: "CONCRETE/fc 280" | property sets: Tekla Quantity, BaseQuantities, QC_Standard, Tekla Common
          4 x IFCFOOTING | object type "650*5000" | names: "EST-E1", "EST-E2" | descriptions: "650*5000" | material: "CONCRETE/fc 280" | property sets: Tekla Quantity, BaseQuantities, QC_Standard, Tekla Common
          1 x IFCWALL | type IFCWALLTYPE "IPSMVB100*202.5*400*2242*2183*100*200*50*277.02" | object type "IPSMVB100*202.5*400*2242*2183*100*200*50*277.02" | names: "DIN-P4" | descriptions: "IPSMVB100*202.5*400*2242*2183*100*200*50*277.02" | material: "CONCRETE/Concrete_Undefined" | property sets: QC_Standard, Tekla Common, Tekla Quantity, Pset_WallCommon, BaseQuantities
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_Tx2InNPleECRYRtQh2Hjng_0" | object type "_Tx2InNPleECRYRtQh2Hjng_0" | names: "EST-E1" | descriptions: "_Tx2InNPleECRYRtQh2Hjng_0" | material: "CONCRETE/Concrete_Undefined" | property sets: Tekla Common, Tekla Quantity, QC_Standard, Pours
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_Cgysq5sgMU-qaFJMdjTZlA_0" | object type "_Cgysq5sgMU-qaFJMdjTZlA_0" | names: "EST-E2" | descriptions: "_Cgysq5sgMU-qaFJMdjTZlA_0" | material: "CONCRETE/Concrete_Undefined" | property sets: QC_Standard, Tekla Common, Tekla Quantity, Pours
      IFCBUILDINGSTOREY "SuperEstructura" | elevation 0.
        contains 1354 elements
          10 x IFCBEAM | type IFCBEAMTYPE "_JDsZU83epEen0TzaihjSSg_0" | object type "_JDsZU83epEen0TzaihjSSg_0" | names: "VID-1a", "VID-1b", "VID-8a" (+3 more) | descriptions: "_JDsZU83epEen0TzaihjSSg_0" | material: "CONCRETE/fc 350" | property sets: Tekla Quantity, QC_Standard, Tekla Common, Pset_BeamCommon, BaseQuantities
          20 x IFCBEAM | type IFCBEAMTYPE "_pgRV1qUE7U6m_HgCCkwbIg_0" | object type "_pgRV1qUE7U6m_HgCCkwbIg_0" | names: "VID-2a", "VID-2b", "VID-7a" (+13 more) | descriptions: "_pgRV1qUE7U6m_HgCCkwbIg_0" | material: "CONCRETE/fc 350" | property sets: Tekla Common, Tekla Quantity, BaseQuantities, Pset_BeamCommon, QC_Standard
          16 x IFCBEAM | type IFCBEAMTYPE "400*1803" | object type "400*1803" | names: "DIA-E1", "DIA-E2", "DIA-P4" | descriptions: "400*1803" | material: "CONCRETE/fc 350" | property sets: Tekla Quantity, Tekla Common, BaseQuantities, Pset_BeamCommon, QC_Standard
          96 x IFCBEAM | type IFCBEAMTYPE "250*1803" | object type "250*1803" | names: "DIA-1", "DIA-2", "DIA-3" (+60 more) | descriptions: "250*1803" | material: "CONCRETE/fc 350" | property sets: Tekla Common, Tekla Quantity, BaseQuantities, Pset_BeamCommon, QC_Standard
          10 x IFCBEAM | type IFCBEAMTYPE "_MY_mTXLcvEqkIjaXhGbUIA_0" | object type "_MY_mTXLcvEqkIjaXhGbUIA_0" | names: "VID-4a", "VID-4b", "VID-5a" (+3 more) | descriptions: "_MY_mTXLcvEqkIjaXhGbUIA_0" | material: "CONCRETE/fc 350" | property sets: Tekla Quantity, Tekla Common, QC_Standard, Pset_BeamCommon, BaseQuantities
          206 x IFCWALL | type IFCWALLTYPE "3000*400" | object type "3000*400" | names: "MNJ-2", "MNJ-1" | descriptions: "3000*400" | material: "CONCRETE/fc 280" | property sets: Tekla Quantity, Tekla Common, Pset_WallCommon, BaseQuantities, QC_Standard
          6 x IFCBEAM | type IFCBEAMTYPE "800*2120" | object type "800*2120" | names: "DIA-P1", "DIA-P2", "DIA-P3" (+3 more) | descriptions: "800*2120" | material: "CONCRETE/fc 350" | property sets: Tekla Common, Tekla Quantity, BaseQuantities, QC_Standard, Pset_BeamCommon
          12 x IFCBEAM | type IFCBEAMTYPE "250*2120" | object type "250*2120" | names: "DIA-P1", "DIA-P2", "DIA-P3" (+6 more) | descriptions: "250*2120" | material: "CONCRETE/fc 350" | property sets: Tekla Common, Tekla Quantity, QC_Standard, Pset_BeamCommon, BaseQuantities
          48 x IFCBEAM | type IFCBEAMTYPE "250*300" | object type "250*300" | names: "DIA-1", "DIA-2", "DIA-3" (+30 more) | descriptions: "250*300" | material: "CONCRETE/Concrete_Undefined" | property sets: Tekla Quantity, Tekla Common, Pset_BeamCommon, BaseQuantities, QC_Standard
          480 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "TUBE76.2*10" | object type "TUBE76.2*10" | names: "Tub-3"" | descriptions: "TUBE76.2*10" | material: "STEEL/Tubo Metalico" | property sets: Tekla Quantity, Tekla Common, QC_Standard, Pours
          120 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "D80" | object type "D80" | names: "Tendon 01", "Tendon 02", "Tendon 03" | descriptions: "D80" | material: "STEEL/Tendon" | property sets: Tekla Common, Tekla Quantity, QC_Standard, Pours
          20 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_iQAmr9z6UkaDmdLvQmn5QQ_0" | object type "_iQAmr9z6UkaDmdLvQmn5QQ_0" | names: "Tendon 01" | descriptions: "_iQAmr9z6UkaDmdLvQmn5QQ_0" | material: "STEEL/Tendon" | property sets: Tekla Common, Tekla Quantity, QC_Standard, Pours
          20 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_APuikTUeQUedexBVPMTNFQ_0" | object type "_APuikTUeQUedexBVPMTNFQ_0" | names: "Tendon 02" | descriptions: "_APuikTUeQUedexBVPMTNFQ_0" | material: "STEEL/Tendon" | property sets: Tekla Quantity, Tekla Common, QC_Standard, Pours
          20 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_zctwP5PVpU2GxoQPSbg4lw_0" | object type "_zctwP5PVpU2GxoQPSbg4lw_0" | names: "Tendon 03" | descriptions: "_zctwP5PVpU2GxoQPSbg4lw_0" | material: "STEEL/Tendon" | property sets: Tekla Common, Tekla Quantity, QC_Standard, Pours
          20 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_WWhurdFeXUWNEXEY9ytvkw_0" | object type "_WWhurdFeXUWNEXEY9ytvkw_0" | names: "Tendon 01" | descriptions: "_WWhurdFeXUWNEXEY9ytvkw_0" | material: "STEEL/Tendon" | property sets: Tekla Common, Tekla Quantity, QC_Standard, Pours
          20 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_WWhurdFeXUWNEXEY9ytvkw_1" | object type "_WWhurdFeXUWNEXEY9ytvkw_1" | names: "Tendon 02" | descriptions: "_WWhurdFeXUWNEXEY9ytvkw_1" | material: "STEEL/Tendon" | property sets: Tekla Quantity, Tekla Common, QC_Standard, Pours
          20 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_WWhurdFeXUWNEXEY9ytvkw_2" | object type "_WWhurdFeXUWNEXEY9ytvkw_2" | names: "Tendon 03" | descriptions: "_WWhurdFeXUWNEXEY9ytvkw_2" | material: "STEEL/Tendon" | property sets: Tekla Common, Tekla Quantity, QC_Standard, Pours
          10 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_xZMV8PGNj0O_GuQtP7XEWQ_0" | object type "_xZMV8PGNj0O_GuQtP7XEWQ_0" | names: "Tendon 01" | descriptions: "_xZMV8PGNj0O_GuQtP7XEWQ_0" | material: "STEEL/Tendon" | property sets: Tekla Common, Tekla Quantity, QC_Standard, Pours
          10 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_xZMV8PGNj0O_GuQtP7XEWQ_1" | object type "_xZMV8PGNj0O_GuQtP7XEWQ_1" | names: "Tendon 02" | descriptions: "_xZMV8PGNj0O_GuQtP7XEWQ_1" | material: "STEEL/Tendon" | property sets: Tekla Common, Tekla Quantity, QC_Standard, Pours
          10 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_zGkkAOtzg0y0avhCB96LKA_0" | object type "_zGkkAOtzg0y0avhCB96LKA_0" | names: "Tendon 01" | descriptions: "_zGkkAOtzg0y0avhCB96LKA_0" | material: "STEEL/Tendon" | property sets: Tekla Common, Tekla Quantity, QC_Standard, Pours
          10 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_zGkkAOtzg0y0avhCB96LKA_1" | object type "_zGkkAOtzg0y0avhCB96LKA_1" | names: "Tendon 02" | descriptions: "_zGkkAOtzg0y0avhCB96LKA_1" | material: "STEEL/Tendon" | property sets: Tekla Common, Tekla Quantity, QC_Standard, Pours
          10 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_zGkkAOtzg0y0avhCB96LKA_2" | object type "_zGkkAOtzg0y0avhCB96LKA_2" | names: "Tendon 03" | descriptions: "_zGkkAOtzg0y0avhCB96LKA_2" | material: "STEEL/Tendon" | property sets: Tekla Common, Tekla Quantity, QC_Standard, Pours
          10 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_xZMV8PGNj0O_GuQtP7XEWQ_2" | object type "_xZMV8PGNj0O_GuQtP7XEWQ_2" | names: "Tendon 03" | descriptions: "_xZMV8PGNj0O_GuQtP7XEWQ_2" | material: "STEEL/Tendon" | property sets: Tekla Common, Tekla Quantity, QC_Standard, Pours
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_W0Q29rrUD0qI3pwUSWdnxA_0" | object type "_W0Q29rrUD0qI3pwUSWdnxA_0" | names: "Grout" | descriptions: "_W0Q29rrUD0qI3pwUSWdnxA_0" | material: "CONCRETE/Grout" | property sets: QC_Standard, Tekla Quantity, Tekla Common, Pours
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_W0Q29rrUD0qI3pwUSWdnxA_1" | object type "_W0Q29rrUD0qI3pwUSWdnxA_1" | names: "Grout" | descriptions: "_W0Q29rrUD0qI3pwUSWdnxA_1" | material: "CONCRETE/Grout" | property sets: QC_Standard, Tekla Quantity, Tekla Common, Pours
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_W0Q29rrUD0qI3pwUSWdnxA_2" | object type "_W0Q29rrUD0qI3pwUSWdnxA_2" | names: "Grout" | descriptions: "_W0Q29rrUD0qI3pwUSWdnxA_2" | material: "CONCRETE/Grout" | property sets: QC_Standard, Tekla Quantity, Tekla Common, Pours
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_W0Q29rrUD0qI3pwUSWdnxA_3" | object type "_W0Q29rrUD0qI3pwUSWdnxA_3" | names: "Grout" | descriptions: "_W0Q29rrUD0qI3pwUSWdnxA_3" | material: "CONCRETE/Grout" | property sets: QC_Standard, Tekla Quantity, Tekla Common, Pours
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_W0Q29rrUD0qI3pwUSWdnxA_4" | object type "_W0Q29rrUD0qI3pwUSWdnxA_4" | names: "Grout" | descriptions: "_W0Q29rrUD0qI3pwUSWdnxA_4" | material: "CONCRETE/Grout" | property sets: QC_Standard, Tekla Common, Tekla Quantity, Pours
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_wCNGqzzxSkuBKOybvcB-mg_0" | object type "_wCNGqzzxSkuBKOybvcB-mg_0" | names: "Grout" | descriptions: "_wCNGqzzxSkuBKOybvcB-mg_0" | material: "CONCRETE/Grout" | property sets: Tekla Quantity, Tekla Common, QC_Standard, Pours
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_wCNGqzzxSkuBKOybvcB-mg_1" | object type "_wCNGqzzxSkuBKOybvcB-mg_1" | names: "Grout" | descriptions: "_wCNGqzzxSkuBKOybvcB-mg_1" | material: "CONCRETE/Grout" | property sets: Tekla Quantity, Tekla Common, QC_Standard, Pours
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_wCNGqzzxSkuBKOybvcB-mg_2" | object type "_wCNGqzzxSkuBKOybvcB-mg_2" | names: "Grout" | descriptions: "_wCNGqzzxSkuBKOybvcB-mg_2" | material: "CONCRETE/Grout" | property sets: Tekla Quantity, Tekla Common, QC_Standard, Pours
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_wCNGqzzxSkuBKOybvcB-mg_3" | object type "_wCNGqzzxSkuBKOybvcB-mg_3" | names: "Grout" | descriptions: "_wCNGqzzxSkuBKOybvcB-mg_3" | material: "CONCRETE/Grout" | property sets: Tekla Quantity, Tekla Common, QC_Standard, Pours
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_wCNGqzzxSkuBKOybvcB-mg_4" | object type "_wCNGqzzxSkuBKOybvcB-mg_4" | names: "Grout" | descriptions: "_wCNGqzzxSkuBKOybvcB-mg_4" | material: "CONCRETE/Grout" | property sets: Tekla Common, Tekla Quantity, QC_Standard, Pours
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_mqotvdKdsE-wiT5oCGDPuw_0" | object type "_mqotvdKdsE-wiT5oCGDPuw_0" | names: "Grout" | descriptions: "_mqotvdKdsE-wiT5oCGDPuw_0" | material: "CONCRETE/Grout" | property sets: Tekla Quantity, Tekla Common, QC_Standard, Pours
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_mqotvdKdsE-wiT5oCGDPuw_1" | object type "_mqotvdKdsE-wiT5oCGDPuw_1" | names: "Grout" | descriptions: "_mqotvdKdsE-wiT5oCGDPuw_1" | material: "CONCRETE/Grout" | property sets: Tekla Quantity, Tekla Common, QC_Standard, Pours
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_mqotvdKdsE-wiT5oCGDPuw_2" | object type "_mqotvdKdsE-wiT5oCGDPuw_2" | names: "Grout" | descriptions: "_mqotvdKdsE-wiT5oCGDPuw_2" | material: "CONCRETE/Grout" | property sets: Tekla Quantity, Tekla Common, QC_Standard, Pours
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_mqotvdKdsE-wiT5oCGDPuw_3" | object type "_mqotvdKdsE-wiT5oCGDPuw_3" | names: "Grout" | descriptions: "_mqotvdKdsE-wiT5oCGDPuw_3" | material: "CONCRETE/Grout" | property sets: Tekla Quantity, Tekla Common, QC_Standard, Pours
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_mqotvdKdsE-wiT5oCGDPuw_4" | object type "_mqotvdKdsE-wiT5oCGDPuw_4" | names: "Grout" | descriptions: "_mqotvdKdsE-wiT5oCGDPuw_4" | material: "CONCRETE/Grout" | property sets: Tekla Common, Tekla Quantity, QC_Standard, Pours
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_RhRq7PJ5BEKGix01TNl22w_0" | object type "_RhRq7PJ5BEKGix01TNl22w_0" | names: "Grout" | descriptions: "_RhRq7PJ5BEKGix01TNl22w_0" | material: "CONCRETE/Grout" | property sets: Tekla Quantity, Tekla Common, QC_Standard, Pours
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_RhRq7PJ5BEKGix01TNl22w_1" | object type "_RhRq7PJ5BEKGix01TNl22w_1" | names: "Grout" | descriptions: "_RhRq7PJ5BEKGix01TNl22w_1" | material: "CONCRETE/Grout" | property sets: Tekla Quantity, Tekla Common, QC_Standard, Pours
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_RhRq7PJ5BEKGix01TNl22w_2" | object type "_RhRq7PJ5BEKGix01TNl22w_2" | names: "Grout" | descriptions: "_RhRq7PJ5BEKGix01TNl22w_2" | material: "CONCRETE/Grout" | property sets: Tekla Quantity, Tekla Common, QC_Standard, Pours
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_RhRq7PJ5BEKGix01TNl22w_3" | object type "_RhRq7PJ5BEKGix01TNl22w_3" | names: "Grout" | descriptions: "_RhRq7PJ5BEKGix01TNl22w_3" | material: "CONCRETE/Grout" | property sets: Tekla Quantity, Tekla Common, QC_Standard, Pours
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_RhRq7PJ5BEKGix01TNl22w_4" | object type "_RhRq7PJ5BEKGix01TNl22w_4" | names: "Grout" | descriptions: "_RhRq7PJ5BEKGix01TNl22w_4" | material: "CONCRETE/Grout" | property sets: Tekla Common, Tekla Quantity, QC_Standard, Pours
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_q7vE1UKJQkSIGwLYHKbz7A_0" | object type "_q7vE1UKJQkSIGwLYHKbz7A_0" | names: "Grout" | descriptions: "_q7vE1UKJQkSIGwLYHKbz7A_0" | material: "CONCRETE/Grout" | property sets: Tekla Quantity, Tekla Common, QC_Standard, Pours
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_q7vE1UKJQkSIGwLYHKbz7A_1" | object type "_q7vE1UKJQkSIGwLYHKbz7A_1" | names: "Grout" | descriptions: "_q7vE1UKJQkSIGwLYHKbz7A_1" | material: "CONCRETE/Grout" | property sets: Tekla Quantity, Tekla Common, QC_Standard, Pours
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_q7vE1UKJQkSIGwLYHKbz7A_2" | object type "_q7vE1UKJQkSIGwLYHKbz7A_2" | names: "Grout" | descriptions: "_q7vE1UKJQkSIGwLYHKbz7A_2" | material: "CONCRETE/Grout" | property sets: Tekla Quantity, Tekla Common, QC_Standard, Pours
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_q7vE1UKJQkSIGwLYHKbz7A_3" | object type "_q7vE1UKJQkSIGwLYHKbz7A_3" | names: "Grout" | descriptions: "_q7vE1UKJQkSIGwLYHKbz7A_3" | material: "CONCRETE/Grout" | property sets: Tekla Quantity, Tekla Common, QC_Standard, Pours
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_q7vE1UKJQkSIGwLYHKbz7A_4" | object type "_q7vE1UKJQkSIGwLYHKbz7A_4" | names: "Grout" | descriptions: "_q7vE1UKJQkSIGwLYHKbz7A_4" | material: "CONCRETE/Grout" | property sets: Tekla Common, Tekla Quantity, QC_Standard, Pours
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_rQh3fPrxo02546su1FUq5g_0" | object type "_rQh3fPrxo02546su1FUq5g_0" | names: "Grout" | descriptions: "_rQh3fPrxo02546su1FUq5g_0" | material: "CONCRETE/Grout" | property sets: Tekla Quantity, Tekla Common, QC_Standard, Pours
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_rQh3fPrxo02546su1FUq5g_1" | object type "_rQh3fPrxo02546su1FUq5g_1" | names: "Grout" | descriptions: "_rQh3fPrxo02546su1FUq5g_1" | material: "CONCRETE/Grout" | property sets: Tekla Quantity, Tekla Common, QC_Standard, Pours
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_rQh3fPrxo02546su1FUq5g_2" | object type "_rQh3fPrxo02546su1FUq5g_2" | names: "Grout" | descriptions: "_rQh3fPrxo02546su1FUq5g_2" | material: "CONCRETE/Grout" | property sets: Tekla Quantity, Tekla Common, QC_Standard, Pours
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_rQh3fPrxo02546su1FUq5g_3" | object type "_rQh3fPrxo02546su1FUq5g_3" | names: "Grout" | descriptions: "_rQh3fPrxo02546su1FUq5g_3" | material: "CONCRETE/Grout" | property sets: Tekla Quantity, Tekla Common, QC_Standard, Pours
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_rQh3fPrxo02546su1FUq5g_4" | object type "_rQh3fPrxo02546su1FUq5g_4" | names: "Grout" | descriptions: "_rQh3fPrxo02546su1FUq5g_4" | material: "CONCRETE/Grout" | property sets: Tekla Common, Tekla Quantity, QC_Standard, Pours
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_bNZjJmYlm0KwoRrWD2MFtw_0" | object type "_bNZjJmYlm0KwoRrWD2MFtw_0" | names: "Grout" | descriptions: "_bNZjJmYlm0KwoRrWD2MFtw_0" | material: "CONCRETE/Grout" | property sets: Tekla Quantity, Tekla Common, QC_Standard, Pours
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_bNZjJmYlm0KwoRrWD2MFtw_1" | object type "_bNZjJmYlm0KwoRrWD2MFtw_1" | names: "Grout" | descriptions: "_bNZjJmYlm0KwoRrWD2MFtw_1" | material: "CONCRETE/Grout" | property sets: Tekla Quantity, Tekla Common, QC_Standard, Pours
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_bNZjJmYlm0KwoRrWD2MFtw_2" | object type "_bNZjJmYlm0KwoRrWD2MFtw_2" | names: "Grout" | descriptions: "_bNZjJmYlm0KwoRrWD2MFtw_2" | material: "CONCRETE/Grout" | property sets: Tekla Quantity, Tekla Common, QC_Standard, Pours
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_bNZjJmYlm0KwoRrWD2MFtw_3" | object type "_bNZjJmYlm0KwoRrWD2MFtw_3" | names: "Grout" | descriptions: "_bNZjJmYlm0KwoRrWD2MFtw_3" | material: "CONCRETE/Grout" | property sets: Tekla Quantity, Tekla Common, QC_Standard, Pours
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_bNZjJmYlm0KwoRrWD2MFtw_4" | object type "_bNZjJmYlm0KwoRrWD2MFtw_4" | names: "Grout" | descriptions: "_bNZjJmYlm0KwoRrWD2MFtw_4" | material: "CONCRETE/Grout" | property sets: Tekla Common, Tekla Quantity, QC_Standard, Pours
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_MKZrQiKvyU-fFOxn3trsng_0" | object type "_MKZrQiKvyU-fFOxn3trsng_0" | names: "Grout" | descriptions: "_MKZrQiKvyU-fFOxn3trsng_0" | material: "CONCRETE/Grout" | property sets: Tekla Quantity, Tekla Common, QC_Standard, Pours
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_MKZrQiKvyU-fFOxn3trsng_1" | object type "_MKZrQiKvyU-fFOxn3trsng_1" | names: "Grout" | descriptions: "_MKZrQiKvyU-fFOxn3trsng_1" | material: "CONCRETE/Grout" | property sets: Tekla Quantity, Tekla Common, QC_Standard, Pours
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_MKZrQiKvyU-fFOxn3trsng_2" | object type "_MKZrQiKvyU-fFOxn3trsng_2" | names: "Grout" | descriptions: "_MKZrQiKvyU-fFOxn3trsng_2" | material: "CONCRETE/Grout" | property sets: Tekla Quantity, Tekla Common, QC_Standard, Pours
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_MKZrQiKvyU-fFOxn3trsng_3" | object type "_MKZrQiKvyU-fFOxn3trsng_3" | names: "Grout" | descriptions: "_MKZrQiKvyU-fFOxn3trsng_3" | material: "CONCRETE/Grout" | property sets: Tekla Quantity, Tekla Common, QC_Standard, Pours
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_MKZrQiKvyU-fFOxn3trsng_4" | object type "_MKZrQiKvyU-fFOxn3trsng_4" | names: "Grout" | descriptions: "_MKZrQiKvyU-fFOxn3trsng_4" | material: "CONCRETE/Grout" | property sets: Tekla Common, Tekla Quantity, QC_Standard, Pours
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_MKZrQiKvyU-fFOxn3trsng_10" | object type "_MKZrQiKvyU-fFOxn3trsng_10" | names: "Grout" | descriptions: "_MKZrQiKvyU-fFOxn3trsng_10" | material: "CONCRETE/Grout" | property sets: Tekla Quantity, Tekla Common, QC_Standard, Pours
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_MKZrQiKvyU-fFOxn3trsng_11" | object type "_MKZrQiKvyU-fFOxn3trsng_11" | names: "Grout" | descriptions: "_MKZrQiKvyU-fFOxn3trsng_11" | material: "CONCRETE/Grout" | property sets: Tekla Quantity, Tekla Common, QC_Standard, Pours
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_MKZrQiKvyU-fFOxn3trsng_12" | object type "_MKZrQiKvyU-fFOxn3trsng_12" | names: "Grout" | descriptions: "_MKZrQiKvyU-fFOxn3trsng_12" | material: "CONCRETE/Grout" | property sets: Tekla Quantity, Tekla Common, QC_Standard, Pours
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_MKZrQiKvyU-fFOxn3trsng_13" | object type "_MKZrQiKvyU-fFOxn3trsng_13" | names: "Grout" | descriptions: "_MKZrQiKvyU-fFOxn3trsng_13" | material: "CONCRETE/Grout" | property sets: Tekla Quantity, Tekla Common, QC_Standard, Pours
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_MKZrQiKvyU-fFOxn3trsng_14" | object type "_MKZrQiKvyU-fFOxn3trsng_14" | names: "Grout" | descriptions: "_MKZrQiKvyU-fFOxn3trsng_14" | material: "CONCRETE/Grout" | property sets: Tekla Common, Tekla Quantity, QC_Standard, Pours
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_MKZrQiKvyU-fFOxn3trsng_20" | object type "_MKZrQiKvyU-fFOxn3trsng_20" | names: "Grout" | descriptions: "_MKZrQiKvyU-fFOxn3trsng_20" | material: "CONCRETE/Grout" | property sets: Tekla Quantity, Tekla Common, QC_Standard, Pours
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_MKZrQiKvyU-fFOxn3trsng_21" | object type "_MKZrQiKvyU-fFOxn3trsng_21" | names: "Grout" | descriptions: "_MKZrQiKvyU-fFOxn3trsng_21" | material: "CONCRETE/Grout" | property sets: Tekla Quantity, Tekla Common, QC_Standard, Pours
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_MKZrQiKvyU-fFOxn3trsng_22" | object type "_MKZrQiKvyU-fFOxn3trsng_22" | names: "Grout" | descriptions: "_MKZrQiKvyU-fFOxn3trsng_22" | material: "CONCRETE/Grout" | property sets: Tekla Quantity, Tekla Common, QC_Standard, Pours
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_MKZrQiKvyU-fFOxn3trsng_23" | object type "_MKZrQiKvyU-fFOxn3trsng_23" | names: "Grout" | descriptions: "_MKZrQiKvyU-fFOxn3trsng_23" | material: "CONCRETE/Grout" | property sets: Tekla Quantity, Tekla Common, QC_Standard, Pours
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_MKZrQiKvyU-fFOxn3trsng_24" | object type "_MKZrQiKvyU-fFOxn3trsng_24" | names: "Grout" | descriptions: "_MKZrQiKvyU-fFOxn3trsng_24" | material: "CONCRETE/Grout" | property sets: Tekla Common, Tekla Quantity, QC_Standard, Pours
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_MKZrQiKvyU-fFOxn3trsng_30" | object type "_MKZrQiKvyU-fFOxn3trsng_30" | names: "Grout" | descriptions: "_MKZrQiKvyU-fFOxn3trsng_30" | material: "CONCRETE/Grout" | property sets: Tekla Quantity, Tekla Common, QC_Standard, Pours
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_MKZrQiKvyU-fFOxn3trsng_31" | object type "_MKZrQiKvyU-fFOxn3trsng_31" | names: "Grout" | descriptions: "_MKZrQiKvyU-fFOxn3trsng_31" | material: "CONCRETE/Grout" | property sets: Tekla Quantity, Tekla Common, QC_Standard, Pours
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_MKZrQiKvyU-fFOxn3trsng_32" | object type "_MKZrQiKvyU-fFOxn3trsng_32" | names: "Grout" | descriptions: "_MKZrQiKvyU-fFOxn3trsng_32" | material: "CONCRETE/Grout" | property sets: Tekla Quantity, Tekla Common, QC_Standard, Pours
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_MKZrQiKvyU-fFOxn3trsng_33" | object type "_MKZrQiKvyU-fFOxn3trsng_33" | names: "Grout" | descriptions: "_MKZrQiKvyU-fFOxn3trsng_33" | material: "CONCRETE/Grout" | property sets: Tekla Quantity, Tekla Common, QC_Standard, Pours
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_MKZrQiKvyU-fFOxn3trsng_34" | object type "_MKZrQiKvyU-fFOxn3trsng_34" | names: "Grout" | descriptions: "_MKZrQiKvyU-fFOxn3trsng_34" | material: "CONCRETE/Grout" | property sets: Tekla Common, Tekla Quantity, QC_Standard, Pours
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_XzVA3TGxA0iQtYZr7oqung_0" | object type "_XzVA3TGxA0iQtYZr7oqung_0" | names: "Grout" | descriptions: "_XzVA3TGxA0iQtYZr7oqung_0" | material: "CONCRETE/Grout" | property sets: Tekla Quantity, Tekla Common, QC_Standard, Pours
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_XzVA3TGxA0iQtYZr7oqung_1" | object type "_XzVA3TGxA0iQtYZr7oqung_1" | names: "Grout" | descriptions: "_XzVA3TGxA0iQtYZr7oqung_1" | material: "CONCRETE/Grout" | property sets: Tekla Quantity, Tekla Common, QC_Standard, Pours
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_XzVA3TGxA0iQtYZr7oqung_2" | object type "_XzVA3TGxA0iQtYZr7oqung_2" | names: "Grout" | descriptions: "_XzVA3TGxA0iQtYZr7oqung_2" | material: "CONCRETE/Grout" | property sets: Tekla Quantity, Tekla Common, QC_Standard, Pours
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_XzVA3TGxA0iQtYZr7oqung_3" | object type "_XzVA3TGxA0iQtYZr7oqung_3" | names: "Grout" | descriptions: "_XzVA3TGxA0iQtYZr7oqung_3" | material: "CONCRETE/Grout" | property sets: Tekla Quantity, Tekla Common, QC_Standard, Pours
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_XzVA3TGxA0iQtYZr7oqung_4" | object type "_XzVA3TGxA0iQtYZr7oqung_4" | names: "Grout" | descriptions: "_XzVA3TGxA0iQtYZr7oqung_4" | material: "CONCRETE/Grout" | property sets: Tekla Common, Tekla Quantity, QC_Standard, Pours
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_XzVA3TGxA0iQtYZr7oqung_10" | object type "_XzVA3TGxA0iQtYZr7oqung_10" | names: "Grout" | descriptions: "_XzVA3TGxA0iQtYZr7oqung_10" | material: "CONCRETE/Grout" | property sets: Tekla Quantity, Tekla Common, QC_Standard, Pours
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_XzVA3TGxA0iQtYZr7oqung_11" | object type "_XzVA3TGxA0iQtYZr7oqung_11" | names: "Grout" | descriptions: "_XzVA3TGxA0iQtYZr7oqung_11" | material: "CONCRETE/Grout" | property sets: Tekla Quantity, Tekla Common, QC_Standard, Pours
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_XzVA3TGxA0iQtYZr7oqung_12" | object type "_XzVA3TGxA0iQtYZr7oqung_12" | names: "Grout" | descriptions: "_XzVA3TGxA0iQtYZr7oqung_12" | material: "CONCRETE/Grout" | property sets: Tekla Quantity, Tekla Common, QC_Standard, Pours
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_XzVA3TGxA0iQtYZr7oqung_13" | object type "_XzVA3TGxA0iQtYZr7oqung_13" | names: "Grout" | descriptions: "_XzVA3TGxA0iQtYZr7oqung_13" | material: "CONCRETE/Grout" | property sets: Tekla Quantity, Tekla Common, QC_Standard, Pours
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_XzVA3TGxA0iQtYZr7oqung_14" | object type "_XzVA3TGxA0iQtYZr7oqung_14" | names: "Grout" | descriptions: "_XzVA3TGxA0iQtYZr7oqung_14" | material: "CONCRETE/Grout" | property sets: Tekla Common, Tekla Quantity, QC_Standard, Pours
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_XzVA3TGxA0iQtYZr7oqung_20" | object type "_XzVA3TGxA0iQtYZr7oqung_20" | names: "Grout" | descriptions: "_XzVA3TGxA0iQtYZr7oqung_20" | material: "CONCRETE/Grout" | property sets: Tekla Quantity, Tekla Common, QC_Standard, Pours
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_XzVA3TGxA0iQtYZr7oqung_21" | object type "_XzVA3TGxA0iQtYZr7oqung_21" | names: "Grout" | descriptions: "_XzVA3TGxA0iQtYZr7oqung_21" | material: "CONCRETE/Grout" | property sets: Tekla Quantity, Tekla Common, QC_Standard, Pours
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_XzVA3TGxA0iQtYZr7oqung_22" | object type "_XzVA3TGxA0iQtYZr7oqung_22" | names: "Grout" | descriptions: "_XzVA3TGxA0iQtYZr7oqung_22" | material: "CONCRETE/Grout" | property sets: Tekla Quantity, Tekla Common, QC_Standard, Pours
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_XzVA3TGxA0iQtYZr7oqung_23" | object type "_XzVA3TGxA0iQtYZr7oqung_23" | names: "Grout" | descriptions: "_XzVA3TGxA0iQtYZr7oqung_23" | material: "CONCRETE/Grout" | property sets: Tekla Quantity, Tekla Common, QC_Standard, Pours
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_XzVA3TGxA0iQtYZr7oqung_24" | object type "_XzVA3TGxA0iQtYZr7oqung_24" | names: "Grout" | descriptions: "_XzVA3TGxA0iQtYZr7oqung_24" | material: "CONCRETE/Grout" | property sets: Tekla Common, Tekla Quantity, QC_Standard, Pours
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_XzVA3TGxA0iQtYZr7oqung_30" | object type "_XzVA3TGxA0iQtYZr7oqung_30" | names: "Grout" | descriptions: "_XzVA3TGxA0iQtYZr7oqung_30" | material: "CONCRETE/Grout" | property sets: Tekla Quantity, Tekla Common, QC_Standard, Pours
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_XzVA3TGxA0iQtYZr7oqung_31" | object type "_XzVA3TGxA0iQtYZr7oqung_31" | names: "Grout" | descriptions: "_XzVA3TGxA0iQtYZr7oqung_31" | material: "CONCRETE/Grout" | property sets: Tekla Quantity, Tekla Common, QC_Standard, Pours
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_XzVA3TGxA0iQtYZr7oqung_32" | object type "_XzVA3TGxA0iQtYZr7oqung_32" | names: "Grout" | descriptions: "_XzVA3TGxA0iQtYZr7oqung_32" | material: "CONCRETE/Grout" | property sets: Tekla Quantity, Tekla Common, QC_Standard, Pours
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_XzVA3TGxA0iQtYZr7oqung_33" | object type "_XzVA3TGxA0iQtYZr7oqung_33" | names: "Grout" | descriptions: "_XzVA3TGxA0iQtYZr7oqung_33" | material: "CONCRETE/Grout" | property sets: Tekla Quantity, Tekla Common, QC_Standard, Pours
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_XzVA3TGxA0iQtYZr7oqung_34" | object type "_XzVA3TGxA0iQtYZr7oqung_34" | names: "Grout" | descriptions: "_XzVA3TGxA0iQtYZr7oqung_34" | material: "CONCRETE/Grout" | property sets: Tekla Common, Tekla Quantity, QC_Standard, Pours
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_Xx3dOakcfUO0IxJF-yvkhA_0" | object type "_Xx3dOakcfUO0IxJF-yvkhA_0" | names: "Grout" | descriptions: "_Xx3dOakcfUO0IxJF-yvkhA_0" | material: "CONCRETE/Grout" | property sets: QC_Standard, Tekla Quantity, Tekla Common, Pours
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_Xx3dOakcfUO0IxJF-yvkhA_1" | object type "_Xx3dOakcfUO0IxJF-yvkhA_1" | names: "Grout" | descriptions: "_Xx3dOakcfUO0IxJF-yvkhA_1" | material: "CONCRETE/Grout" | property sets: QC_Standard, Tekla Quantity, Tekla Common, Pours
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_Xx3dOakcfUO0IxJF-yvkhA_2" | object type "_Xx3dOakcfUO0IxJF-yvkhA_2" | names: "Grout" | descriptions: "_Xx3dOakcfUO0IxJF-yvkhA_2" | material: "CONCRETE/Grout" | property sets: QC_Standard, Tekla Quantity, Tekla Common, Pours
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_Xx3dOakcfUO0IxJF-yvkhA_3" | object type "_Xx3dOakcfUO0IxJF-yvkhA_3" | names: "Grout" | descriptions: "_Xx3dOakcfUO0IxJF-yvkhA_3" | material: "CONCRETE/Grout" | property sets: QC_Standard, Tekla Quantity, Tekla Common, Pours
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_Xx3dOakcfUO0IxJF-yvkhA_4" | object type "_Xx3dOakcfUO0IxJF-yvkhA_4" | names: "Grout" | descriptions: "_Xx3dOakcfUO0IxJF-yvkhA_4" | material: "CONCRETE/Grout" | property sets: QC_Standard, Tekla Common, Tekla Quantity, Pours
          10 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_xM0e5Dp4S02OamZVnlEJYA_2_1" | object type "_xM0e5Dp4S02OamZVnlEJYA_2_1" | names: "Tendon 03" | descriptions: "_xM0e5Dp4S02OamZVnlEJYA_2_1" | material: "STEEL/Tendon" | property sets: Tekla Quantity, Tekla Common, QC_Standard, Pours
          10 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_o5V_7SDI4k-TInVG-m3yJQ_1_1" | object type "_o5V_7SDI4k-TInVG-m3yJQ_1_1" | names: "Tendon 02" | descriptions: "_o5V_7SDI4k-TInVG-m3yJQ_1_1" | material: "STEEL/Tendon" | property sets: Tekla Quantity, Tekla Common, QC_Standard, Pours
          10 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_o5V_7SDI4k-TInVG-m3yJQ_0" | object type "_o5V_7SDI4k-TInVG-m3yJQ_0" | names: "Tendon 01" | descriptions: "_o5V_7SDI4k-TInVG-m3yJQ_0" | material: "STEEL/Tendon" | property sets: Tekla Quantity, Tekla Common, QC_Standard, Pours
          10 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_o5V_7SDI4k-TInVG-m3yJQ_2_1" | object type "_o5V_7SDI4k-TInVG-m3yJQ_2_1" | names: "Tendon 03" | descriptions: "_o5V_7SDI4k-TInVG-m3yJQ_2_1" | material: "STEEL/Tendon" | property sets: Tekla Quantity, Tekla Common, QC_Standard, Pours
          10 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_xM0e5Dp4S02OamZVnlEJYA_1_1" | object type "_xM0e5Dp4S02OamZVnlEJYA_1_1" | names: "Tendon 02" | descriptions: "_xM0e5Dp4S02OamZVnlEJYA_1_1" | material: "STEEL/Tendon" | property sets: Tekla Quantity, Tekla Common, QC_Standard, Pours
          10 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_xM0e5Dp4S02OamZVnlEJYA_0" | object type "_xM0e5Dp4S02OamZVnlEJYA_0" | names: "Tendon 01" | descriptions: "_xM0e5Dp4S02OamZVnlEJYA_0" | material: "STEEL/Tendon" | property sets: Tekla Quantity, Tekla Common, QC_Standard, Pours
          4 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_Ytsq9ZJl6kKIcPhQQVUMXA_0" | object type "_Ytsq9ZJl6kKIcPhQQVUMXA_0" | names: "TBL-2", "TBL-3", "TBL-6" (+1 more) | descriptions: "_Ytsq9ZJl6kKIcPhQQVUMXA_0" | material: "CONCRETE/Concrete_Undefined" | property sets: Tekla Common, Tekla Quantity, QC_Standard, Pours
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_NC7kOKz8QEKJmJ5mCongMA_0" | object type "_NC7kOKz8QEKJmJ5mCongMA_0" | names: "TBL-4" | descriptions: "_NC7kOKz8QEKJmJ5mCongMA_0" | material: "CONCRETE/Concrete_Undefined" | property sets: Tekla Common, Tekla Quantity, QC_Standard, Pours
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_aJiu3r_V90SDTop659Lqxg_0" | object type "_aJiu3r_V90SDTop659Lqxg_0" | names: "TBL-5" | descriptions: "_aJiu3r_V90SDTop659Lqxg_0" | material: "CONCRETE/Concrete_Undefined" | property sets: Tekla Common, QC_Standard, Tekla Quantity, Pours
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_Qegs1zYFkECFEu_6lD-C8g_0" | object type "_Qegs1zYFkECFEu_6lD-C8g_0" | names: "TBL-8" | descriptions: "_Qegs1zYFkECFEu_6lD-C8g_0" | material: "CONCRETE/Concrete_Undefined" | property sets: Tekla Common, QC_Standard, Tekla Quantity, Pours
          2 x IFCPLATE | type IFCPLATETYPE "PL1110*119" | object type "PL1110*119" | names: "JD-1" | descriptions: "PL1110*119" | material: "STEEL/S235JR" | property sets: Tekla Common, Tekla Quantity, Pset_PlateCommon, BaseQuantities, QC_Standard
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_FBY1Et6deUytYuY0PxOVbg_0" | object type "_FBY1Et6deUytYuY0PxOVbg_0" | names: "TBL-1" | descriptions: "_FBY1Et6deUytYuY0PxOVbg_0" | material: "CONCRETE/fc 280" | property sets: QC_Standard, Tekla Common, Tekla Quantity, Pours

Types
  IFCPLATETYPE "PL10*600" | 2 occurrences
  IFCPLATETYPE "PL10*552" | 2 occurrences
  IFCPLATETYPE "PL160*499" | 1 occurrence
  IFCCOLUMNTYPE "D41.28" | 4 occurrences
  IFCCOLUMNTYPE "D25.96" | 12 occurrences
  IFCCOLUMNTYPE "EPD57*15.52" | 4 occurrences
  IFCCOLUMNTYPE "EPD52.4*13.22" | 4 occurrences
  IFCCOLUMNTYPE "EPD50.8*12.42" | 8 occurrences
  IFCBEAMTYPE "D41.28" | 4 occurrences
  IFCBEAMTYPE "D25.96" | 8 occurrences
  IFCBEAMTYPE "EPD57*15.52" | 4 occurrences
  IFCBEAMTYPE "EPD52.4*13.22" | 4 occurrences
  IFCBEAMTYPE "EPD50.8*12.42" | 4 occurrences
  IFCBUILDINGELEMENTPROXYTYPE "TUBE76.2*10" | 504 occurrences
  IFCBUILDINGELEMENTPROXYTYPE "TUBE50.8*10" | 12 occurrences
  IFCBUILDINGELEMENTPROXYTYPE "TUBE101.6*10" | 12 occurrences
  IFCWALLTYPE "IPSMVB100*202.5*400*2242*2183*100*200*50*277.02" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "_Tx2InNPleECRYRtQh2Hjng_0" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "_Cgysq5sgMU-qaFJMdjTZlA_0" | 1 occurrence
  IFCBEAMTYPE "_JDsZU83epEen0TzaihjSSg_0" | 10 occurrences
  IFCBEAMTYPE "_pgRV1qUE7U6m_HgCCkwbIg_0" | 20 occurrences
  IFCBEAMTYPE "400*1803" | 16 occurrences
  IFCBEAMTYPE "250*1803" | 96 occurrences
  IFCBEAMTYPE "_MY_mTXLcvEqkIjaXhGbUIA_0" | 10 occurrences
  IFCWALLTYPE "3000*400" | 206 occurrences
  IFCBEAMTYPE "800*2120" | 6 occurrences
  IFCBEAMTYPE "250*2120" | 12 occurrences
  IFCBEAMTYPE "250*300" | 48 occurrences
  IFCBUILDINGELEMENTPROXYTYPE "D80" | 120 occurrences
  IFCBUILDINGELEMENTPROXYTYPE "_iQAmr9z6UkaDmdLvQmn5QQ_0" | 20 occurrences
  IFCBUILDINGELEMENTPROXYTYPE "_APuikTUeQUedexBVPMTNFQ_0" | 20 occurrences
  IFCBUILDINGELEMENTPROXYTYPE "_zctwP5PVpU2GxoQPSbg4lw_0" | 20 occurrences
  IFCBUILDINGELEMENTPROXYTYPE "_WWhurdFeXUWNEXEY9ytvkw_0" | 20 occurrences
  IFCBUILDINGELEMENTPROXYTYPE "_WWhurdFeXUWNEXEY9ytvkw_1" | 20 occurrences
  IFCBUILDINGELEMENTPROXYTYPE "_WWhurdFeXUWNEXEY9ytvkw_2" | 20 occurrences
  IFCBUILDINGELEMENTPROXYTYPE "_xZMV8PGNj0O_GuQtP7XEWQ_0" | 10 occurrences
  IFCBUILDINGELEMENTPROXYTYPE "_xZMV8PGNj0O_GuQtP7XEWQ_1" | 10 occurrences
  IFCBUILDINGELEMENTPROXYTYPE "_zGkkAOtzg0y0avhCB96LKA_0" | 10 occurrences
  IFCBUILDINGELEMENTPROXYTYPE "_zGkkAOtzg0y0avhCB96LKA_1" | 10 occurrences
  IFCBUILDINGELEMENTPROXYTYPE "_zGkkAOtzg0y0avhCB96LKA_2" | 10 occurrences
  IFCBUILDINGELEMENTPROXYTYPE "_xZMV8PGNj0O_GuQtP7XEWQ_2" | 10 occurrences
  IFCBUILDINGELEMENTPROXYTYPE "_W0Q29rrUD0qI3pwUSWdnxA_0" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "_W0Q29rrUD0qI3pwUSWdnxA_1" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "_W0Q29rrUD0qI3pwUSWdnxA_2" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "_W0Q29rrUD0qI3pwUSWdnxA_3" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "_W0Q29rrUD0qI3pwUSWdnxA_4" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "_wCNGqzzxSkuBKOybvcB-mg_0" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "_wCNGqzzxSkuBKOybvcB-mg_1" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "_wCNGqzzxSkuBKOybvcB-mg_2" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "_wCNGqzzxSkuBKOybvcB-mg_3" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "_wCNGqzzxSkuBKOybvcB-mg_4" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "_mqotvdKdsE-wiT5oCGDPuw_0" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "_mqotvdKdsE-wiT5oCGDPuw_1" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "_mqotvdKdsE-wiT5oCGDPuw_2" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "_mqotvdKdsE-wiT5oCGDPuw_3" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "_mqotvdKdsE-wiT5oCGDPuw_4" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "_RhRq7PJ5BEKGix01TNl22w_0" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "_RhRq7PJ5BEKGix01TNl22w_1" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "_RhRq7PJ5BEKGix01TNl22w_2" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "_RhRq7PJ5BEKGix01TNl22w_3" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "_RhRq7PJ5BEKGix01TNl22w_4" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "_q7vE1UKJQkSIGwLYHKbz7A_0" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "_q7vE1UKJQkSIGwLYHKbz7A_1" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "_q7vE1UKJQkSIGwLYHKbz7A_2" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "_q7vE1UKJQkSIGwLYHKbz7A_3" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "_q7vE1UKJQkSIGwLYHKbz7A_4" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "_rQh3fPrxo02546su1FUq5g_0" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "_rQh3fPrxo02546su1FUq5g_1" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "_rQh3fPrxo02546su1FUq5g_2" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "_rQh3fPrxo02546su1FUq5g_3" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "_rQh3fPrxo02546su1FUq5g_4" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "_bNZjJmYlm0KwoRrWD2MFtw_0" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "_bNZjJmYlm0KwoRrWD2MFtw_1" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "_bNZjJmYlm0KwoRrWD2MFtw_2" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "_bNZjJmYlm0KwoRrWD2MFtw_3" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "_bNZjJmYlm0KwoRrWD2MFtw_4" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "_MKZrQiKvyU-fFOxn3trsng_0" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "_MKZrQiKvyU-fFOxn3trsng_1" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "_MKZrQiKvyU-fFOxn3trsng_2" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "_MKZrQiKvyU-fFOxn3trsng_3" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "_MKZrQiKvyU-fFOxn3trsng_4" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "_MKZrQiKvyU-fFOxn3trsng_10" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "_MKZrQiKvyU-fFOxn3trsng_11" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "_MKZrQiKvyU-fFOxn3trsng_12" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "_MKZrQiKvyU-fFOxn3trsng_13" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "_MKZrQiKvyU-fFOxn3trsng_14" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "_MKZrQiKvyU-fFOxn3trsng_20" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "_MKZrQiKvyU-fFOxn3trsng_21" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "_MKZrQiKvyU-fFOxn3trsng_22" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "_MKZrQiKvyU-fFOxn3trsng_23" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "_MKZrQiKvyU-fFOxn3trsng_24" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "_MKZrQiKvyU-fFOxn3trsng_30" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "_MKZrQiKvyU-fFOxn3trsng_31" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "_MKZrQiKvyU-fFOxn3trsng_32" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "_MKZrQiKvyU-fFOxn3trsng_33" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "_MKZrQiKvyU-fFOxn3trsng_34" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "_XzVA3TGxA0iQtYZr7oqung_0" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "_XzVA3TGxA0iQtYZr7oqung_1" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "_XzVA3TGxA0iQtYZr7oqung_2" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "_XzVA3TGxA0iQtYZr7oqung_3" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "_XzVA3TGxA0iQtYZr7oqung_4" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "_XzVA3TGxA0iQtYZr7oqung_10" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "_XzVA3TGxA0iQtYZr7oqung_11" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "_XzVA3TGxA0iQtYZr7oqung_12" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "_XzVA3TGxA0iQtYZr7oqung_13" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "_XzVA3TGxA0iQtYZr7oqung_14" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "_XzVA3TGxA0iQtYZr7oqung_20" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "_XzVA3TGxA0iQtYZr7oqung_21" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "_XzVA3TGxA0iQtYZr7oqung_22" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "_XzVA3TGxA0iQtYZr7oqung_23" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "_XzVA3TGxA0iQtYZr7oqung_24" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "_XzVA3TGxA0iQtYZr7oqung_30" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "_XzVA3TGxA0iQtYZr7oqung_31" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "_XzVA3TGxA0iQtYZr7oqung_32" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "_XzVA3TGxA0iQtYZr7oqung_33" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "_XzVA3TGxA0iQtYZr7oqung_34" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "_Xx3dOakcfUO0IxJF-yvkhA_0" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "_Xx3dOakcfUO0IxJF-yvkhA_1" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "_Xx3dOakcfUO0IxJF-yvkhA_2" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "_Xx3dOakcfUO0IxJF-yvkhA_3" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "_Xx3dOakcfUO0IxJF-yvkhA_4" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "_xM0e5Dp4S02OamZVnlEJYA_2_1" | 10 occurrences
  IFCBUILDINGELEMENTPROXYTYPE "_o5V_7SDI4k-TInVG-m3yJQ_1_1" | 10 occurrences
  IFCBUILDINGELEMENTPROXYTYPE "_o5V_7SDI4k-TInVG-m3yJQ_0" | 10 occurrences
  IFCBUILDINGELEMENTPROXYTYPE "_o5V_7SDI4k-TInVG-m3yJQ_2_1" | 10 occurrences
  IFCBUILDINGELEMENTPROXYTYPE "_xM0e5Dp4S02OamZVnlEJYA_1_1" | 10 occurrences
  IFCBUILDINGELEMENTPROXYTYPE "_xM0e5Dp4S02OamZVnlEJYA_0" | 10 occurrences
  IFCBUILDINGELEMENTPROXYTYPE "_Ytsq9ZJl6kKIcPhQQVUMXA_0" | 4 occurrences
  IFCBUILDINGELEMENTPROXYTYPE "_NC7kOKz8QEKJmJ5mCongMA_0" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "_aJiu3r_V90SDTop659Lqxg_0" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "_Qegs1zYFkECFEu_6lD-C8g_0" | 1 occurrence
  IFCPLATETYPE "PL1110*119" | 2 occurrences
  IFCBUILDINGELEMENTPROXYTYPE "_FBY1Et6deUytYuY0PxOVbg_0" | 1 occurrence

Property sets
  QC_Standard | properties | on 60 objects (60 IFCBUILDINGELEMENTPROXY)
    A (no value)
    Alfa (no value)
    Aplicacion (no value)
    Aplicacion = "Tuberia" (IFCLABEL)
    B (no value)
    Beta (no value)
    Bloque = "Calzada Derecha" (IFCLABEL)
    C (no value)
    CC (no value)
    Cantidad (no value)
    Clase (no value)
    Creado en = "13.08.2021 18:49:49" (IFCLABEL)
    Creado por = "DESKTOP-TK2EL9U\QC-PC-JAMES" (IFCLABEL)
    D (no value)
    E (no value)
    Encofrado (no value)
    Estado (no value)
    F (no value)
    Fecha de Inicio (no value)
    Fecha de estado (no value)
    Fecha de termino (no value)
    Forma (no value)
    G (no value)
    Gamma (no value)
    H (no value)
    Habilitado (no value)
    I (no value)
    ID concreto (no value)
    Longitud = 800. (IFCLENGTHMEASURE) [MILLI METRE]
    Marca (no value)
    Material = "Tubo Metalico" (IFCLABEL)
    Modificacion (no value)
    Modificado en (no value)
    Modificado por (no value)
    Nivel = "SuperEstructura" (IFCLABEL)
    Nombre = "Tub-3"" (IFCLABEL)
    Orden de Produccion (no value)
    Peso = 0. (IFCMASSMEASURE) [KILO GRAM]
    Peso Total (no value)
    Plano (no value)
    Posicion (no value)
    QC_ID_UNIQUE (no value)
    QC_LOOKAHEAD (no value)
    QC_PUBLISH (no value)
    Tamaño (no value)
    Tipo (no value)
    Ubicacion = "P7-E2" (IFCLABEL)
    Vaciado (no value)
    Volumen = 0. (IFCVOLUMEMEASURE) [CUBIC_METRE]
  QC_Standard | properties | on 60 objects (60 IFCBUILDINGELEMENTPROXY)
    A (no value)
    Alfa (no value)
    Aplicacion (no value)
    Aplicacion = "Tuberia" (IFCLABEL)
    B (no value)
    Beta (no value)
    Bloque = "Calzada Derecha" (IFCLABEL)
    C (no value)
    CC (no value)
    Cantidad (no value)
    Clase (no value)
    Creado en = "13.08.2021 18:49:49" (IFCLABEL)
    Creado por = "DESKTOP-TK2EL9U\QC-PC-JAMES" (IFCLABEL)
    D (no value)
    E (no value)
    Encofrado (no value)
    Estado (no value)
    F (no value)
    Fecha de Inicio (no value)
    Fecha de estado (no value)
    Fecha de termino (no value)
    Forma (no value)
    G (no value)
    Gamma (no value)
    H (no value)
    Habilitado (no value)
    I (no value)
    ID concreto (no value)
    Longitud = 800. (IFCLENGTHMEASURE) [MILLI METRE]
    Marca (no value)
    Material = "Tubo Metalico" (IFCLABEL)
    Modificacion (no value)
    Modificado en (no value)
    Modificado por (no value)
    Nivel = "SuperEstructura" (IFCLABEL)
    Nombre = "Tub-3"" (IFCLABEL)
    Orden de Produccion (no value)
    Peso = 0. (IFCMASSMEASURE) [KILO GRAM]
    Peso Total (no value)
    Plano (no value)
    Posicion (no value)
    QC_ID_UNIQUE (no value)
    QC_LOOKAHEAD (no value)
    QC_PUBLISH (no value)
    Tamaño (no value)
    Tipo (no value)
    Ubicacion = "P6-P7" (IFCLABEL)
    Vaciado (no value)
    Volumen = 0. (IFCVOLUMEMEASURE) [CUBIC_METRE]
  QC_Standard | properties | on 60 objects (60 IFCBUILDINGELEMENTPROXY)
    A (no value)
    Alfa (no value)
    Aplicacion (no value)
    Aplicacion = "Tuberia" (IFCLABEL)
    B (no value)
    Beta (no value)
    Bloque = "Calzada Derecha" (IFCLABEL)
    C (no value)
    CC (no value)
    Cantidad (no value)
    Clase (no value)
    Creado en = "13.08.2021 18:49:49" (IFCLABEL)
    Creado por = "DESKTOP-TK2EL9U\QC-PC-JAMES" (IFCLABEL)
    D (no value)
    E (no value)
    Encofrado (no value)
    Estado (no value)
    F (no value)
    Fecha de Inicio (no value)
    Fecha de estado (no value)
    Fecha de termino (no value)
    Forma (no value)
    G (no value)
    Gamma (no value)
    H (no value)
    Habilitado (no value)
    I (no value)
    ID concreto (no value)
    Longitud = 800. (IFCLENGTHMEASURE) [MILLI METRE]
    Marca (no value)
    Material = "Tubo Metalico" (IFCLABEL)
    Modificacion (no value)
    Modificado en (no value)
    Modificado por (no value)
    Nivel = "SuperEstructura" (IFCLABEL)
    Nombre = "Tub-3"" (IFCLABEL)
    Orden de Produccion (no value)
    Peso = 0. (IFCMASSMEASURE) [KILO GRAM]
    Peso Total (no value)
    Plano (no value)
    Posicion (no value)
    QC_ID_UNIQUE (no value)
    QC_LOOKAHEAD (no value)
    QC_PUBLISH (no value)
    Tamaño (no value)
    Tipo (no value)
    Ubicacion = "P5-P6" (IFCLABEL)
    Vaciado (no value)
    Volumen = 0. (IFCVOLUMEMEASURE) [CUBIC_METRE]
  QC_Standard | properties | on 60 objects (60 IFCBUILDINGELEMENTPROXY)
    A (no value)
    Alfa (no value)
    Aplicacion (no value)
    Aplicacion = "Tuberia" (IFCLABEL)
    B (no value)
    Beta (no value)
    Bloque = "Calzada Derecha" (IFCLABEL)
    C (no value)
    CC (no value)
    Cantidad (no value)
    Clase (no value)
    Creado en = "13.08.2021 18:49:49" (IFCLABEL)
    Creado por = "DESKTOP-TK2EL9U\QC-PC-JAMES" (IFCLABEL)
    D (no value)
    E (no value)
    Encofrado (no value)
    Estado (no value)
    F (no value)
    Fecha de Inicio (no value)
    Fecha de estado (no value)
    Fecha de termino (no value)
    Forma (no value)
    G (no value)
    Gamma (no value)
    H (no value)
    Habilitado (no value)
    I (no value)
    ID concreto (no value)
    Longitud = 800. (IFCLENGTHMEASURE) [MILLI METRE]
    Marca (no value)
    Material = "Tubo Metalico" (IFCLABEL)
    Modificacion (no value)
    Modificado en (no value)
    Modificado por (no value)
    Nivel = "SuperEstructura" (IFCLABEL)
    Nombre = "Tub-3"" (IFCLABEL)
    Orden de Produccion (no value)
    Peso = 0. (IFCMASSMEASURE) [KILO GRAM]
    Peso Total (no value)
    Plano (no value)
    Posicion (no value)
    QC_ID_UNIQUE (no value)
    QC_LOOKAHEAD (no value)
    QC_PUBLISH (no value)
    Tamaño (no value)
    Tipo (no value)
    Ubicacion = "P4-P5" (IFCLABEL)
    Vaciado (no value)
    Volumen = 0. (IFCVOLUMEMEASURE) [CUBIC_METRE]
  QC_Standard | properties | on 60 objects (60 IFCBUILDINGELEMENTPROXY)
    A (no value)
    Alfa (no value)
    Aplicacion (no value)
    Aplicacion = "Tuberia" (IFCLABEL)
    B (no value)
    Beta (no value)
    Bloque = "Calzada Derecha" (IFCLABEL)
    C (no value)
    CC (no value)
    Cantidad (no value)
    Clase (no value)
    Creado en = "13.08.2021 18:49:49" (IFCLABEL)
    Creado por = "DESKTOP-TK2EL9U\QC-PC-JAMES" (IFCLABEL)
    D (no value)
    E (no value)
    Encofrado (no value)
    Estado (no value)
    F (no value)
    Fecha de Inicio (no value)
    Fecha de estado (no value)
    Fecha de termino (no value)
    Forma (no value)
    G (no value)
    Gamma (no value)
    H (no value)
    Habilitado (no value)
    I (no value)
    ID concreto (no value)
    Longitud = 800. (IFCLENGTHMEASURE) [MILLI METRE]
    Marca (no value)
    Material = "Tubo Metalico" (IFCLABEL)
    Modificacion (no value)
    Modificado en (no value)
    Modificado por (no value)
    Nivel = "SuperEstructura" (IFCLABEL)
    Nombre = "Tub-3"" (IFCLABEL)
    Orden de Produccion (no value)
    Peso = 0. (IFCMASSMEASURE) [KILO GRAM]
    Peso Total (no value)
    Plano (no value)
    Posicion (no value)
    QC_ID_UNIQUE (no value)
    QC_LOOKAHEAD (no value)
    QC_PUBLISH (no value)
    Tamaño (no value)
    Tipo (no value)
    Ubicacion = "P3-P4" (IFCLABEL)
    Vaciado (no value)
    Volumen = 0. (IFCVOLUMEMEASURE) [CUBIC_METRE]
  QC_Standard | properties | on 60 objects (60 IFCBUILDINGELEMENTPROXY)
    A (no value)
    Alfa (no value)
    Aplicacion (no value)
    Aplicacion = "Tuberia" (IFCLABEL)
    B (no value)
    Beta (no value)
    Bloque = "Calzada Derecha" (IFCLABEL)
    C (no value)
    CC (no value)
    Cantidad (no value)
    Clase (no value)
    Creado en = "13.08.2021 18:49:49" (IFCLABEL)
    Creado por = "DESKTOP-TK2EL9U\QC-PC-JAMES" (IFCLABEL)
    D (no value)
    E (no value)
    Encofrado (no value)
    Estado (no value)
    F (no value)
    Fecha de Inicio (no value)
    Fecha de estado (no value)
    Fecha de termino (no value)
    Forma (no value)
    G (no value)
    Gamma (no value)
    H (no value)
    Habilitado (no value)
    I (no value)
    ID concreto (no value)
    Longitud = 800. (IFCLENGTHMEASURE) [MILLI METRE]
    Marca (no value)
    Material = "Tubo Metalico" (IFCLABEL)
    Modificacion (no value)
    Modificado en (no value)
    Modificado por (no value)
    Nivel = "SuperEstructura" (IFCLABEL)
    Nombre = "Tub-3"" (IFCLABEL)
    Orden de Produccion (no value)
    Peso = 0. (IFCMASSMEASURE) [KILO GRAM]
    Peso Total (no value)
    Plano (no value)
    Posicion (no value)
    QC_ID_UNIQUE (no value)
    QC_LOOKAHEAD (no value)
    QC_PUBLISH (no value)
    Tamaño (no value)
    Tipo (no value)
    Ubicacion = "P2-P3" (IFCLABEL)
    Vaciado (no value)
    Volumen = 0. (IFCVOLUMEMEASURE) [CUBIC_METRE]
  QC_Standard | properties | on 60 objects (60 IFCBUILDINGELEMENTPROXY)
    A (no value)
    Alfa (no value)
    Aplicacion (no value)
    Aplicacion = "Tuberia" (IFCLABEL)
    B (no value)
    Beta (no value)
    Bloque = "Calzada Derecha" (IFCLABEL)
    C (no value)
    CC (no value)
    Cantidad (no value)
    Clase (no value)
    Creado en = "13.08.2021 18:49:49" (IFCLABEL)
    Creado por = "DESKTOP-TK2EL9U\QC-PC-JAMES" (IFCLABEL)
    D (no value)
    E (no value)
    Encofrado (no value)
    Estado (no value)
    F (no value)
    Fecha de Inicio (no value)
    Fecha de estado (no value)
    Fecha de termino (no value)
    Forma (no value)
    G (no value)
    Gamma (no value)
    H (no value)
    Habilitado (no value)
    I (no value)
    ID concreto (no value)
    Longitud = 800. (IFCLENGTHMEASURE) [MILLI METRE]
    Marca (no value)
    Material = "Tubo Metalico" (IFCLABEL)
    Modificacion (no value)
    Modificado en (no value)
    Modificado por (no value)
    Nivel = "SuperEstructura" (IFCLABEL)
    Nombre = "Tub-3"" (IFCLABEL)
    Orden de Produccion (no value)
    Peso = 0. (IFCMASSMEASURE) [KILO GRAM]
    Peso Total (no value)
    Plano (no value)
    Posicion (no value)
    QC_ID_UNIQUE (no value)
    QC_LOOKAHEAD (no value)
    QC_PUBLISH (no value)
    Tamaño (no value)
    Tipo (no value)
    Ubicacion = "P1-P2" (IFCLABEL)
    Vaciado (no value)
    Volumen = 0. (IFCVOLUMEMEASURE) [CUBIC_METRE]
  QC_Standard | properties | on 60 objects (60 IFCBUILDINGELEMENTPROXY)
    A (no value)
    Alfa (no value)
    Aplicacion (no value)
    Aplicacion = "Tuberia" (IFCLABEL)
    B (no value)
    Beta (no value)
    Bloque = "Calzada Derecha" (IFCLABEL)
    C (no value)
    CC (no value)
    Cantidad (no value)
    Clase (no value)
    Creado en = "13.08.2021 18:49:49" (IFCLABEL)
    Creado por = "DESKTOP-TK2EL9U\QC-PC-JAMES" (IFCLABEL)
    D (no value)
    E (no value)
    Encofrado (no value)
    Estado (no value)
    F (no value)
    Fecha de Inicio (no value)
    Fecha de estado (no value)
    Fecha de termino (no value)
    Forma (no value)
    G (no value)
    Gamma (no value)
    H (no value)
    Habilitado (no value)
    I (no value)
    ID concreto (no value)
    Longitud = 800. (IFCLENGTHMEASURE) [MILLI METRE]
    Marca (no value)
    Material = "Tubo Metalico" (IFCLABEL)
    Modificacion (no value)
    Modificado en (no value)
    Modificado por (no value)
    Nivel = "SuperEstructura" (IFCLABEL)
    Nombre = "Tub-3"" (IFCLABEL)
    Orden de Produccion (no value)
    Peso = 0. (IFCMASSMEASURE) [KILO GRAM]
    Peso Total (no value)
    Plano (no value)
    Posicion (no value)
    QC_ID_UNIQUE (no value)
    QC_LOOKAHEAD (no value)
    QC_PUBLISH (no value)
    Tamaño (no value)
    Tipo (no value)
    Ubicacion = "E1-P1" (IFCLABEL)
    Vaciado (no value)
    Volumen = 0. (IFCVOLUMEMEASURE) [CUBIC_METRE]
  QC_Standard: 275 more contents on 1136 objects not shown
  Tekla Common | properties | on 103 objects (103 IFCWALL)
    Bottom elevation = "+27.508" (IFCLABEL)
    Class = "2" (IFCLABEL)
    Initial GUID (no value)
    Phase = 1 (IFCINTEGER)
    Preliminary mark = "" (IFCLABEL)
    Top elevation = "+28.158" (IFCLABEL)
  Tekla Common | properties | on 103 objects (103 IFCWALL)
    Bottom elevation = "+27.290" (IFCLABEL)
    Class = "2" (IFCLABEL)
    Initial GUID (no value)
    Phase = 1 (IFCINTEGER)
    Preliminary mark = "" (IFCLABEL)
    Top elevation = "+27.940" (IFCLABEL)
  Tekla Common | properties | on 48 objects (48 IFCBUILDINGELEMENTPROXY)
    Bottom elevation = "+25.406" (IFCLABEL)
    Class = "1" (IFCLABEL)
    Initial GUID (no value)
    Phase = 1 (IFCINTEGER)
    Preliminary mark = "" (IFCLABEL)
    Top elevation = "+25.482" (IFCLABEL)
  Tekla Common | properties | on 48 objects (48 IFCBUILDINGELEMENTPROXY)
    Bottom elevation = "+25.300" (IFCLABEL)
    Class = "1" (IFCLABEL)
    Initial GUID (no value)
    Phase = 1 (IFCINTEGER)
    Preliminary mark = "" (IFCLABEL)
    Top elevation = "+25.376" (IFCLABEL)
  Tekla Common | properties | on 48 objects (48 IFCBUILDINGELEMENTPROXY)
    Bottom elevation = "+25.344" (IFCLABEL)
    Class = "1" (IFCLABEL)
    Initial GUID (no value)
    Phase = 1 (IFCINTEGER)
    Preliminary mark = "" (IFCLABEL)
    Top elevation = "+25.420" (IFCLABEL)
  Tekla Common | properties | on 48 objects (48 IFCBUILDINGELEMENTPROXY)
    Bottom elevation = "+25.238" (IFCLABEL)
    Class = "1" (IFCLABEL)
    Initial GUID (no value)
    Phase = 1 (IFCINTEGER)
    Preliminary mark = "" (IFCLABEL)
    Top elevation = "+25.314" (IFCLABEL)
  Tekla Common | properties | on 48 objects (48 IFCBUILDINGELEMENTPROXY)
    Bottom elevation = "+25.285" (IFCLABEL)
    Class = "1" (IFCLABEL)
    Initial GUID (no value)
    Phase = 1 (IFCINTEGER)
    Preliminary mark = "" (IFCLABEL)
    Top elevation = "+25.361" (IFCLABEL)
  Tekla Common | properties | on 48 objects (48 IFCBUILDINGELEMENTPROXY)
    Bottom elevation = "+25.179" (IFCLABEL)
    Class = "1" (IFCLABEL)
    Initial GUID (no value)
    Phase = 1 (IFCINTEGER)
    Preliminary mark = "" (IFCLABEL)
    Top elevation = "+25.255" (IFCLABEL)
  Tekla Common: 135 more contents on 1122 objects not shown
  Tekla Quantity | properties | on 480 objects (480 IFCBUILDINGELEMENTPROXY)
    Area per tons = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Gross footprint area = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Height = 76.2 (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 800. (IFCLENGTHMEASURE) [MILLI METRE]
    Net surface area = 0.2 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0. (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Weight = 0. (IFCMASSMEASURE) [KILO GRAM]
    Width = 76.2 (IFCLENGTHMEASURE) [MILLI METRE]
  Tekla Quantity | properties | on 206 objects (206 IFCWALL)
    Area per tons = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Gross footprint area = 0.4 (IFCAREAMEASURE) [SQUARE_METRE]
    Height = 400. (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 650. (IFCLENGTHMEASURE) [MILLI METRE]
    Net surface area = 6.2 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.5 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Weight = 0. (IFCMASSMEASURE) [KILO GRAM]
    Width = 3000. (IFCLENGTHMEASURE) [MILLI METRE]
  Tekla Quantity | properties | on 80 objects (80 IFCBUILDINGELEMENTPROXY)
    Area per tons = 5. (IFCAREAMEASURE) [SQUARE_METRE]
    Gross footprint area = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Height = 250.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 322. (IFCLENGTHMEASURE) [MILLI METRE]
    Net surface area = 0.3 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0. (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Weight = 52.3 (IFCMASSMEASURE) [KILO GRAM]
    Width = 250. (IFCLENGTHMEASURE) [MILLI METRE]
  Tekla Quantity | properties | on 80 objects (80 IFCBUILDINGELEMENTPROXY)
    Area per tons = 5. (IFCAREAMEASURE) [SQUARE_METRE]
    Gross footprint area = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Height = 249.8 (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 327.2 (IFCLENGTHMEASURE) [MILLI METRE]
    Net surface area = 0.3 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0. (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Weight = 52.3 (IFCMASSMEASURE) [KILO GRAM]
    Width = 250. (IFCLENGTHMEASURE) [MILLI METRE]
  Tekla Quantity | properties | on 80 objects (80 IFCBUILDINGELEMENTPROXY)
    Area per tons = 5. (IFCAREAMEASURE) [SQUARE_METRE]
    Gross footprint area = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Height = 249. (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 331.7 (IFCLENGTHMEASURE) [MILLI METRE]
    Net surface area = 0.3 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0. (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Weight = 52.3 (IFCMASSMEASURE) [KILO GRAM]
    Width = 250. (IFCLENGTHMEASURE) [MILLI METRE]
  Tekla Quantity | properties | on 80 objects (80 IFCBUILDINGELEMENTPROXY)
    Area per tons = 8.6 (IFCAREAMEASURE) [SQUARE_METRE]
    Gross footprint area = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Height = 1468. (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 175. (IFCLENGTHMEASURE) [MILLI METRE]
    Net surface area = 1.9 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.1 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Weight = 220.9 (IFCMASSMEASURE) [KILO GRAM]
    Width = 533. (IFCLENGTHMEASURE) [MILLI METRE]
  Tekla Quantity | properties | on 72 objects (72 IFCBEAM)
    Area per tons = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Gross footprint area = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Height = 1803.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 2784.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Net surface area = 11.6 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 1.3 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Weight = 0. (IFCMASSMEASURE) [KILO GRAM]
    Width = 250. (IFCLENGTHMEASURE) [MILLI METRE]
  Tekla Quantity | properties | on 48 objects (48 IFCBEAM)
    Area per tons = 6.7 (IFCAREAMEASURE) [SQUARE_METRE]
    Gross footprint area = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Height = 300. (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 1681.2 (IFCLENGTHMEASURE) [MILLI METRE]
    Net surface area = 1.7 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.1 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Weight = 271.5 (IFCMASSMEASURE) [KILO GRAM]
    Width = 250. (IFCLENGTHMEASURE) [MILLI METRE]
  Tekla Quantity: 59 more contents on 490 objects not shown
  Pours | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Pour Actual End Date (no value)
    Pour Actual End Form (no value)
    Pour Actual End Rebar (no value)
    Pour Actual Start Date (no value)
    Pour Actual Start Form (no value)
    Pour Actual Start Rebar (no value)
    Pour Area = 1056.9 (IFCAREAMEASURE) [SQUARE_METRE]
    Pour Area NGY = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Pour Area NGZ = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Pour Area NXG = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Pour Area PGX = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Pour Area PGY = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Pour Area PGZ = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Pour Bottom Level = "+26.969" (IFCLABEL)
    Pour Break Comment (no value)
    Pour Break GUID = "82315272-d39b-4bc5-8d7f-5d61d2e6c362" (IFCLABEL)
    Pour Break ID (no value)
    Pour Break Type (no value)
    Pour Check Date (no value)
    Pour Checked By (no value)
    Pour Comment (no value)
    Pour Comment (no value)
    Pour Concrete Mixture (no value)
    Pour Content Type = "PART" (IFCLABEL)
    Pour Formwork Check Date (no value)
    Pour Formwork Checked By (no value)
    Pour Formwork Comment (no value)
    Pour Formwork Status (no value)
    Pour GUID = "82315272-d39b-4bc5-8d7f-5d61d2e6c362" (IFCLABEL)
    Pour ID (no value)
    Pour Material = "fc 280" (IFCLABEL)
    Pour Number (no value)
    Pour Planned End Date (no value)
    Pour Planned End Form (no value)
    Pour Planned End Rebar (no value)
    Pour Planned Start Date (no value)
    Pour Planned Start Form (no value)
    Pour Planned Start Rebar (no value)
    Pour Rebar Check Date (no value)
    Pour Rebar CheckedBy (no value)
    Pour Rebar Comment (no value)
    Pour Rebar Release Number (no value)
    Pour Rebar Shipment Number (no value)
    Pour Rebar Status (no value)
    Pour Status (no value)
    Pour Top Level = "+27.508" (IFCLABEL)
    Pour Type (no value)
    Pour User Field1 (no value)
    Pour User Field2 (no value)
    Pour User Field3 (no value)
    Pour User Field4 (no value)
    Pour Volume = 106.7 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Pour Weight = 0. (IFCMASSMEASURE) [KILO GRAM]
    Pour Weight Net = 0. (IFCMASSMEASURE) [KILO GRAM]
  Pours | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Pour Actual End Date (no value)
    Pour Actual End Form (no value)
    Pour Actual End Rebar (no value)
    Pour Actual Start Date (no value)
    Pour Actual Start Form (no value)
    Pour Actual Start Rebar (no value)
    Pour Area = 214.8 (IFCAREAMEASURE) [SQUARE_METRE]
    Pour Area NGY = 8.5 (IFCAREAMEASURE) [SQUARE_METRE]
    Pour Area NGZ = 23.2 (IFCAREAMEASURE) [SQUARE_METRE]
    Pour Area NXG = 71.8 (IFCAREAMEASURE) [SQUARE_METRE]
    Pour Area PGX = 66.6 (IFCAREAMEASURE) [SQUARE_METRE]
    Pour Area PGY = 8.9 (IFCAREAMEASURE) [SQUARE_METRE]
    Pour Area PGZ = 28.4 (IFCAREAMEASURE) [SQUARE_METRE]
    Pour Bottom Level = "+21.200" (IFCLABEL)
    Pour Break Comment (no value)
    Pour Break GUID = "2c3bc737-f72c-4ba4-b581-c3d0f4c37ae7" (IFCLABEL)
    Pour Break ID (no value)
    Pour Break Type (no value)
    Pour Check Date (no value)
    Pour Checked By (no value)
    Pour Comment (no value)
    Pour Comment (no value)
    Pour Concrete Mixture (no value)
    Pour Content Type = "PART" (IFCLABEL)
    Pour Formwork Check Date (no value)
    Pour Formwork Checked By (no value)
    Pour Formwork Comment (no value)
    Pour Formwork Status (no value)
    Pour GUID = "2c3bc737-f72c-4ba4-b581-c3d0f4c37ae7" (IFCLABEL)
    Pour ID (no value)
    Pour Material = "Concrete_Undefined" (IFCLABEL)
    Pour Number (no value)
    Pour Planned End Date (no value)
    Pour Planned End Form (no value)
    Pour Planned End Rebar (no value)
    Pour Planned Start Date (no value)
    Pour Planned Start Form (no value)
    Pour Planned Start Rebar (no value)
    Pour Rebar Check Date (no value)
    Pour Rebar CheckedBy (no value)
    Pour Rebar Comment (no value)
    Pour Rebar Release Number (no value)
    Pour Rebar Shipment Number (no value)
    Pour Rebar Status (no value)
    Pour Status (no value)
    Pour Top Level = "+27.508" (IFCLABEL)
    Pour Type (no value)
    Pour User Field1 (no value)
    Pour User Field2 (no value)
    Pour User Field3 (no value)
    Pour User Field4 (no value)
    Pour Volume = 100.7 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Pour Weight = 241758.6 (IFCMASSMEASURE) [KILO GRAM]
    Pour Weight Net = 241758.6 (IFCMASSMEASURE) [KILO GRAM]
  Pours | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Pour Actual End Date (no value)
    Pour Actual End Form (no value)
    Pour Actual End Rebar (no value)
    Pour Actual Start Date (no value)
    Pour Actual Start Form (no value)
    Pour Actual Start Rebar (no value)
    Pour Area = 214.8 (IFCAREAMEASURE) [SQUARE_METRE]
    Pour Area NGY = 8.5 (IFCAREAMEASURE) [SQUARE_METRE]
    Pour Area NGZ = 23.2 (IFCAREAMEASURE) [SQUARE_METRE]
    Pour Area NXG = 66.6 (IFCAREAMEASURE) [SQUARE_METRE]
    Pour Area PGX = 71.8 (IFCAREAMEASURE) [SQUARE_METRE]
    Pour Area PGY = 8.9 (IFCAREAMEASURE) [SQUARE_METRE]
    Pour Area PGZ = 28.4 (IFCAREAMEASURE) [SQUARE_METRE]
    Pour Bottom Level = "+21.200" (IFCLABEL)
    Pour Break Comment (no value)
    Pour Break GUID = "149ec76a-77b3-4623-b1df-1c97418ae9aa" (IFCLABEL)
    Pour Break ID (no value)
    Pour Break Type (no value)
    Pour Check Date (no value)
    Pour Checked By (no value)
    Pour Comment (no value)
    Pour Comment (no value)
    Pour Concrete Mixture (no value)
    Pour Content Type = "PART" (IFCLABEL)
    Pour Formwork Check Date (no value)
    Pour Formwork Checked By (no value)
    Pour Formwork Comment (no value)
    Pour Formwork Status (no value)
    Pour GUID = "149ec76a-77b3-4623-b1df-1c97418ae9aa" (IFCLABEL)
    Pour ID (no value)
    Pour Material = "Concrete_Undefined" (IFCLABEL)
    Pour Number (no value)
    Pour Planned End Date (no value)
    Pour Planned End Form (no value)
    Pour Planned End Rebar (no value)
    Pour Planned Start Date (no value)
    Pour Planned Start Form (no value)
    Pour Planned Start Rebar (no value)
    Pour Rebar Check Date (no value)
    Pour Rebar CheckedBy (no value)
    Pour Rebar Comment (no value)
    Pour Rebar Release Number (no value)
    Pour Rebar Shipment Number (no value)
    Pour Rebar Status (no value)
    Pour Status (no value)
    Pour Top Level = "+27.508" (IFCLABEL)
    Pour Type (no value)
    Pour User Field1 (no value)
    Pour User Field2 (no value)
    Pour User Field3 (no value)
    Pour User Field4 (no value)
    Pour Volume = 100.7 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Pour Weight = 241758.6 (IFCMASSMEASURE) [KILO GRAM]
    Pour Weight Net = 241758.6 (IFCMASSMEASURE) [KILO GRAM]
  Pours | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Pour Actual End Date (no value)
    Pour Actual End Form (no value)
    Pour Actual End Rebar (no value)
    Pour Actual Start Date (no value)
    Pour Actual Start Form (no value)
    Pour Actual Start Rebar (no value)
    Pour Area = 1056.9 (IFCAREAMEASURE) [SQUARE_METRE]
    Pour Area NGY = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Pour Area NGZ = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Pour Area NXG = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Pour Area PGX = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Pour Area PGY = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Pour Area PGZ = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Pour Bottom Level = "+26.969" (IFCLABEL)
    Pour Break Comment (no value)
    Pour Break GUID = "17d736bf-bbb7-46c4-986c-19b64df9e1ac" (IFCLABEL)
    Pour Break ID (no value)
    Pour Break Type (no value)
    Pour Check Date (no value)
    Pour Checked By (no value)
    Pour Comment (no value)
    Pour Comment (no value)
    Pour Concrete Mixture (no value)
    Pour Content Type = "PART" (IFCLABEL)
    Pour Formwork Check Date (no value)
    Pour Formwork Checked By (no value)
    Pour Formwork Comment (no value)
    Pour Formwork Status (no value)
    Pour GUID = "17d736bf-bbb7-46c4-986c-19b64df9e1ac" (IFCLABEL)
    Pour ID (no value)
    Pour Material = "Concrete_Undefined" (IFCLABEL)
    Pour Number (no value)
    Pour Planned End Date (no value)
    Pour Planned End Form (no value)
    Pour Planned End Rebar (no value)
    Pour Planned Start Date (no value)
    Pour Planned Start Form (no value)
    Pour Planned Start Rebar (no value)
    Pour Rebar Check Date (no value)
    Pour Rebar CheckedBy (no value)
    Pour Rebar Comment (no value)
    Pour Rebar Release Number (no value)
    Pour Rebar Shipment Number (no value)
    Pour Rebar Status (no value)
    Pour Status (no value)
    Pour Top Level = "+27.508" (IFCLABEL)
    Pour Type (no value)
    Pour User Field1 (no value)
    Pour User Field2 (no value)
    Pour User Field3 (no value)
    Pour User Field4 (no value)
    Pour Volume = 106.7 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Pour Weight = 256199. (IFCMASSMEASURE) [KILO GRAM]
    Pour Weight Net = 256199. (IFCMASSMEASURE) [KILO GRAM]
  Pours | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Pour Actual End Date (no value)
    Pour Actual End Form (no value)
    Pour Actual End Rebar (no value)
    Pour Actual Start Date (no value)
    Pour Actual Start Form (no value)
    Pour Actual Start Rebar (no value)
    Pour Area = 1069. (IFCAREAMEASURE) [SQUARE_METRE]
    Pour Area NGY = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Pour Area NGZ = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Pour Area NXG = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Pour Area PGX = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Pour Area PGY = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Pour Area PGZ = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Pour Bottom Level = "+26.969" (IFCLABEL)
    Pour Break Comment (no value)
    Pour Break GUID = "870b048f-ab9d-4b8c-884a-0418be53ca87" (IFCLABEL)
    Pour Break ID (no value)
    Pour Break Type (no value)
    Pour Check Date (no value)
    Pour Checked By (no value)
    Pour Comment (no value)
    Pour Comment (no value)
    Pour Concrete Mixture (no value)
    Pour Content Type = "PART" (IFCLABEL)
    Pour Formwork Check Date (no value)
    Pour Formwork Checked By (no value)
    Pour Formwork Comment (no value)
    Pour Formwork Status (no value)
    Pour GUID = "870b048f-ab9d-4b8c-884a-0418be53ca87" (IFCLABEL)
    Pour ID (no value)
    Pour Material = "Concrete_Undefined" (IFCLABEL)
    Pour Number (no value)
    Pour Planned End Date (no value)
    Pour Planned End Form (no value)
    Pour Planned End Rebar (no value)
    Pour Planned Start Date (no value)
    Pour Planned Start Form (no value)
    Pour Planned Start Rebar (no value)
    Pour Rebar Check Date (no value)
    Pour Rebar CheckedBy (no value)
    Pour Rebar Comment (no value)
    Pour Rebar Release Number (no value)
    Pour Rebar Shipment Number (no value)
    Pour Rebar Status (no value)
    Pour Status (no value)
    Pour Top Level = "+27.508" (IFCLABEL)
    Pour Type (no value)
    Pour User Field1 (no value)
    Pour User Field2 (no value)
    Pour User Field3 (no value)
    Pour User Field4 (no value)
    Pour Volume = 108.3 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Pour Weight = 259886.2 (IFCMASSMEASURE) [KILO GRAM]
    Pour Weight Net = 259886.2 (IFCMASSMEASURE) [KILO GRAM]
  Pours | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Pour Actual End Date (no value)
    Pour Actual End Form (no value)
    Pour Actual End Rebar (no value)
    Pour Actual Start Date (no value)
    Pour Actual Start Form (no value)
    Pour Actual Start Rebar (no value)
    Pour Area = 1069. (IFCAREAMEASURE) [SQUARE_METRE]
    Pour Area NGY = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Pour Area NGZ = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Pour Area NXG = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Pour Area PGX = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Pour Area PGY = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Pour Area PGZ = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Pour Bottom Level = "+26.969" (IFCLABEL)
    Pour Break Comment (no value)
    Pour Break GUID = "5725995e-3c72-4702-9012-4f3f1bc9a187" (IFCLABEL)
    Pour Break ID (no value)
    Pour Break Type (no value)
    Pour Check Date (no value)
    Pour Checked By (no value)
    Pour Comment (no value)
    Pour Comment (no value)
    Pour Concrete Mixture (no value)
    Pour Content Type = "PART" (IFCLABEL)
    Pour Formwork Check Date (no value)
    Pour Formwork Checked By (no value)
    Pour Formwork Comment (no value)
    Pour Formwork Status (no value)
    Pour GUID = "5725995e-3c72-4702-9012-4f3f1bc9a187" (IFCLABEL)
    Pour ID (no value)
    Pour Material = "Concrete_Undefined" (IFCLABEL)
    Pour Number (no value)
    Pour Planned End Date (no value)
    Pour Planned End Form (no value)
    Pour Planned End Rebar (no value)
    Pour Planned Start Date (no value)
    Pour Planned Start Form (no value)
    Pour Planned Start Rebar (no value)
    Pour Rebar Check Date (no value)
    Pour Rebar CheckedBy (no value)
    Pour Rebar Comment (no value)
    Pour Rebar Release Number (no value)
    Pour Rebar Shipment Number (no value)
    Pour Rebar Status (no value)
    Pour Status (no value)
    Pour Top Level = "+27.508" (IFCLABEL)
    Pour Type (no value)
    Pour User Field1 (no value)
    Pour User Field2 (no value)
    Pour User Field3 (no value)
    Pour User Field4 (no value)
    Pour Volume = 108.3 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Pour Weight = 259886.2 (IFCMASSMEASURE) [KILO GRAM]
    Pour Weight Net = 259886.2 (IFCMASSMEASURE) [KILO GRAM]
  Pours | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Pour Actual End Date (no value)
    Pour Actual End Form (no value)
    Pour Actual End Rebar (no value)
    Pour Actual Start Date (no value)
    Pour Actual Start Form (no value)
    Pour Actual Start Rebar (no value)
    Pour Area = 1048.5 (IFCAREAMEASURE) [SQUARE_METRE]
    Pour Area NGY = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Pour Area NGZ = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Pour Area NXG = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Pour Area PGX = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Pour Area PGY = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Pour Area PGZ = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Pour Bottom Level = "+26.969" (IFCLABEL)
    Pour Break Comment (no value)
    Pour Break GUID = "8633e817-c09d-497d-a75f-461ab2d8ff25" (IFCLABEL)
    Pour Break ID (no value)
    Pour Break Type (no value)
    Pour Check Date (no value)
    Pour Checked By (no value)
    Pour Comment (no value)
    Pour Comment (no value)
    Pour Concrete Mixture (no value)
    Pour Content Type = "PART" (IFCLABEL)
    Pour Formwork Check Date (no value)
    Pour Formwork Checked By (no value)
    Pour Formwork Comment (no value)
    Pour Formwork Status (no value)
    Pour GUID = "8633e817-c09d-497d-a75f-461ab2d8ff25" (IFCLABEL)
    Pour ID (no value)
    Pour Material = "Concrete_Undefined" (IFCLABEL)
    Pour Number (no value)
    Pour Planned End Date (no value)
    Pour Planned End Form (no value)
    Pour Planned End Rebar (no value)
    Pour Planned Start Date (no value)
    Pour Planned Start Form (no value)
    Pour Planned Start Rebar (no value)
    Pour Rebar Check Date (no value)
    Pour Rebar CheckedBy (no value)
    Pour Rebar Comment (no value)
    Pour Rebar Release Number (no value)
    Pour Rebar Shipment Number (no value)
    Pour Rebar Status (no value)
    Pour Status (no value)
    Pour Top Level = "+27.508" (IFCLABEL)
    Pour Type (no value)
    Pour User Field1 (no value)
    Pour User Field2 (no value)
    Pour User Field3 (no value)
    Pour User Field4 (no value)
    Pour Volume = 106.1 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Pour Weight = 254587.5 (IFCMASSMEASURE) [KILO GRAM]
    Pour Weight Net = 254587.5 (IFCMASSMEASURE) [KILO GRAM]
  Pours | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Pour Actual End Date (no value)
    Pour Actual End Form (no value)
    Pour Actual End Rebar (no value)
    Pour Actual Start Date (no value)
    Pour Actual Start Form (no value)
    Pour Actual Start Rebar (no value)
    Pour Area = 1048.5 (IFCAREAMEASURE) [SQUARE_METRE]
    Pour Area NGY = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Pour Area NGZ = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Pour Area NXG = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Pour Area PGX = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Pour Area PGY = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Pour Area PGZ = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Pour Bottom Level = "+26.969" (IFCLABEL)
    Pour Break Comment (no value)
    Pour Break GUID = "6721a632-0680-417c-9753-2c78eabf1293" (IFCLABEL)
    Pour Break ID (no value)
    Pour Break Type (no value)
    Pour Check Date (no value)
    Pour Checked By (no value)
    Pour Comment (no value)
    Pour Comment (no value)
    Pour Concrete Mixture (no value)
    Pour Content Type = "PART" (IFCLABEL)
    Pour Formwork Check Date (no value)
    Pour Formwork Checked By (no value)
    Pour Formwork Comment (no value)
    Pour Formwork Status (no value)
    Pour GUID = "6721a632-0680-417c-9753-2c78eabf1293" (IFCLABEL)
    Pour ID (no value)
    Pour Material = "Concrete_Undefined" (IFCLABEL)
    Pour Number (no value)
    Pour Planned End Date (no value)
    Pour Planned End Form (no value)
    Pour Planned End Rebar (no value)
    Pour Planned Start Date (no value)
    Pour Planned Start Form (no value)
    Pour Planned Start Rebar (no value)
    Pour Rebar Check Date (no value)
    Pour Rebar CheckedBy (no value)
    Pour Rebar Comment (no value)
    Pour Rebar Release Number (no value)
    Pour Rebar Shipment Number (no value)
    Pour Rebar Status (no value)
    Pour Status (no value)
    Pour Top Level = "+27.508" (IFCLABEL)
    Pour Type (no value)
    Pour User Field1 (no value)
    Pour User Field2 (no value)
    Pour User Field3 (no value)
    Pour User Field4 (no value)
    Pour Volume = 106.1 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Pour Weight = 254587.5 (IFCMASSMEASURE) [KILO GRAM]
    Pour Weight Net = 254587.5 (IFCMASSMEASURE) [KILO GRAM]
  Pours: 970 more contents on 970 objects not shown
  Pset_PlateCommon | properties | on 2 objects (2 IFCPLATE)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "1010(?)" (IFCIDENTIFIER)
  Pset_PlateCommon | properties | on 2 objects (2 IFCPLATE)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "1001" (IFCIDENTIFIER)
  Pset_PlateCommon | properties | on 2 objects (2 IFCPLATE)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "1002" (IFCIDENTIFIER)
  Pset_PlateCommon | properties | on 1 object (1 IFCPLATE)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "1003" (IFCIDENTIFIER)
  BaseQuantities | quantities | on 103 objects (103 IFCWALL)
    Length = 650.000743096745 [MILLI METRE]
    NetVolume = 0.535649508531252 [CUBIC_METRE]
    NetWeight = 0. [KILO GRAM]
    OuterSurfaceArea = 6.18304994262435 [SQUARE_METRE]
  BaseQuantities | quantities | on 103 objects (103 IFCWALL)
    Length = 650.001525878906 [MILLI METRE]
    NetVolume = 0.535649552479527 [CUBIC_METRE]
    NetWeight = 0. [KILO GRAM]
    OuterSurfaceArea = 6.18304506431037 [SQUARE_METRE]
  BaseQuantities | quantities | on 30 objects (30 IFCFOOTING)
    CrossSectionArea = 0.6084 [SQUARE_METRE]
    GrossSurfaceArea = 1.58808 [SQUARE_METRE]
    GrossVolume = 0.0723996 [CUBIC_METRE]
    GrossWeight = 0. [KILO GRAM]
    Height = 780. [MILLI METRE]
    Length = 119. [MILLI METRE]
    NetVolume = 0.0723996 [CUBIC_METRE]
    NetWeight = 0. [KILO GRAM]
    OuterSurfaceArea = 1.58808 [SQUARE_METRE]
    Width = 780. [MILLI METRE]
  BaseQuantities | quantities | on 24 objects (24 IFCBEAM)
    Length = 2785.05729634471 [MILLI METRE]
    NetVolume = 1.18594993869118 [CUBIC_METRE]
    NetWeight = 0. [KILO GRAM]
    OuterSurfaceArea = 11.6203352450169 [SQUARE_METRE]
  BaseQuantities | quantities | on 20 objects (20 IFCFOOTING)
    CrossSectionArea = 0.6084 [SQUARE_METRE]
    GrossSurfaceArea = 1.5912 [SQUARE_METRE]
    GrossVolume = 0.073008 [CUBIC_METRE]
    GrossWeight = 0. [KILO GRAM]
    Height = 780. [MILLI METRE]
    Length = 120. [MILLI METRE]
    NetVolume = 0.073008 [CUBIC_METRE]
    NetWeight = 0. [KILO GRAM]
    OuterSurfaceArea = 1.5912 [SQUARE_METRE]
    Width = 780. [MILLI METRE]
  BaseQuantities | quantities | on 16 objects (16 IFCBEAM)
    Length = 1681.23293155984 [MILLI METRE]
    NetVolume = 0.113139384127731 [CUBIC_METRE]
    NetWeight = 271.534521906554 [KILO GRAM]
    OuterSurfaceArea = 1.83088331626895 [SQUARE_METRE]
  BaseQuantities | quantities | on 16 objects (16 IFCBEAM)
    Length = 2784.89660529768 [MILLI METRE]
    NetVolume = 1.18594996065412 [CUBIC_METRE]
    NetWeight = 0. [KILO GRAM]
    OuterSurfaceArea = 11.620331387473 [SQUARE_METRE]
  BaseQuantities | quantities | on 15 objects (15 IFCBEAM)
    Length = 2784.84869133385 [MILLI METRE]
    NetVolume = 1.18594991667141 [CUBIC_METRE]
    NetWeight = 0. [KILO GRAM]
    OuterSurfaceArea = 11.6203297942679 [SQUARE_METRE]
  BaseQuantities: 84 more contents on 311 objects not shown
  Pset_BeamCommon | properties | on 12 objects (12 IFCBEAM)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Hormigón_S-1/74" (IFCIDENTIFIER)
  Pset_BeamCommon | properties | on 12 objects (12 IFCBEAM)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Hormigón_S-1/73" (IFCIDENTIFIER)
  Pset_BeamCommon | properties | on 12 objects (12 IFCBEAM)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Hormigón_S-1/72" (IFCIDENTIFIER)
  Pset_BeamCommon | properties | on 12 objects (12 IFCBEAM)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Hormigón_S-1/71" (IFCIDENTIFIER)
  Pset_BeamCommon | properties | on 12 objects (12 IFCBEAM)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Hormigón_S-1/70" (IFCIDENTIFIER)
  Pset_BeamCommon | properties | on 12 objects (12 IFCBEAM)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Hormigón_S-1/69" (IFCIDENTIFIER)
  Pset_BeamCommon | properties | on 12 objects (12 IFCBEAM)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Hormigón_S-1/68" (IFCIDENTIFIER)
  Pset_BeamCommon | properties | on 12 objects (12 IFCBEAM)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Hormigón_S-1/9" (IFCIDENTIFIER)
  Pset_BeamCommon: 49 more contents on 146 objects not shown
  Pset_WallCommon | properties | on 103 objects (103 IFCWALL)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Hormigón_S-1/39" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 103 objects (103 IFCWALL)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Hormigón_S-1/38" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 1 object (1 IFCWALL)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Hormigón_W-1/1" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 8 objects (8 IFCCOLUMN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "1009" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 8 objects (8 IFCCOLUMN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "1008" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 4 objects (4 IFCCOLUMN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "1007" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 4 objects (4 IFCCOLUMN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "1006" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 4 objects (4 IFCCOLUMN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "1005" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 4 objects (4 IFCCOLUMN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "1004" (IFCIDENTIFIER)