IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
Description: "Option [Drawing Scale: 100.000000]"
Description: "Option [Global Unique Identifiers (GUID): Keep existing]"
Description: "Option [Elements to export: Visible elements (on all stories)]"
Description: "Option [Partial Structure Display: Entire Model]"
Description: "Option [IFC Domain: All]"
Description: "Option [Structural Function: All Elements]"
Description: "Option [Convert Grid elements: On]"
Description: "Option [Convert IFC Annotations and ARCHICAD 2D elements: On]"
Description: "Option [Convert 2D symbols of Doors and Windows: On]"
Description: "Option [Explode Composite and Complex Profile elements into parts: Off]"
Description: "Option [Export geometries that Participates in Collision Detection only: On]"
Description: "Option [Multi-skin complex geometries: Building element parts]"
Description: "Option [Elements in Solid Element Operations: Extruded/revolved]"
Description: "Option [Elements with junctions: Extruded/revolved without junctions]"
Description: "Option [Slabs with slanted edge(s): Extruded]"
File name: "C:\Users\luca\Desktop\IFC.ifc"
Time stamp: "2020-08-27T15:03:39"
Author: "Architect"
Organization: "Building Designer Office"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.09 : 26 Sep 2013"
Originating system: "IFC file generated by GRAPHISOFT ARCHICAD-64 20.0.0 AUS FULL Windows version (IFC add-on version: 8005 AUS FULL)."
Authorization: "The authorising person"
Application: "ARCHICAD-64" version "20.0.0" identifier "IFC add-on version: 8005 AUS FULL" by Organization "GRAPHISOFT" id "GS" description "GRAPHISOFT"

People and organizations
  Person "Undefined" of Organization "Undefined"
  Owner history of Person "Undefined" of Organization "Undefined" | application "ARCHICAD-64" version "20.0.0" identifier "IFC add-on version: 8005 AUS FULL" by Organization "GRAPHISOFT" id "GS" description "GRAPHISOFT" | change ADDED | created 1598511818 (2020-08-27T07:03:38Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  SOLIDANGLEUNIT: STERADIAN
  CURRENCY: AUD
  TIMEUNIT: SECOND
  MASSUNIT: GRAM
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  LUMINOUSINTENSITYUNIT: LUMEN

Spatial structure
IFCPROJECT "Project"
  IFCSITE "Site" | latitude -31° 57′ 0″ | longitude 115° 52′ 0″ | elevation above sea level 0.
    IFCBUILDING "Building"
      IFCBUILDINGSTOREY "SUBFLOOR" | elevation -172.
        contains 15 elements
          3 x IFCSLAB | type IFCSLABTYPE "Paving | 60mm 60" | FLOOR | names: "Slab006" | material: layers "Paving | 60mm" ("Brick Paving" 60.) | property sets: AC_Pset_RenovationAndPhasing, Pset_SlabCommon
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Wall | s090 | Rndr 1 90" | names: "Wall179", "Wall178", "Wall181" (+1 more) | material: layers "Wall | s090 | Rndr 1" ("Wall - Render - Colour 1" 90.) | property sets: AC_Pset_RenovationAndPhasing, Pset_WallCommon
          5 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Wall | s090 | Face 90" | names: "Wall162", "Wall163", "Wall165" (+2 more) | material: layers "Wall | s090 | Face" ("Wall - 2c Face Brick" 90.) | property sets: AC_Pset_RenovationAndPhasing, Pset_WallCommon
          1 x IFCSLAB | type IFCSLABTYPE "Slab | Concrete | 85mm 86" | FLOOR | names: "Slab017" | material: layers "Slab | Concrete | 85mm" ("Concrete - Grano" 86.) | property sets: AC_Pset_RenovationAndPhasing, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Slab | Grano | 85mm 86" | FLOOR | names: "Slab016" | material: layers "Slab | Grano | 85mm" ("Concrete - Grano" 86.) | property sets: AC_Pset_RenovationAndPhasing, Pset_SlabCommon
          1 x IFCBEAM | type IFCBEAMTYPE "Cabinetwork - Laminate 90 x 90" | object type "Cabinetwork - Laminate 90 x 90" | names: "Beam0037" | material: "Cabinetwork - Laminate" | property sets: AC_Pset_RenovationAndPhasing, Pset_BeamCommon
      IFCBUILDINGSTOREY "F.F.L." | elevation 0.
        contains 123 elements
          7 x IFCCOLUMN | type IFCCOLUMNTYPE "Wall - 2c Face Brick 290 x 100" | object type "Wall - 2c Face Brick 290 x 100" | names: "Col-001" | material: "Wall - 2c Face Brick" | property sets: AC_Pset_RenovationAndPhasing, Pset_ColumnCommon
          10 x IFCFURNISHINGELEMENT | type IFCFURNISHINGELEMENTTYPE "Robe & Linen shelves 4D" | names: "R002", "R010", "R011" | material: "Solid" | property sets: AC_Pset_RenovationAndPhasing
          32 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Wall | s090 | F&S 90" | names: "Wall242", "Wall257", "Wall245" (+27 more) | material: layers "Wall | s090 | F&S" ("Wall - Internal Float & Set" 90.) | property sets: AC_Pset_RenovationAndPhasing, Pset_WallCommon
          1 x IFCFURNISHINGELEMENT | type IFCFURNISHINGELEMENTTYPE "Vents 3de" | names: "W051" | material: "Solid" | property sets: AC_Pset_RenovationAndPhasing
          1 x IFCFURNISHINGELEMENT | type IFCFURNISHINGELEMENTTYPE "Laundry tub 4D" | names: "W050" | material: "Solid" | property sets: AC_Pset_RenovationAndPhasing
          2 x IFCFURNISHINGELEMENT | type IFCFURNISHINGELEMENTTYPE "Towel Rail 4D" | names: "W046", "R007" | material: "Solid" | property sets: AC_Pset_RenovationAndPhasing
          1 x IFCFURNISHINGELEMENT | type IFCFURNISHINGELEMENTTYPE "Baths 4D" | names: "R015" | material: "Solid" | property sets: AC_Pset_RenovationAndPhasing
          3 x IFCFURNISHINGELEMENT | type IFCFURNISHINGELEMENTTYPE "Cupboard 4D" | names: "W045" | material: "Solid" | property sets: AC_Pset_RenovationAndPhasing
          2 x IFCFURNISHINGELEMENT | type IFCFURNISHINGELEMENTTYPE "Vanity Cupboard 4D" | names: "W045", "R005" | material: "Solid" | property sets: AC_Pset_RenovationAndPhasing
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Wall | s090 | F&S/Face 90" | names: "Wall231", "Wall230" | material: layers "Wall | s090 | F&S/Face" ("Wall - 2c Face Brick" 45., "Wall - Internal Float & Set" 45.) | property sets: AC_Pset_RenovationAndPhasing, Pset_WallCommon
          14 x IFCDOOR | type IFCDOORSTYLE "Internal Swing door 4D" | names: "D52", "D43", "D50" (+9 more) | material: materials ("face brick") | property sets: AC_Pset_RenovationAndPhasing, Pset_DoorCommon
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Wall | s090 | Face 90" | names: "Wall212", "Wall213" | material: layers "Wall | s090 | Face" ("Wall - 2c Face Brick" 90.) | property sets: AC_Pset_RenovationAndPhasing, Pset_WallCommon
          2 x IFCFURNISHINGELEMENT | type IFCFURNISHINGELEMENTTYPE "Benchtop | Laminate 33mm 33" | names: "Slab014" | material: "Cabinetwork - Laminate" | property sets: AC_Pset_RenovationAndPhasing
          1 x IFCFURNISHINGELEMENT | type IFCFURNISHINGELEMENTTYPE "drawers 4D" | names: "W044" | material: "Solid" | property sets: AC_Pset_RenovationAndPhasing
          2 x IFCFURNISHINGELEMENT | type IFCFURNISHINGELEMENTTYPE "Toilet 4D" | names: "R006", "R012" | material: "Solid" | property sets: AC_Pset_RenovationAndPhasing
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Wall | c230 | F&S/Rndr 1 230" | names: "Wall240", "Wall237", "Wall238" (+1 more) | material: layers "Wall | c230 | F&S/Rndr 1" ("Wall - Render - Colour 1" 90., "Air Space" 50., "Wall - Internal Float & Set" 90.) | property sets: AC_Pset_RenovationAndPhasing, Pset_WallCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Meterbox VHG" | names: "W053" | material: "Roof Colorbond" | property sets: AC_Pset_RenovationAndPhasing
          5 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Wall | c230 | F&S/Face 230" | names: "Wall230", "Wall228", "Wall232" (+2 more) | material: layers "Wall | c230 | F&S/Face" ("Wall - 2c Face Brick" 90., "Air Space" 50., "Wall - Internal Float & Set" 90.) | property sets: AC_Pset_RenovationAndPhasing, Pset_WallCommon
          1 x IFCFURNISHINGELEMENT | type IFCFURNISHINGELEMENTTYPE "Dishwasher recess 4D" | names: "W054" | material: "Roof Colorbond" | property sets: AC_Pset_RenovationAndPhasing
          2 x IFCFURNISHINGELEMENT | type IFCFURNISHINGELEMENTTYPE "Toilet Roll Holder" | names: "R013", "R008" | material: "Solid" | property sets: AC_Pset_RenovationAndPhasing
          1 x IFCFURNISHINGELEMENT | type IFCFURNISHINGELEMENTTYPE "Underbench oven 4D" | names: "W043" | material: "Solid" | property sets: AC_Pset_RenovationAndPhasing
          1 x IFCDOOR | type IFCDOORSTYLE "External Multi door 4D" | names: "D40" | material: materials ("Empty", "Empty") | property sets: AC_Pset_RenovationAndPhasing, Pset_DoorCommon
          1 x IFCFURNISHINGELEMENT | type IFCFURNISHINGELEMENTTYPE "Hotplate 4D" | names: "W047" | material: "Solid" | property sets: AC_Pset_RenovationAndPhasing
          1 x IFCFURNISHINGELEMENT | type IFCFURNISHINGELEMENTTYPE "Rangehood Canopy VHG" | names: "W041" | material: "Empty" | property sets: AC_Pset_RenovationAndPhasing
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Post 90 x 90" | object type "Post 90 x 90" | names: "Col-001" | material: "Post" | property sets: AC_Pset_RenovationAndPhasing, Pset_ColumnCommon
          11 x IFCWINDOW | type IFCWINDOWSTYLE "Multi Window 4D" | names: "W-58", "W-57", "W-56" (+8 more) | material: materials ("Empty", "wood", "wood", "Empty") | property sets: AC_Pset_RenovationAndPhasing, Pset_WindowCommon
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Wall | s090 | Face/Rndr 1 90" | names: "Wall211", "Wall210" | material: layers "Wall | s090 | Face/Rndr 1" ("Wall - Render - Colour 1" 45., "Wall - 2c Face Brick" 45.) | property sets: AC_Pset_RenovationAndPhasing, Pset_WallCommon
          1 x IFCFURNISHINGELEMENT | type IFCFURNISHINGELEMENTTYPE "Manhole 4D" | names: "R022" | material: "Solid" | property sets: AC_Pset_RenovationAndPhasing
          1 x IFCFURNISHINGELEMENT | type IFCFURNISHINGELEMENTTYPE "HWU 3de" | names: "R024" | material: "Solid Fill" | property sets: AC_Pset_RenovationAndPhasing
          2 x IFCFURNISHINGELEMENT | type IFCFURNISHINGELEMENTTYPE "Multi Shower 4D" | names: "W044", "R004" | material: "Solid" | property sets: AC_Pset_RenovationAndPhasing
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Wall - 2c Face Brick 300 x 100" | object type "Wall - 2c Face Brick 300 x 100" | names: "Col-001" | material: "Wall - 2c Face Brick" | property sets: AC_Pset_RenovationAndPhasing, Pset_ColumnCommon
          2 x IFCWINDOW | type IFCWINDOWSTYLE "Sliding door 4D" | names: "W-61", "W-59" | material: materials ("Empty", "wood", "wood", "Empty") | property sets: AC_Pset_RenovationAndPhasing, Pset_WindowCommon
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Wall | s190 | Face/Rndr 1 190" | names: "Wall208" | material: layers "Wall | s190 | Face/Rndr 1" ("Wall - Render - Colour 1" 95., "Wall - 2c Face Brick" 95.) | property sets: AC_Pset_RenovationAndPhasing, Pset_WallCommon
          1 x IFCDOOR | type IFCDOORSTYLE "Garage door 4D" | names: "D39" | property sets: AC_Pset_RenovationAndPhasing, Pset_DoorCommon
          1 x IFCFURNISHINGELEMENT | type IFCFURNISHINGELEMENTTYPE "kitchen sink 4D" | names: "W037" | material: "Solid" | property sets: AC_Pset_RenovationAndPhasing
      IFCBUILDINGSTOREY "CEILING" | elevation 2435.
        contains 65 elements
          15 x IFCFURNISHINGELEMENT | type IFCFURNISHINGELEMENTTYPE "Cornice 4D" | names: "S001" | material: "Empty Fill" | property sets: AC_Pset_RenovationAndPhasing
          20 x IFCSLAB | type IFCSLABTYPE "Ceiling | Lining 10" | FLOOR | names: "Slab067", "Slab061", "Slab065" (+17 more) | material: layers "Ceiling | Lining" ("Ceiling - Plasterboard" 10.) | property sets: AC_Pset_RenovationAndPhasing, Pset_SlabCommon
          8 x IFCWALL | type IFCWALLTYPE "INT | 90s | F&S/Rough | Plate 230 x 292" | names: "Wall217", "Wall212", "Wall214" (+5 more) | parts: 72 IFCBUILDINGELEMENTPART | property sets: AC_Pset_RenovationAndPhasing, Pset_WallCommon
          6 x IFCSLAB | type IFCSLABTYPE "Roof | Tiled 178" | ROOF | names: "Roof0009" | material: layers "Roof | Tiled" ("Roof Cover - Tiled" 20., "Air Space" 38., "Roof - Timber" 120.) | property sets: AC_Pset_RenovationAndPhasing, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Eave Lining 76" | FLOOR | names: "Slab010" | material: layers "Eave Lining" ("Roof - Timber" 70., "Ceiling - Fibre Cement Sheet" 6.) | property sets: AC_Pset_RenovationAndPhasing, Pset_SlabCommon
          1 x IFCBEAM | type IFCBEAMTYPE "BEAM | UB | 250 UB 26 124 x 248" | object type "BEAM | UB | 250 UB 26 124 x 248" | names: "Beam0041" | material: "Steel - Structural" | property sets: AC_Pset_RenovationAndPhasing, Pset_BeamCommon
          2 x IFCBEAM | type IFCBEAMTYPE "BEAM | LVL | 300X63 LVL 63 x 300" | object type "BEAM | LVL | 300X63 LVL 63 x 300" | names: "Beam0042", "Beam0043" | material: "Drop Beam" | property sets: AC_Pset_RenovationAndPhasing, Pset_BeamCommon
          4 x IFCSLAB | type IFCSLABTYPE "Ceiling | Joists 90" | FLOOR | names: "Slab008", "Slab009", "Slab010" | material: layers "Ceiling | Joists" ("Roof - Timber" 90.) | property sets: AC_Pset_RenovationAndPhasing, Pset_SlabCommon
          1 x IFCBEAM | type IFCBEAMTYPE "BEAM | LVL | 200X63 LVL 63 x 200" | object type "BEAM | LVL | 200X63 LVL 63 x 200" | names: "Beam0042" | material: "Drop Beam" | property sets: AC_Pset_RenovationAndPhasing, Pset_BeamCommon
          6 x IFCFURNISHINGELEMENT | type IFCFURNISHINGELEMENTTYPE "4D Roofing" | names: "R001" | material: "Empty Fill" | property sets: AC_Pset_RenovationAndPhasing
          1 x IFCBEAM | type IFCBEAMTYPE "B'HEAD | Framed 650 x 292" | object type "B'HEAD | Framed 650 x 292" | names: "Beam0043" | parts: 8 IFCBUILDINGELEMENTPART | property sets: AC_Pset_RenovationAndPhasing, Pset_BeamCommon

Types
  IFCSLABTYPE "Paving | 60mm 60" | FLOOR | 3 occurrences
  IFCWALLTYPE "Wall | s090 | Rndr 1 90" | 4 occurrences
  IFCWALLTYPE "Wall | s090 | Face 90" | 7 occurrences
  IFCSLABTYPE "Slab | Concrete | 85mm 86" | FLOOR | 1 occurrence
  IFCSLABTYPE "Slab | Grano | 85mm 86" | FLOOR | 1 occurrence
  IFCBEAMTYPE "Cabinetwork - Laminate 90 x 90" | 1 occurrence
  IFCCOLUMNTYPE "Wall - 2c Face Brick 290 x 100" | 7 occurrences
  IFCFURNISHINGELEMENTTYPE "Robe & Linen shelves 4D" | 10 occurrences
  IFCWALLTYPE "Wall | s090 | F&S 90" | 32 occurrences
  IFCFURNISHINGELEMENTTYPE "Vents 3de" | 1 occurrence
  IFCFURNISHINGELEMENTTYPE "Laundry tub 4D" | 1 occurrence
  IFCFURNISHINGELEMENTTYPE "Towel Rail 4D" | 2 occurrences
  IFCFURNISHINGELEMENTTYPE "Baths 4D" | 1 occurrence
  IFCFURNISHINGELEMENTTYPE "Cupboard 4D" | 3 occurrences
  IFCFURNISHINGELEMENTTYPE "Vanity Cupboard 4D" | 2 occurrences
  IFCWALLTYPE "Wall | s090 | F&S/Face 90" | 2 occurrences
  IFCDOORSTYLE "Internal Swing door 4D" | 14 occurrences
  IFCFURNISHINGELEMENTTYPE "Benchtop | Laminate 33mm 33" | 2 occurrences
  IFCFURNISHINGELEMENTTYPE "drawers 4D" | 1 occurrence
  IFCFURNISHINGELEMENTTYPE "Toilet 4D" | 2 occurrences
  IFCWALLTYPE "Wall | c230 | F&S/Rndr 1 230" | 4 occurrences
  IFCBUILDINGELEMENTPROXYTYPE "Meterbox VHG" | 1 occurrence
  IFCWALLTYPE "Wall | c230 | F&S/Face 230" | 5 occurrences
  IFCFURNISHINGELEMENTTYPE "Dishwasher recess 4D" | 1 occurrence
  IFCFURNISHINGELEMENTTYPE "Toilet Roll Holder" | 2 occurrences
  IFCFURNISHINGELEMENTTYPE "Underbench oven 4D" | 1 occurrence
  IFCDOORSTYLE "External Multi door 4D" | 1 occurrence
  IFCFURNISHINGELEMENTTYPE "Hotplate 4D" | 1 occurrence
  IFCFURNISHINGELEMENTTYPE "Rangehood Canopy VHG" | 1 occurrence
  IFCCOLUMNTYPE "Post 90 x 90" | 1 occurrence
  IFCWINDOWSTYLE "Multi Window 4D" | 11 occurrences
  IFCWALLTYPE "Wall | s090 | Face/Rndr 1 90" | 2 occurrences
  IFCFURNISHINGELEMENTTYPE "Manhole 4D" | 1 occurrence
  IFCFURNISHINGELEMENTTYPE "HWU 3de" | 1 occurrence
  IFCFURNISHINGELEMENTTYPE "Multi Shower 4D" | 2 occurrences
  IFCCOLUMNTYPE "Wall - 2c Face Brick 300 x 100" | 1 occurrence
  IFCWINDOWSTYLE "Sliding door 4D" | 2 occurrences
  IFCWALLTYPE "Wall | s190 | Face/Rndr 1 190" | 1 occurrence
  IFCDOORSTYLE "Garage door 4D" | 1 occurrence
  IFCFURNISHINGELEMENTTYPE "kitchen sink 4D" | 1 occurrence
  IFCFURNISHINGELEMENTTYPE "Cornice 4D" | 15 occurrences
  IFCSLABTYPE "Ceiling | Lining 10" | FLOOR | 20 occurrences
  IFCWALLTYPE "INT | 90s | F&S/Rough | Plate 230 x 292" | 8 occurrences
  IFCSLABTYPE "Roof | Tiled 178" | ROOF | 6 occurrences
  IFCSLABTYPE "Eave Lining 76" | FLOOR | 1 occurrence
  IFCBEAMTYPE "BEAM | UB | 250 UB 26 124 x 248" | 1 occurrence
  IFCBEAMTYPE "BEAM | LVL | 300X63 LVL 63 x 300" | 2 occurrences
  IFCSLABTYPE "Ceiling | Joists 90" | FLOOR | 4 occurrences
  IFCBEAMTYPE "BEAM | LVL | 200X63 LVL 63 x 200" | 1 occurrence
  IFCFURNISHINGELEMENTTYPE "4D Roofing" | 6 occurrences
  IFCBEAMTYPE "B'HEAD | Framed 650 x 292" | 1 occurrence

Property sets
  AC_Pset_RenovationAndPhasing | properties | on 203 objects (57 IFCFURNISHINGELEMENT, 57 IFCWALLSTANDARDCASE, 36 IFCSLAB, 16 IFCDOOR)
    Renovation Status = "Existing" (IFCLABEL)
  Pset_SlabCommon | properties | on 23 objects (23 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
  Pset_SlabCommon | properties | on 9 objects (9 IFCSLAB)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
  Pset_SlabCommon | properties | on 4 objects (4 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
  Pset_WallCommon | properties | on 34 objects (34 IFCWALLSTANDARDCASE)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
  Pset_WallCommon | properties | on 31 objects (23 IFCWALLSTANDARDCASE, 8 IFCWALL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
  Pset_BeamCommon | properties | on 2 objects (2 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "BEAM | LVL | 300X63 LVL 63 x 300" (IFCIDENTIFIER)
  Pset_BeamCommon | properties | on 1 object (1 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Cabinetwork - Laminate 90 x 90" (IFCIDENTIFIER)
  Pset_BeamCommon | properties | on 1 object (1 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "BEAM | UB | 250 UB 26 124 x 248" (IFCIDENTIFIER)
  Pset_BeamCommon | properties | on 1 object (1 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "BEAM | LVL | 200X63 LVL 63 x 200" (IFCIDENTIFIER)
  Pset_BeamCommon | properties | on 1 object (1 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "B'HEAD | Framed 650 x 292" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 7 objects (7 IFCCOLUMN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Wall - 2c Face Brick 290 x 100" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 1 object (1 IFCCOLUMN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Post 90 x 90" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 1 object (1 IFCCOLUMN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Wall - 2c Face Brick 300 x 100" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 14 objects (14 IFCDOOR)
    IsExternal = FALSE (IFCBOOLEAN)
  Pset_DoorCommon | properties | on 2 objects (2 IFCDOOR)
    IsExternal = TRUE (IFCBOOLEAN)
  Pset_WindowCommon | properties | on 13 objects (13 IFCWINDOW)
    IsExternal = TRUE (IFCBOOLEAN)