IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "Project Number"
Time stamp: "2021-02-01T19:40:18"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "21.0.0.383 - Exporter 21.0.0.383 - IU alternativa 21.0.0.383"
Application: "Autodesk Revit 2021 (ENU)" version "2021" identifier "Revit" by Organization "Autodesk Revit 2021 (ENU)"

People and organizations
  Person "CYPE" of Organization (no name given)
  Owner history of Person "CYPE" of Organization (no name given) | application "Autodesk Revit 2021 (ENU)" version "2021" identifier "Revit" by Organization "Autodesk Revit 2021 (ENU)" | change NOCHANGE | created 1610653983 (2021-01-14T19:53:03Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived

Spatial structure
IFCPROJECT "Project Number" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 48° 7′ 58.799999″ | longitude 11° 34′ 58.799999″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "Munich", "Germany"
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Nivel:8mm Head" | elevation 94.1717368783468
        contains 1214 elements
          4 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "M_Supply Diffuser - Sidewall:450 x 200" | object type "M_Supply Diffuser - Sidewall:450 x 200" | names: "M_Supply Diffuser - Sidewall:450 x 200:383543", "M_Supply Diffuser - Sidewall:450 x 200:386464", "M_Supply Diffuser - Sidewall:450 x 200:396193" (+1 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:14 kW" | object type "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:14 kW" | names: "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:14 kW:386031" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          5 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "M_Supply Diffuser - Sidewall:450 x 200" | object type "M_Supply Diffuser - Sidewall:450 x 200" | names: "M_Supply Diffuser - Sidewall:450 x 200:386293", "M_Supply Diffuser - Sidewall:450 x 200:386336", "M_Supply Diffuser - Sidewall:450 x 200:386552" (+2 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "M_Supply Diffuser - Sidewall:450 x 200" | object type "M_Supply Diffuser - Sidewall:450 x 200" | names: "M_Supply Diffuser - Sidewall:450 x 200:386707" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          255 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "Conducto rectangular:Mitered Elbows / Taps" | object type "Conducto rectangular:Mitered Elbows / Taps" | names: "Conducto rectangular:Mitered Elbows / Taps:392168", "Conducto rectangular:Mitered Elbows / Taps:392170", "Conducto rectangular:Mitered Elbows / Taps:392174" (+252 more) | property sets: Pset_DistributionFlowElementCommon, Pset_DuctSegmentTypeCommon, Pset_FlowSegmentDuctSegment, Pset_FlowSegmentPipeSegment, Pset_QuantityTakeOff
          6 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Elbow - Mitered:Standard" | object type "M_Rectangular Duct Elbow - Mitered:Standard" | names: "M_Rectangular Duct Elbow - Mitered:Standard:392203", "M_Rectangular Duct Elbow - Mitered:Standard:393779", "M_Rectangular Duct Elbow - Mitered:Standard:399432" (+3 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          38 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Takeoff:Standard" | object type "M_Rectangular Duct Takeoff:Standard" | names: "M_Rectangular Duct Takeoff:Standard:392234", "M_Rectangular Duct Takeoff:Standard:392628", "M_Rectangular Duct Takeoff:Standard:393777" (+35 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          6 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Endcap:Standard" | object type "M_Rectangular Duct Endcap:Standard" | names: "M_Rectangular Duct Endcap:Standard:392633", "M_Rectangular Duct Endcap:Standard:393378", "M_Rectangular Duct Endcap:Standard:401776" (+3 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Endcap:Standard" | object type "M_Rectangular Duct Endcap:Standard" | names: "M_Rectangular Duct Endcap:Standard:392961" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          3 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Takeoff:Standard" | object type "M_Rectangular Duct Takeoff:Standard" | names: "M_Rectangular Duct Takeoff:Standard:393174", "M_Rectangular Duct Takeoff:Standard:395684", "M_Rectangular Duct Takeoff:Standard:971582" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:393414" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:393568" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Elbow - Mitered:Standard" | object type "M_Rectangular Duct Elbow - Mitered:Standard" | names: "M_Rectangular Duct Elbow - Mitered:Standard:393577", "M_Rectangular Duct Elbow - Mitered:Standard:805267" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:393607" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          4 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Endcap:Standard" | object type "M_Rectangular Duct Endcap:Standard" | names: "M_Rectangular Duct Endcap:Standard:393645", "M_Rectangular Duct Endcap:Standard:395938", "M_Rectangular Duct Endcap:Standard:395946" (+1 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:393674" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          7 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Endcap:Standard" | object type "M_Rectangular Duct Endcap:Standard" | names: "M_Rectangular Duct Endcap:Standard:393702", "M_Rectangular Duct Endcap:Standard:401446", "M_Rectangular Duct Endcap:Standard:401454" (+4 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          32 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Takeoff:Standard" | object type "M_Rectangular Duct Takeoff:Standard" | names: "M_Rectangular Duct Takeoff:Standard:393747", "M_Rectangular Duct Takeoff:Standard:393916", "M_Rectangular Duct Takeoff:Standard:393947" (+29 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          11 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "M_Supply Diffuser - Sidewall:450 x 200" | object type "M_Supply Diffuser - Sidewall:450 x 200" | names: "M_Supply Diffuser - Sidewall:450 x 200:393958", "M_Supply Diffuser - Sidewall:450 x 200:393959", "M_Supply Diffuser - Sidewall:450 x 200:393983" (+8 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          8 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "M_Supply Diffuser - Sidewall:450 x 200" | object type "M_Supply Diffuser - Sidewall:450 x 200" | names: "M_Supply Diffuser - Sidewall:450 x 200:393972", "M_Supply Diffuser - Sidewall:450 x 200:401772", "M_Supply Diffuser - Sidewall:450 x 200:401773" (+5 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:14 kW" | object type "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:14 kW" | names: "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:14 kW:394114" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Takeoff:Standard" | object type "M_Rectangular Duct Takeoff:Standard" | names: "M_Rectangular Duct Takeoff:Standard:395719", "M_Rectangular Duct Takeoff:Standard:805256" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Endcap:Standard" | object type "M_Rectangular Duct Endcap:Standard" | names: "M_Rectangular Duct Endcap:Standard:395764" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:395778", "M_Rectangular Duct Transition - Angle:45 Degree:401648" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Elbow - Mitered:Standard" | object type "M_Rectangular Duct Elbow - Mitered:Standard" | names: "M_Rectangular Duct Elbow - Mitered:Standard:395795", "M_Rectangular Duct Elbow - Mitered:Standard:395836" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:395796" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          3 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:395961", "M_Rectangular Duct Transition - Angle:45 Degree:395962", "M_Rectangular Duct Transition - Angle:45 Degree:412733" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:395963", "M_Rectangular Duct Transition - Angle:45 Degree:805268" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Back Discharge:7 kW" | object type "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Back Discharge:7 kW" | names: "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Back Discharge:7 kW:395978" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          3 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "M_Supply Diffuser - Sidewall:450 x 200" | object type "M_Supply Diffuser - Sidewall:450 x 200" | names: "M_Supply Diffuser - Sidewall:450 x 200:396293", "M_Supply Diffuser - Sidewall:450 x 200:412940", "M_Supply Diffuser - Sidewall:450 x 200:413125" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          8 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "M_Supply Diffuser - Sidewall:450 x 200" | object type "M_Supply Diffuser - Sidewall:450 x 200" | names: "M_Supply Diffuser - Sidewall:450 x 200:399597", "M_Supply Diffuser - Sidewall:450 x 200:399643", "M_Supply Diffuser - Sidewall:450 x 200:403378" (+5 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          11 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "M_Supply Diffuser - Sidewall:450 x 200" | object type "M_Supply Diffuser - Sidewall:450 x 200" | names: "M_Supply Diffuser - Sidewall:450 x 200:399662", "M_Supply Diffuser - Sidewall:450 x 200:399663", "M_Supply Diffuser - Sidewall:450 x 200:399690" (+8 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:14 kW" | object type "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:14 kW" | names: "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:14 kW:399752" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Takeoff:Standard" | object type "M_Rectangular Duct Takeoff:Standard" | names: "M_Rectangular Duct Takeoff:Standard:401412", "M_Rectangular Duct Takeoff:Standard:404371" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Elbow - Mitered:Standard" | object type "M_Rectangular Duct Elbow - Mitered:Standard" | names: "M_Rectangular Duct Elbow - Mitered:Standard:401424", "M_Rectangular Duct Elbow - Mitered:Standard:404373" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:401700" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:11 kW" | object type "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:11 kW" | names: "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:11 kW:401918", "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:11 kW:403750" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:402637" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Elbow - Mitered:Standard" | object type "M_Rectangular Duct Elbow - Mitered:Standard" | names: "M_Rectangular Duct Elbow - Mitered:Standard:402646", "M_Rectangular Duct Elbow - Mitered:Standard:402886" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:402887" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "M_Supply Diffuser - Sidewall:450 x 200" | object type "M_Supply Diffuser - Sidewall:450 x 200" | names: "M_Supply Diffuser - Sidewall:450 x 200:402932", "M_Supply Diffuser - Sidewall:450 x 200:402933" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:7 kW" | object type "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:7 kW" | names: "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:7 kW:402967" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:403118" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:403180" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Elbow - Mitered:Standard" | object type "M_Rectangular Duct Elbow - Mitered:Standard" | names: "M_Rectangular Duct Elbow - Mitered:Standard:403291", "M_Rectangular Duct Elbow - Mitered:Standard:403301" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:403299" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:403393" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:11 kW" | object type "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:11 kW" | names: "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:11 kW:403487" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          3 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:403749", "M_Rectangular Duct Transition - Angle:45 Degree:404487", "M_Rectangular Duct Transition - Angle:45 Degree:710237" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          3 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:403909", "M_Rectangular Duct Transition - Angle:45 Degree:403921", "M_Rectangular Duct Transition - Angle:45 Degree:404216" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "M_Supply Diffuser - Sidewall:450 x 200" | object type "M_Supply Diffuser - Sidewall:450 x 200" | names: "M_Supply Diffuser - Sidewall:450 x 200:404203" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:11 kW" | object type "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:11 kW" | names: "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:11 kW:404215", "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:11 kW:404284" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:404488" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:7 kW" | object type "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:7 kW" | names: "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:7 kW:404570" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:405051" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          5 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "M_Return Grille - Rectangular - Hosted:Standard" | object type "M_Return Grille - Rectangular - Hosted:Standard" | names: "M_Return Grille - Rectangular - Hosted:Standard:408521", "M_Return Grille - Rectangular - Hosted:Standard:408625", "M_Return Grille - Rectangular - Hosted:Standard:408652" (+2 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          3 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Endcap:Standard" | object type "M_Rectangular Duct Endcap:Standard" | names: "M_Rectangular Duct Endcap:Standard:408713", "M_Rectangular Duct Endcap:Standard:410819", "M_Rectangular Duct Endcap:Standard:411974" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          6 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Takeoff:Standard" | object type "M_Rectangular Duct Takeoff:Standard" | names: "M_Rectangular Duct Takeoff:Standard:408801", "M_Rectangular Duct Takeoff:Standard:410953", "M_Rectangular Duct Takeoff:Standard:411494" (+3 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:409027" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          7 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Elbow - Mitered:Standard" | object type "M_Rectangular Duct Elbow - Mitered:Standard" | names: "M_Rectangular Duct Elbow - Mitered:Standard:409029", "M_Rectangular Duct Elbow - Mitered:Standard:410812", "M_Rectangular Duct Elbow - Mitered:Standard:411002" (+4 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          5 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Takeoff:Standard" | object type "M_Rectangular Duct Takeoff:Standard" | names: "M_Rectangular Duct Takeoff:Standard:409045", "M_Rectangular Duct Takeoff:Standard:409060", "M_Rectangular Duct Takeoff:Standard:410442" (+2 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          3 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "M_Return Grille - Rectangular - Hosted:Standard" | object type "M_Return Grille - Rectangular - Hosted:Standard" | names: "M_Return Grille - Rectangular - Hosted:Standard:409174", "M_Return Grille - Rectangular - Hosted:Standard:410535", "M_Return Grille - Rectangular - Hosted:Standard:412008" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          3 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Endcap:Standard" | object type "M_Rectangular Duct Endcap:Standard" | names: "M_Rectangular Duct Endcap:Standard:410471", "M_Rectangular Duct Endcap:Standard:411277", "M_Rectangular Duct Endcap:Standard:414225" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "M_Return Grille - Rectangular - Hosted:Standard" | object type "M_Return Grille - Rectangular - Hosted:Standard" | names: "M_Return Grille - Rectangular - Hosted:Standard:410510", "M_Return Grille - Rectangular - Hosted:Standard:412006" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:410810", "M_Rectangular Duct Transition - Angle:45 Degree:412557" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:411001" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          3 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Takeoff:Standard" | object type "M_Rectangular Duct Takeoff:Standard" | names: "M_Rectangular Duct Takeoff:Standard:411083", "M_Rectangular Duct Takeoff:Standard:411873", "M_Rectangular Duct Takeoff:Standard:411898" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          6 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Elbow - Mitered:Standard" | object type "M_Rectangular Duct Elbow - Mitered:Standard" | names: "M_Rectangular Duct Elbow - Mitered:Standard:411090", "M_Rectangular Duct Elbow - Mitered:Standard:411100", "M_Rectangular Duct Elbow - Mitered:Standard:411575" (+3 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "M_Return Grille - Rectangular - Hosted:Standard" | object type "M_Return Grille - Rectangular - Hosted:Standard" | names: "M_Return Grille - Rectangular - Hosted:Standard:411147", "M_Return Grille - Rectangular - Hosted:Standard:412802" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:411207" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          7 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Endcap:Standard" | object type "M_Rectangular Duct Endcap:Standard" | names: "M_Rectangular Duct Endcap:Standard:411268", "M_Rectangular Duct Endcap:Standard:411580", "M_Rectangular Duct Endcap:Standard:411609" (+4 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          5 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "M_Return Grille - Rectangular - Hosted:Standard" | object type "M_Return Grille - Rectangular - Hosted:Standard" | names: "M_Return Grille - Rectangular - Hosted:Standard:411303", "M_Return Grille - Rectangular - Hosted:Standard:411451", "M_Return Grille - Rectangular - Hosted:Standard:411617" (+2 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          3 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Takeoff:Standard" | object type "M_Rectangular Duct Takeoff:Standard" | names: "M_Rectangular Duct Takeoff:Standard:411550", "M_Rectangular Duct Takeoff:Standard:411604", "M_Rectangular Duct Takeoff:Standard:411623" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:411574", "M_Rectangular Duct Transition - Angle:45 Degree:411607" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          4 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "M_Return Grille - Rectangular - Hosted:Standard" | object type "M_Return Grille - Rectangular - Hosted:Standard" | names: "M_Return Grille - Rectangular - Hosted:Standard:411597", "M_Return Grille - Rectangular - Hosted:Standard:411600", "M_Return Grille - Rectangular - Hosted:Standard:411656" (+1 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:411851" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          10 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "M_Return Grille - Rectangular - Hosted:Standard" | object type "M_Return Grille - Rectangular - Hosted:Standard" | names: "M_Return Grille - Rectangular - Hosted:Standard:412078", "M_Return Grille - Rectangular - Hosted:Standard:412118", "M_Return Grille - Rectangular - Hosted:Standard:412141" (+7 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          4 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "M_Supply Diffuser - Sidewall:450 x 200" | object type "M_Supply Diffuser - Sidewall:450 x 200" | names: "M_Supply Diffuser - Sidewall:450 x 200:412613", "M_Supply Diffuser - Sidewall:450 x 200:412614", "M_Supply Diffuser - Sidewall:450 x 200:412707" (+1 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Takeoff:Standard" | object type "M_Rectangular Duct Takeoff:Standard" | names: "M_Rectangular Duct Takeoff:Standard:412728" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Takeoff:Standard" | object type "M_Rectangular Duct Takeoff:Standard" | names: "M_Rectangular Duct Takeoff:Standard:412835", "M_Rectangular Duct Takeoff:Standard:414007" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "M_Supply Diffuser - Sidewall:450 x 200" | object type "M_Supply Diffuser - Sidewall:450 x 200" | names: "M_Supply Diffuser - Sidewall:450 x 200:412912", "M_Supply Diffuser - Sidewall:450 x 200:413124" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "M_Supply Diffuser - Sidewall:450 x 200" | object type "M_Supply Diffuser - Sidewall:450 x 200" | names: "M_Supply Diffuser - Sidewall:450 x 200:413134", "M_Supply Diffuser - Sidewall:450 x 200:413135" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:11 kW" | object type "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:11 kW" | names: "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:11 kW:413239" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:413535" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:413536" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "M_Return Grille - Rectangular - Hosted:Standard" | object type "M_Return Grille - Rectangular - Hosted:Standard" | names: "M_Return Grille - Rectangular - Hosted:Standard:413899" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "M_Return Grille - Rectangular - Hosted:Standard" | object type "M_Return Grille - Rectangular - Hosted:Standard" | names: "M_Return Grille - Rectangular - Hosted:Standard:413949" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:445022" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:445044" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          4 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Elbow - Mitered:Standard" | object type "M_Rectangular Duct Elbow - Mitered:Standard" | names: "M_Rectangular Duct Elbow - Mitered:Standard:445046", "M_Rectangular Duct Elbow - Mitered:Standard:517806", "M_Rectangular Duct Elbow - Mitered:Standard:520552" (+1 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          22 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "M_Sconce Light - Flat Round:60W - 277V" | object type "M_Sconce Light - Flat Round:60W - 277V" | names: "M_Sconce Light - Flat Round:60W - 277V:447049", "M_Sconce Light - Flat Round:60W - 277V:447165", "M_Sconce Light - Flat Round:60W - 277V:447199" (+19 more) | material: "Glass - Frosted" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Elbow - Mitered:Standard" | object type "M_Rectangular Duct Elbow - Mitered:Standard" | names: "M_Rectangular Duct Elbow - Mitered:Standard:448747", "M_Rectangular Duct Elbow - Mitered:Standard:448748" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          18 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_Wall Occupancy Sensor - Regular Voltage:Passive Infrared - 277 V" | object type "M_Wall Occupancy Sensor - Regular Voltage:Passive Infrared - 277 V" | names: "M_Wall Occupancy Sensor - Regular Voltage:Passive Infrared - 277 V:448880", "M_Wall Occupancy Sensor - Regular Voltage:Passive Infrared - 277 V:448919", "M_Wall Occupancy Sensor - Regular Voltage:Passive Infrared - 277 V:448998" (+15 more) | material: materials ("<Unnamed>", "<Unnamed>") | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          3 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_Lighting Switches:Single Pole" | object type "M_Lighting Switches:Single Pole" | names: "M_Lighting Switches:Single Pole:452699", "M_Lighting Switches:Single Pole:452731", "M_Lighting Switches:Single Pole:452792" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          12 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Takeoff:Standard" | object type "M_Rectangular Duct Takeoff:Standard" | names: "M_Rectangular Duct Takeoff:Standard:478951", "M_Rectangular Duct Takeoff:Standard:478970", "M_Rectangular Duct Takeoff:Standard:479033" (+9 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          12 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Elbow - Mitered:Standard" | object type "M_Rectangular Duct Elbow - Mitered:Standard" | names: "M_Rectangular Duct Elbow - Mitered:Standard:478971", "M_Rectangular Duct Elbow - Mitered:Standard:479050", "M_Rectangular Duct Elbow - Mitered:Standard:479079" (+9 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          9 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Elbow - Mitered:Standard" | object type "M_Rectangular Duct Elbow - Mitered:Standard" | names: "M_Rectangular Duct Elbow - Mitered:Standard:478974", "M_Rectangular Duct Elbow - Mitered:Standard:479053", "M_Rectangular Duct Elbow - Mitered:Standard:479082" (+6 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Takeoff:Standard" | object type "M_Rectangular Duct Takeoff:Standard" | names: "M_Rectangular Duct Takeoff:Standard:479183" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          9 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Takeoff:Standard" | object type "M_Rectangular Duct Takeoff:Standard" | names: "M_Rectangular Duct Takeoff:Standard:479418", "M_Rectangular Duct Takeoff:Standard:479499", "M_Rectangular Duct Takeoff:Standard:479530" (+6 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Elbow - Mitered:Standard" | object type "M_Rectangular Duct Elbow - Mitered:Standard" | names: "M_Rectangular Duct Elbow - Mitered:Standard:479601", "M_Rectangular Duct Elbow - Mitered:Standard:709693" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:479621" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Elbow - Mitered:Standard" | object type "M_Rectangular Duct Elbow - Mitered:Standard" | names: "M_Rectangular Duct Elbow - Mitered:Standard:479718" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          8 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "M_Supply Diffuser - Sidewall:450 x 200" | object type "M_Supply Diffuser - Sidewall:450 x 200" | names: "M_Supply Diffuser - Sidewall:450 x 200:480021", "M_Supply Diffuser - Sidewall:450 x 200:480165", "M_Supply Diffuser - Sidewall:450 x 200:480184" (+5 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Right Return - Back Discharge:11 kW" | object type "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Right Return - Back Discharge:11 kW" | names: "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Right Return - Back Discharge:11 kW:480517", "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Right Return - Back Discharge:11 kW:481056" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:480979" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Endcap:Standard" | object type "M_Rectangular Duct Endcap:Standard" | names: "M_Rectangular Duct Endcap:Standard:481014" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Elbow - Mitered:Standard" | object type "M_Rectangular Duct Elbow - Mitered:Standard" | names: "M_Rectangular Duct Elbow - Mitered:Standard:481396" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:481437" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Endcap:Standard" | object type "M_Rectangular Duct Endcap:Standard" | names: "M_Rectangular Duct Endcap:Standard:481460" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Right Return - Back Discharge:11 kW" | object type "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Right Return - Back Discharge:11 kW" | names: "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Right Return - Back Discharge:11 kW:481927" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Endcap:Standard" | object type "M_Rectangular Duct Endcap:Standard" | names: "M_Rectangular Duct Endcap:Standard:482274" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          4 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Elbow - Mitered:Standard" | object type "M_Rectangular Duct Elbow - Mitered:Standard" | names: "M_Rectangular Duct Elbow - Mitered:Standard:517427", "M_Rectangular Duct Elbow - Mitered:Standard:517437", "M_Rectangular Duct Elbow - Mitered:Standard:517590" (+1 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          3 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Elbow - Mitered:Standard" | object type "M_Rectangular Duct Elbow - Mitered:Standard" | names: "M_Rectangular Duct Elbow - Mitered:Standard:517610", "M_Rectangular Duct Elbow - Mitered:Standard:517618", "M_Rectangular Duct Elbow - Mitered:Standard:532663" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Elbow - Mitered:Standard" | object type "M_Rectangular Duct Elbow - Mitered:Standard" | names: "M_Rectangular Duct Elbow - Mitered:Standard:517823", "M_Rectangular Duct Elbow - Mitered:Standard:518256" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Takeoff:Standard" | object type "M_Rectangular Duct Takeoff:Standard" | names: "M_Rectangular Duct Takeoff:Standard:518386" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "Exhaust Grille - Rectangular - Hosted - Horizontal:Standard" | object type "Exhaust Grille - Rectangular - Hosted - Horizontal:Standard" | names: "Exhaust Grille - Rectangular - Hosted - Horizontal:Standard:520071", "Exhaust Grille - Rectangular - Hosted - Horizontal:Standard:520483" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Union:Standard" | object type "M_Rectangular Duct Union:Standard" | names: "M_Rectangular Duct Union:Standard:520224" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Elbow - Mitered:Standard" | object type "M_Rectangular Duct Elbow - Mitered:Standard" | names: "M_Rectangular Duct Elbow - Mitered:Standard:520413", "M_Rectangular Duct Elbow - Mitered:Standard:520417" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:520696" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          133 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "Tipos de tubería:Standard" | object type "Tipos de tubería:Standard" | names: "Tipos de tubería:Standard:530080", "Tipos de tubería:Standard:530081", "Tipos de tubería:Standard:530082" (+130 more) | property sets: Pset_DistributionFlowElementCommon, Pset_FlowSegmentDuctSegment, Pset_FlowSegmentPipeSegment, Pset_QuantityTakeOff
          57 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Pipe Elbow:Standard" | object type "M_Pipe Elbow:Standard" | names: "M_Pipe Elbow:Standard:530086", "M_Pipe Elbow:Standard:530088", "M_Pipe Elbow:Standard:530090" (+54 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          6 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Pipe Transition:Standard" | object type "M_Pipe Transition:Standard" | names: "M_Pipe Transition:Standard:530102", "M_Pipe Transition:Standard:530115", "M_Pipe Transition:Standard:530137" (+3 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          12 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Pipe Elbow:Standard" | object type "M_Pipe Elbow:Standard" | names: "M_Pipe Elbow:Standard:530103", "M_Pipe Elbow:Standard:530105", "M_Pipe Elbow:Standard:530116" (+9 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          21 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Pipe Tee:Standard" | object type "M_Pipe Tee:Standard" | names: "M_Pipe Tee:Standard:530236", "M_Pipe Tee:Standard:530252", "M_Pipe Tee:Standard:530260" (+18 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          6 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Pipe Tee:Standard" | object type "M_Pipe Tee:Standard" | names: "M_Pipe Tee:Standard:530240", "M_Pipe Tee:Standard:530245", "M_Pipe Tee:Standard:530255" (+3 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          12 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Pipe Transition:Standard" | object type "M_Pipe Transition:Standard" | names: "M_Pipe Transition:Standard:530242", "M_Pipe Transition:Standard:530243", "M_Pipe Transition:Standard:530247" (+9 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:534710", "M_Rectangular Duct Transition - Angle:45 Degree:534711" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:534756" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          43 x IFCCOLUMN | type IFCCOLUMNTYPE "STB Stütze - rund:STB d=30" | object type "STB Stütze - rund:STB d=30" | names: "STB Stütze - rund:STB d=30:573295", "STB Stütze - rund:STB d=30:573327", "STB Stütze - rund:STB d=30:573328" (+40 more) | material: "Stahlbeton - Fertigbeton" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Muro básico:STB 30.0 Rot" | object type "Muro básico:STB 30.0 Rot" | names: "Muro básico:STB 30.0 Rot:573298", "Muro básico:STB 30.0 Rot:573316" | material: layers "Muro básico:STB 30.0 Rot" ("Stahlbeton - Ortbeton - Rot" 300.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Muro básico:STB 30.0" | object type "Muro básico:STB 30.0" | names: "Muro básico:STB 30.0:573299", "Muro básico:STB 30.0:573321", "Muro básico:STB 30.0:573662" (+1 more) | material: layers "Muro básico:STB 30.0" ("Stahlbeton - Ortbeton" 300.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:STB 30.0" | object type "Suelo:STB 30.0" | FLOOR | names: "Suelo:STB 30.0:573302" | material: layers "Suelo:STB 30.0" ("Stahlbeton - Ortbeton" 300.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          7 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Muro básico:STB 20.0" | object type "Muro básico:STB 20.0" | names: "Muro básico:STB 20.0:573317", "Muro básico:STB 20.0:573318", "Muro básico:STB 20.0:573319" (+4 more) | material: layers "Muro básico:STB 20.0" ("Stahlbeton - Ortbeton" 200.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Muro básico:STB 30.0" | object type "Muro básico:STB 30.0" | names: "Muro básico:STB 30.0:573322" | material: layers "Muro básico:STB 30.0" ("Stahlbeton - Ortbeton" 300.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          4 x IFCWALL | type IFCWALLTYPE "Muro básico:STB 20.0" | object type "Muro básico:STB 20.0" | names: "Muro básico:STB 20.0:573323", "Muro básico:STB 20.0:573324", "Muro básico:STB 20.0:573325" (+1 more) | material: layers "Muro básico:STB 20.0" ("Stahlbeton - Ortbeton" 200.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          10 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Muro básico:MW 17.5" | object type "Muro básico:MW 17.5" | names: "Muro básico:MW 17.5:573574", "Muro básico:MW 17.5:573575", "Muro básico:MW 17.5:573576" (+7 more) | material: layers "Muro básico:MW 17.5" ("Mauerwerk - Ziegel" 175.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          9 x IFCDOOR | type IFCDOORSTYLE "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26" | object type "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26" | names: "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26:573577", "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26:573578", "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26:573579" (+6 more) | material: materials ("Tür - Stahl Griff", "Tür - Stahl Zarge") | property sets: Pset_DoorCommon, Pset_QuantityTakeOff
          4 x IFCDOOR | type IFCDOORSTYLE "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26" | object type "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26" | names: "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26:573583", "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26:573584", "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26:573669" (+1 more) | material: materials ("Tür - Stahl Griff", "Tür - Stahl Zarge") | property sets: Pset_DoorCommon, Pset_QuantityTakeOff
          14 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Muro básico:MW 11.5" | object type "Muro básico:MW 11.5" | names: "Muro básico:MW 11.5:573588", "Muro básico:MW 11.5:573589", "Muro básico:MW 11.5:573590" (+11 more) | material: layers "Muro básico:MW 11.5" ("Mauerwerk - Ziegel" 115.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Muro básico:Lamelle 11.5" | object type "Muro básico:Lamelle 11.5" | names: "Muro básico:Lamelle 11.5:573595", "Muro básico:Lamelle 11.5:575086" | material: layers "Muro básico:Lamelle 11.5" ("Mauerwerk - Lamellen" 115.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          22 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Muro cortina:Standard" | object type "Muro cortina:Standard" | names: "Muro cortina:Standard:573596", "Muro cortina:Standard:573598", "Muro cortina:Standard:573600" (+19 more) | parts: 1297 IFCMEMBER, 588 IFCPLATE, 8 IFCDOOR | property sets: Pset_OpeningElementCommon, Pset_QuantityTakeOff, Pset_CurtainWallCommon
          2 x IFCDOOR | type IFCDOORSTYLE "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26" | object type "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26" | names: "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26:573668", "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26:573674" | material: materials ("Tür - Stahl Griff", "Tür - Stahl Zarge") | property sets: Pset_DoorCommon, Pset_QuantityTakeOff
          4 x IFCDOOR | type IFCDOORSTYLE "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26" | object type "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26" | names: "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26:573673", "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26:573676", "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26:573677" (+1 more) | material: materials ("Tür - Stahl Griff", "Tür - Stahl Zarge") | property sets: Pset_DoorCommon, Pset_QuantityTakeOff
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Muro básico:WC Trennwand 5.0" | object type "Muro básico:WC Trennwand 5.0" | names: "Muro básico:WC Trennwand 5.0:573780", "Muro básico:WC Trennwand 5.0:573781", "Muro básico:WC Trennwand 5.0:573782" (+1 more) | material: layers "Muro básico:WC Trennwand 5.0" ("WC Trennwand" 50.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          4 x IFCDOOR | type IFCDOORSTYLE "Drehflügel 1-flg - Stahlzarge:76 x 2.26" | object type "Drehflügel 1-flg - Stahlzarge:76 x 2.26" | names: "Drehflügel 1-flg - Stahlzarge:76 x 2.26:573783", "Drehflügel 1-flg - Stahlzarge:76 x 2.26:573784", "Drehflügel 1-flg - Stahlzarge:76 x 2.26:577953" (+1 more) | material: materials ("Tür - Stahl Griff", "Tür - Stahl Zarge") | property sets: Pset_DoorCommon, Pset_QuantityTakeOff
          3 x IFCCOLUMN | type IFCCOLUMNTYPE "STB Stütze - rund:STB d=30" | object type "STB Stütze - rund:STB d=30" | names: "STB Stütze - rund:STB d=30:574557", "STB Stütze - rund:STB d=30:577494", "STB Stütze - rund:STB d=30:577495" | material: "Stahlbeton - Fertigbeton" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Aufzug 2-flg:Aufzug 2-flg" | object type "Aufzug 2-flg:Aufzug 2-flg" | names: "Aufzug 2-flg:Aufzug 2-flg:575085" | material: "Tür - Aufzug Metall" | property sets: Pset_OpeningElementCommon, Pset_QuantityTakeOff
          7 x IFCDOOR | type IFCDOORSTYLE "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26" | object type "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26" | names: "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26:575087", "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26:575088", "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26:575090" (+4 more) | material: materials ("Tür - Stahl Griff", "Tür - Stahl Zarge") | property sets: Pset_DoorCommon, Pset_QuantityTakeOff
          6 x IFCDOOR | type IFCDOORSTYLE "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26" | object type "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26" | names: "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26:575089", "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26:575091", "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26:575093" (+3 more) | material: materials ("Tür - Stahl Griff", "Tür - Stahl Zarge") | property sets: Pset_DoorCommon, Pset_QuantityTakeOff
          5 x IFCSTAIR | object type "Escalera:Massiv - Stufen Naturstein" | names: "Escalera:Massiv - Stufen Naturstein:576198", "Escalera:Massiv - Stufen Naturstein:576328", "Escalera:Massiv - Stufen Naturstein:576464" (+2 more) | parts: 4 IFCRAILING, 4 IFCSTAIRFLIGHT, 3 IFCSTAIR, 2 IFCSLAB | property sets: Pset_QuantityTakeOff, Pset_StairCommon
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:FB 15.0 - Holzdielen" | object type "Suelo:FB 15.0 - Holzdielen" | FLOOR | names: "Suelo:FB 15.0 - Holzdielen:577501" | material: layers "Suelo:FB 15.0 - Holzdielen" ("Bodenbelag Holzdielen" 30., "Decke - Estrich" 40., "Default Floor" 80.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:FB 15.0 - Teppich" | object type "Suelo:FB 15.0 - Teppich" | FLOOR | names: "Suelo:FB 15.0 - Teppich:577894" | material: layers "Suelo:FB 15.0 - Teppich" ("Bodenbelag Teppich" 10., "Decke - Estrich" 60., "Wärmedämmung - hart" 80.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:FB 15.0 - Teppich" | object type "Suelo:FB 15.0 - Teppich" | FLOOR | names: "Suelo:FB 15.0 - Teppich:577894:2" | material: layers "Suelo:FB 15.0 - Teppich" ("Bodenbelag Teppich" 10., "Decke - Estrich" 60., "Wärmedämmung - hart" 80.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:FB 15.0 - Teppich" | object type "Suelo:FB 15.0 - Teppich" | FLOOR | names: "Suelo:FB 15.0 - Teppich:577894:3" | material: layers "Suelo:FB 15.0 - Teppich" ("Bodenbelag Teppich" 10., "Decke - Estrich" 60., "Wärmedämmung - hart" 80.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:FB 15.0 - Teppich" | object type "Suelo:FB 15.0 - Teppich" | FLOOR | names: "Suelo:FB 15.0 - Teppich:577894:4" | material: layers "Suelo:FB 15.0 - Teppich" ("Bodenbelag Teppich" 10., "Decke - Estrich" 60., "Wärmedämmung - hart" 80.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:FB 15.0 - Teppich" | object type "Suelo:FB 15.0 - Teppich" | FLOOR | names: "Suelo:FB 15.0 - Teppich:577894:5" | material: layers "Suelo:FB 15.0 - Teppich" ("Bodenbelag Teppich" 10., "Decke - Estrich" 60., "Wärmedämmung - hart" 80.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:FB 15.0 - Teppich" | object type "Suelo:FB 15.0 - Teppich" | FLOOR | names: "Suelo:FB 15.0 - Teppich:577894:6" | material: layers "Suelo:FB 15.0 - Teppich" ("Bodenbelag Teppich" 10., "Decke - Estrich" 60., "Wärmedämmung - hart" 80.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:FB 15.0 - Teppich" | object type "Suelo:FB 15.0 - Teppich" | FLOOR | names: "Suelo:FB 15.0 - Teppich:577894:7" | material: layers "Suelo:FB 15.0 - Teppich" ("Bodenbelag Teppich" 10., "Decke - Estrich" 60., "Wärmedämmung - hart" 80.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:FB 15.0 - Teppich" | object type "Suelo:FB 15.0 - Teppich" | FLOOR | names: "Suelo:FB 15.0 - Teppich:577894:8" | material: layers "Suelo:FB 15.0 - Teppich" ("Bodenbelag Teppich" 10., "Decke - Estrich" 60., "Wärmedämmung - hart" 80.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:FB 15.0 - Teppich" | object type "Suelo:FB 15.0 - Teppich" | FLOOR | names: "Suelo:FB 15.0 - Teppich:577894:9" | material: layers "Suelo:FB 15.0 - Teppich" ("Bodenbelag Teppich" 10., "Decke - Estrich" 60., "Wärmedämmung - hart" 80.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:FB 15.0 - Teppich" | object type "Suelo:FB 15.0 - Teppich" | FLOOR | names: "Suelo:FB 15.0 - Teppich:577894:10" | material: layers "Suelo:FB 15.0 - Teppich" ("Bodenbelag Teppich" 10., "Decke - Estrich" 60., "Wärmedämmung - hart" 80.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:FB 15.0 - Teppich" | object type "Suelo:FB 15.0 - Teppich" | FLOOR | names: "Suelo:FB 15.0 - Teppich:577894:11" | material: layers "Suelo:FB 15.0 - Teppich" ("Bodenbelag Teppich" 10., "Decke - Estrich" 60., "Wärmedämmung - hart" 80.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:FB 15.0 - Teppich" | object type "Suelo:FB 15.0 - Teppich" | FLOOR | names: "Suelo:FB 15.0 - Teppich:577894:12" | material: layers "Suelo:FB 15.0 - Teppich" ("Bodenbelag Teppich" 10., "Decke - Estrich" 60., "Wärmedämmung - hart" 80.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:FB 15.0 - Teppich" | object type "Suelo:FB 15.0 - Teppich" | FLOOR | names: "Suelo:FB 15.0 - Teppich:577894:13" | material: layers "Suelo:FB 15.0 - Teppich" ("Bodenbelag Teppich" 10., "Decke - Estrich" 60., "Wärmedämmung - hart" 80.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:FB 15.0 - Teppich" | object type "Suelo:FB 15.0 - Teppich" | FLOOR | names: "Suelo:FB 15.0 - Teppich:577894:14" | material: layers "Suelo:FB 15.0 - Teppich" ("Bodenbelag Teppich" 10., "Decke - Estrich" 60., "Wärmedämmung - hart" 80.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:FB 15.0 - Teppich" | object type "Suelo:FB 15.0 - Teppich" | FLOOR | names: "Suelo:FB 15.0 - Teppich:577894:15" | material: layers "Suelo:FB 15.0 - Teppich" ("Bodenbelag Teppich" 10., "Decke - Estrich" 60., "Wärmedämmung - hart" 80.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:FB 10.0 - Fliesen 15 x 15" | object type "Suelo:FB 10.0 - Fliesen 15 x 15" | FLOOR | names: "Suelo:FB 10.0 - Fliesen 15 x 15:577947" | material: layers "Suelo:FB 10.0 - Fliesen 15 x 15" ("Decke - Fliesen 15 x 15" 10., "Decke - Estrich" 60., "Wärmedämmung - hart" 80.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:FB 10.0 - Fliesen 15 x 15" | object type "Suelo:FB 10.0 - Fliesen 15 x 15" | FLOOR | names: "Suelo:FB 10.0 - Fliesen 15 x 15:577947:2" | material: layers "Suelo:FB 10.0 - Fliesen 15 x 15" ("Decke - Fliesen 15 x 15" 10., "Decke - Estrich" 60., "Wärmedämmung - hart" 80.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:FB 10.0 - Fliesen 15 x 15" | object type "Suelo:FB 10.0 - Fliesen 15 x 15" | FLOOR | names: "Suelo:FB 10.0 - Fliesen 15 x 15:577947:3" | material: layers "Suelo:FB 10.0 - Fliesen 15 x 15" ("Decke - Fliesen 15 x 15" 10., "Decke - Estrich" 60., "Wärmedämmung - hart" 80.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:FB 10.0 - Fliesen 15 x 15" | object type "Suelo:FB 10.0 - Fliesen 15 x 15" | FLOOR | names: "Suelo:FB 10.0 - Fliesen 15 x 15:577947:4" | material: layers "Suelo:FB 10.0 - Fliesen 15 x 15" ("Decke - Fliesen 15 x 15" 10., "Decke - Estrich" 60., "Wärmedämmung - hart" 80.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:FB 15.0 - Holzdielen" | object type "Suelo:FB 15.0 - Holzdielen" | FLOOR | names: "Suelo:FB 15.0 - Holzdielen:577961" | material: layers "Suelo:FB 15.0 - Holzdielen" ("Bodenbelag Holzdielen" 30., "Decke - Estrich" 40., "Default Floor" 80.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:FB 15.0 - Fliesen 50 x 50" | object type "Suelo:FB 15.0 - Fliesen 50 x 50" | FLOOR | names: "Suelo:FB 15.0 - Fliesen 50 x 50:578008" | material: layers "Suelo:FB 15.0 - Fliesen 50 x 50" ("Bodenbelag Fliesen 50 x 50" 10., "Decke - Estrich" 60., "Wärmedämmung - hart" 80.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:FB 15.0 - Fliesen 50 x 50" | object type "Suelo:FB 15.0 - Fliesen 50 x 50" | FLOOR | names: "Suelo:FB 15.0 - Fliesen 50 x 50:578008:2" | material: layers "Suelo:FB 15.0 - Fliesen 50 x 50" ("Bodenbelag Fliesen 50 x 50" 10., "Decke - Estrich" 60., "Wärmedämmung - hart" 80.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:FB 15.0 - Holzdielen" | object type "Suelo:FB 15.0 - Holzdielen" | FLOOR | names: "Suelo:FB 15.0 - Holzdielen:578071" | material: layers "Suelo:FB 15.0 - Holzdielen" ("Bodenbelag Holzdielen" 30., "Decke - Estrich" 40., "Default Floor" 80.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_Lighting and Appliance Panelboard - 480V MLO - Surface:125 A" | object type "M_Lighting and Appliance Panelboard - 480V MLO - Surface:125 A" | names: "M_Lighting and Appliance Panelboard - 480V MLO - Surface:LP-1:581482" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff, Pset_ProvisionForVoid
          3 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_Lighting and Appliance Panelboard - 208V MLO - Surface:400 A" | object type "M_Lighting and Appliance Panelboard - 208V MLO - Surface:400 A" | names: "M_Lighting and Appliance Panelboard - 208V MLO - Surface:PP-1B:581483", "M_Lighting and Appliance Panelboard - 208V MLO - Surface:EP-1A:581484", "M_Lighting and Appliance Panelboard - 208V MLO - Surface:EP-1B:581485" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff, Pset_ProvisionForVoid
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_Lighting and Appliance Panelboard - 480V MCB - Surface:100 A" | object type "M_Lighting and Appliance Panelboard - 480V MCB - Surface:100 A" | names: "M_Lighting and Appliance Panelboard - 480V MCB - Surface:LP-1B:622023", "M_Lighting and Appliance Panelboard - 480V MCB - Surface:MP-1B:622026" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff, Pset_ProvisionForVoid
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_Lighting and Appliance Panelboard - 208V MCB - Surface:100 A" | object type "M_Lighting and Appliance Panelboard - 208V MCB - Surface:100 A" | names: "M_Lighting and Appliance Panelboard - 208V MCB - Surface:PP-1A:622027" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff, Pset_ProvisionForVoid
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_Dry Type Transformer - 480-208Y120 - NEMA Type 3R:15 kVA" | object type "M_Dry Type Transformer - 480-208Y120 - NEMA Type 3R:15 kVA" | names: "M_Dry Type Transformer - 480-208Y120 - NEMA Type 3R:TP-1A:622028" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff, Pset_ProvisionForVoid
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_Dry Type Transformer - 480-208Y120 - NEMA Type 2:500 kVA" | object type "M_Dry Type Transformer - 480-208Y120 - NEMA Type 2:500 kVA" | names: "M_Dry Type Transformer - 480-208Y120 - NEMA Type 2:T-SVC:624416" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_Circuit Breaker Switchboard:762mmx965mm" | object type "M_Circuit Breaker Switchboard:762mmx965mm" | names: "M_Circuit Breaker Switchboard:SWB:630241" | material: materials ("<Unnamed>", "<Unnamed>") | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          19 x IFCFLOWSEGMENT | type IFCCABLECARRIERSEGMENTTYPE "Tubo sin uniones:Rigid Nonmetallic Conduit (RNC Sch 80)" | object type "Tubo sin uniones:Rigid Nonmetallic Conduit (RNC Sch 80)" | names: "Tubo sin uniones:Rigid Nonmetallic Conduit (RNC Sch 80):678659", "Tubo sin uniones:Rigid Nonmetallic Conduit (RNC Sch 80):679071", "Tubo sin uniones:Rigid Nonmetallic Conduit (RNC Sch 80):679170" (+16 more) | property sets: Pset_DistributionFlowElementCommon, Pset_FlowSegmentDuctSegment, Pset_FlowSegmentPipeSegment, Pset_QuantityTakeOff
          12 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "Conduit Elbow - without Fittings - RNC:Standard" | object type "Conduit Elbow - without Fittings - RNC:Standard" | names: "Conduit Elbow - without Fittings - RNC:Standard:679174", "Conduit Elbow - without Fittings - RNC:Standard:683664", "Conduit Elbow - without Fittings - RNC:Standard:683837" (+9 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "Conduit Body - Type L - Aluminum:Standard" | object type "Conduit Body - Type L - Aluminum:Standard" | names: "Conduit Body - Type L - Aluminum:Standard:685902" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "Conducto redondo:Taps" | object type "Conducto redondo:Taps" | names: "Conducto redondo:Taps:686628" | property sets: Pset_DistributionFlowElementCommon, Pset_DuctSegmentTypeCommon, Pset_FlowSegmentDuctSegment, Pset_FlowSegmentPipeSegment, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:712162" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Tee - Generic:Standard" | object type "M_Tee - Generic:Standard" | names: "M_Tee - Generic:Standard:712287" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          17 x IFCFLOWSEGMENT | type IFCCABLECARRIERSEGMENTTYPE "Bandeja de cables con uniones:Ladder Cable Tray" | object type "Bandeja de cables con uniones:Ladder Cable Tray" | names: "Bandeja de cables con uniones:Ladder Cable Tray:797605", "Bandeja de cables con uniones:Ladder Cable Tray:797611", "Bandeja de cables con uniones:Ladder Cable Tray:797663" (+14 more) | property sets: Pset_DistributionFlowElementCommon, Pset_FlowSegmentDuctSegment, Pset_FlowSegmentPipeSegment, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "M_Ladder Horizontal Tee:300mm Radius" | object type "M_Ladder Horizontal Tee:300mm Radius" | names: "M_Ladder Horizontal Tee:300mm Radius:797649" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          4 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "M_Ladder Vertical Outside Bend:Standard" | object type "M_Ladder Vertical Outside Bend:Standard" | names: "M_Ladder Vertical Outside Bend:Standard:798053", "M_Ladder Vertical Outside Bend:Standard:798344", "M_Ladder Vertical Outside Bend:Standard:798873" (+1 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "M_Ladder Horizontal Bend:Standard" | object type "M_Ladder Horizontal Bend:Standard" | names: "M_Ladder Horizontal Bend:Standard:798526", "M_Ladder Horizontal Bend:Standard:799607" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Union:Standard" | object type "M_Rectangular Duct Union:Standard" | names: "M_Rectangular Duct Union:Standard:798761" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          5 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "M_Ladder Vertical Inside Bend:Standard" | object type "M_Ladder Vertical Inside Bend:Standard" | names: "M_Ladder Vertical Inside Bend:Standard:798871", "M_Ladder Vertical Inside Bend:Standard:799010", "M_Ladder Vertical Inside Bend:Standard:799012" (+2 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "M_Ladder Vertical Inside Bend:Standard" | object type "M_Ladder Vertical Inside Bend:Standard" | names: "M_Ladder Vertical Inside Bend:Standard:800100" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "M_Ladder Vertical Outside Bend:Standard" | object type "M_Ladder Vertical Outside Bend:Standard" | names: "M_Ladder Vertical Outside Bend:Standard:800193" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:805257" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Takeoff:Standard" | object type "M_Rectangular Duct Takeoff:Standard" | names: "M_Rectangular Duct Takeoff:Standard:805265" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Takeoff:Standard" | object type "M_Rectangular Duct Takeoff:Standard" | names: "M_Rectangular Duct Takeoff:Standard:805494", "M_Rectangular Duct Takeoff:Standard:805546" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Tee - Generic:Standard" | object type "M_Tee - Generic:Standard" | names: "M_Tee - Generic:Standard:812876" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Transition - Generic:Standard" | object type "M_Transition - Generic:Standard" | names: "M_Transition - Generic:Standard:812884" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          4 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Elbow - Generic:Standard" | object type "M_Elbow - Generic:Standard" | names: "M_Elbow - Generic:Standard:812887", "M_Elbow - Generic:Standard:817502", "M_Elbow - Generic:Standard:818363" (+1 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Tee - Generic:Standard" | object type "M_Tee - Generic:Standard" | names: "M_Tee - Generic:Standard:817492" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Transition - Generic:Standard" | object type "M_Transition - Generic:Standard" | names: "M_Transition - Generic:Standard:817500" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Elbow - Generic:Standard" | object type "M_Elbow - Generic:Standard" | names: "M_Elbow - Generic:Standard:818367" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_Lighting and Appliance Panelboard - 480V MCB - Surface:400 A" | object type "M_Lighting and Appliance Panelboard - 480V MCB - Surface:400 A" | names: "M_Lighting and Appliance Panelboard - 480V MCB - Surface:MDP-1:822681" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff, Pset_ProvisionForVoid
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Elbow - Mitered:Standard" | object type "M_Rectangular Duct Elbow - Mitered:Standard" | names: "M_Rectangular Duct Elbow - Mitered:Standard:971584", "M_Rectangular Duct Elbow - Mitered:Standard:971590" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
      IFCBUILDINGSTOREY "Level 2" | long name "Level 2" | object type "Nivel:8mm Head" | elevation 3799.99999999989
        contains 1771 elements
          13 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "M_Supply Diffuser - Rectangular Face Round Neck:600x600 - 250 Neck" | object type "M_Supply Diffuser - Rectangular Face Round Neck:600x600 - 250 Neck" | names: "M_Supply Diffuser - Rectangular Face Round Neck:600x600 - 250 Neck:379463", "M_Supply Diffuser - Rectangular Face Round Neck:600x600 - 250 Neck:414276", "M_Supply Diffuser - Rectangular Face Round Neck:600x600 - 250 Neck:414296" (+10 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          7 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "M_Supply Diffuser - Rectangular Face Round Neck:600x600 - 250 Neck" | object type "M_Supply Diffuser - Rectangular Face Round Neck:600x600 - 250 Neck" | names: "M_Supply Diffuser - Rectangular Face Round Neck:600x600 - 250 Neck:414359", "M_Supply Diffuser - Rectangular Face Round Neck:600x600 - 250 Neck:414759", "M_Supply Diffuser - Rectangular Face Round Neck:600x600 - 250 Neck:414855" (+4 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          9 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "M_Supply Diffuser - Rectangular Face Round Neck:600x600 - 250 Neck" | object type "M_Supply Diffuser - Rectangular Face Round Neck:600x600 - 250 Neck" | names: "M_Supply Diffuser - Rectangular Face Round Neck:600x600 - 250 Neck:414379", "M_Supply Diffuser - Rectangular Face Round Neck:600x600 - 250 Neck:414584", "M_Supply Diffuser - Rectangular Face Round Neck:600x600 - 250 Neck:414585" (+6 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          8 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "M_Supply Diffuser - Rectangular Face Round Neck:600x600 - 250 Neck" | object type "M_Supply Diffuser - Rectangular Face Round Neck:600x600 - 250 Neck" | names: "M_Supply Diffuser - Rectangular Face Round Neck:600x600 - 250 Neck:414680", "M_Supply Diffuser - Rectangular Face Round Neck:600x600 - 250 Neck:414681", "M_Supply Diffuser - Rectangular Face Round Neck:600x600 - 250 Neck:414682" (+5 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          6 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "M_Supply Diffuser - Rectangular Face Round Neck:600x600 - 250 Neck" | object type "M_Supply Diffuser - Rectangular Face Round Neck:600x600 - 250 Neck" | names: "M_Supply Diffuser - Rectangular Face Round Neck:600x600 - 250 Neck:414731", "M_Supply Diffuser - Rectangular Face Round Neck:600x600 - 250 Neck:414854", "M_Supply Diffuser - Rectangular Face Round Neck:600x600 - 250 Neck:415007" (+3 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "M_Supply Diffuser - Rectangular Face Round Neck:600x600 - 250 Neck" | object type "M_Supply Diffuser - Rectangular Face Round Neck:600x600 - 250 Neck" | names: "M_Supply Diffuser - Rectangular Face Round Neck:600x600 - 250 Neck:415060", "M_Supply Diffuser - Rectangular Face Round Neck:600x600 - 250 Neck:415061" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "M_Supply Diffuser - Sidewall:450 x 200" | object type "M_Supply Diffuser - Sidewall:450 x 200" | names: "M_Supply Diffuser - Sidewall:450 x 200:415095", "M_Supply Diffuser - Sidewall:450 x 200:415183" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          4 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "M_Supply Diffuser - Sidewall:450 x 200" | object type "M_Supply Diffuser - Sidewall:450 x 200" | names: "M_Supply Diffuser - Sidewall:450 x 200:415223", "M_Supply Diffuser - Sidewall:450 x 200:415224", "M_Supply Diffuser - Sidewall:450 x 200:415247" (+1 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          4 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "M_Supply Diffuser - Sidewall:450 x 200" | object type "M_Supply Diffuser - Sidewall:450 x 200" | names: "M_Supply Diffuser - Sidewall:450 x 200:415232", "M_Supply Diffuser - Sidewall:450 x 200:415233", "M_Supply Diffuser - Sidewall:450 x 200:415249" (+1 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          8 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "M_Supply Diffuser - Sidewall:450 x 200" | object type "M_Supply Diffuser - Sidewall:450 x 200" | names: "M_Supply Diffuser - Sidewall:450 x 200:415480", "M_Supply Diffuser - Sidewall:450 x 200:415481", "M_Supply Diffuser - Sidewall:450 x 200:415513" (+5 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Back Discharge:14 kW" | object type "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Back Discharge:14 kW" | names: "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Back Discharge:14 kW:415572", "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Back Discharge:14 kW:415895" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:14 kW" | object type "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:14 kW" | names: "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:14 kW:418911" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          43 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "Conducto rectangular:Mitered Elbows / Tees" | object type "Conducto rectangular:Mitered Elbows / Tees" | names: "Conducto rectangular:Mitered Elbows / Tees:419031", "Conducto rectangular:Mitered Elbows / Tees:419032", "Conducto rectangular:Mitered Elbows / Tees:419035" (+40 more) | property sets: Pset_DistributionFlowElementCommon, Pset_DuctSegmentTypeCommon, Pset_FlowSegmentDuctSegment, Pset_FlowSegmentPipeSegment, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:419033", "M_Rectangular Duct Transition - Angle:45 Degree:419948" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          193 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "Conducto rectangular:Mitered Elbows / Taps" | object type "Conducto rectangular:Mitered Elbows / Taps" | names: "Conducto rectangular:Mitered Elbows / Taps:419038", "Conducto rectangular:Mitered Elbows / Taps:419045", "Conducto rectangular:Mitered Elbows / Taps:419052" (+190 more) | property sets: Pset_DistributionFlowElementCommon, Pset_DuctSegmentTypeCommon, Pset_FlowSegmentDuctSegment, Pset_FlowSegmentPipeSegment, Pset_QuantityTakeOff
          54 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "Conducto flexible redondo:Flex - Round" | object type "Conducto flexible redondo:Flex - Round" | names: "Conducto flexible redondo:Flex - Round:419042", "Conducto flexible redondo:Flex - Round:419049", "Conducto flexible redondo:Flex - Round:419056" (+51 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          38 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular to Round Duct Transition - Angle:45 Degree" | object type "M_Rectangular to Round Duct Transition - Angle:45 Degree" | names: "M_Rectangular to Round Duct Transition - Angle:45 Degree:419078", "M_Rectangular to Round Duct Transition - Angle:45 Degree:419137", "M_Rectangular to Round Duct Transition - Angle:45 Degree:419345" (+35 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Tee:Standard" | object type "M_Rectangular Duct Tee:Standard" | names: "M_Rectangular Duct Tee:Standard:419084" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          10 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Takeoff:Standard" | object type "M_Rectangular Duct Takeoff:Standard" | names: "M_Rectangular Duct Takeoff:Standard:419097", "M_Rectangular Duct Takeoff:Standard:419136", "M_Rectangular Duct Takeoff:Standard:419344" (+7 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          6 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Endcap:Standard" | object type "M_Rectangular Duct Endcap:Standard" | names: "M_Rectangular Duct Endcap:Standard:419171", "M_Rectangular Duct Endcap:Standard:419270", "M_Rectangular Duct Endcap:Standard:419994" (+3 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          3 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:419285", "M_Rectangular Duct Transition - Angle:45 Degree:419930", "M_Rectangular Duct Transition - Angle:45 Degree:422279" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:419286" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:419302" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          3 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:419303", "M_Rectangular Duct Transition - Angle:45 Degree:419931", "M_Rectangular Duct Transition - Angle:45 Degree:426122" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          15 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Takeoff:Standard" | object type "M_Rectangular Duct Takeoff:Standard" | names: "M_Rectangular Duct Takeoff:Standard:419368", "M_Rectangular Duct Takeoff:Standard:419392", "M_Rectangular Duct Takeoff:Standard:420693" (+12 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:14 kW" | object type "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:14 kW" | names: "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:14 kW:419678" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular to Round Duct Transition - Angle:45 Degree" | object type "M_Rectangular to Round Duct Transition - Angle:45 Degree" | names: "M_Rectangular to Round Duct Transition - Angle:45 Degree:419806", "M_Rectangular to Round Duct Transition - Angle:45 Degree:420072" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Tee:Standard" | object type "M_Rectangular Duct Tee:Standard" | names: "M_Rectangular Duct Tee:Standard:419860" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          3 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Cross:Standard" | object type "M_Rectangular Duct Cross:Standard" | names: "M_Rectangular Duct Cross:Standard:419863", "M_Rectangular Duct Cross:Standard:422578", "M_Rectangular Duct Cross:Standard:422792" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Cross:Standard" | object type "M_Rectangular Duct Cross:Standard" | names: "M_Rectangular Duct Cross:Standard:419868", "M_Rectangular Duct Cross:Standard:426056" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Takeoff:Standard" | object type "M_Rectangular Duct Takeoff:Standard" | names: "M_Rectangular Duct Takeoff:Standard:419874", "M_Rectangular Duct Takeoff:Standard:420071" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Endcap:Standard" | object type "M_Rectangular Duct Endcap:Standard" | names: "M_Rectangular Duct Endcap:Standard:419910", "M_Rectangular Duct Endcap:Standard:423894" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:420010" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:420011" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          4 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:420026", "M_Rectangular Duct Transition - Angle:45 Degree:420033", "M_Rectangular Duct Transition - Angle:45 Degree:426131" (+1 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          8 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:420041", "M_Rectangular Duct Transition - Angle:45 Degree:420048", "M_Rectangular Duct Transition - Angle:45 Degree:422293" (+5 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:7 kW" | object type "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:7 kW" | names: "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:7 kW:420143" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:11 kW" | object type "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:11 kW" | names: "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:11 kW:421392" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:421904" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Elbow - Mitered:Standard" | object type "M_Rectangular Duct Elbow - Mitered:Standard" | names: "M_Rectangular Duct Elbow - Mitered:Standard:421906" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Cross:Standard" | object type "M_Rectangular Duct Cross:Standard" | names: "M_Rectangular Duct Cross:Standard:421953" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:422280" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:422282", "M_Rectangular Duct Transition - Angle:45 Degree:536815" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:11 kW" | object type "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:11 kW" | names: "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:11 kW:422382", "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:11 kW:422679" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:422547", "M_Rectangular Duct Transition - Angle:45 Degree:422761" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          4 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Endcap:Standard" | object type "M_Rectangular Duct Endcap:Standard" | names: "M_Rectangular Duct Endcap:Standard:422592", "M_Rectangular Duct Endcap:Standard:422826", "M_Rectangular Duct Endcap:Standard:425329" (+1 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          5 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:422609", "M_Rectangular Duct Transition - Angle:45 Degree:422838", "M_Rectangular Duct Transition - Angle:45 Degree:423961" (+2 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:422610", "M_Rectangular Duct Transition - Angle:45 Degree:422839" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:11 kW" | object type "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:11 kW" | names: "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:11 kW:422922" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Elbow - Mitered:Standard" | object type "M_Rectangular Duct Elbow - Mitered:Standard" | names: "M_Rectangular Duct Elbow - Mitered:Standard:423710" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          20 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Takeoff:Standard" | object type "M_Rectangular Duct Takeoff:Standard" | names: "M_Rectangular Duct Takeoff:Standard:423829", "M_Rectangular Duct Takeoff:Standard:423983", "M_Rectangular Duct Takeoff:Standard:424008" (+17 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          12 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Takeoff:Standard" | object type "M_Rectangular Duct Takeoff:Standard" | names: "M_Rectangular Duct Takeoff:Standard:423844", "M_Rectangular Duct Takeoff:Standard:423857", "M_Rectangular Duct Takeoff:Standard:424542" (+9 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Endcap:Standard" | object type "M_Rectangular Duct Endcap:Standard" | names: "M_Rectangular Duct Endcap:Standard:423905" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:423960" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:423962" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Endcap:Standard" | object type "M_Rectangular Duct Endcap:Standard" | names: "M_Rectangular Duct Endcap:Standard:424341" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Right Return - Back Discharge:7 kW" | object type "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Right Return - Back Discharge:7 kW" | names: "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Right Return - Back Discharge:7 kW:424651" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:424853" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:424984" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Elbow - Mitered:Standard" | object type "M_Rectangular Duct Elbow - Mitered:Standard" | names: "M_Rectangular Duct Elbow - Mitered:Standard:424986" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:425366" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:425367" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Endcap:Standard" | object type "M_Rectangular Duct Endcap:Standard" | names: "M_Rectangular Duct Endcap:Standard:425689", "M_Rectangular Duct Endcap:Standard:429632" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Back Discharge:14 kW" | object type "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Back Discharge:14 kW" | names: "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Back Discharge:14 kW:425729" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:426024" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Elbow - Mitered:Standard" | object type "M_Rectangular Duct Elbow - Mitered:Standard" | names: "M_Rectangular Duct Elbow - Mitered:Standard:426026" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:426121" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Elbow - Mitered:Standard" | object type "M_Rectangular Duct Elbow - Mitered:Standard" | names: "M_Rectangular Duct Elbow - Mitered:Standard:426532", "M_Rectangular Duct Elbow - Mitered:Standard:536446" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:426681" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:11 kW" | object type "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:11 kW" | names: "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:11 kW:426761" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:427620" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Tee:Standard" | object type "M_Rectangular Duct Tee:Standard" | names: "M_Rectangular Duct Tee:Standard:427660" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Tee:Standard" | object type "M_Rectangular Duct Tee:Standard" | names: "M_Rectangular Duct Tee:Standard:427667" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:427919" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:427932" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:427933" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          6 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Endcap:Standard" | object type "M_Rectangular Duct Endcap:Standard" | names: "M_Rectangular Duct Endcap:Standard:428849", "M_Rectangular Duct Endcap:Standard:429084", "M_Rectangular Duct Endcap:Standard:429244" (+3 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          12 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Elbow - Mitered:Standard" | object type "M_Rectangular Duct Elbow - Mitered:Standard" | names: "M_Rectangular Duct Elbow - Mitered:Standard:428928", "M_Rectangular Duct Elbow - Mitered:Standard:429023", "M_Rectangular Duct Elbow - Mitered:Standard:429119" (+9 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          5 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Endcap:Standard" | object type "M_Rectangular Duct Endcap:Standard" | names: "M_Rectangular Duct Endcap:Standard:428986", "M_Rectangular Duct Endcap:Standard:429448", "M_Rectangular Duct Endcap:Standard:429738" (+2 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Takeoff:Standard" | object type "M_Rectangular Duct Takeoff:Standard" | names: "M_Rectangular Duct Takeoff:Standard:429821", "M_Rectangular Duct Takeoff:Standard:430038" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:429908", "M_Rectangular Duct Transition - Angle:45 Degree:430074" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          28 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "M_Return Diffuser:600 x 600 Face 300 x 300 Connection" | object type "M_Return Diffuser:600 x 600 Face 300 x 300 Connection" | names: "M_Return Diffuser:600 x 600 Face 300 x 300 Connection:430641", "M_Return Diffuser:600 x 600 Face 300 x 300 Connection:430655", "M_Return Diffuser:600 x 600 Face 300 x 300 Connection:430663" (+25 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          84 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "M_Plain Recessed Lighting Fixture:600x600 - 277" | object type "M_Plain Recessed Lighting Fixture:600x600 - 277" | names: "M_Plain Recessed Lighting Fixture:600x600 - 277:431650", "M_Plain Recessed Lighting Fixture:600x600 - 277:431663", "M_Plain Recessed Lighting Fixture:600x600 - 277:431703" (+81 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          19 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "M_Pendant Light - Linear - 2 Lamp:1200mm - 277V" | object type "M_Pendant Light - Linear - 2 Lamp:1200mm - 277V" | names: "M_Pendant Light - Linear - 2 Lamp:1200mm - 277V:431863", "M_Pendant Light - Linear - 2 Lamp:1200mm - 277V:431864", "M_Pendant Light - Linear - 2 Lamp:1200mm - 277V:431865" (+16 more) | material: materials ("Metal - Paint Finish - Ivory, Glossy", "Glass - White, High Luminance") | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          65 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "M_Pendant Light - Disk:100W - 277V" | object type "M_Pendant Light - Disk:100W - 277V" | names: "M_Pendant Light - Disk:100W - 277V:433693", "M_Pendant Light - Disk:100W - 277V:433946", "M_Pendant Light - Disk:100W - 277V:433966" (+62 more) | material: materials ("Metal - Chrome", "Plastic - Blue", "Glass - Clear, Grey") | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          20 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "M_Sconce Light - Flat Round:60W - 277V" | object type "M_Sconce Light - Flat Round:60W - 277V" | names: "M_Sconce Light - Flat Round:60W - 277V:435210", "M_Sconce Light - Flat Round:60W - 277V:435288", "M_Sconce Light - Flat Round:60W - 277V:435295" (+17 more) | material: "Glass - Frosted" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          65 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "M_Pendant Light - Linear - 2 Lamp:2400mm - 277V" | object type "M_Pendant Light - Linear - 2 Lamp:2400mm - 277V" | names: "M_Pendant Light - Linear - 2 Lamp:2400mm - 277V:436700", "M_Pendant Light - Linear - 2 Lamp:2400mm - 277V:436786", "M_Pendant Light - Linear - 2 Lamp:2400mm - 277V:436813" (+62 more) | material: materials ("Metal - Paint Finish - Ivory, Glossy", "Glass - White, High Luminance") | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          21 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_Wall Occupancy Sensor - Regular Voltage:Passive Infrared - 277 V" | object type "M_Wall Occupancy Sensor - Regular Voltage:Passive Infrared - 277 V" | names: "M_Wall Occupancy Sensor - Regular Voltage:Passive Infrared - 277 V:438026", "M_Wall Occupancy Sensor - Regular Voltage:Passive Infrared - 277 V:438198", "M_Wall Occupancy Sensor - Regular Voltage:Passive Infrared - 277 V:438697" (+18 more) | material: materials ("<Unnamed>", "<Unnamed>") | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff, Pset_ProvisionForVoid
          4 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_Lighting Switches:Single Pole" | object type "M_Lighting Switches:Single Pole" | names: "M_Lighting Switches:Single Pole:438062", "M_Lighting Switches:Single Pole:440544", "M_Lighting Switches:Single Pole:440668" (+1 more) | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff, Pset_ProvisionForVoid
          4 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "M_Exhaust Grill:600 x 600 Face 300 x 300 Connection" | object type "M_Exhaust Grill:600 x 600 Face 300 x 300 Connection" | names: "M_Exhaust Grill:600 x 600 Face 300 x 300 Connection:442050", "M_Exhaust Grill:600 x 600 Face 300 x 300 Connection:442138", "M_Exhaust Grill:600 x 600 Face 300 x 300 Connection:521663" (+1 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_Lighting and Appliance Panelboard - 208V MLO - Surface:400 A" | object type "M_Lighting and Appliance Panelboard - 208V MLO - Surface:400 A" | names: "M_Lighting and Appliance Panelboard - 208V MLO - Surface:EP-2:471580", "M_Lighting and Appliance Panelboard - 208V MLO - Surface:PP-2B:471596" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff, Pset_ProvisionForVoid
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_Lighting and Appliance Panelboard - 480V MLO - Surface:400 A" | object type "M_Lighting and Appliance Panelboard - 480V MLO - Surface:400 A" | names: "M_Lighting and Appliance Panelboard - 480V MLO - Surface:LP-2:471705" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff, Pset_ProvisionForVoid
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Takeoff:Standard" | object type "M_Rectangular Duct Takeoff:Standard" | names: "M_Rectangular Duct Takeoff:Standard:479828" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          5 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Elbow - Mitered:Standard" | object type "M_Rectangular Duct Elbow - Mitered:Standard" | names: "M_Rectangular Duct Elbow - Mitered:Standard:483221", "M_Rectangular Duct Elbow - Mitered:Standard:483623", "M_Rectangular Duct Elbow - Mitered:Standard:483915" (+2 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          7 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Takeoff:Standard" | object type "M_Rectangular Duct Takeoff:Standard" | names: "M_Rectangular Duct Takeoff:Standard:483267", "M_Rectangular Duct Takeoff:Standard:483649", "M_Rectangular Duct Takeoff:Standard:483686" (+4 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          17 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Takeoff:Standard" | object type "M_Rectangular Duct Takeoff:Standard" | names: "M_Rectangular Duct Takeoff:Standard:483521", "M_Rectangular Duct Takeoff:Standard:483538", "M_Rectangular Duct Takeoff:Standard:483543" (+14 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          15 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Elbow - Mitered:Standard" | object type "M_Rectangular Duct Elbow - Mitered:Standard" | names: "M_Rectangular Duct Elbow - Mitered:Standard:483522", "M_Rectangular Duct Elbow - Mitered:Standard:483544", "M_Rectangular Duct Elbow - Mitered:Standard:483586" (+12 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          9 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Elbow - Mitered:Standard" | object type "M_Rectangular Duct Elbow - Mitered:Standard" | names: "M_Rectangular Duct Elbow - Mitered:Standard:483525", "M_Rectangular Duct Elbow - Mitered:Standard:483673", "M_Rectangular Duct Elbow - Mitered:Standard:483704" (+6 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:484029" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Right Return - Back Discharge:11 kW" | object type "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Right Return - Back Discharge:11 kW" | names: "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Right Return - Back Discharge:11 kW:484101" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Endcap:Standard" | object type "M_Rectangular Duct Endcap:Standard" | names: "M_Rectangular Duct Endcap:Standard:484336" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:484542", "M_Rectangular Duct Transition - Angle:45 Degree:484945" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:484881" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Takeoff:Standard" | object type "M_Rectangular Duct Takeoff:Standard" | names: "M_Rectangular Duct Takeoff:Standard:484903" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:485035" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Elbow - Mitered:Standard" | object type "M_Rectangular Duct Elbow - Mitered:Standard" | names: "M_Rectangular Duct Elbow - Mitered:Standard:507830", "M_Rectangular Duct Elbow - Mitered:Standard:507834" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          6 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Elbow - Mitered:Standard" | object type "M_Rectangular Duct Elbow - Mitered:Standard" | names: "M_Rectangular Duct Elbow - Mitered:Standard:520873", "M_Rectangular Duct Elbow - Mitered:Standard:520891", "M_Rectangular Duct Elbow - Mitered:Standard:521216" (+3 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          4 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Union:Standard" | object type "M_Rectangular Duct Union:Standard" | names: "M_Rectangular Duct Union:Standard:521369", "M_Rectangular Duct Union:Standard:521383", "M_Rectangular Duct Union:Standard:521391" (+1 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Elbow - Mitered:Standard" | object type "M_Rectangular Duct Elbow - Mitered:Standard" | names: "M_Rectangular Duct Elbow - Mitered:Standard:521506", "M_Rectangular Duct Elbow - Mitered:Standard:521510" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Elbow - Mitered:Standard" | object type "M_Rectangular Duct Elbow - Mitered:Standard" | names: "M_Rectangular Duct Elbow - Mitered:Standard:521634", "M_Rectangular Duct Elbow - Mitered:Standard:521637" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Takeoff:Standard" | object type "M_Rectangular Duct Takeoff:Standard" | names: "M_Rectangular Duct Takeoff:Standard:521986" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          3 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Elbow - Mitered:Standard" | object type "M_Rectangular Duct Elbow - Mitered:Standard" | names: "M_Rectangular Duct Elbow - Mitered:Standard:521988", "M_Rectangular Duct Elbow - Mitered:Standard:522040", "M_Rectangular Duct Elbow - Mitered:Standard:522043" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:522009" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          212 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "Tipos de tubería:Standard" | object type "Tipos de tubería:Standard" | names: "Tipos de tubería:Standard:529090", "Tipos de tubería:Standard:529091", "Tipos de tubería:Standard:529092" (+209 more) | property sets: Pset_DistributionFlowElementCommon, Pset_FlowSegmentDuctSegment, Pset_FlowSegmentPipeSegment, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Pipe Transition:Standard" | object type "M_Pipe Transition:Standard" | names: "M_Pipe Transition:Standard:529096" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          20 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Pipe Elbow:Standard" | object type "M_Pipe Elbow:Standard" | names: "M_Pipe Elbow:Standard:529097", "M_Pipe Elbow:Standard:529099", "M_Pipe Elbow:Standard:529102" (+17 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          10 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Pipe Transition:Standard" | object type "M_Pipe Transition:Standard" | names: "M_Pipe Transition:Standard:529113", "M_Pipe Transition:Standard:529126", "M_Pipe Transition:Standard:529152" (+7 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          25 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Pipe Elbow:Standard" | object type "M_Pipe Elbow:Standard" | names: "M_Pipe Elbow:Standard:529114", "M_Pipe Elbow:Standard:529116", "M_Pipe Elbow:Standard:529127" (+22 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          35 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Pipe Elbow:Standard" | object type "M_Pipe Elbow:Standard" | names: "M_Pipe Elbow:Standard:529179", "M_Pipe Elbow:Standard:529181", "M_Pipe Elbow:Standard:529188" (+32 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          5 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Pipe Tee:Standard" | object type "M_Pipe Tee:Standard" | names: "M_Pipe Tee:Standard:529259", "M_Pipe Tee:Standard:545865", "M_Pipe Tee:Standard:591797" (+2 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          6 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Pipe Tee:Standard" | object type "M_Pipe Tee:Standard" | names: "M_Pipe Tee:Standard:529267", "M_Pipe Tee:Standard:529272", "M_Pipe Tee:Standard:529315" (+3 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          6 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Pipe Transition:Standard" | object type "M_Pipe Transition:Standard" | names: "M_Pipe Transition:Standard:529269", "M_Pipe Transition:Standard:529270", "M_Pipe Transition:Standard:529274" (+3 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          14 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Pipe Tee:Standard" | object type "M_Pipe Tee:Standard" | names: "M_Pipe Tee:Standard:529284", "M_Pipe Tee:Standard:529290", "M_Pipe Tee:Standard:529295" (+11 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          12 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Pipe Transition:Standard" | object type "M_Pipe Transition:Standard" | names: "M_Pipe Transition:Standard:529286", "M_Pipe Transition:Standard:529292", "M_Pipe Transition:Standard:529293" (+9 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          6 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Pipe Transition:Standard" | object type "M_Pipe Transition:Standard" | names: "M_Pipe Transition:Standard:529732", "M_Pipe Transition:Standard:529733", "M_Pipe Transition:Standard:529737" (+3 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:531658" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Pipe Transition:Standard" | object type "M_Pipe Transition:Standard" | names: "M_Pipe Transition:Standard:532528", "M_Pipe Transition:Standard:532529" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Back Discharge:14 kW" | object type "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Back Discharge:14 kW" | names: "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Back Discharge:14 kW:536194" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
          4 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "M_Supply Diffuser - Rectangular Face Round Neck:600x600 - 250 Neck" | object type "M_Supply Diffuser - Rectangular Face Round Neck:600x600 - 250 Neck" | names: "M_Supply Diffuser - Rectangular Face Round Neck:600x600 - 250 Neck:536266", "M_Supply Diffuser - Rectangular Face Round Neck:600x600 - 250 Neck:536319", "M_Supply Diffuser - Rectangular Face Round Neck:600x600 - 250 Neck:536336" (+1 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Elbow - Mitered:Standard" | object type "M_Rectangular Duct Elbow - Mitered:Standard" | names: "M_Rectangular Duct Elbow - Mitered:Standard:536435" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          8 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "Conducto redondo:Taps" | object type "Conducto redondo:Taps" | names: "Conducto redondo:Taps:536476", "Conducto redondo:Taps:536520", "Conducto redondo:Taps:536547" (+5 more) | property sets: Pset_DistributionFlowElementCommon, Pset_DuctSegmentTypeCommon, Pset_FlowSegmentDuctSegment, Pset_FlowSegmentPipeSegment, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Round Duct Takeoff:Standard" | object type "M_Round Duct Takeoff:Standard" | names: "M_Round Duct Takeoff:Standard:536489", "M_Round Duct Takeoff:Standard:536560" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          4 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Round Duct Takeoff:Standard" | object type "M_Round Duct Takeoff:Standard" | names: "M_Round Duct Takeoff:Standard:536533", "M_Round Duct Takeoff:Standard:976804", "M_Round Duct Takeoff:Standard:976808" (+1 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Round Duct Takeoff:Standard" | object type "M_Round Duct Takeoff:Standard" | names: "M_Round Duct Takeoff:Standard:536656" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Round Duct Takeoff:Standard" | object type "M_Round Duct Takeoff:Standard" | names: "M_Round Duct Takeoff:Standard:536672" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Round Duct Transition - Angle:45 Degree" | object type "M_Round Duct Transition - Angle:45 Degree" | names: "M_Round Duct Transition - Angle:45 Degree:536733", "M_Round Duct Transition - Angle:45 Degree:536814" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:536812" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:536813" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:536816" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "M_Supply Diffuser - Rectangular Face Round Neck:600x600 - 200 Neck" | object type "M_Supply Diffuser - Rectangular Face Round Neck:600x600 - 200 Neck" | names: "M_Supply Diffuser - Rectangular Face Round Neck:600x600 - 200 Neck:536867" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "M_Supply Diffuser - Rectangular Face Round Neck:600x600 - 200 Neck" | object type "M_Supply Diffuser - Rectangular Face Round Neck:600x600 - 200 Neck" | names: "M_Supply Diffuser - Rectangular Face Round Neck:600x600 - 200 Neck:536984" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          3 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "M_Supply Diffuser - Rectangular Face Round Neck:600x600 - 200 Neck" | object type "M_Supply Diffuser - Rectangular Face Round Neck:600x600 - 200 Neck" | names: "M_Supply Diffuser - Rectangular Face Round Neck:600x600 - 200 Neck:536994", "M_Supply Diffuser - Rectangular Face Round Neck:600x600 - 200 Neck:537002", "M_Supply Diffuser - Rectangular Face Round Neck:600x600 - 200 Neck:537010" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Back Discharge:11 kW" | object type "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Back Discharge:11 kW" | names: "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Back Discharge:11 kW:537029" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:539500" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Elbow - Mitered:Standard" | object type "M_Rectangular Duct Elbow - Mitered:Standard" | names: "M_Rectangular Duct Elbow - Mitered:Standard:539501" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          5 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular to Round Duct Transition - Angle:45 Degree" | object type "M_Rectangular to Round Duct Transition - Angle:45 Degree" | names: "M_Rectangular to Round Duct Transition - Angle:45 Degree:539513", "M_Rectangular to Round Duct Transition - Angle:45 Degree:539523", "M_Rectangular to Round Duct Transition - Angle:45 Degree:539533" (+2 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Elbow - Mitered:Standard" | object type "M_Rectangular Duct Elbow - Mitered:Standard" | names: "M_Rectangular Duct Elbow - Mitered:Standard:539514", "M_Rectangular Duct Elbow - Mitered:Standard:539534" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Tee:Standard" | object type "M_Rectangular Duct Tee:Standard" | names: "M_Rectangular Duct Tee:Standard:539559", "M_Rectangular Duct Tee:Standard:539562" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          3 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:539564", "M_Rectangular Duct Transition - Angle:45 Degree:539569", "M_Rectangular Duct Transition - Angle:45 Degree:539574" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Tee:Standard" | object type "M_Rectangular Duct Tee:Standard" | names: "M_Rectangular Duct Tee:Standard:539566", "M_Rectangular Duct Tee:Standard:539572" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:539570", "M_Rectangular Duct Transition - Angle:45 Degree:539575" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          5 x IFCFLOWTERMINAL | type IFCDISTRIBUTIONELEMENTTYPE "M_Water Closet - Flush Valve - Wall Mounted:Public - 6.1 Lpf" | object type "M_Water Closet - Flush Valve - Wall Mounted:Public - 6.1 Lpf" | names: "M_Water Closet - Flush Valve - Wall Mounted:Public - 6.1 Lpf:543273", "M_Water Closet - Flush Valve - Wall Mounted:Public - 6.1 Lpf:543313", "M_Water Closet - Flush Valve - Wall Mounted:Public - 6.1 Lpf:543332" (+2 more) | material: materials ("<Unnamed>", "<Unnamed>", "<Unnamed>") | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWTERMINAL | type IFCDISTRIBUTIONELEMENTTYPE "M_Urinal - Wall Hung:20 mm Flush Valve" | object type "M_Urinal - Wall Hung:20 mm Flush Valve" | names: "M_Urinal - Wall Hung:20 mm Flush Valve:543319", "M_Urinal - Wall Hung:20 mm Flush Valve:593903" | material: materials ("<Unnamed>", "<Unnamed>") | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          4 x IFCFLOWTERMINAL | type IFCDISTRIBUTIONELEMENTTYPE "M_Lavatory - Wall Mounted:485 mmx355 mm - Public" | object type "M_Lavatory - Wall Mounted:485 mmx355 mm - Public" | names: "M_Lavatory - Wall Mounted:485 mmx355 mm - Public:543393", "M_Lavatory - Wall Mounted:485 mmx355 mm - Public:543403", "M_Lavatory - Wall Mounted:485 mmx355 mm - Public:543504" (+1 more) | material: materials ("<Unnamed>", "<Unnamed>") | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          6 x IFCFLOWTERMINAL | type IFCFIRESUPPRESSIONTERMINALTYPE "M_Sprinkler - Pendent - Hosted:15 mm Pendent on Drop with Guard" | object type "M_Sprinkler - Pendent - Hosted:15 mm Pendent on Drop with Guard" | names: "M_Sprinkler - Pendent - Hosted:15 mm Pendent on Drop with Guard:545673", "M_Sprinkler - Pendent - Hosted:15 mm Pendent on Drop with Guard:545696", "M_Sprinkler - Pendent - Hosted:15 mm Pendent on Drop with Guard:545726" (+3 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Pipe Cross:Standard" | object type "M_Pipe Cross:Standard" | names: "M_Pipe Cross:Standard:545863" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          7 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Muro básico:STB 20.0" | object type "Muro básico:STB 20.0" | names: "Muro básico:STB 20.0:573378", "Muro básico:STB 20.0:573379", "Muro básico:STB 20.0:573380" (+4 more) | material: layers "Muro básico:STB 20.0" ("Stahlbeton - Ortbeton" 200.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          29 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Muro básico:MW 11.5" | object type "Muro básico:MW 11.5" | names: "Muro básico:MW 11.5:573383", "Muro básico:MW 11.5:573731", "Muro básico:MW 11.5:573732" (+26 more) | material: layers "Muro básico:MW 11.5" ("Mauerwerk - Ziegel" 115.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Muro básico:STB 30.0" | object type "Muro básico:STB 30.0" | names: "Muro básico:STB 30.0:573384", "Muro básico:STB 30.0:573385", "Muro básico:STB 30.0:573387" | material: layers "Muro básico:STB 30.0" ("Stahlbeton - Ortbeton" 300.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:STB 30.0" | object type "Suelo:STB 30.0" | FLOOR | names: "Suelo:STB 30.0:573390" | material: layers "Suelo:STB 30.0" ("Stahlbeton - Ortbeton" 300.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          37 x IFCCOLUMN | type IFCCOLUMNTYPE "STB Stütze - rund:STB d=30" | object type "STB Stütze - rund:STB d=30" | names: "STB Stütze - rund:STB d=30:573463", "STB Stütze - rund:STB d=30:573464", "STB Stütze - rund:STB d=30:573465" (+34 more) | material: "Stahlbeton - Fertigbeton" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          2 x IFCCOLUMN | type IFCCOLUMNTYPE "STB Stütze - rund:STB d=30" | object type "STB Stütze - rund:STB d=30" | names: "STB Stütze - rund:STB d=30:573481", "STB Stütze - rund:STB d=30:577498" | material: "Stahlbeton - Fertigbeton" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "STB Stütze - rund:STB d=30" | object type "STB Stütze - rund:STB d=30" | names: "STB Stütze - rund:STB d=30:573495" | material: "Stahlbeton - Fertigbeton" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "STB Stütze - rund:STB d=30" | object type "STB Stütze - rund:STB d=30" | names: "STB Stütze - rund:STB d=30:573496" | material: "Stahlbeton - Fertigbeton" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "STB Stütze - rund:STB d=30" | object type "STB Stütze - rund:STB d=30" | names: "STB Stütze - rund:STB d=30:573503" | material: "Stahlbeton - Fertigbeton" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "STB Stütze - rund:STB d=30" | object type "STB Stütze - rund:STB d=30" | names: "STB Stütze - rund:STB d=30:573504" | material: "Stahlbeton - Fertigbeton" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          8 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Muro cortina:Standard" | object type "Muro cortina:Standard" | names: "Muro cortina:Standard:573660", "Muro cortina:Standard:573664", "Muro cortina:Standard:575890" (+5 more) | parts: 111 IFCMEMBER, 32 IFCPLATE, 6 IFCDOOR | property sets: Pset_CurtainWallCommon, Pset_QuantityTakeOff
          9 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Muro básico:MW 17.5" | object type "Muro básico:MW 17.5" | names: "Muro básico:MW 17.5:573689", "Muro básico:MW 17.5:573690", "Muro básico:MW 17.5:573691" (+6 more) | material: layers "Muro básico:MW 17.5" ("Mauerwerk - Ziegel" 175.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          6 x IFCDOOR | type IFCDOORSTYLE "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26" | object type "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26" | names: "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26:573692", "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26:573693", "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26:573694" (+3 more) | material: materials ("Tür - Stahl Griff", "Tür - Stahl Zarge") | property sets: Pset_DoorCommon, Pset_QuantityTakeOff
          2 x IFCDOOR | type IFCDOORSTYLE "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26" | object type "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26" | names: "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26:573698", "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26:573699" | material: materials ("Tür - Stahl Griff", "Tür - Stahl Zarge") | property sets: Pset_DoorCommon, Pset_QuantityTakeOff
          4 x IFCDOOR | type IFCDOORSTYLE "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26" | object type "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26" | names: "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26:573747", "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26:573749", "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26:577823" (+1 more) | material: materials ("Tür - Stahl Griff", "Tür - Stahl Zarge") | property sets: Pset_DoorCommon, Pset_QuantityTakeOff
          4 x IFCDOOR | type IFCDOORSTYLE "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26" | object type "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26" | names: "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26:573748", "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26:573757", "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26:573760" (+1 more) | material: materials ("Tür - Stahl Griff", "Tür - Stahl Zarge") | property sets: Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26" | object type "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26" | names: "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26:573750" | material: materials ("Tür - Stahl Griff", "Tür - Stahl Zarge") | property sets: Pset_DoorCommon, Pset_QuantityTakeOff
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Muro básico:WC Trennwand 5.0" | object type "Muro básico:WC Trennwand 5.0" | names: "Muro básico:WC Trennwand 5.0:573751", "Muro básico:WC Trennwand 5.0:578639", "Muro básico:WC Trennwand 5.0:578640" | material: layers "Muro básico:WC Trennwand 5.0" ("WC Trennwand" 50.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          6 x IFCDOOR | type IFCDOORSTYLE "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26" | object type "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26" | names: "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26:573758", "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26:573759", "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26:573761" (+3 more) | material: materials ("Tür - Stahl Griff", "Tür - Stahl Zarge") | property sets: Pset_DoorCommon, Pset_QuantityTakeOff
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Muro básico:Lamelle 11.5" | object type "Muro básico:Lamelle 11.5" | names: "Muro básico:Lamelle 11.5:575419", "Muro básico:Lamelle 11.5:575883" | material: layers "Muro básico:Lamelle 11.5" ("Mauerwerk - Lamellen" 115.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          6 x IFCDOOR | type IFCDOORSTYLE "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26" | object type "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26" | names: "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26:575420", "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26:575421", "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26:575423" (+3 more) | material: materials ("Tür - Stahl Griff", "Tür - Stahl Zarge") | property sets: Pset_DoorCommon, Pset_QuantityTakeOff
          7 x IFCDOOR | type IFCDOORSTYLE "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26" | object type "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26" | names: "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26:575422", "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26:575424", "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26:575425" (+4 more) | material: materials ("Tür - Stahl Griff", "Tür - Stahl Zarge") | property sets: Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Aufzug 2-flg:Aufzug 2-flg" | object type "Aufzug 2-flg:Aufzug 2-flg" | names: "Aufzug 2-flg:Aufzug 2-flg:575428" | material: "Tür - Aufzug Metall" | property sets: Pset_OpeningElementCommon, Pset_QuantityTakeOff
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:FB 15.0 - Fliesen 50 x 50" | object type "Suelo:FB 15.0 - Fliesen 50 x 50" | FLOOR | names: "Suelo:FB 15.0 - Fliesen 50 x 50:576071" | material: layers "Suelo:FB 15.0 - Fliesen 50 x 50" ("Bodenbelag Fliesen 50 x 50" 10., "Decke - Estrich" 60., "Wärmedämmung - hart" 80.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          3 x IFCSTAIR | object type "Escalera:Massiv - Stufen Naturstein" | names: "Escalera:Massiv - Stufen Naturstein:576926", "Escalera:Massiv - Stufen Naturstein:577000", "Escalera:Massiv - Stufen Naturstein:579611" | parts: 4 IFCRAILING, 4 IFCSTAIRFLIGHT, 2 IFCSLAB, 1 IFCSTAIR | property sets: Pset_QuantityTakeOff, Pset_StairCommon
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "STB Stütze - rund:STB d=30" | object type "STB Stütze - rund:STB d=30" | names: "STB Stütze - rund:STB d=30:577497" | material: "Stahlbeton - Fertigbeton" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          66 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Stahlbalkon:Stahlbalkon" | object type "Stahlbalkon:Stahlbalkon" | names: "Stahlbalkon:Stahlbalkon:577533", "Stahlbalkon:Stahlbalkon:577535", "Stahlbalkon:Stahlbalkon:577536" (+63 more) | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff, Pset_ProvisionForVoid
          15 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Stahlbalkon:Stahlbalkon" | object type "Stahlbalkon:Stahlbalkon" | names: "Stahlbalkon:Stahlbalkon:577538", "Stahlbalkon:Stahlbalkon:577539", "Stahlbalkon:Stahlbalkon:577540" (+12 more) | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff, Pset_ProvisionForVoid
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:Sonnenschutz" | object type "Suelo:Sonnenschutz" | FLOOR | names: "Suelo:Sonnenschutz:577552" | material: layers "Suelo:Sonnenschutz" ("Gitterrost" 100.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:Sonnenschutz" | object type "Suelo:Sonnenschutz" | FLOOR | names: "Suelo:Sonnenschutz:577552:2" | material: layers "Suelo:Sonnenschutz" ("Gitterrost" 100.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:Sonnenschutz" | object type "Suelo:Sonnenschutz" | FLOOR | names: "Suelo:Sonnenschutz:577552:3" | material: layers "Suelo:Sonnenschutz" ("Gitterrost" 100.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:Sonnenschutz" | object type "Suelo:Sonnenschutz" | FLOOR | names: "Suelo:Sonnenschutz:577552:4" | material: layers "Suelo:Sonnenschutz" ("Gitterrost" 100.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:Sonnenschutz" | object type "Suelo:Sonnenschutz" | FLOOR | names: "Suelo:Sonnenschutz:577552:5" | material: layers "Suelo:Sonnenschutz" ("Gitterrost" 100.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:Sonnenschutz" | object type "Suelo:Sonnenschutz" | FLOOR | names: "Suelo:Sonnenschutz:577552:6" | material: layers "Suelo:Sonnenschutz" ("Gitterrost" 100.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Texto de modelo:Logo" | object type "Texto de modelo:Logo" | names: "Texto de modelo:Logo:577821" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff, Pset_ProvisionForVoid
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:FB 15.0 - Holzdielen" | object type "Suelo:FB 15.0 - Holzdielen" | FLOOR | names: "Suelo:FB 15.0 - Holzdielen:578097" | material: layers "Suelo:FB 15.0 - Holzdielen" ("Bodenbelag Holzdielen" 30., "Decke - Estrich" 40., "Default Floor" 80.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:FB 15.0 - Holzdielen" | object type "Suelo:FB 15.0 - Holzdielen" | FLOOR | names: "Suelo:FB 15.0 - Holzdielen:578407" | material: layers "Suelo:FB 15.0 - Holzdielen" ("Bodenbelag Holzdielen" 30., "Decke - Estrich" 40., "Default Floor" 80.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:FB 15.0 - Teppich" | object type "Suelo:FB 15.0 - Teppich" | FLOOR | names: "Suelo:FB 15.0 - Teppich:578433" | material: layers "Suelo:FB 15.0 - Teppich" ("Bodenbelag Teppich" 10., "Decke - Estrich" 60., "Wärmedämmung - hart" 80.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:FB 15.0 - Teppich" | object type "Suelo:FB 15.0 - Teppich" | FLOOR | names: "Suelo:FB 15.0 - Teppich:578433:2" | material: layers "Suelo:FB 15.0 - Teppich" ("Bodenbelag Teppich" 10., "Decke - Estrich" 60., "Wärmedämmung - hart" 80.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:FB 15.0 - Teppich" | object type "Suelo:FB 15.0 - Teppich" | FLOOR | names: "Suelo:FB 15.0 - Teppich:578433:3" | material: layers "Suelo:FB 15.0 - Teppich" ("Bodenbelag Teppich" 10., "Decke - Estrich" 60., "Wärmedämmung - hart" 80.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:FB 15.0 - Teppich" | object type "Suelo:FB 15.0 - Teppich" | FLOOR | names: "Suelo:FB 15.0 - Teppich:578433:4" | material: layers "Suelo:FB 15.0 - Teppich" ("Bodenbelag Teppich" 10., "Decke - Estrich" 60., "Wärmedämmung - hart" 80.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:FB 15.0 - Teppich" | object type "Suelo:FB 15.0 - Teppich" | FLOOR | names: "Suelo:FB 15.0 - Teppich:578433:5" | material: layers "Suelo:FB 15.0 - Teppich" ("Bodenbelag Teppich" 10., "Decke - Estrich" 60., "Wärmedämmung - hart" 80.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:FB 15.0 - Teppich" | object type "Suelo:FB 15.0 - Teppich" | FLOOR | names: "Suelo:FB 15.0 - Teppich:578433:6" | material: layers "Suelo:FB 15.0 - Teppich" ("Bodenbelag Teppich" 10., "Decke - Estrich" 60., "Wärmedämmung - hart" 80.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:FB 15.0 - Teppich" | object type "Suelo:FB 15.0 - Teppich" | FLOOR | names: "Suelo:FB 15.0 - Teppich:578433:7" | material: layers "Suelo:FB 15.0 - Teppich" ("Bodenbelag Teppich" 10., "Decke - Estrich" 60., "Wärmedämmung - hart" 80.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:FB 15.0 - Teppich" | object type "Suelo:FB 15.0 - Teppich" | FLOOR | names: "Suelo:FB 15.0 - Teppich:578433:8" | material: layers "Suelo:FB 15.0 - Teppich" ("Bodenbelag Teppich" 10., "Decke - Estrich" 60., "Wärmedämmung - hart" 80.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:FB 15.0 - Teppich" | object type "Suelo:FB 15.0 - Teppich" | FLOOR | names: "Suelo:FB 15.0 - Teppich:578433:9" | material: layers "Suelo:FB 15.0 - Teppich" ("Bodenbelag Teppich" 10., "Decke - Estrich" 60., "Wärmedämmung - hart" 80.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:FB 15.0 - Teppich" | object type "Suelo:FB 15.0 - Teppich" | FLOOR | names: "Suelo:FB 15.0 - Teppich:578433:10" | material: layers "Suelo:FB 15.0 - Teppich" ("Bodenbelag Teppich" 10., "Decke - Estrich" 60., "Wärmedämmung - hart" 80.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:FB 15.0 - Teppich" | object type "Suelo:FB 15.0 - Teppich" | FLOOR | names: "Suelo:FB 15.0 - Teppich:578433:11" | material: layers "Suelo:FB 15.0 - Teppich" ("Bodenbelag Teppich" 10., "Decke - Estrich" 60., "Wärmedämmung - hart" 80.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:FB 15.0 - Teppich" | object type "Suelo:FB 15.0 - Teppich" | FLOOR | names: "Suelo:FB 15.0 - Teppich:578433:12" | material: layers "Suelo:FB 15.0 - Teppich" ("Bodenbelag Teppich" 10., "Decke - Estrich" 60., "Wärmedämmung - hart" 80.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:FB 15.0 - Teppich" | object type "Suelo:FB 15.0 - Teppich" | FLOOR | names: "Suelo:FB 15.0 - Teppich:578433:13" | material: layers "Suelo:FB 15.0 - Teppich" ("Bodenbelag Teppich" 10., "Decke - Estrich" 60., "Wärmedämmung - hart" 80.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:FB 15.0 - Teppich" | object type "Suelo:FB 15.0 - Teppich" | FLOOR | names: "Suelo:FB 15.0 - Teppich:578433:14" | material: layers "Suelo:FB 15.0 - Teppich" ("Bodenbelag Teppich" 10., "Decke - Estrich" 60., "Wärmedämmung - hart" 80.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:FB 15.0 - Teppich" | object type "Suelo:FB 15.0 - Teppich" | FLOOR | names: "Suelo:FB 15.0 - Teppich:578433:15" | material: layers "Suelo:FB 15.0 - Teppich" ("Bodenbelag Teppich" 10., "Decke - Estrich" 60., "Wärmedämmung - hart" 80.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:FB 15.0 - Teppich" | object type "Suelo:FB 15.0 - Teppich" | FLOOR | names: "Suelo:FB 15.0 - Teppich:578433:16" | material: layers "Suelo:FB 15.0 - Teppich" ("Bodenbelag Teppich" 10., "Decke - Estrich" 60., "Wärmedämmung - hart" 80.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:FB 15.0 - Teppich" | object type "Suelo:FB 15.0 - Teppich" | FLOOR | names: "Suelo:FB 15.0 - Teppich:578433:17" | material: layers "Suelo:FB 15.0 - Teppich" ("Bodenbelag Teppich" 10., "Decke - Estrich" 60., "Wärmedämmung - hart" 80.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:FB 15.0 - Teppich" | object type "Suelo:FB 15.0 - Teppich" | FLOOR | names: "Suelo:FB 15.0 - Teppich:578433:18" | material: layers "Suelo:FB 15.0 - Teppich" ("Bodenbelag Teppich" 10., "Decke - Estrich" 60., "Wärmedämmung - hart" 80.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:FB 10.0 - Fliesen 15 x 15" | object type "Suelo:FB 10.0 - Fliesen 15 x 15" | FLOOR | names: "Suelo:FB 10.0 - Fliesen 15 x 15:578586" | material: layers "Suelo:FB 10.0 - Fliesen 15 x 15" ("Decke - Fliesen 15 x 15" 10., "Decke - Estrich" 60., "Wärmedämmung - hart" 80.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:FB 10.0 - Fliesen 15 x 15" | object type "Suelo:FB 10.0 - Fliesen 15 x 15" | FLOOR | names: "Suelo:FB 10.0 - Fliesen 15 x 15:578586:2" | material: layers "Suelo:FB 10.0 - Fliesen 15 x 15" ("Decke - Fliesen 15 x 15" 10., "Decke - Estrich" 60., "Wärmedämmung - hart" 80.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:FB 10.0 - Fliesen 15 x 15" | object type "Suelo:FB 10.0 - Fliesen 15 x 15" | FLOOR | names: "Suelo:FB 10.0 - Fliesen 15 x 15:578586:3" | material: layers "Suelo:FB 10.0 - Fliesen 15 x 15" ("Decke - Fliesen 15 x 15" 10., "Decke - Estrich" 60., "Wärmedämmung - hart" 80.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:FB 10.0 - Fliesen 15 x 15" | object type "Suelo:FB 10.0 - Fliesen 15 x 15" | FLOOR | names: "Suelo:FB 10.0 - Fliesen 15 x 15:578586:4" | material: layers "Suelo:FB 10.0 - Fliesen 15 x 15" ("Decke - Fliesen 15 x 15" 10., "Decke - Estrich" 60., "Wärmedämmung - hart" 80.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:FB 10.0 - Fliesen 15 x 15" | object type "Suelo:FB 10.0 - Fliesen 15 x 15" | FLOOR | names: "Suelo:FB 10.0 - Fliesen 15 x 15:578586:5" | material: layers "Suelo:FB 10.0 - Fliesen 15 x 15" ("Decke - Fliesen 15 x 15" 10., "Decke - Estrich" 60., "Wärmedämmung - hart" 80.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          2 x IFCDOOR | type IFCDOORSTYLE "Drehflügel 1-flg - Stahlzarge:76 x 2.26" | object type "Drehflügel 1-flg - Stahlzarge:76 x 2.26" | names: "Drehflügel 1-flg - Stahlzarge:76 x 2.26:578641", "Drehflügel 1-flg - Stahlzarge:76 x 2.26:578642" | material: materials ("Tür - Stahl Griff", "Tür - Stahl Zarge") | property sets: Pset_DoorCommon, Pset_QuantityTakeOff
          2 x IFCDOOR | type IFCDOORSTYLE "Drehflügel 1-flg - Stahlzarge:76 x 2.26" | object type "Drehflügel 1-flg - Stahlzarge:76 x 2.26" | names: "Drehflügel 1-flg - Stahlzarge:76 x 2.26:578643", "Drehflügel 1-flg - Stahlzarge:76 x 2.26:578644" | material: materials ("Tür - Stahl Griff", "Tür - Stahl Zarge") | property sets: Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:FB 15.0 - Holzdielen" | object type "Suelo:FB 15.0 - Holzdielen" | FLOOR | names: "Suelo:FB 15.0 - Holzdielen:578704" | material: layers "Suelo:FB 15.0 - Holzdielen" ("Bodenbelag Holzdielen" 30., "Decke - Estrich" 40., "Default Floor" 80.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:FB 15.0 - Holzdielen" | object type "Suelo:FB 15.0 - Holzdielen" | FLOOR | names: "Suelo:FB 15.0 - Holzdielen:578704:2" | material: layers "Suelo:FB 15.0 - Holzdielen" ("Bodenbelag Holzdielen" 30., "Decke - Estrich" 40., "Default Floor" 80.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | object type "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | CEILING | names: "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600:580427" | material: layers "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" ("Decke - Gipskarton" 20., "Decke - Deckenraster" 30.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | object type "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | CEILING | names: "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600:580450" | material: layers "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" ("Decke - Gipskarton" 20., "Decke - Deckenraster" 30.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | object type "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | CEILING | names: "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600:580461" | material: layers "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" ("Decke - Gipskarton" 20., "Decke - Deckenraster" 30.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | object type "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | CEILING | names: "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600:580472" | material: layers "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" ("Decke - Gipskarton" 20., "Decke - Deckenraster" 30.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | object type "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | CEILING | names: "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600:580483" | material: layers "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" ("Decke - Gipskarton" 20., "Decke - Deckenraster" 30.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | object type "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | CEILING | names: "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600:580494" | material: layers "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" ("Decke - Gipskarton" 20., "Decke - Deckenraster" 30.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | object type "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | CEILING | names: "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600:580505" | material: layers "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" ("Decke - Gipskarton" 20., "Decke - Deckenraster" 30.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | object type "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | CEILING | names: "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600:580516" | material: layers "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" ("Decke - Gipskarton" 20., "Decke - Deckenraster" 30.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | object type "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | CEILING | names: "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600:580527" | material: layers "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" ("Decke - Gipskarton" 20., "Decke - Deckenraster" 30.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | object type "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | CEILING | names: "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600:580538" | material: layers "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" ("Decke - Gipskarton" 20., "Decke - Deckenraster" 30.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | object type "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | CEILING | names: "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600:580545" | material: layers "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" ("Decke - Gipskarton" 20., "Decke - Deckenraster" 30.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | object type "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | CEILING | names: "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600:580556" | material: layers "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" ("Decke - Gipskarton" 20., "Decke - Deckenraster" 30.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | object type "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | CEILING | names: "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600:580567" | material: layers "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" ("Decke - Gipskarton" 20., "Decke - Deckenraster" 30.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | object type "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | CEILING | names: "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600:580582" | material: layers "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" ("Decke - Gipskarton" 20., "Decke - Deckenraster" 30.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | object type "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | CEILING | names: "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600:580593" | material: layers "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" ("Decke - Gipskarton" 20., "Decke - Deckenraster" 30.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | object type "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | CEILING | names: "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600:580604" | material: layers "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" ("Decke - Gipskarton" 20., "Decke - Deckenraster" 30.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | object type "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | CEILING | names: "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600:580619" | material: layers "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" ("Decke - Gipskarton" 20., "Decke - Deckenraster" 30.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | object type "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | CEILING | names: "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600:580634" | material: layers "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" ("Decke - Gipskarton" 20., "Decke - Deckenraster" 30.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | object type "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | CEILING | names: "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600:580645" | material: layers "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" ("Decke - Gipskarton" 20., "Decke - Deckenraster" 30.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | object type "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | CEILING | names: "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600:580656" | material: layers "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" ("Decke - Gipskarton" 20., "Decke - Deckenraster" 30.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | object type "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | CEILING | names: "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600:580667" | material: layers "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" ("Decke - Gipskarton" 20., "Decke - Deckenraster" 30.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | object type "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | CEILING | names: "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600:580678" | material: layers "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" ("Decke - Gipskarton" 20., "Decke - Deckenraster" 30.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | object type "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | CEILING | names: "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600:580689" | material: layers "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" ("Decke - Gipskarton" 20., "Decke - Deckenraster" 30.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | object type "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | CEILING | names: "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600:580700" | material: layers "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" ("Decke - Gipskarton" 20., "Decke - Deckenraster" 30.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | object type "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | CEILING | names: "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600:580711" | material: layers "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" ("Decke - Gipskarton" 20., "Decke - Deckenraster" 30.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_Water Heater - Tankless:2.3 L" | object type "M_Water Heater - Tankless:2.3 L" | names: "M_Water Heater - Tankless:2.3 L:591320" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          5 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Pipe Tee:Standard" | object type "M_Pipe Tee:Standard" | names: "M_Pipe Tee:Standard:593147", "M_Pipe Tee:Standard:593669", "M_Pipe Tee:Standard:593958" (+2 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Pipe Transition:Standard" | object type "M_Pipe Transition:Standard" | names: "M_Pipe Transition:Standard:593151" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          5 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Pipe Elbow:Standard" | object type "M_Pipe Elbow:Standard" | names: "M_Pipe Elbow:Standard:593407", "M_Pipe Elbow:Standard:593558", "M_Pipe Elbow:Standard:594380" (+2 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Pipe Transition:Standard" | object type "M_Pipe Transition:Standard" | names: "M_Pipe Transition:Standard:593673", "M_Pipe Transition:Standard:593962" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Pipe Cross:Standard" | object type "M_Pipe Cross:Standard" | names: "M_Pipe Cross:Standard:594020" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Pipe Elbow:Standard" | object type "M_Pipe Elbow:Standard" | names: "M_Pipe Elbow:Standard:594561" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Pipe Tee:Standard" | object type "M_Pipe Tee:Standard" | names: "M_Pipe Tee:Standard:595371" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Tee - Generic:Standard" | object type "M_Tee - Generic:Standard" | names: "M_Tee - Generic:Standard:605110", "M_Tee - Generic:Standard:818204" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          4 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Tee Sanitary - PVC - Sch 40 - DWV:Standard" | object type "M_Tee Sanitary - PVC - Sch 40 - DWV:Standard" | names: "M_Tee Sanitary - PVC - Sch 40 - DWV:Standard:605224", "M_Tee Sanitary - PVC - Sch 40 - DWV:Standard:605237", "M_Tee Sanitary - PVC - Sch 40 - DWV:Standard:605738" (+1 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          4 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Pipe Transition:Standard" | object type "M_Pipe Transition:Standard" | names: "M_Pipe Transition:Standard:605227", "M_Pipe Transition:Standard:605228", "M_Pipe Transition:Standard:605239" (+1 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Bend - PVC - Sch 40 - DWV:Standard" | object type "M_Bend - PVC - Sch 40 - DWV:Standard" | names: "M_Bend - PVC - Sch 40 - DWV:Standard:605388" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Transition - Generic:Standard" | object type "M_Transition - Generic:Standard" | names: "M_Transition - Generic:Standard:605740" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Bend - PVC - Sch 40 - DWV:Standard" | object type "M_Bend - PVC - Sch 40 - DWV:Standard" | names: "M_Bend - PVC - Sch 40 - DWV:Standard:606536" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Bend - PVC - Sch 40 - DWV:Standard" | object type "M_Bend - PVC - Sch 40 - DWV:Standard" | names: "M_Bend - PVC - Sch 40 - DWV:Standard:606539" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Bend - PVC - Sch 40 - DWV:Standard" | object type "M_Bend - PVC - Sch 40 - DWV:Standard" | names: "M_Bend - PVC - Sch 40 - DWV:Standard:606548" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Bend - PVC - Sch 40 - DWV:Standard" | object type "M_Bend - PVC - Sch 40 - DWV:Standard" | names: "M_Bend - PVC - Sch 40 - DWV:Standard:606559" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Bend - PVC - Sch 40 - DWV:Standard" | object type "M_Bend - PVC - Sch 40 - DWV:Standard" | names: "M_Bend - PVC - Sch 40 - DWV:Standard:606564" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Transition - Generic:Standard" | object type "M_Transition - Generic:Standard" | names: "M_Transition - Generic:Standard:606586" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_Lighting and Appliance Panelboard - 480V MCB - Surface:100 A" | object type "M_Lighting and Appliance Panelboard - 480V MCB - Surface:100 A" | names: "M_Lighting and Appliance Panelboard - 480V MCB - Surface:LP-2B:625731", "M_Lighting and Appliance Panelboard - 480V MCB - Surface:MP-2B:625733" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff, Pset_ProvisionForVoid
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_Lighting and Appliance Panelboard - 208V MCB - Surface:100 A" | object type "M_Lighting and Appliance Panelboard - 208V MCB - Surface:100 A" | names: "M_Lighting and Appliance Panelboard - 208V MCB - Surface:PP-2A:625734" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff, Pset_ProvisionForVoid
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_Dry Type Transformer - 480-208Y120 - NEMA Type 3R:15 kVA" | object type "M_Dry Type Transformer - 480-208Y120 - NEMA Type 3R:15 kVA" | names: "M_Dry Type Transformer - 480-208Y120 - NEMA Type 3R:TP-2A:625735" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "Conduit Body - Type L - Aluminum:Standard" | object type "Conduit Body - Type L - Aluminum:Standard" | names: "Conduit Body - Type L - Aluminum:Standard:687956" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          4 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Tee - Generic:Standard" | object type "M_Tee - Generic:Standard" | names: "M_Tee - Generic:Standard:711660", "M_Tee - Generic:Standard:711712", "M_Tee - Generic:Standard:711766" (+1 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          4 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Transition - Generic:Standard" | object type "M_Transition - Generic:Standard" | names: "M_Transition - Generic:Standard:711664", "M_Transition - Generic:Standard:711716", "M_Transition - Generic:Standard:711770" (+1 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Pipe Tee:Standard" | object type "M_Pipe Tee:Standard" | names: "M_Pipe Tee:Standard:812969" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Elbow - Generic:Standard" | object type "M_Elbow - Generic:Standard" | names: "M_Elbow - Generic:Standard:812982" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          7 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Elbow - Generic:Standard" | object type "M_Elbow - Generic:Standard" | names: "M_Elbow - Generic:Standard:813093", "M_Elbow - Generic:Standard:816090", "M_Elbow - Generic:Standard:816092" (+4 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Transition - Generic:Standard" | object type "M_Transition - Generic:Standard" | names: "M_Transition - Generic:Standard:813095" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Transition - Generic:Standard" | object type "M_Transition - Generic:Standard" | names: "M_Transition - Generic:Standard:813567", "M_Transition - Generic:Standard:818704" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          3 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Tee - Generic:Standard" | object type "M_Tee - Generic:Standard" | names: "M_Tee - Generic:Standard:813612", "M_Tee - Generic:Standard:818608", "M_Tee - Generic:Standard:818730" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Transition - Generic:Standard" | object type "M_Transition - Generic:Standard" | names: "M_Transition - Generic:Standard:813616" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Transition - Generic:Standard" | object type "M_Transition - Generic:Standard" | names: "M_Transition - Generic:Standard:813619" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          5 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Elbow - Generic:Standard" | object type "M_Elbow - Generic:Standard" | names: "M_Elbow - Generic:Standard:813623", "M_Elbow - Generic:Standard:813627", "M_Elbow - Generic:Standard:818614" (+2 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Transition - Generic:Standard" | object type "M_Transition - Generic:Standard" | names: "M_Transition - Generic:Standard:815983" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          4 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Tee - Generic:Standard" | object type "M_Tee - Generic:Standard" | names: "M_Tee - Generic:Standard:816082", "M_Tee - Generic:Standard:816188", "M_Tee - Generic:Standard:818215" (+1 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Transition - Generic:Standard" | object type "M_Transition - Generic:Standard" | names: "M_Transition - Generic:Standard:816163" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Transition - Generic:Standard" | object type "M_Transition - Generic:Standard" | names: "M_Transition - Generic:Standard:818212" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Transition - Generic:Standard" | object type "M_Transition - Generic:Standard" | names: "M_Transition - Generic:Standard:818592" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:819767" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:819902" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Endcap:Standard" | object type "M_Rectangular Duct Endcap:Standard" | names: "M_Rectangular Duct Endcap:Standard:820071" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_Lighting and Appliance Panelboard - 480V MCB - Surface:400 A" | object type "M_Lighting and Appliance Panelboard - 480V MCB - Surface:400 A" | names: "M_Lighting and Appliance Panelboard - 480V MCB - Surface:MDP-2:823239" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff, Pset_ProvisionForVoid
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Cross - Generic:Standard" | object type "M_Cross - Generic:Standard" | names: "M_Cross - Generic:Standard:972753" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular to Round Duct Transition - Angle:45 Degree" | object type "M_Rectangular to Round Duct Transition - Angle:45 Degree" | names: "M_Rectangular to Round Duct Transition - Angle:45 Degree:973977" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          3 x IFCRAILING | object type "Barandilla:Stahl (1) - Horizontal" | names: "Barandilla:Stahl (1) - Horizontal:576320", "Barandilla:Stahl (1) - Horizontal:576379", "Barandilla:Stahl (1) - Horizontal:576915" | material: materials ("Geländer - Holz", "Geländer - Stahl") | property sets: Pset_QuantityTakeOff, Pset_RailingCommon
      IFCBUILDINGSTOREY "Level 3" | long name "Level 3" | object type "Nivel:8mm Head" | elevation 7299.99999999989
        contains 1258 elements
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:18 kW" | object type "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:18 kW" | names: "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:18 kW:488402" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:14 kW" | object type "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:14 kW" | names: "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:14 kW:488482" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:14 kW" | object type "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:14 kW" | names: "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:14 kW:488611" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:14 kW" | object type "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:14 kW" | names: "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:14 kW:488732", "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:14 kW:489000" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Right Return - Back Discharge:11 kW" | object type "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Right Return - Back Discharge:11 kW" | names: "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Right Return - Back Discharge:11 kW:488842" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Back Discharge:14 kW" | object type "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Back Discharge:14 kW" | names: "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Back Discharge:14 kW:489125" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:7 kW" | object type "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:7 kW" | names: "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:7 kW:489297" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:7 kW" | object type "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:7 kW" | names: "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:7 kW:489559" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:7 kW" | object type "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:7 kW" | names: "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:7 kW:489653" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          27 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "M_Supply Diffuser - Rectangular Face Round Neck:600x600 - 250 Neck" | object type "M_Supply Diffuser - Rectangular Face Round Neck:600x600 - 250 Neck" | names: "M_Supply Diffuser - Rectangular Face Round Neck:600x600 - 250 Neck:489769", "M_Supply Diffuser - Rectangular Face Round Neck:600x600 - 250 Neck:490068", "M_Supply Diffuser - Rectangular Face Round Neck:600x600 - 250 Neck:490089" (+24 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          8 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "M_Supply Diffuser - Rectangular Face Round Neck:600x600 - 250 Neck" | object type "M_Supply Diffuser - Rectangular Face Round Neck:600x600 - 250 Neck" | names: "M_Supply Diffuser - Rectangular Face Round Neck:600x600 - 250 Neck:490116", "M_Supply Diffuser - Rectangular Face Round Neck:600x600 - 250 Neck:490117", "M_Supply Diffuser - Rectangular Face Round Neck:600x600 - 250 Neck:490195" (+5 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          4 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "M_Supply Diffuser - Rectangular Face Round Neck:600x600 - 250 Neck" | object type "M_Supply Diffuser - Rectangular Face Round Neck:600x600 - 250 Neck" | names: "M_Supply Diffuser - Rectangular Face Round Neck:600x600 - 250 Neck:490149", "M_Supply Diffuser - Rectangular Face Round Neck:600x600 - 250 Neck:490150", "M_Supply Diffuser - Rectangular Face Round Neck:600x600 - 250 Neck:490169" (+1 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          4 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "M_Supply Diffuser - Rectangular Face Round Neck:600x600 - 250 Neck" | object type "M_Supply Diffuser - Rectangular Face Round Neck:600x600 - 250 Neck" | names: "M_Supply Diffuser - Rectangular Face Round Neck:600x600 - 250 Neck:490378", "M_Supply Diffuser - Rectangular Face Round Neck:600x600 - 250 Neck:490379", "M_Supply Diffuser - Rectangular Face Round Neck:600x600 - 250 Neck:490380" (+1 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          16 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "M_Supply Diffuser - Rectangular Face Round Neck:600x600 - 250 Neck" | object type "M_Supply Diffuser - Rectangular Face Round Neck:600x600 - 250 Neck" | names: "M_Supply Diffuser - Rectangular Face Round Neck:600x600 - 250 Neck:490420", "M_Supply Diffuser - Rectangular Face Round Neck:600x600 - 250 Neck:490421", "M_Supply Diffuser - Rectangular Face Round Neck:600x600 - 250 Neck:490435" (+13 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          42 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "Conducto rectangular:Mitered Elbows / Tees" | object type "Conducto rectangular:Mitered Elbows / Tees" | names: "Conducto rectangular:Mitered Elbows / Tees:490577", "Conducto rectangular:Mitered Elbows / Tees:490578", "Conducto rectangular:Mitered Elbows / Tees:490579" (+39 more) | property sets: Pset_DistributionFlowElementCommon, Pset_DuctSegmentTypeCommon, Pset_FlowSegmentDuctSegment, Pset_FlowSegmentPipeSegment, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:490580" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          5 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Elbow - Mitered:Standard" | object type "M_Rectangular Duct Elbow - Mitered:Standard" | names: "M_Rectangular Duct Elbow - Mitered:Standard:490582", "M_Rectangular Duct Elbow - Mitered:Standard:522434", "M_Rectangular Duct Elbow - Mitered:Standard:522451" (+2 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          176 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "Conducto rectangular:Mitered Elbows / Taps" | object type "Conducto rectangular:Mitered Elbows / Taps" | names: "Conducto rectangular:Mitered Elbows / Taps:490585", "Conducto rectangular:Mitered Elbows / Taps:490606", "Conducto rectangular:Mitered Elbows / Taps:490828" (+173 more) | property sets: Pset_DistributionFlowElementCommon, Pset_DuctSegmentTypeCommon, Pset_FlowSegmentDuctSegment, Pset_FlowSegmentPipeSegment, Pset_QuantityTakeOff
          59 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "Conducto flexible redondo:Flex - Round" | object type "Conducto flexible redondo:Flex - Round" | names: "Conducto flexible redondo:Flex - Round:490589", "Conducto flexible redondo:Flex - Round:490596", "Conducto flexible redondo:Flex - Round:490603" (+56 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          48 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular to Round Duct Transition - Angle:45 Degree" | object type "M_Rectangular to Round Duct Transition - Angle:45 Degree" | names: "M_Rectangular to Round Duct Transition - Angle:45 Degree:490590", "M_Rectangular to Round Duct Transition - Angle:45 Degree:490655", "M_Rectangular to Round Duct Transition - Angle:45 Degree:490833" (+45 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          7 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Cross:Standard" | object type "M_Rectangular Duct Cross:Standard" | names: "M_Rectangular Duct Cross:Standard:490612", "M_Rectangular Duct Cross:Standard:492725", "M_Rectangular Duct Cross:Standard:493202" (+4 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          14 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:490615", "M_Rectangular Duct Transition - Angle:45 Degree:490654", "M_Rectangular Duct Transition - Angle:45 Degree:492965" (+11 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          5 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Endcap:Standard" | object type "M_Rectangular Duct Endcap:Standard" | names: "M_Rectangular Duct Endcap:Standard:490629", "M_Rectangular Duct Endcap:Standard:492755", "M_Rectangular Duct Endcap:Standard:493249" (+2 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:490644" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          3 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:490645", "M_Rectangular Duct Transition - Angle:45 Degree:492953", "M_Rectangular Duct Transition - Angle:45 Degree:493270" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:490825" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Elbow - Mitered:Standard" | object type "M_Rectangular Duct Elbow - Mitered:Standard" | names: "M_Rectangular Duct Elbow - Mitered:Standard:490842", "M_Rectangular Duct Elbow - Mitered:Standard:493668" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:490843" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          10 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Takeoff:Standard" | object type "M_Rectangular Duct Takeoff:Standard" | names: "M_Rectangular Duct Takeoff:Standard:490850", "M_Rectangular Duct Takeoff:Standard:492903", "M_Rectangular Duct Takeoff:Standard:493216" (+7 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:490886" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Elbow - Mitered:Standard" | object type "M_Rectangular Duct Elbow - Mitered:Standard" | names: "M_Rectangular Duct Elbow - Mitered:Standard:490887" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Cross:Standard" | object type "M_Rectangular Duct Cross:Standard" | names: "M_Rectangular Duct Cross:Standard:490917" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          5 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Endcap:Standard" | object type "M_Rectangular Duct Endcap:Standard" | names: "M_Rectangular Duct Endcap:Standard:490934", "M_Rectangular Duct Endcap:Standard:494028", "M_Rectangular Duct Endcap:Standard:494044" (+2 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:490958" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:490959" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          4 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:490972", "M_Rectangular Duct Transition - Angle:45 Degree:490979", "M_Rectangular Duct Transition - Angle:45 Degree:492329" (+1 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Tee:Standard" | object type "M_Rectangular Duct Tee:Standard" | names: "M_Rectangular Duct Tee:Standard:491917" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Tee:Standard" | object type "M_Rectangular Duct Tee:Standard" | names: "M_Rectangular Duct Tee:Standard:491920" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:491925" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Cross:Standard" | object type "M_Rectangular Duct Cross:Standard" | names: "M_Rectangular Duct Cross:Standard:491927", "M_Rectangular Duct Cross:Standard:493554" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular to Round Duct Transition - Angle:45 Degree" | object type "M_Rectangular to Round Duct Transition - Angle:45 Degree" | names: "M_Rectangular to Round Duct Transition - Angle:45 Degree:491931" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Tee:Standard" | object type "M_Rectangular Duct Tee:Standard" | names: "M_Rectangular Duct Tee:Standard:491933" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          3 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:492210", "M_Rectangular Duct Transition - Angle:45 Degree:494077", "M_Rectangular Duct Transition - Angle:45 Degree:494330" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          9 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Takeoff:Standard" | object type "M_Rectangular Duct Takeoff:Standard" | names: "M_Rectangular Duct Takeoff:Standard:492291", "M_Rectangular Duct Takeoff:Standard:492928", "M_Rectangular Duct Takeoff:Standard:493215" (+6 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:492313" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          3 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:492323", "M_Rectangular Duct Transition - Angle:45 Degree:493972", "M_Rectangular Duct Transition - Angle:45 Degree:493979" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:492331" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:492338" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:492655" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Cross:Standard" | object type "M_Rectangular Duct Cross:Standard" | names: "M_Rectangular Duct Cross:Standard:492722" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Elbow - Mitered:Standard" | object type "M_Rectangular Duct Elbow - Mitered:Standard" | names: "M_Rectangular Duct Elbow - Mitered:Standard:492861" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:492951", "M_Rectangular Duct Transition - Angle:45 Degree:493328" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          4 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:492973", "M_Rectangular Duct Transition - Angle:45 Degree:492980", "M_Rectangular Duct Transition - Angle:45 Degree:493362" (+1 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Tee:Standard" | object type "M_Rectangular Duct Tee:Standard" | names: "M_Rectangular Duct Tee:Standard:493199" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Cross:Standard" | object type "M_Rectangular Duct Cross:Standard" | names: "M_Rectangular Duct Cross:Standard:493207" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:493329" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:493341" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:493414" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:493522" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Elbow - Mitered:Standard" | object type "M_Rectangular Duct Elbow - Mitered:Standard" | names: "M_Rectangular Duct Elbow - Mitered:Standard:493524" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:493651" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:493669" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:493881", "M_Rectangular Duct Transition - Angle:45 Degree:494213" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          8 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular to Round Duct Transition - Angle:45 Degree" | object type "M_Rectangular to Round Duct Transition - Angle:45 Degree" | names: "M_Rectangular to Round Duct Transition - Angle:45 Degree:493898", "M_Rectangular to Round Duct Transition - Angle:45 Degree:493933", "M_Rectangular to Round Duct Transition - Angle:45 Degree:494163" (+5 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Tee:Standard" | object type "M_Rectangular Duct Tee:Standard" | names: "M_Rectangular Duct Tee:Standard:493945", "M_Rectangular Duct Tee:Standard:494277" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          6 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Takeoff:Standard" | object type "M_Rectangular Duct Takeoff:Standard" | names: "M_Rectangular Duct Takeoff:Standard:493957", "M_Rectangular Duct Takeoff:Standard:493959", "M_Rectangular Duct Takeoff:Standard:494421" (+3 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:493962" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:493963" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          4 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:493982", "M_Rectangular Duct Transition - Angle:45 Degree:493988", "M_Rectangular Duct Transition - Angle:45 Degree:494331" (+1 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          4 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:494079", "M_Rectangular Duct Transition - Angle:45 Degree:494089", "M_Rectangular Duct Transition - Angle:45 Degree:494334" (+1 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          4 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Takeoff:Standard" | object type "M_Rectangular Duct Takeoff:Standard" | names: "M_Rectangular Duct Takeoff:Standard:494162", "M_Rectangular Duct Takeoff:Standard:494293", "M_Rectangular Duct Takeoff:Standard:806483" (+1 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:18 kW" | object type "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:18 kW" | names: "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:18 kW:494453" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          8 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Elbow - Mitered:Standard" | object type "M_Rectangular Duct Elbow - Mitered:Standard" | names: "M_Rectangular Duct Elbow - Mitered:Standard:495016", "M_Rectangular Duct Elbow - Mitered:Standard:495038", "M_Rectangular Duct Elbow - Mitered:Standard:522127" (+5 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:495040" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Endcap:Standard" | object type "M_Rectangular Duct Endcap:Standard" | names: "M_Rectangular Duct Endcap:Standard:495335" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:495345" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Endcap:Standard" | object type "M_Rectangular Duct Endcap:Standard" | names: "M_Rectangular Duct Endcap:Standard:495536", "M_Rectangular Duct Endcap:Standard:495642" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          6 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Takeoff:Standard" | object type "M_Rectangular Duct Takeoff:Standard" | names: "M_Rectangular Duct Takeoff:Standard:495558", "M_Rectangular Duct Takeoff:Standard:495669", "M_Rectangular Duct Takeoff:Standard:495813" (+3 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          13 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Elbow - Mitered:Standard" | object type "M_Rectangular Duct Elbow - Mitered:Standard" | names: "M_Rectangular Duct Elbow - Mitered:Standard:495608", "M_Rectangular Duct Elbow - Mitered:Standard:495677", "M_Rectangular Duct Elbow - Mitered:Standard:495717" (+10 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          8 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Takeoff:Standard" | object type "M_Rectangular Duct Takeoff:Standard" | names: "M_Rectangular Duct Takeoff:Standard:495711", "M_Rectangular Duct Takeoff:Standard:495849", "M_Rectangular Duct Takeoff:Standard:495946" (+5 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          5 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Endcap:Standard" | object type "M_Rectangular Duct Endcap:Standard" | names: "M_Rectangular Duct Endcap:Standard:495907", "M_Rectangular Duct Endcap:Standard:495917", "M_Rectangular Duct Endcap:Standard:496238" (+2 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          3 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Endcap:Standard" | object type "M_Rectangular Duct Endcap:Standard" | names: "M_Rectangular Duct Endcap:Standard:496109", "M_Rectangular Duct Endcap:Standard:507169", "M_Rectangular Duct Endcap:Standard:507227" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Takeoff:Standard" | object type "M_Rectangular Duct Takeoff:Standard" | names: "M_Rectangular Duct Takeoff:Standard:496408" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:496489" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          3 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Endcap:Standard" | object type "M_Rectangular Duct Endcap:Standard" | names: "M_Rectangular Duct Endcap:Standard:496699", "M_Rectangular Duct Endcap:Standard:496815", "M_Rectangular Duct Endcap:Standard:496911" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          8 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "M_Supply Diffuser - Sidewall:450 x 200" | object type "M_Supply Diffuser - Sidewall:450 x 200" | names: "M_Supply Diffuser - Sidewall:450 x 200:496980", "M_Supply Diffuser - Sidewall:450 x 200:497146", "M_Supply Diffuser - Sidewall:450 x 200:497165" (+5 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Back Discharge:11 kW" | object type "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Back Discharge:11 kW" | names: "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Back Discharge:11 kW:497273" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Elbow - Mitered:Standard" | object type "M_Rectangular Duct Elbow - Mitered:Standard" | names: "M_Rectangular Duct Elbow - Mitered:Standard:497581", "M_Rectangular Duct Elbow - Mitered:Standard:497951" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Endcap:Standard" | object type "M_Rectangular Duct Endcap:Standard" | names: "M_Rectangular Duct Endcap:Standard:497599", "M_Rectangular Duct Endcap:Standard:498023" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          4 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Takeoff:Standard" | object type "M_Rectangular Duct Takeoff:Standard" | names: "M_Rectangular Duct Takeoff:Standard:497707", "M_Rectangular Duct Takeoff:Standard:497749", "M_Rectangular Duct Takeoff:Standard:498303" (+1 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Right Return - Back Discharge:11 kW" | object type "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Right Return - Back Discharge:11 kW" | names: "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Right Return - Back Discharge:11 kW:497783" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          4 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Takeoff:Standard" | object type "M_Rectangular Duct Takeoff:Standard" | names: "M_Rectangular Duct Takeoff:Standard:498056", "M_Rectangular Duct Takeoff:Standard:498072", "M_Rectangular Duct Takeoff:Standard:498104" (+1 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:498237", "M_Rectangular Duct Transition - Angle:45 Degree:498329" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:498238", "M_Rectangular Duct Transition - Angle:45 Degree:498330" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          111 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "M_Plain Recessed Lighting Fixture:600x600 - 277" | object type "M_Plain Recessed Lighting Fixture:600x600 - 277" | names: "M_Plain Recessed Lighting Fixture:600x600 - 277:498911", "M_Plain Recessed Lighting Fixture:600x600 - 277:498941", "M_Plain Recessed Lighting Fixture:600x600 - 277:498954" (+108 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          15 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_Wall Occupancy Sensor - Regular Voltage:Passive Infrared - 277 V" | object type "M_Wall Occupancy Sensor - Regular Voltage:Passive Infrared - 277 V" | names: "M_Wall Occupancy Sensor - Regular Voltage:Passive Infrared - 277 V:500207", "M_Wall Occupancy Sensor - Regular Voltage:Passive Infrared - 277 V:500227", "M_Wall Occupancy Sensor - Regular Voltage:Passive Infrared - 277 V:500295" (+12 more) | material: materials ("<Unnamed>", "<Unnamed>") | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_Lighting Switches:Single Pole" | object type "M_Lighting Switches:Single Pole" | names: "M_Lighting Switches:Single Pole:502446", "M_Lighting Switches:Single Pole:502464" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          24 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "M_Sconce Light - Flat Round:60W - 277V" | object type "M_Sconce Light - Flat Round:60W - 277V" | names: "M_Sconce Light - Flat Round:60W - 277V:502493", "M_Sconce Light - Flat Round:60W - 277V:502513", "M_Sconce Light - Flat Round:60W - 277V:502612" (+21 more) | material: "Glass - Frosted" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_Lighting and Appliance Panelboard - 208V MLO - Surface:400 A" | object type "M_Lighting and Appliance Panelboard - 208V MLO - Surface:400 A" | names: "M_Lighting and Appliance Panelboard - 208V MLO - Surface:PP-3B:503195", "M_Lighting and Appliance Panelboard - 208V MLO - Surface:EP-3:503251" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff, Pset_ProvisionForVoid
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_Lighting and Appliance Panelboard - 480V MLO - Surface:400 A" | object type "M_Lighting and Appliance Panelboard - 480V MLO - Surface:400 A" | names: "M_Lighting and Appliance Panelboard - 480V MLO - Surface:LP-3:503257" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff, Pset_ProvisionForVoid
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Takeoff:Standard" | object type "M_Rectangular Duct Takeoff:Standard" | names: "M_Rectangular Duct Takeoff:Standard:507346" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Elbow - Mitered:Standard" | object type "M_Rectangular Duct Elbow - Mitered:Standard" | names: "M_Rectangular Duct Elbow - Mitered:Standard:508033", "M_Rectangular Duct Elbow - Mitered:Standard:508036" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          3 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Elbow - Mitered:Standard" | object type "M_Rectangular Duct Elbow - Mitered:Standard" | names: "M_Rectangular Duct Elbow - Mitered:Standard:508055", "M_Rectangular Duct Elbow - Mitered:Standard:508063", "M_Rectangular Duct Elbow - Mitered:Standard:508153" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:508165" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          7 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Elbow - Mitered:Standard" | object type "M_Rectangular Duct Elbow - Mitered:Standard" | names: "M_Rectangular Duct Elbow - Mitered:Standard:508175", "M_Rectangular Duct Elbow - Mitered:Standard:508558", "M_Rectangular Duct Elbow - Mitered:Standard:508749" (+4 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          17 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Takeoff:Standard" | object type "M_Rectangular Duct Takeoff:Standard" | names: "M_Rectangular Duct Takeoff:Standard:508322", "M_Rectangular Duct Takeoff:Standard:508539", "M_Rectangular Duct Takeoff:Standard:508572" (+14 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          10 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Elbow - Mitered:Standard" | object type "M_Rectangular Duct Elbow - Mitered:Standard" | names: "M_Rectangular Duct Elbow - Mitered:Standard:508516", "M_Rectangular Duct Elbow - Mitered:Standard:508519", "M_Rectangular Duct Elbow - Mitered:Standard:508555" (+7 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:508520", "M_Rectangular Duct Transition - Angle:45 Degree:522246" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          4 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Takeoff:Standard" | object type "M_Rectangular Duct Takeoff:Standard" | names: "M_Rectangular Duct Takeoff:Standard:508554", "M_Rectangular Duct Takeoff:Standard:508626", "M_Rectangular Duct Takeoff:Standard:508698" (+1 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Takeoff:Standard" | object type "M_Rectangular Duct Takeoff:Standard" | names: "M_Rectangular Duct Takeoff:Standard:508585" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Elbow - Mitered:Standard" | object type "M_Rectangular Duct Elbow - Mitered:Standard" | names: "M_Rectangular Duct Elbow - Mitered:Standard:508586" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Tee:Standard" | object type "M_Rectangular Duct Tee:Standard" | names: "M_Rectangular Duct Tee:Standard:508602" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:508655", "M_Rectangular Duct Transition - Angle:45 Degree:508656" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Takeoff:Standard" | object type "M_Rectangular Duct Takeoff:Standard" | names: "M_Rectangular Duct Takeoff:Standard:508903" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Elbow - Mitered:Standard" | object type "M_Rectangular Duct Elbow - Mitered:Standard" | names: "M_Rectangular Duct Elbow - Mitered:Standard:508904" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Tee:Standard" | object type "M_Rectangular Duct Tee:Standard" | names: "M_Rectangular Duct Tee:Standard:508949" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:508953" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:508986" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          12 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "M_Return Diffuser:600 x 600 Face 300 x 300 Connection" | object type "M_Return Diffuser:600 x 600 Face 300 x 300 Connection" | names: "M_Return Diffuser:600 x 600 Face 300 x 300 Connection:509286", "M_Return Diffuser:600 x 600 Face 300 x 300 Connection:509375", "M_Return Diffuser:600 x 600 Face 300 x 300 Connection:509638" (+9 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "M_Return Diffuser:600 x 600 Face 300 x 300 Connection" | object type "M_Return Diffuser:600 x 600 Face 300 x 300 Connection" | names: "M_Return Diffuser:600 x 600 Face 300 x 300 Connection:509416", "M_Return Diffuser:600 x 600 Face 300 x 300 Connection:509417" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "M_Return Diffuser:600 x 600 Face 300 x 300 Connection" | object type "M_Return Diffuser:600 x 600 Face 300 x 300 Connection" | names: "M_Return Diffuser:600 x 600 Face 300 x 300 Connection:509486", "M_Return Diffuser:600 x 600 Face 300 x 300 Connection:509487" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          4 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "M_Return Diffuser:600 x 600 Face 300 x 300 Connection" | object type "M_Return Diffuser:600 x 600 Face 300 x 300 Connection" | names: "M_Return Diffuser:600 x 600 Face 300 x 300 Connection:509511", "M_Return Diffuser:600 x 600 Face 300 x 300 Connection:509543", "M_Return Diffuser:600 x 600 Face 300 x 300 Connection:509564" (+1 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "M_Return Diffuser:600 x 600 Face 300 x 300 Connection" | object type "M_Return Diffuser:600 x 600 Face 300 x 300 Connection" | names: "M_Return Diffuser:600 x 600 Face 300 x 300 Connection:509639" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "M_Return Diffuser:600 x 600 Face 300 x 300 Connection" | object type "M_Return Diffuser:600 x 600 Face 300 x 300 Connection" | names: "M_Return Diffuser:600 x 600 Face 300 x 300 Connection:509803", "M_Return Diffuser:600 x 600 Face 300 x 300 Connection:509804" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          8 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "M_Return Diffuser:600 x 600 Face 300 x 300 Connection" | object type "M_Return Diffuser:600 x 600 Face 300 x 300 Connection" | names: "M_Return Diffuser:600 x 600 Face 300 x 300 Connection:509826", "M_Return Diffuser:600 x 600 Face 300 x 300 Connection:509866", "M_Return Diffuser:600 x 600 Face 300 x 300 Connection:509899" (+5 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "M_Exhaust Grill:600 x 600 Face 300 x 300 Connection" | object type "M_Exhaust Grill:600 x 600 Face 300 x 300 Connection" | names: "M_Exhaust Grill:600 x 600 Face 300 x 300 Connection:522312", "M_Exhaust Grill:600 x 600 Face 300 x 300 Connection:522330" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Takeoff:Standard" | object type "M_Rectangular Duct Takeoff:Standard" | names: "M_Rectangular Duct Takeoff:Standard:522450" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:522461" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          119 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "Tipos de tubería:Standard" | object type "Tipos de tubería:Standard" | names: "Tipos de tubería:Standard:527395", "Tipos de tubería:Standard:527396", "Tipos de tubería:Standard:527397" (+116 more) | property sets: Pset_DistributionFlowElementCommon, Pset_FlowSegmentDuctSegment, Pset_FlowSegmentPipeSegment, Pset_QuantityTakeOff
          26 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Pipe Elbow:Standard" | object type "M_Pipe Elbow:Standard" | names: "M_Pipe Elbow:Standard:527398", "M_Pipe Elbow:Standard:527400", "M_Pipe Elbow:Standard:527404" (+23 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          14 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Pipe Transition:Standard" | object type "M_Pipe Transition:Standard" | names: "M_Pipe Transition:Standard:527427", "M_Pipe Transition:Standard:527441", "M_Pipe Transition:Standard:527455" (+11 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          32 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Pipe Elbow:Standard" | object type "M_Pipe Elbow:Standard" | names: "M_Pipe Elbow:Standard:527428", "M_Pipe Elbow:Standard:527430", "M_Pipe Elbow:Standard:527442" (+29 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          12 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Pipe Tee:Standard" | object type "M_Pipe Tee:Standard" | names: "M_Pipe Tee:Standard:527549", "M_Pipe Tee:Standard:527554", "M_Pipe Tee:Standard:527569" (+9 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          22 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Pipe Transition:Standard" | object type "M_Pipe Transition:Standard" | names: "M_Pipe Transition:Standard:527551", "M_Pipe Transition:Standard:527553", "M_Pipe Transition:Standard:527556" (+19 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          12 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Pipe Tee:Standard" | object type "M_Pipe Tee:Standard" | names: "M_Pipe Tee:Standard:527561", "M_Pipe Tee:Standard:527564", "M_Pipe Tee:Standard:527584" (+9 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Pipe Elbow:Standard" | object type "M_Pipe Elbow:Standard" | names: "M_Pipe Elbow:Standard:528309" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Pipe Elbow:Standard" | object type "M_Pipe Elbow:Standard" | names: "M_Pipe Elbow:Standard:528329" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Pipe Elbow:Standard" | object type "M_Pipe Elbow:Standard" | names: "M_Pipe Elbow:Standard:528337" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Pipe Elbow:Standard" | object type "M_Pipe Elbow:Standard" | names: "M_Pipe Elbow:Standard:528360" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Pipe Elbow:Standard" | object type "M_Pipe Elbow:Standard" | names: "M_Pipe Elbow:Standard:533913" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:STB 30.0" | object type "Suelo:STB 30.0" | FLOOR | names: "Suelo:STB 30.0:573418" | material: layers "Suelo:STB 30.0" ("Stahlbeton - Ortbeton" 300.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          41 x IFCCOLUMN | type IFCCOLUMNTYPE "STB Stütze - rund:STB d=30" | object type "STB Stütze - rund:STB d=30" | names: "STB Stütze - rund:STB d=30:573505", "STB Stütze - rund:STB d=30:573506", "STB Stütze - rund:STB d=30:573507" (+38 more) | material: "Stahlbeton - Fertigbeton" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          10 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Muro básico:MW 17.5" | object type "Muro básico:MW 17.5" | names: "Muro básico:MW 17.5:573704", "Muro básico:MW 17.5:573706", "Muro básico:MW 17.5:573707" (+7 more) | material: layers "Muro básico:MW 17.5" ("Mauerwerk - Ziegel" 175.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          3 x IFCDOOR | type IFCDOORSTYLE "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26" | object type "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26" | names: "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26:573705", "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26:573711", "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26:573712" | material: materials ("Tür - Stahl Griff", "Tür - Stahl Zarge") | property sets: Pset_DoorCommon, Pset_QuantityTakeOff
          4 x IFCDOOR | type IFCDOORSTYLE "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26" | object type "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26" | names: "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26:573708", "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26:573709", "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26:573725" (+1 more) | material: materials ("Tür - Stahl Griff", "Tür - Stahl Zarge") | property sets: Pset_DoorCommon, Pset_QuantityTakeOff
          18 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Muro básico:MW 11.5" | object type "Muro básico:MW 11.5" | names: "Muro básico:MW 11.5:573713", "Muro básico:MW 11.5:573718", "Muro básico:MW 11.5:573719" (+15 more) | material: layers "Muro básico:MW 11.5" ("Mauerwerk - Ziegel" 115.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCDOOR | type IFCDOORSTYLE "Drehflügel 1-flg - Stahlzarge:76 x 2.26" | object type "Drehflügel 1-flg - Stahlzarge:76 x 2.26" | names: "Drehflügel 1-flg - Stahlzarge:76 x 2.26:573721" | material: materials ("Tür - Stahl Griff", "Tür - Stahl Zarge") | property sets: Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "Drehflügel 1-flg - Stahlzarge:76 x 2.26" | object type "Drehflügel 1-flg - Stahlzarge:76 x 2.26" | names: "Drehflügel 1-flg - Stahlzarge:76 x 2.26:573722" | material: materials ("Tür - Stahl Griff", "Tür - Stahl Zarge") | property sets: Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "Drehflügel 1-flg - Stahlzarge:76 x 2.26" | object type "Drehflügel 1-flg - Stahlzarge:76 x 2.26" | names: "Drehflügel 1-flg - Stahlzarge:76 x 2.26:573723" | material: materials ("Tür - Stahl Griff", "Tür - Stahl Zarge") | property sets: Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "Drehflügel 1-flg - Stahlzarge:76 x 2.26" | object type "Drehflügel 1-flg - Stahlzarge:76 x 2.26" | names: "Drehflügel 1-flg - Stahlzarge:76 x 2.26:573724" | material: materials ("Tür - Stahl Griff", "Tür - Stahl Zarge") | property sets: Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Muro básico:STB 25.0 WD 12.0" | object type "Muro básico:STB 25.0 WD 12.0" | names: "Muro básico:STB 25.0 WD 12.0:575873" | material: layers "Muro básico:STB 25.0 WD 12.0" ("Wärmedämmung - hart" 120., "Stahlbeton - Ortbeton" 250.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Muro básico:Lamelle 11.5" | object type "Muro básico:Lamelle 11.5" | names: "Muro básico:Lamelle 11.5:576022", "Muro básico:Lamelle 11.5:576044", "Muro básico:Lamelle 11.5:576054" | material: layers "Muro básico:Lamelle 11.5" ("Mauerwerk - Lamellen" 115.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          9 x IFCDOOR | type IFCDOORSTYLE "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26" | object type "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26" | names: "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26:576023", "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26:576024", "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26:576025" (+6 more) | material: materials ("Tür - Stahl Griff", "Tür - Stahl Zarge") | property sets: Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Aufzug 2-flg:Aufzug 2-flg" | object type "Aufzug 2-flg:Aufzug 2-flg" | names: "Aufzug 2-flg:Aufzug 2-flg:576034" | material: "Tür - Aufzug Metall" | property sets: Pset_OpeningElementCommon, Pset_QuantityTakeOff
          5 x IFCDOOR | type IFCDOORSTYLE "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26" | object type "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26" | names: "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26:576046", "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26:576047", "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26:576050" (+2 more) | material: materials ("Tür - Stahl Griff", "Tür - Stahl Zarge") | property sets: Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:FB 15.0 - Fliesen 50 x 50" | object type "Suelo:FB 15.0 - Fliesen 50 x 50" | FLOOR | names: "Suelo:FB 15.0 - Fliesen 50 x 50:576122" | material: layers "Suelo:FB 15.0 - Fliesen 50 x 50" ("Bodenbelag Fliesen 50 x 50" 10., "Decke - Estrich" 60., "Wärmedämmung - hart" 80.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          3 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Muro cortina:Standard" | object type "Muro cortina:Standard" | names: "Muro cortina:Standard:576765", "Muro cortina:Standard:576813", "Muro cortina:Standard:576861" | parts: 42 IFCMEMBER, 9 IFCPLATE, 3 IFCDOOR | property sets: Pset_CurtainWallCommon, Pset_QuantityTakeOff
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:Sonnenschutz" | object type "Suelo:Sonnenschutz" | FLOOR | names: "Suelo:Sonnenschutz:577724" | material: layers "Suelo:Sonnenschutz" ("Gitterrost" 100.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:Sonnenschutz" | object type "Suelo:Sonnenschutz" | FLOOR | names: "Suelo:Sonnenschutz:577724:2" | material: layers "Suelo:Sonnenschutz" ("Gitterrost" 100.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:Sonnenschutz" | object type "Suelo:Sonnenschutz" | FLOOR | names: "Suelo:Sonnenschutz:577724:3" | material: layers "Suelo:Sonnenschutz" ("Gitterrost" 100.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:Sonnenschutz" | object type "Suelo:Sonnenschutz" | FLOOR | names: "Suelo:Sonnenschutz:577724:4" | material: layers "Suelo:Sonnenschutz" ("Gitterrost" 100.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:Sonnenschutz" | object type "Suelo:Sonnenschutz" | FLOOR | names: "Suelo:Sonnenschutz:577724:5" | material: layers "Suelo:Sonnenschutz" ("Gitterrost" 100.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:Sonnenschutz" | object type "Suelo:Sonnenschutz" | FLOOR | names: "Suelo:Sonnenschutz:577724:6" | material: layers "Suelo:Sonnenschutz" ("Gitterrost" 100.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:FB 10.0 - Fliesen 15 x 15" | object type "Suelo:FB 10.0 - Fliesen 15 x 15" | FLOOR | names: "Suelo:FB 10.0 - Fliesen 15 x 15:579067" | material: layers "Suelo:FB 10.0 - Fliesen 15 x 15" ("Decke - Fliesen 15 x 15" 10., "Decke - Estrich" 60., "Wärmedämmung - hart" 80.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:FB 10.0 - Fliesen 15 x 15" | object type "Suelo:FB 10.0 - Fliesen 15 x 15" | FLOOR | names: "Suelo:FB 10.0 - Fliesen 15 x 15:579067:2" | material: layers "Suelo:FB 10.0 - Fliesen 15 x 15" ("Decke - Fliesen 15 x 15" 10., "Decke - Estrich" 60., "Wärmedämmung - hart" 80.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:FB 10.0 - Fliesen 15 x 15" | object type "Suelo:FB 10.0 - Fliesen 15 x 15" | FLOOR | names: "Suelo:FB 10.0 - Fliesen 15 x 15:579067:3" | material: layers "Suelo:FB 10.0 - Fliesen 15 x 15" ("Decke - Fliesen 15 x 15" 10., "Decke - Estrich" 60., "Wärmedämmung - hart" 80.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:FB 10.0 - Fliesen 15 x 15" | object type "Suelo:FB 10.0 - Fliesen 15 x 15" | FLOOR | names: "Suelo:FB 10.0 - Fliesen 15 x 15:579067:4" | material: layers "Suelo:FB 10.0 - Fliesen 15 x 15" ("Decke - Fliesen 15 x 15" 10., "Decke - Estrich" 60., "Wärmedämmung - hart" 80.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          2 x IFCDOOR | type IFCDOORSTYLE "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26" | object type "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26" | names: "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26:579164", "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26:579168" | material: materials ("Tür - Stahl Griff", "Tür - Stahl Zarge") | property sets: Pset_DoorCommon, Pset_QuantityTakeOff
          3 x IFCDOOR | type IFCDOORSTYLE "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26" | object type "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26" | names: "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26:579165", "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26:579166", "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26:579167" | material: materials ("Tür - Stahl Griff", "Tür - Stahl Zarge") | property sets: Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | object type "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | CEILING | names: "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600:579747" | material: layers "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" ("Decke - Gipskarton" 20., "Decke - Deckenraster" 30.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | object type "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | CEILING | names: "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600:580723" | material: layers "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" ("Decke - Gipskarton" 20., "Decke - Deckenraster" 30.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | object type "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | CEILING | names: "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600:580730" | material: layers "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" ("Decke - Gipskarton" 20., "Decke - Deckenraster" 30.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | object type "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | CEILING | names: "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600:580741" | material: layers "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" ("Decke - Gipskarton" 20., "Decke - Deckenraster" 30.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | object type "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | CEILING | names: "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600:580748" | material: layers "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" ("Decke - Gipskarton" 20., "Decke - Deckenraster" 30.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | object type "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | CEILING | names: "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600:580767" | material: layers "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" ("Decke - Gipskarton" 20., "Decke - Deckenraster" 30.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | object type "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | CEILING | names: "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600:580778" | material: layers "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" ("Decke - Gipskarton" 20., "Decke - Deckenraster" 30.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | object type "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | CEILING | names: "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600:580789" | material: layers "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" ("Decke - Gipskarton" 20., "Decke - Deckenraster" 30.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | object type "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | CEILING | names: "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600:580800" | material: layers "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" ("Decke - Gipskarton" 20., "Decke - Deckenraster" 30.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | object type "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | CEILING | names: "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600:580811" | material: layers "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" ("Decke - Gipskarton" 20., "Decke - Deckenraster" 30.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | object type "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | CEILING | names: "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600:580822" | material: layers "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" ("Decke - Gipskarton" 20., "Decke - Deckenraster" 30.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | object type "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | CEILING | names: "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600:580829" | material: layers "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" ("Decke - Gipskarton" 20., "Decke - Deckenraster" 30.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | object type "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | CEILING | names: "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600:580844" | material: layers "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" ("Decke - Gipskarton" 20., "Decke - Deckenraster" 30.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | object type "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | CEILING | names: "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600:580853" | material: layers "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" ("Decke - Gipskarton" 20., "Decke - Deckenraster" 30.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | object type "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | CEILING | names: "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600:580860" | material: layers "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" ("Decke - Gipskarton" 20., "Decke - Deckenraster" 30.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | object type "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | CEILING | names: "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600:580871" | material: layers "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" ("Decke - Gipskarton" 20., "Decke - Deckenraster" 30.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | object type "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | CEILING | names: "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600:580882" | material: layers "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" ("Decke - Gipskarton" 20., "Decke - Deckenraster" 30.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | object type "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | CEILING | names: "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600:580889" | material: layers "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" ("Decke - Gipskarton" 20., "Decke - Deckenraster" 30.) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26" | object type "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26" | names: "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26:580927" | material: materials ("Tür - Stahl Griff", "Tür - Stahl Zarge") | property sets: Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Bend - PVC - Sch 40 - DWV:Standard" | object type "M_Bend - PVC - Sch 40 - DWV:Standard" | names: "M_Bend - PVC - Sch 40 - DWV:Standard:606528" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Tee - Generic:Standard" | object type "M_Tee - Generic:Standard" | names: "M_Tee - Generic:Standard:606570" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Tee Sanitary - PVC - Sch 40 - DWV:Standard" | object type "M_Tee Sanitary - PVC - Sch 40 - DWV:Standard" | names: "M_Tee Sanitary - PVC - Sch 40 - DWV:Standard:606576" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Tee Sanitary - PVC - Sch 40 - DWV:Standard" | object type "M_Tee Sanitary - PVC - Sch 40 - DWV:Standard" | names: "M_Tee Sanitary - PVC - Sch 40 - DWV:Standard:606578" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Tee Sanitary - PVC - Sch 40 - DWV:Standard" | object type "M_Tee Sanitary - PVC - Sch 40 - DWV:Standard" | names: "M_Tee Sanitary - PVC - Sch 40 - DWV:Standard:606581" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Tee Sanitary - PVC - Sch 40 - DWV:Standard" | object type "M_Tee Sanitary - PVC - Sch 40 - DWV:Standard" | names: "M_Tee Sanitary - PVC - Sch 40 - DWV:Standard:606588" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_Lighting and Appliance Panelboard - 480V MCB - Surface:100 A" | object type "M_Lighting and Appliance Panelboard - 480V MCB - Surface:100 A" | names: "M_Lighting and Appliance Panelboard - 480V MCB - Surface:LP-3B:626004", "M_Lighting and Appliance Panelboard - 480V MCB - Surface:MP-3B:626006" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff, Pset_ProvisionForVoid
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_Lighting and Appliance Panelboard - 208V MCB - Surface:100 A" | object type "M_Lighting and Appliance Panelboard - 208V MCB - Surface:100 A" | names: "M_Lighting and Appliance Panelboard - 208V MCB - Surface:PP-3A:626007" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff, Pset_ProvisionForVoid
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_Dry Type Transformer - 480-208Y120 - NEMA Type 3R:15 kVA" | object type "M_Dry Type Transformer - 480-208Y120 - NEMA Type 3R:15 kVA" | names: "M_Dry Type Transformer - 480-208Y120 - NEMA Type 3R:TP-3A:626008" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Transition - Generic:Standard" | object type "M_Transition - Generic:Standard" | names: "M_Transition - Generic:Standard:711816" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular to Round Duct Transition - Angle:45 Degree" | object type "M_Rectangular to Round Duct Transition - Angle:45 Degree" | names: "M_Rectangular to Round Duct Transition - Angle:45 Degree:806485", "M_Rectangular to Round Duct Transition - Angle:45 Degree:806550" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:812650" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_Lighting and Appliance Panelboard - 480V MCB - Surface:400 A" | object type "M_Lighting and Appliance Panelboard - 480V MCB - Surface:400 A" | names: "M_Lighting and Appliance Panelboard - 480V MCB - Surface:MDP-3:824070" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff, Pset_ProvisionForVoid
          3 x IFCRAILING | object type "Barandilla:Stahl (1) - Horizontal" | names: "Barandilla:Stahl (1) - Horizontal:576887", "Barandilla:Stahl (1) - Horizontal:576896", "Barandilla:Stahl (1) - Horizontal:577484" | material: materials ("Geländer - Holz", "Geländer - Stahl") | property sets: Pset_QuantityTakeOff, Pset_RailingCommon
      IFCBUILDINGSTOREY "Roof Level" | long name "Roof Level" | object type "Nivel:8mm Head" | elevation 10899.9999999999
        contains 79 elements
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_Outdoor AHU - Horizontal:5.7 Square Meters of Coil" | object type "M_Outdoor AHU - Horizontal:5.7 Square Meters of Coil" | names: "M_Outdoor AHU - Horizontal:5.7 Square Meters of Coil:477676" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff, Pset_ProvisionForVoid
          10 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "Conducto rectangular:Mitered Elbows / Taps" | object type "Conducto rectangular:Mitered Elbows / Taps" | names: "Conducto rectangular:Mitered Elbows / Taps:477769", "Conducto rectangular:Mitered Elbows / Taps:477782", "Conducto rectangular:Mitered Elbows / Taps:477829" (+7 more) | property sets: Pset_DistributionFlowElementCommon, Pset_DuctSegmentTypeCommon, Pset_FlowSegmentDuctSegment, Pset_FlowSegmentPipeSegment, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:477828" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Elbow - Mitered:Standard" | object type "M_Rectangular Duct Elbow - Mitered:Standard" | names: "M_Rectangular Duct Elbow - Mitered:Standard:477865" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:477882" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Elbow - Mitered:Standard" | object type "M_Rectangular Duct Elbow - Mitered:Standard" | names: "M_Rectangular Duct Elbow - Mitered:Standard:478146" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Elbow - Mitered:Standard" | object type "M_Rectangular Duct Elbow - Mitered:Standard" | names: "M_Rectangular Duct Elbow - Mitered:Standard:478440" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Union:Standard" | object type "M_Rectangular Duct Union:Standard" | names: "M_Rectangular Duct Union:Standard:478588" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:478789" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_Cooling Tower - Closed Circuit - Counterflow - 67-189 kW:177 kW" | object type "M_Cooling Tower - Closed Circuit - Counterflow - 67-189 kW:177 kW" | names: "M_Cooling Tower - Closed Circuit - Counterflow - 67-189 kW:177 kW:513637" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          24 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "Tipos de tubería:Standard" | object type "Tipos de tubería:Standard" | names: "Tipos de tubería:Standard:513756", "Tipos de tubería:Standard:513770", "Tipos de tubería:Standard:513840" (+21 more) | property sets: Pset_DistributionFlowElementCommon, Pset_FlowSegmentDuctSegment, Pset_FlowSegmentPipeSegment, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Pipe Transition:Standard" | object type "M_Pipe Transition:Standard" | names: "M_Pipe Transition:Standard:513769" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Pipe Elbow:Standard" | object type "M_Pipe Elbow:Standard" | names: "M_Pipe Elbow:Standard:513778", "M_Pipe Elbow:Standard:513911" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Pipe Elbow:Standard" | object type "M_Pipe Elbow:Standard" | names: "M_Pipe Elbow:Standard:513854", "M_Pipe Elbow:Standard:513871" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_Centrifugal Fan - Rooftop - Upblast:1383-2808 LPS" | object type "M_Centrifugal Fan - Rooftop - Upblast:1383-2808 LPS" | names: "M_Centrifugal Fan - Rooftop - Upblast:1383-2808 LPS:516686" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:517064" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Pipe Tee:Standard" | object type "M_Pipe Tee:Standard" | names: "M_Pipe Tee:Standard:528301" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Pipe Transition:Standard" | object type "M_Pipe Transition:Standard" | names: "M_Pipe Transition:Standard:528306" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Pipe Tee:Standard" | object type "M_Pipe Tee:Standard" | names: "M_Pipe Tee:Standard:528351" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Pipe Transition:Standard" | object type "M_Pipe Transition:Standard" | names: "M_Pipe Transition:Standard:528356" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_Lighting and Appliance Panelboard - 480V MLO - Surface:400 A" | object type "M_Lighting and Appliance Panelboard - 480V MLO - Surface:400 A" | names: "M_Lighting and Appliance Panelboard - 480V MLO - Surface:CTP:532001" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff, Pset_ProvisionForVoid
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_Lighting and Appliance Panelboard - 208V MLO - Surface:400 A" | object type "M_Lighting and Appliance Panelboard - 208V MLO - Surface:400 A" | names: "M_Lighting and Appliance Panelboard - 208V MLO - Surface:AHP:532120" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff, Pset_ProvisionForVoid
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | object type "M_Rectangular Duct Transition - Angle:45 Degree" | names: "M_Rectangular Duct Transition - Angle:45 Degree:532661" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:STB 30.0" | object type "Suelo:STB 30.0" | FLOOR | names: "Suelo:STB 30.0:573547" | material: layers "Suelo:STB 30.0" ("Stahlbeton - Ortbeton" 300.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:Sonnenschutz" | object type "Suelo:Sonnenschutz" | FLOOR | names: "Suelo:Sonnenschutz:577773" | material: layers "Suelo:Sonnenschutz" ("Gitterrost" 100.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:Sonnenschutz" | object type "Suelo:Sonnenschutz" | FLOOR | names: "Suelo:Sonnenschutz:577773:2" | material: layers "Suelo:Sonnenschutz" ("Gitterrost" 100.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:Sonnenschutz" | object type "Suelo:Sonnenschutz" | FLOOR | names: "Suelo:Sonnenschutz:577773:3" | material: layers "Suelo:Sonnenschutz" ("Gitterrost" 100.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:Sonnenschutz" | object type "Suelo:Sonnenschutz" | FLOOR | names: "Suelo:Sonnenschutz:577773:4" | material: layers "Suelo:Sonnenschutz" ("Gitterrost" 100.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:Sonnenschutz" | object type "Suelo:Sonnenschutz" | FLOOR | names: "Suelo:Sonnenschutz:577773:5" | material: layers "Suelo:Sonnenschutz" ("Gitterrost" 100.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Suelo:Sonnenschutz" | object type "Suelo:Sonnenschutz" | FLOOR | names: "Suelo:Sonnenschutz:577773:6" | material: layers "Suelo:Sonnenschutz" ("Gitterrost" 100.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          4 x IFCCOLUMN | type IFCCOLUMNTYPE "Strut:1.5" x 1.5"" | object type "Strut:1.5" x 1.5"" | names: "Strut:1.5" x 1.5":691053", "Strut:1.5" x 1.5":691545", "Strut:1.5" x 1.5":692874" (+1 more) | material: "<Unnamed>" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "M_Rectangular Duct Elbow - Mitered:Standard" | object type "M_Rectangular Duct Elbow - Mitered:Standard" | names: "M_Rectangular Duct Elbow - Mitered:Standard:709694" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          8 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Elbow - Generic:Standard" | object type "M_Elbow - Generic:Standard" | names: "M_Elbow - Generic:Standard:711565", "M_Elbow - Generic:Standard:711687", "M_Elbow - Generic:Standard:711719" (+5 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Cap - Generic:Standard" | object type "M_Cap - Generic:Standard" | names: "M_Cap - Generic:Standard:815270" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Cap - Generic:Standard" | object type "M_Cap - Generic:Standard" | names: "M_Cap - Generic:Standard:817389" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff

Types
  IFCAIRTERMINALTYPE "M_Supply Diffuser - Sidewall:450 x 200" | 4 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:14 kW" | 1 occurrence | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
  IFCAIRTERMINALTYPE "M_Supply Diffuser - Sidewall:450 x 200" | 5 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCAIRTERMINALTYPE "M_Supply Diffuser - Sidewall:450 x 200" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTSEGMENTTYPE "Conducto rectangular:Mitered Elbows / Taps" | 634 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Elbow - Mitered:Standard" | 18 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Takeoff:Standard" | 62 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Endcap:Standard" | 17 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Endcap:Standard" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Takeoff:Standard" | 23 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Elbow - Mitered:Standard" | 10 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Endcap:Standard" | 5 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Endcap:Standard" | 13 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Takeoff:Standard" | 48 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCAIRTERMINALTYPE "M_Supply Diffuser - Sidewall:450 x 200" | 11 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCAIRTERMINALTYPE "M_Supply Diffuser - Sidewall:450 x 200" | 8 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:14 kW" | 1 occurrence | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Takeoff:Standard" | 2 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Endcap:Standard" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 4 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Elbow - Mitered:Standard" | 5 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 5 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 4 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 2 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Back Discharge:7 kW" | 1 occurrence | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
  IFCAIRTERMINALTYPE "M_Supply Diffuser - Sidewall:450 x 200" | 3 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCAIRTERMINALTYPE "M_Supply Diffuser - Sidewall:450 x 200" | 16 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCAIRTERMINALTYPE "M_Supply Diffuser - Sidewall:450 x 200" | 11 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:14 kW" | 1 occurrence | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Takeoff:Standard" | 2 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Elbow - Mitered:Standard" | 3 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:11 kW" | 2 occurrences | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 3 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Elbow - Mitered:Standard" | 4 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 3 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCAIRTERMINALTYPE "M_Supply Diffuser - Sidewall:450 x 200" | 2 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:7 kW" | 2 occurrences | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Elbow - Mitered:Standard" | 2 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 3 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:11 kW" | 1 occurrence | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 3 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 6 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCAIRTERMINALTYPE "M_Supply Diffuser - Sidewall:450 x 200" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:11 kW" | 2 occurrences | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:7 kW" | 1 occurrence | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCAIRTERMINALTYPE "M_Return Grille - Rectangular - Hosted:Standard" | 5 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Endcap:Standard" | 13 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Takeoff:Standard" | 6 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Elbow - Mitered:Standard" | 20 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Takeoff:Standard" | 11 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCAIRTERMINALTYPE "M_Return Grille - Rectangular - Hosted:Standard" | 3 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Endcap:Standard" | 8 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCAIRTERMINALTYPE "M_Return Grille - Rectangular - Hosted:Standard" | 2 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 2 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 2 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Takeoff:Standard" | 3 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Elbow - Mitered:Standard" | 6 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCAIRTERMINALTYPE "M_Return Grille - Rectangular - Hosted:Standard" | 2 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Endcap:Standard" | 16 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCAIRTERMINALTYPE "M_Return Grille - Rectangular - Hosted:Standard" | 5 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Takeoff:Standard" | 3 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 2 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCAIRTERMINALTYPE "M_Return Grille - Rectangular - Hosted:Standard" | 4 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCAIRTERMINALTYPE "M_Return Grille - Rectangular - Hosted:Standard" | 10 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCAIRTERMINALTYPE "M_Supply Diffuser - Sidewall:450 x 200" | 4 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Takeoff:Standard" | 25 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Takeoff:Standard" | 10 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCAIRTERMINALTYPE "M_Supply Diffuser - Sidewall:450 x 200" | 2 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCAIRTERMINALTYPE "M_Supply Diffuser - Sidewall:450 x 200" | 2 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:11 kW" | 1 occurrence | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 2 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 2 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCAIRTERMINALTYPE "M_Return Grille - Rectangular - Hosted:Standard" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCAIRTERMINALTYPE "M_Return Grille - Rectangular - Hosted:Standard" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Elbow - Mitered:Standard" | 18 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCLIGHTFIXTURETYPE "M_Sconce Light - Flat Round:60W - 277V" | 66 occurrences | material: "Glass - Frosted" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Elbow - Mitered:Standard" | 3 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "M_Wall Occupancy Sensor - Regular Voltage:Passive Infrared - 277 V" | 54 occurrences | material: materials ("<Unnamed>", "<Unnamed>") | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "M_Lighting Switches:Single Pole" | 9 occurrences | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Takeoff:Standard" | 23 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Elbow - Mitered:Standard" | 37 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Elbow - Mitered:Standard" | 25 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Takeoff:Standard" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Takeoff:Standard" | 43 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Elbow - Mitered:Standard" | 10 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 2 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Elbow - Mitered:Standard" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCAIRTERMINALTYPE "M_Supply Diffuser - Sidewall:450 x 200" | 16 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Right Return - Back Discharge:11 kW" | 2 occurrences | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Endcap:Standard" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Elbow - Mitered:Standard" | 2 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Endcap:Standard" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Right Return - Back Discharge:11 kW" | 1 occurrence | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Endcap:Standard" | 2 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Elbow - Mitered:Standard" | 4 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Elbow - Mitered:Standard" | 3 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Elbow - Mitered:Standard" | 2 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Takeoff:Standard" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCAIRTERMINALTYPE "Exhaust Grille - Rectangular - Hosted - Horizontal:Standard" | 2 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Union:Standard" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Elbow - Mitered:Standard" | 2 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCPIPESEGMENTTYPE "Tipos de tubería:Standard" | 488 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCPIPEFITTINGTYPE "M_Pipe Elbow:Standard" | 118 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCPIPEFITTINGTYPE "M_Pipe Transition:Standard" | 30 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCPIPEFITTINGTYPE "M_Pipe Elbow:Standard" | 69 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCPIPEFITTINGTYPE "M_Pipe Tee:Standard" | 47 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCPIPEFITTINGTYPE "M_Pipe Tee:Standard" | 24 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCPIPEFITTINGTYPE "M_Pipe Transition:Standard" | 40 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 2 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCCOLUMNTYPE "STB Stütze - rund:STB d=30" | COLUMN | 43 occurrences | material: "Stahlbeton - Fertigbeton" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
  IFCWALLTYPE "Muro básico:STB 30.0 Rot" | STANDARD | 2 occurrences | material: layers "Muro básico:STB 30.0 Rot" ("Stahlbeton - Ortbeton - Rot" 300.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Muro básico:STB 30.0" | STANDARD | 8 occurrences | material: layers "Muro básico:STB 30.0" ("Stahlbeton - Ortbeton" 300.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCSLABTYPE "Suelo:STB 30.0" | FLOOR | 1 occurrence | material: layers "Suelo:STB 30.0" ("Stahlbeton - Ortbeton" 300.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCWALLTYPE "Muro básico:STB 20.0" | STANDARD | 18 occurrences | material: layers "Muro básico:STB 20.0" ("Stahlbeton - Ortbeton" 200.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Muro básico:MW 17.5" | STANDARD | 29 occurrences | material: layers "Muro básico:MW 17.5" ("Mauerwerk - Ziegel" 175.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCDOORSTYLE "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26" | SINGLE_SWING_LEFT | 18 occurrences | material: materials ("<Unnamed>", "Tür - Stahl Zarge", "<Unnamed>", "Tür - Stahl Griff") | property sets: Drehflügel 1-flg - Stahlzarge:88.5 x 2.26:573577, Pset_DoorCommon, Pset_QuantityTakeOff
  IFCDOORSTYLE "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26" | SINGLE_SWING_RIGHT | 10 occurrences | material: materials ("<Unnamed>", "Tür - Stahl Zarge", "<Unnamed>", "Tür - Stahl Griff") | property sets: Drehflügel 1-flg - Stahlzarge:88.5 x 2.26:573583, Pset_DoorCommon, Pset_QuantityTakeOff
  IFCWALLTYPE "Muro básico:MW 11.5" | STANDARD | 61 occurrences | material: layers "Muro básico:MW 11.5" ("Mauerwerk - Ziegel" 115.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Muro básico:Lamelle 11.5" | STANDARD | 7 occurrences | material: layers "Muro básico:Lamelle 11.5" ("Mauerwerk - Lamellen" 115.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCCURTAINWALLTYPE "Muro cortina:Standard" | 33 occurrences | property sets: Pset_CurtainWallCommon, Pset_QuantityTakeOff
  IFCDOORSTYLE "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26" | SINGLE_SWING_RIGHT | 3 occurrences | material: materials ("<Unnamed>", "<Unnamed>", "Tür - Stahl Zarge", "Tür - Stahl Griff") | property sets: Drehflügel 1-flg - Stahlzarge:88.5 x 2.26:573668, Pset_DoorCommon, Pset_QuantityTakeOff
  IFCDOORSTYLE "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26" | SINGLE_SWING_LEFT | 10 occurrences | material: materials ("<Unnamed>", "Tür - Stahl Zarge", "<Unnamed>", "Tür - Stahl Griff") | property sets: Drehflügel 1-flg - Stahlzarge:88.5 x 2.26:573673, Pset_DoorCommon, Pset_QuantityTakeOff
  IFCWALLTYPE "Muro básico:WC Trennwand 5.0" | STANDARD | 7 occurrences | material: layers "Muro básico:WC Trennwand 5.0" ("WC Trennwand" 50.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCDOORSTYLE "Drehflügel 1-flg - Stahlzarge:76 x 2.26" | SINGLE_SWING_RIGHT | 4 occurrences | material: materials ("Tür - Stahl Zarge", "<Unnamed>", "<Unnamed>", "Tür - Stahl Griff") | property sets: Drehflügel 1-flg - Stahlzarge:76 x 2.26:573783, Pset_DoorCommon, Pset_QuantityTakeOff
  IFCCOLUMNTYPE "STB Stütze - rund:STB d=30" | COLUMN | 3 occurrences | material: "Stahlbeton - Fertigbeton" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
  IFCBUILDINGELEMENTPROXYTYPE "Aufzug 2-flg:Aufzug 2-flg" | 3 occurrences | material: materials ("<Unnamed>", "Tür - Aufzug Metall") | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
  IFCDOORSTYLE "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26" | SINGLE_SWING_LEFT | 19 occurrences | material: materials ("<Unnamed>", "<Unnamed>", "Tür - Stahl Zarge", "Tür - Stahl Griff") | property sets: Drehflügel 1-flg - Stahlzarge:88.5 x 2.26:575087, Pset_DoorCommon, Pset_QuantityTakeOff
  IFCDOORSTYLE "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26" | SINGLE_SWING_RIGHT | 21 occurrences | material: materials ("<Unnamed>", "<Unnamed>", "Tür - Stahl Zarge", "Tür - Stahl Griff") | property sets: Drehflügel 1-flg - Stahlzarge:88.5 x 2.26:575089, Pset_DoorCommon, Pset_QuantityTakeOff
  IFCSLABTYPE "Suelo:FB 15.0 - Holzdielen" | FLOOR | 1 occurrence | material: layers "Suelo:FB 15.0 - Holzdielen" ("Bodenbelag Holzdielen" 30., "Decke - Estrich" 40., "Default Floor" 80.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Suelo:FB 15.0 - Teppich" | FLOOR | 1 occurrence | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Suelo:FB 15.0 - Teppich" | FLOOR | 1 occurrence | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Suelo:FB 15.0 - Teppich" | FLOOR | 1 occurrence | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Suelo:FB 15.0 - Teppich" | FLOOR | 1 occurrence | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Suelo:FB 15.0 - Teppich" | FLOOR | 1 occurrence | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Suelo:FB 15.0 - Teppich" | FLOOR | 1 occurrence | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Suelo:FB 15.0 - Teppich" | FLOOR | 1 occurrence | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Suelo:FB 15.0 - Teppich" | FLOOR | 1 occurrence | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Suelo:FB 15.0 - Teppich" | FLOOR | 1 occurrence | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Suelo:FB 15.0 - Teppich" | FLOOR | 1 occurrence | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Suelo:FB 15.0 - Teppich" | FLOOR | 1 occurrence | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Suelo:FB 15.0 - Teppich" | FLOOR | 1 occurrence | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Suelo:FB 15.0 - Teppich" | FLOOR | 1 occurrence | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Suelo:FB 15.0 - Teppich" | FLOOR | 1 occurrence | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Suelo:FB 15.0 - Teppich" | FLOOR | 1 occurrence | material: layers "Suelo:FB 15.0 - Teppich" ("Bodenbelag Teppich" 10., "Decke - Estrich" 60., "Wärmedämmung - hart" 80.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Suelo:FB 10.0 - Fliesen 15 x 15" | FLOOR | 1 occurrence | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Suelo:FB 10.0 - Fliesen 15 x 15" | FLOOR | 1 occurrence | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Suelo:FB 10.0 - Fliesen 15 x 15" | FLOOR | 1 occurrence | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Suelo:FB 10.0 - Fliesen 15 x 15" | FLOOR | 1 occurrence | material: layers "Suelo:FB 10.0 - Fliesen 15 x 15" ("Decke - Fliesen 15 x 15" 10., "Decke - Estrich" 60., "Wärmedämmung - hart" 80.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Suelo:FB 15.0 - Holzdielen" | FLOOR | 1 occurrence | material: layers "Suelo:FB 15.0 - Holzdielen" ("Bodenbelag Holzdielen" 30., "Decke - Estrich" 40., "Default Floor" 80.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Suelo:FB 15.0 - Fliesen 50 x 50" | FLOOR | 1 occurrence | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Suelo:FB 15.0 - Fliesen 50 x 50" | FLOOR | 1 occurrence | material: layers "Suelo:FB 15.0 - Fliesen 50 x 50" ("Bodenbelag Fliesen 50 x 50" 10., "Decke - Estrich" 60., "Wärmedämmung - hart" 80.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Suelo:FB 15.0 - Holzdielen" | FLOOR | 1 occurrence | material: layers "Suelo:FB 15.0 - Holzdielen" ("Bodenbelag Holzdielen" 30., "Decke - Estrich" 40., "Default Floor" 80.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCBUILDINGELEMENTPROXYTYPE "M_Lighting and Appliance Panelboard - 480V MLO - Surface:125 A" | 1 occurrence | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff, Pset_ProvisionForVoid
  IFCBUILDINGELEMENTPROXYTYPE "M_Lighting and Appliance Panelboard - 208V MLO - Surface:400 A" | 7 occurrences | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff, Pset_ProvisionForVoid
  IFCBUILDINGELEMENTPROXYTYPE "M_Lighting and Appliance Panelboard - 480V MCB - Surface:100 A" | 6 occurrences | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff, Pset_ProvisionForVoid
  IFCBUILDINGELEMENTPROXYTYPE "M_Lighting and Appliance Panelboard - 208V MCB - Surface:100 A" | 3 occurrences | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff, Pset_ProvisionForVoid
  IFCBUILDINGELEMENTPROXYTYPE "M_Dry Type Transformer - 480-208Y120 - NEMA Type 3R:15 kVA" | 3 occurrences | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "M_Dry Type Transformer - 480-208Y120 - NEMA Type 2:500 kVA" | 1 occurrence | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "M_Circuit Breaker Switchboard:762mmx965mm" | 1 occurrence | material: materials ("<Unnamed>", "<Unnamed>") | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
  IFCCABLECARRIERSEGMENTTYPE "Tubo sin uniones:Rigid Nonmetallic Conduit (RNC Sch 80)" | CONDUITSEGMENT | 19 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCCABLECARRIERFITTINGTYPE "Conduit Elbow - without Fittings - RNC:Standard" | 12 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCCABLECARRIERFITTINGTYPE "Conduit Body - Type L - Aluminum:Standard" | 2 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTSEGMENTTYPE "Conducto redondo:Taps" | 9 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCPIPEFITTINGTYPE "M_Tee - Generic:Standard" | 5 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCCABLECARRIERSEGMENTTYPE "Bandeja de cables con uniones:Ladder Cable Tray" | CABLETRAYSEGMENT | 17 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCCABLECARRIERFITTINGTYPE "M_Ladder Horizontal Tee:300mm Radius" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCCABLECARRIERFITTINGTYPE "M_Ladder Vertical Outside Bend:Standard" | 4 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCCABLECARRIERFITTINGTYPE "M_Ladder Horizontal Bend:Standard" | 2 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Union:Standard" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCCABLECARRIERFITTINGTYPE "M_Ladder Vertical Inside Bend:Standard" | 5 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCCABLECARRIERFITTINGTYPE "M_Ladder Vertical Inside Bend:Standard" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCCABLECARRIERFITTINGTYPE "M_Ladder Vertical Outside Bend:Standard" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 2 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Takeoff:Standard" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Takeoff:Standard" | 2 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCPIPEFITTINGTYPE "M_Tee - Generic:Standard" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCPIPEFITTINGTYPE "M_Transition - Generic:Standard" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCPIPEFITTINGTYPE "M_Elbow - Generic:Standard" | 11 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCPIPEFITTINGTYPE "M_Tee - Generic:Standard" | 3 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCPIPEFITTINGTYPE "M_Transition - Generic:Standard" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCPIPEFITTINGTYPE "M_Elbow - Generic:Standard" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "M_Lighting and Appliance Panelboard - 480V MCB - Surface:400 A" | 3 occurrences | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff, Pset_ProvisionForVoid
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Elbow - Mitered:Standard" | 2 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCAIRTERMINALTYPE "M_Supply Diffuser - Rectangular Face Round Neck:600x600 - 250 Neck" | 13 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCAIRTERMINALTYPE "M_Supply Diffuser - Rectangular Face Round Neck:600x600 - 250 Neck" | 34 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCAIRTERMINALTYPE "M_Supply Diffuser - Rectangular Face Round Neck:600x600 - 250 Neck" | 9 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCAIRTERMINALTYPE "M_Supply Diffuser - Rectangular Face Round Neck:600x600 - 250 Neck" | 8 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCAIRTERMINALTYPE "M_Supply Diffuser - Rectangular Face Round Neck:600x600 - 250 Neck" | 6 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCAIRTERMINALTYPE "M_Supply Diffuser - Rectangular Face Round Neck:600x600 - 250 Neck" | 2 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCAIRTERMINALTYPE "M_Supply Diffuser - Sidewall:450 x 200" | 2 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCAIRTERMINALTYPE "M_Supply Diffuser - Sidewall:450 x 200" | 4 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCAIRTERMINALTYPE "M_Supply Diffuser - Sidewall:450 x 200" | 4 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Back Discharge:14 kW" | 2 occurrences | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:14 kW" | 1 occurrence | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
  IFCDUCTSEGMENTTYPE "Conducto rectangular:Mitered Elbows / Tees" | 85 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 2 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTSEGMENTTYPE "Conducto flexible redondo:Flex - Round" | FLEXIBLESEGMENT | 113 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular to Round Duct Transition - Angle:45 Degree" | 86 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Tee:Standard" | 2 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 6 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 2 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 2 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 4 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:14 kW" | 1 occurrence | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular to Round Duct Transition - Angle:45 Degree" | 10 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Tee:Standard" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Cross:Standard" | 4 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Cross:Standard" | 4 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Takeoff:Standard" | 8 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Endcap:Standard" | 7 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 7 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 12 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:11 kW" | 1 occurrence | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Elbow - Mitered:Standard" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Cross:Standard" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:11 kW" | 2 occurrences | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 2 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 5 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 2 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:11 kW" | 1 occurrence | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Endcap:Standard" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Right Return - Back Discharge:7 kW" | 1 occurrence | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Back Discharge:14 kW" | 1 occurrence | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Elbow - Mitered:Standard" | 2 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:11 kW" | 1 occurrence | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Tee:Standard" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Tee:Standard" | 2 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 5 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Takeoff:Standard" | 2 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 2 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCAIRTERMINALTYPE "M_Return Diffuser:600 x 600 Face 300 x 300 Connection" | 28 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCLIGHTFIXTURETYPE "M_Plain Recessed Lighting Fixture:600x600 - 277" | 195 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCLIGHTFIXTURETYPE "M_Pendant Light - Linear - 2 Lamp:1200mm - 277V" | 19 occurrences | material: materials ("Metal - Paint Finish - Ivory, Glossy", "Metal - Paint Finish - Ivory, Glossy", "Glass - White, High Luminance") | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCLIGHTFIXTURETYPE "M_Pendant Light - Disk:100W - 277V" | 65 occurrences | material: materials ("Plastic - Blue", "Glass - Clear, Grey", "Metal - Chrome") | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCLIGHTFIXTURETYPE "M_Pendant Light - Linear - 2 Lamp:2400mm - 277V" | 65 occurrences | material: materials ("Glass - White, High Luminance", "Metal - Paint Finish - Ivory, Glossy", "Metal - Paint Finish - Ivory, Glossy") | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCAIRTERMINALTYPE "M_Exhaust Grill:600 x 600 Face 300 x 300 Connection" | 4 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "M_Lighting and Appliance Panelboard - 480V MLO - Surface:400 A" | 2 occurrences | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff, Pset_ProvisionForVoid
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Takeoff:Standard" | 2 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Right Return - Back Discharge:11 kW" | 1 occurrence | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 2 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 3 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Takeoff:Standard" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Elbow - Mitered:Standard" | 2 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Union:Standard" | 4 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Elbow - Mitered:Standard" | 2 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Elbow - Mitered:Standard" | 2 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Takeoff:Standard" | 2 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 2 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCPIPEFITTINGTYPE "M_Pipe Transition:Standard" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCPIPEFITTINGTYPE "M_Pipe Elbow:Standard" | 20 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCPIPEFITTINGTYPE "M_Pipe Tee:Standard" | 5 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCPIPEFITTINGTYPE "M_Pipe Transition:Standard" | 6 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCPIPEFITTINGTYPE "M_Pipe Transition:Standard" | 12 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCPIPEFITTINGTYPE "M_Pipe Transition:Standard" | 2 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Back Discharge:14 kW" | 1 occurrence | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
  IFCAIRTERMINALTYPE "M_Supply Diffuser - Rectangular Face Round Neck:600x600 - 250 Neck" | 4 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Elbow - Mitered:Standard" | 3 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Round Duct Takeoff:Standard" | 2 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Round Duct Takeoff:Standard" | 4 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Round Duct Takeoff:Standard" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Round Duct Takeoff:Standard" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Round Duct Transition - Angle:45 Degree" | 2 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCAIRTERMINALTYPE "M_Supply Diffuser - Rectangular Face Round Neck:600x600 - 200 Neck" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCAIRTERMINALTYPE "M_Supply Diffuser - Rectangular Face Round Neck:600x600 - 200 Neck" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCAIRTERMINALTYPE "M_Supply Diffuser - Rectangular Face Round Neck:600x600 - 200 Neck" | 3 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Back Discharge:11 kW" | 1 occurrence | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 2 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular to Round Duct Transition - Angle:45 Degree" | 5 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Elbow - Mitered:Standard" | 2 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Tee:Standard" | 2 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 3 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Tee:Standard" | 2 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 2 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDISTRIBUTIONELEMENTTYPE "M_Water Closet - Flush Valve - Wall Mounted:Public - 6.1 Lpf" | 5 occurrences | material: materials ("<Unnamed>", "<Unnamed>", "<Unnamed>") | property sets: Pset_QuantityTakeOff
  IFCDISTRIBUTIONELEMENTTYPE "M_Urinal - Wall Hung:20 mm Flush Valve" | 2 occurrences | material: materials ("<Unnamed>", "<Unnamed>") | property sets: Pset_QuantityTakeOff
  IFCDISTRIBUTIONELEMENTTYPE "M_Lavatory - Wall Mounted:485 mmx355 mm - Public" | 4 occurrences | material: materials ("<Unnamed>", "<Unnamed>") | property sets: Pset_QuantityTakeOff
  IFCFIRESUPPRESSIONTERMINALTYPE "M_Sprinkler - Pendent - Hosted:15 mm Pendent on Drop with Guard" | 6 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCPIPEFITTINGTYPE "M_Pipe Cross:Standard" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCSLABTYPE "Suelo:STB 30.0" | FLOOR | 1 occurrence | material: layers "Suelo:STB 30.0" ("Stahlbeton - Ortbeton" 300.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCCOLUMNTYPE "STB Stütze - rund:STB d=30" | COLUMN | 37 occurrences | material: "Stahlbeton - Fertigbeton" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "STB Stütze - rund:STB d=30" | COLUMN | 2 occurrences | material: "Stahlbeton - Fertigbeton" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "STB Stütze - rund:STB d=30" | COLUMN | 1 occurrence | material: "Stahlbeton - Fertigbeton" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "STB Stütze - rund:STB d=30" | COLUMN | 1 occurrence | material: "Stahlbeton - Fertigbeton" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "STB Stütze - rund:STB d=30" | COLUMN | 1 occurrence | material: "Stahlbeton - Fertigbeton" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
  IFCCOLUMNTYPE "STB Stütze - rund:STB d=30" | COLUMN | 1 occurrence | material: "Stahlbeton - Fertigbeton" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
  IFCDOORSTYLE "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26" | SINGLE_SWING_RIGHT | 4 occurrences | material: materials ("<Unnamed>", "<Unnamed>", "Tür - Stahl Zarge", "Tür - Stahl Griff") | property sets: Drehflügel 1-flg - Stahlzarge:88.5 x 2.26:573747, Pset_DoorCommon, Pset_QuantityTakeOff
  IFCDOORSTYLE "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26" | SINGLE_SWING_LEFT | 4 occurrences | material: materials ("Tür - Stahl Zarge", "<Unnamed>", "<Unnamed>", "Tür - Stahl Griff") | property sets: Drehflügel 1-flg - Stahlzarge:88.5 x 2.26:573748, Pset_DoorCommon, Pset_QuantityTakeOff
  IFCSLABTYPE "Suelo:FB 15.0 - Fliesen 50 x 50" | FLOOR | 1 occurrence | material: layers "Suelo:FB 15.0 - Fliesen 50 x 50" ("Bodenbelag Fliesen 50 x 50" 10., "Decke - Estrich" 60., "Wärmedämmung - hart" 80.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCCOLUMNTYPE "STB Stütze - rund:STB d=30" | COLUMN | 1 occurrence | material: "Stahlbeton - Fertigbeton" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
  IFCBUILDINGELEMENTPROXYTYPE "Stahlbalkon:Stahlbalkon" | 66 occurrences | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Stahlbalkon:Stahlbalkon" | 15 occurrences | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
  IFCSLABTYPE "Suelo:Sonnenschutz" | FLOOR | 1 occurrence | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Suelo:Sonnenschutz" | FLOOR | 1 occurrence | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Suelo:Sonnenschutz" | FLOOR | 1 occurrence | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Suelo:Sonnenschutz" | FLOOR | 1 occurrence | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Suelo:Sonnenschutz" | FLOOR | 1 occurrence | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Suelo:Sonnenschutz" | FLOOR | 1 occurrence | material: layers "Suelo:Sonnenschutz" ("Gitterrost" 100.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCBUILDINGELEMENTPROXYTYPE "Texto de modelo:Logo" | 1 occurrence | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
  IFCSLABTYPE "Suelo:FB 15.0 - Holzdielen" | FLOOR | 1 occurrence | material: layers "Suelo:FB 15.0 - Holzdielen" ("Bodenbelag Holzdielen" 30., "Decke - Estrich" 40., "Default Floor" 80.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Suelo:FB 15.0 - Holzdielen" | FLOOR | 1 occurrence | material: layers "Suelo:FB 15.0 - Holzdielen" ("Bodenbelag Holzdielen" 30., "Decke - Estrich" 40., "Default Floor" 80.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Suelo:FB 15.0 - Teppich" | FLOOR | 1 occurrence | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Suelo:FB 15.0 - Teppich" | FLOOR | 1 occurrence | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Suelo:FB 15.0 - Teppich" | FLOOR | 1 occurrence | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Suelo:FB 15.0 - Teppich" | FLOOR | 1 occurrence | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Suelo:FB 15.0 - Teppich" | FLOOR | 1 occurrence | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Suelo:FB 15.0 - Teppich" | FLOOR | 1 occurrence | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Suelo:FB 15.0 - Teppich" | FLOOR | 1 occurrence | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Suelo:FB 15.0 - Teppich" | FLOOR | 1 occurrence | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Suelo:FB 15.0 - Teppich" | FLOOR | 1 occurrence | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Suelo:FB 15.0 - Teppich" | FLOOR | 1 occurrence | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Suelo:FB 15.0 - Teppich" | FLOOR | 1 occurrence | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Suelo:FB 15.0 - Teppich" | FLOOR | 1 occurrence | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Suelo:FB 15.0 - Teppich" | FLOOR | 1 occurrence | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Suelo:FB 15.0 - Teppich" | FLOOR | 1 occurrence | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Suelo:FB 15.0 - Teppich" | FLOOR | 1 occurrence | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Suelo:FB 15.0 - Teppich" | FLOOR | 1 occurrence | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Suelo:FB 15.0 - Teppich" | FLOOR | 1 occurrence | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Suelo:FB 15.0 - Teppich" | FLOOR | 1 occurrence | material: layers "Suelo:FB 15.0 - Teppich" ("Bodenbelag Teppich" 10., "Decke - Estrich" 60., "Wärmedämmung - hart" 80.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Suelo:FB 10.0 - Fliesen 15 x 15" | FLOOR | 1 occurrence | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Suelo:FB 10.0 - Fliesen 15 x 15" | FLOOR | 1 occurrence | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Suelo:FB 10.0 - Fliesen 15 x 15" | FLOOR | 1 occurrence | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Suelo:FB 10.0 - Fliesen 15 x 15" | FLOOR | 1 occurrence | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Suelo:FB 10.0 - Fliesen 15 x 15" | FLOOR | 1 occurrence | material: layers "Suelo:FB 10.0 - Fliesen 15 x 15" ("Decke - Fliesen 15 x 15" 10., "Decke - Estrich" 60., "Wärmedämmung - hart" 80.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCDOORSTYLE "Drehflügel 1-flg - Stahlzarge:76 x 2.26" | SINGLE_SWING_RIGHT | 2 occurrences | material: materials ("<Unnamed>", "Tür - Stahl Zarge", "<Unnamed>", "Tür - Stahl Griff") | property sets: Drehflügel 1-flg - Stahlzarge:76 x 2.26:578641, Pset_DoorCommon, Pset_QuantityTakeOff
  IFCDOORSTYLE "Drehflügel 1-flg - Stahlzarge:76 x 2.26" | SINGLE_SWING_LEFT | 2 occurrences | material: materials ("Tür - Stahl Zarge", "<Unnamed>", "<Unnamed>", "Tür - Stahl Griff") | property sets: Drehflügel 1-flg - Stahlzarge:76 x 2.26:578643, Pset_DoorCommon, Pset_QuantityTakeOff
  IFCSLABTYPE "Suelo:FB 15.0 - Holzdielen" | FLOOR | 1 occurrence | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Suelo:FB 15.0 - Holzdielen" | FLOOR | 1 occurrence | material: layers "Suelo:FB 15.0 - Holzdielen" ("Bodenbelag Holzdielen" 30., "Decke - Estrich" 40., "Default Floor" 80.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCCOVERINGTYPE "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "M_Water Heater - Tankless:2.3 L" | 1 occurrence | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
  IFCPIPEFITTINGTYPE "M_Pipe Tee:Standard" | 5 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCPIPEFITTINGTYPE "M_Pipe Transition:Standard" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCPIPEFITTINGTYPE "M_Pipe Elbow:Standard" | 5 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCPIPEFITTINGTYPE "M_Pipe Transition:Standard" | 2 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCPIPEFITTINGTYPE "M_Pipe Cross:Standard" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCPIPEFITTINGTYPE "M_Pipe Elbow:Standard" | 3 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCPIPEFITTINGTYPE "M_Pipe Tee:Standard" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCPIPEFITTINGTYPE "M_Tee Sanitary - PVC - Sch 40 - DWV:Standard" | 4 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCPIPEFITTINGTYPE "M_Pipe Transition:Standard" | 4 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCPIPEFITTINGTYPE "M_Bend - PVC - Sch 40 - DWV:Standard" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCPIPEFITTINGTYPE "M_Transition - Generic:Standard" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCPIPEFITTINGTYPE "M_Bend - PVC - Sch 40 - DWV:Standard" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCPIPEFITTINGTYPE "M_Bend - PVC - Sch 40 - DWV:Standard" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCPIPEFITTINGTYPE "M_Bend - PVC - Sch 40 - DWV:Standard" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCPIPEFITTINGTYPE "M_Bend - PVC - Sch 40 - DWV:Standard" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCPIPEFITTINGTYPE "M_Bend - PVC - Sch 40 - DWV:Standard" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCPIPEFITTINGTYPE "M_Transition - Generic:Standard" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCPIPEFITTINGTYPE "M_Tee - Generic:Standard" | 4 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCPIPEFITTINGTYPE "M_Transition - Generic:Standard" | 4 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCPIPEFITTINGTYPE "M_Pipe Tee:Standard" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCPIPEFITTINGTYPE "M_Elbow - Generic:Standard" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCPIPEFITTINGTYPE "M_Transition - Generic:Standard" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCPIPEFITTINGTYPE "M_Transition - Generic:Standard" | 2 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCPIPEFITTINGTYPE "M_Tee - Generic:Standard" | 3 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCPIPEFITTINGTYPE "M_Transition - Generic:Standard" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCPIPEFITTINGTYPE "M_Transition - Generic:Standard" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCPIPEFITTINGTYPE "M_Elbow - Generic:Standard" | 5 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCPIPEFITTINGTYPE "M_Transition - Generic:Standard" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCPIPEFITTINGTYPE "M_Transition - Generic:Standard" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCPIPEFITTINGTYPE "M_Transition - Generic:Standard" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCPIPEFITTINGTYPE "M_Transition - Generic:Standard" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 2 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Endcap:Standard" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCPIPEFITTINGTYPE "M_Cross - Generic:Standard" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular to Round Duct Transition - Angle:45 Degree" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:18 kW" | 1 occurrence | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:14 kW" | 1 occurrence | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:14 kW" | 1 occurrence | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:14 kW" | 2 occurrences | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Right Return - Back Discharge:11 kW" | 1 occurrence | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Back Discharge:14 kW" | 1 occurrence | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:7 kW" | 1 occurrence | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:7 kW" | 1 occurrence | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:7 kW" | 1 occurrence | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
  IFCAIRTERMINALTYPE "M_Supply Diffuser - Rectangular Face Round Neck:600x600 - 250 Neck" | 8 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCAIRTERMINALTYPE "M_Supply Diffuser - Rectangular Face Round Neck:600x600 - 250 Neck" | 4 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCAIRTERMINALTYPE "M_Supply Diffuser - Rectangular Face Round Neck:600x600 - 250 Neck" | 4 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCAIRTERMINALTYPE "M_Supply Diffuser - Rectangular Face Round Neck:600x600 - 250 Neck" | 16 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Cross:Standard" | 7 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 14 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Cross:Standard" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 4 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Tee:Standard" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular to Round Duct Transition - Angle:45 Degree" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Cross:Standard" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Elbow - Mitered:Standard" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Tee:Standard" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 2 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Tee:Standard" | 2 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 4 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Takeoff:Standard" | 4 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Right Discharge:18 kW" | 1 occurrence | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Endcap:Standard" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Endcap:Standard" | 2 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Takeoff:Standard" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Left Return - Back Discharge:11 kW" | 1 occurrence | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "M_WSHP - Horizontal - High Efficiency - 7-18 kW - Right Return - Back Discharge:11 kW" | 1 occurrence | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Elbow - Mitered:Standard" | 2 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Takeoff:Standard" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Elbow - Mitered:Standard" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Tee:Standard" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 2 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Takeoff:Standard" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Elbow - Mitered:Standard" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Tee:Standard" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCAIRTERMINALTYPE "M_Return Diffuser:600 x 600 Face 300 x 300 Connection" | 12 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCAIRTERMINALTYPE "M_Return Diffuser:600 x 600 Face 300 x 300 Connection" | 2 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCAIRTERMINALTYPE "M_Return Diffuser:600 x 600 Face 300 x 300 Connection" | 2 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCAIRTERMINALTYPE "M_Return Diffuser:600 x 600 Face 300 x 300 Connection" | 4 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCAIRTERMINALTYPE "M_Return Diffuser:600 x 600 Face 300 x 300 Connection" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCAIRTERMINALTYPE "M_Return Diffuser:600 x 600 Face 300 x 300 Connection" | 2 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCAIRTERMINALTYPE "M_Return Diffuser:600 x 600 Face 300 x 300 Connection" | 8 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCAIRTERMINALTYPE "M_Exhaust Grill:600 x 600 Face 300 x 300 Connection" | 2 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCPIPEFITTINGTYPE "M_Pipe Elbow:Standard" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCPIPEFITTINGTYPE "M_Pipe Elbow:Standard" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCPIPEFITTINGTYPE "M_Pipe Elbow:Standard" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCPIPEFITTINGTYPE "M_Pipe Elbow:Standard" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCPIPEFITTINGTYPE "M_Pipe Elbow:Standard" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCSLABTYPE "Suelo:STB 30.0" | FLOOR | 1 occurrence | material: layers "Suelo:STB 30.0" ("Stahlbeton - Ortbeton" 300.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCCOLUMNTYPE "STB Stütze - rund:STB d=30" | COLUMN | 41 occurrences | material: "Stahlbeton - Fertigbeton" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
  IFCDOORSTYLE "Drehflügel 1-flg - Stahlzarge:76 x 2.26" | SINGLE_SWING_RIGHT | 1 occurrence | material: materials ("Tür - Stahl Zarge", "<Unnamed>", "<Unnamed>", "Tür - Stahl Griff") | property sets: Drehflügel 1-flg - Stahlzarge:76 x 2.26:573721, Pset_DoorCommon, Pset_QuantityTakeOff
  IFCDOORSTYLE "Drehflügel 1-flg - Stahlzarge:76 x 2.26" | SINGLE_SWING_LEFT | 1 occurrence | material: materials ("<Unnamed>", "<Unnamed>", "Tür - Stahl Zarge", "Tür - Stahl Griff") | property sets: Drehflügel 1-flg - Stahlzarge:76 x 2.26:573722, Pset_DoorCommon, Pset_QuantityTakeOff
  IFCDOORSTYLE "Drehflügel 1-flg - Stahlzarge:76 x 2.26" | SINGLE_SWING_RIGHT | 1 occurrence | material: materials ("<Unnamed>", "Tür - Stahl Zarge", "<Unnamed>", "Tür - Stahl Griff") | property sets: Drehflügel 1-flg - Stahlzarge:76 x 2.26:573723, Pset_DoorCommon, Pset_QuantityTakeOff
  IFCDOORSTYLE "Drehflügel 1-flg - Stahlzarge:76 x 2.26" | SINGLE_SWING_LEFT | 1 occurrence | material: materials ("<Unnamed>", "<Unnamed>", "Tür - Stahl Zarge", "Tür - Stahl Griff") | property sets: Drehflügel 1-flg - Stahlzarge:76 x 2.26:573724, Pset_DoorCommon, Pset_QuantityTakeOff
  IFCWALLTYPE "Muro básico:STB 25.0 WD 12.0" | STANDARD | 1 occurrence | material: layers "Muro básico:STB 25.0 WD 12.0" ("Wärmedämmung - hart" 120., "Stahlbeton - Ortbeton" 250.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCSLABTYPE "Suelo:FB 15.0 - Fliesen 50 x 50" | FLOOR | 1 occurrence | material: layers "Suelo:FB 15.0 - Fliesen 50 x 50" ("Bodenbelag Fliesen 50 x 50" 10., "Decke - Estrich" 60., "Wärmedämmung - hart" 80.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Suelo:Sonnenschutz" | FLOOR | 1 occurrence | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Suelo:Sonnenschutz" | FLOOR | 1 occurrence | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Suelo:Sonnenschutz" | FLOOR | 1 occurrence | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Suelo:Sonnenschutz" | FLOOR | 1 occurrence | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Suelo:Sonnenschutz" | FLOOR | 1 occurrence | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Suelo:Sonnenschutz" | FLOOR | 1 occurrence | material: layers "Suelo:Sonnenschutz" ("Gitterrost" 100.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Suelo:FB 10.0 - Fliesen 15 x 15" | FLOOR | 1 occurrence | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Suelo:FB 10.0 - Fliesen 15 x 15" | FLOOR | 1 occurrence | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Suelo:FB 10.0 - Fliesen 15 x 15" | FLOOR | 1 occurrence | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Suelo:FB 10.0 - Fliesen 15 x 15" | FLOOR | 1 occurrence | material: layers "Suelo:FB 10.0 - Fliesen 15 x 15" ("Decke - Fliesen 15 x 15" 10., "Decke - Estrich" 60., "Wärmedämmung - hart" 80.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCDOORSTYLE "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26" | SINGLE_SWING_RIGHT | 2 occurrences | material: materials ("<Unnamed>", "<Unnamed>", "Tür - Stahl Zarge", "Tür - Stahl Griff") | property sets: Drehflügel 1-flg - Stahlzarge:88.5 x 2.26:579164, Pset_DoorCommon, Pset_QuantityTakeOff
  IFCDOORSTYLE "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26" | SINGLE_SWING_LEFT | 3 occurrences | material: materials ("<Unnamed>", "Tür - Stahl Zarge", "<Unnamed>", "Tür - Stahl Griff") | property sets: Drehflügel 1-flg - Stahlzarge:88.5 x 2.26:579165, Pset_DoorCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Techo compuesto:Abgehängte Decke 5.0cm - 600 x 600" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
  IFCDOORSTYLE "Drehflügel 1-flg - Stahlzarge:88.5 x 2.26" | SINGLE_SWING_LEFT | 1 occurrence | material: materials ("<Unnamed>", "<Unnamed>", "Tür - Stahl Zarge", "Tür - Stahl Griff") | property sets: Drehflügel 1-flg - Stahlzarge:88.5 x 2.26:580927, Pset_DoorCommon, Pset_QuantityTakeOff
  IFCPIPEFITTINGTYPE "M_Bend - PVC - Sch 40 - DWV:Standard" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCPIPEFITTINGTYPE "M_Tee - Generic:Standard" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCPIPEFITTINGTYPE "M_Tee Sanitary - PVC - Sch 40 - DWV:Standard" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCPIPEFITTINGTYPE "M_Tee Sanitary - PVC - Sch 40 - DWV:Standard" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCPIPEFITTINGTYPE "M_Tee Sanitary - PVC - Sch 40 - DWV:Standard" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCPIPEFITTINGTYPE "M_Tee Sanitary - PVC - Sch 40 - DWV:Standard" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCPIPEFITTINGTYPE "M_Transition - Generic:Standard" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular to Round Duct Transition - Angle:45 Degree" | 2 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "M_Outdoor AHU - Horizontal:5.7 Square Meters of Coil" | 1 occurrence | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Elbow - Mitered:Standard" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Elbow - Mitered:Standard" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Elbow - Mitered:Standard" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Union:Standard" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "M_Cooling Tower - Closed Circuit - Counterflow - 67-189 kW:177 kW" | 1 occurrence | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
  IFCPIPEFITTINGTYPE "M_Pipe Transition:Standard" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCPIPEFITTINGTYPE "M_Pipe Elbow:Standard" | 2 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "M_Centrifugal Fan - Rooftop - Upblast:1383-2808 LPS" | 1 occurrence | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCPIPEFITTINGTYPE "M_Pipe Tee:Standard" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCPIPEFITTINGTYPE "M_Pipe Transition:Standard" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCPIPEFITTINGTYPE "M_Pipe Tee:Standard" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCPIPEFITTINGTYPE "M_Pipe Transition:Standard" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "M_Lighting and Appliance Panelboard - 480V MLO - Surface:400 A" | 1 occurrence | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff, Pset_ProvisionForVoid
  IFCBUILDINGELEMENTPROXYTYPE "M_Lighting and Appliance Panelboard - 208V MLO - Surface:400 A" | 1 occurrence | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff, Pset_ProvisionForVoid
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Transition - Angle:45 Degree" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCSLABTYPE "Suelo:STB 30.0" | FLOOR | 1 occurrence | material: layers "Suelo:STB 30.0" ("Stahlbeton - Ortbeton" 300.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Suelo:Sonnenschutz" | FLOOR | 1 occurrence | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Suelo:Sonnenschutz" | FLOOR | 1 occurrence | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Suelo:Sonnenschutz" | FLOOR | 1 occurrence | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Suelo:Sonnenschutz" | FLOOR | 1 occurrence | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Suelo:Sonnenschutz" | FLOOR | 1 occurrence | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Suelo:Sonnenschutz" | FLOOR | 1 occurrence | material: layers "Suelo:Sonnenschutz" ("Gitterrost" 100.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCCOLUMNTYPE "Strut:1.5" x 1.5"" | COLUMN | 4 occurrences | material: "<Unnamed>" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
  IFCDUCTFITTINGTYPE "M_Rectangular Duct Elbow - Mitered:Standard" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCPIPEFITTINGTYPE "M_Elbow - Generic:Standard" | 8 occurrences | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCPIPEFITTINGTYPE "M_Cap - Generic:Standard" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
  IFCPIPEFITTINGTYPE "M_Cap - Generic:Standard" | 1 occurrence | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff

Property sets
  Pset_DistributionFlowElementCommon | properties | on 1666 objects (1143 IFCFLOWFITTING, 488 IFCFLOWSEGMENT, 35 IFCFLOWTERMINAL) | on 194 type objects
    Reference = "Standard" (IFCIDENTIFIER)
  Pset_DistributionFlowElementCommon | properties | on 634 objects (634 IFCFLOWSEGMENT) | on 2 type objects
    Reference = "Mitered Elbows / Taps" (IFCIDENTIFIER)
  Pset_DistributionFlowElementCommon | properties | on 309 objects (309 IFCFLOWFITTING) | on 108 type objects
    Reference = "45 Degree" (IFCIDENTIFIER)
  Pset_DistributionFlowElementCommon | properties | on 195 objects (195 IFCFLOWTERMINAL) | on 1 type object
    Reference = "600x600 - 277" (IFCIDENTIFIER)
  Pset_DistributionFlowElementCommon | properties | on 113 objects (113 IFCFLOWSEGMENT) | on 2 type objects
    Reference = "Flex - Round" (IFCIDENTIFIER)
  Pset_DistributionFlowElementCommon | properties | on 108 objects (108 IFCFLOWTERMINAL) | on 11 type objects
    Reference = "600x600 - 250 Neck" (IFCIDENTIFIER)
  Pset_DistributionFlowElementCommon | properties | on 96 objects (96 IFCFLOWTERMINAL) | on 17 type objects
    Reference = "450 x 200" (IFCIDENTIFIER)
  Pset_DistributionFlowElementCommon | properties | on 85 objects (85 IFCFLOWSEGMENT) | on 2 type objects
    Reference = "Mitered Elbows / Tees" (IFCIDENTIFIER)
  Pset_DistributionFlowElementCommon: 14 more contents on 348 objects not shown
  Pset_QuantityTakeOff | properties | on 1702 objects (1143 IFCFLOWFITTING, 488 IFCFLOWSEGMENT, 35 IFCFLOWTERMINAL, 33 IFCCURTAINWALL) | on 195 type objects
    Reference = "Standard" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 1063 objects (1063 IFCMEMBER)
    Reference = "6 x 15 mit Deckprofil" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 634 objects (634 IFCFLOWSEGMENT) | on 2 type objects
    Reference = "Mitered Elbows / Taps" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 438 objects (438 IFCPLATE)
    Reference = "Verglasung" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 309 objects (309 IFCFLOWFITTING) | on 108 type objects
    Reference = "45 Degree" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 216 objects (216 IFCMEMBER)
    Reference = "6 x 12" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 195 objects (195 IFCFLOWTERMINAL) | on 1 type object
    Reference = "600x600 - 277" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 191 objects (191 IFCPLATE)
    Reference = "Metallpanel" (IFCIDENTIFIER)
  Pset_QuantityTakeOff: 60 more contents on 1842 objects not shown
  Pset_BuildingElementProxyCommon | properties | on 81 objects (81 IFCBUILDINGELEMENTPROXY) | on 2 type objects
    Reference = "Stahlbalkon" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 54 objects (54 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "Passive Infrared - 277 V" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 19 objects (19 IFCBUILDINGELEMENTPROXY) | on 15 type objects
    Reference = "11 kW" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 14 objects (14 IFCBUILDINGELEMENTPROXY) | on 12 type objects
    Reference = "14 kW" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 14 objects (14 IFCBUILDINGELEMENTPROXY) | on 5 type objects
    Reference = "400 A" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 9 objects (9 IFCBUILDINGELEMENTPROXY) | on 2 type objects
    Reference = "100 A" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 9 objects (9 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "Single Pole" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 8 objects (8 IFCBUILDINGELEMENTPROXY) | on 7 type objects
    Reference = "7 kW" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon: 11 more contents on 13 objects not shown
  Pset_DuctSegmentTypeCommon | properties | on 143 objects (143 IFCFLOWSEGMENT)
    Length = 249.999999999999 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    Shape in {"Rectangle"} (IFCLABEL)
  Pset_DuctSegmentTypeCommon | properties | on 138 objects (138 IFCFLOWSEGMENT)
    Length = 200. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    Shape in {"Rectangle"} (IFCLABEL)
  Pset_DuctSegmentTypeCommon | properties | on 54 objects (54 IFCFLOWSEGMENT)
    Length = 150.000000000001 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    Shape in {"Rectangle"} (IFCLABEL)
  Pset_DuctSegmentTypeCommon | properties | on 42 objects (42 IFCFLOWSEGMENT)
    Length = 300.000000000001 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    Shape in {"Rectangle"} (IFCLABEL)
  Pset_DuctSegmentTypeCommon | properties | on 39 objects (39 IFCFLOWSEGMENT)
    Length = 350.000000000001 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    Shape in {"Rectangle"} (IFCLABEL)
  Pset_DuctSegmentTypeCommon | properties | on 33 objects (33 IFCFLOWSEGMENT)
    Length = 300. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    Shape in {"Rectangle"} (IFCLABEL)
  Pset_DuctSegmentTypeCommon | properties | on 30 objects (30 IFCFLOWSEGMENT)
    Length = 250.000000000001 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    Shape in {"Rectangle"} (IFCLABEL)
  Pset_DuctSegmentTypeCommon | properties | on 26 objects (26 IFCFLOWSEGMENT)
    Length = 325. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    Shape in {"Rectangle"} (IFCLABEL)
  Pset_DuctSegmentTypeCommon: 67 more contents on 223 objects not shown
  Pset_FlowSegmentDuctSegment | properties | on 143 objects (143 IFCFLOWSEGMENT)
    Length = 249.999999999999 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentDuctSegment | properties | on 138 objects (138 IFCFLOWSEGMENT)
    Length = 200. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentDuctSegment | properties | on 54 objects (54 IFCFLOWSEGMENT)
    Length = 150.000000000001 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentDuctSegment | properties | on 43 objects (43 IFCFLOWSEGMENT)
    Length = 300.000000000001 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentDuctSegment | properties | on 39 objects (39 IFCFLOWSEGMENT)
    Length = 350.000000000001 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentDuctSegment | properties | on 35 objects (35 IFCFLOWSEGMENT)
    Length = 300. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentDuctSegment | properties | on 30 objects (30 IFCFLOWSEGMENT)
    Length = 250.000000000001 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentDuctSegment | properties | on 26 objects (26 IFCFLOWSEGMENT)
    Length = 325. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentDuctSegment: 461 more contents on 744 objects not shown
  Pset_FlowSegmentPipeSegment | properties | on 143 objects (143 IFCFLOWSEGMENT)
    Length = 249.999999999999 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentPipeSegment | properties | on 138 objects (138 IFCFLOWSEGMENT)
    Length = 200. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentPipeSegment | properties | on 54 objects (54 IFCFLOWSEGMENT)
    Length = 150.000000000001 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentPipeSegment | properties | on 43 objects (43 IFCFLOWSEGMENT)
    Length = 300.000000000001 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentPipeSegment | properties | on 39 objects (39 IFCFLOWSEGMENT)
    Length = 350.000000000001 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentPipeSegment | properties | on 35 objects (35 IFCFLOWSEGMENT)
    Length = 300. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentPipeSegment | properties | on 30 objects (30 IFCFLOWSEGMENT)
    Length = 250.000000000001 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentPipeSegment | properties | on 26 objects (26 IFCFLOWSEGMENT)
    Length = 325. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentPipeSegment: 461 more contents on 744 objects not shown
  Pset_ManufacturerTypeInformation | properties | on 5 objects (5 IFCBUILDINGELEMENTPROXY) | on 4 type objects
    Manufacturer = "ACME" (IFCLABEL)
  Pset_ProvisionForVoid | properties | on 7 objects (7 IFCBUILDINGELEMENTPROXY)
    Depth = 146.1 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    Height = 1346.2 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    Width = 508. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_ProvisionForVoid | properties | on 6 objects (6 IFCBUILDINGELEMENTPROXY)
    Depth = 146.1 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    Height = 965.2 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    Width = 508. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_ProvisionForVoid | properties | on 3 objects (3 IFCBUILDINGELEMENTPROXY)
    Depth = 146.1 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    Height = 584.2 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    Width = 508. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_ProvisionForVoid | properties | on 3 objects (3 IFCBUILDINGELEMENTPROXY)
    Depth = 146.1 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    Height = 1727.2 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    Width = 508. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_ProvisionForVoid | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    Depth = 146.1 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    Height = 1422.4 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    Width = 508. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_ProvisionForVoid | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    Depth = 146.1 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    Height = 1270. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    Width = 508. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_ProvisionForVoid | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Depth = 46.434374999969 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    Height = 69.3539062500087 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    Width = 46.434374999969 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_ProvisionForVoid | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Depth = 53.9750000000356 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    Height = 76.2000000000049 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    Width = 53.9750000000356 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_ProvisionForVoid: 7 more contents on 6 objects not shown
  Pset_ColumnCommon | properties | on 131 objects (131 IFCCOLUMN) | on 10 type objects
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "STB d=30" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 4 objects (4 IFCCOLUMN) | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "1.5" x 1.5"" (IFCIDENTIFIER)
  Pset_ReinforcementBarPitchOfColumn | properties | on 131 objects (131 IFCCOLUMN) | on 10 type objects
    Reference = "STB d=30" (IFCLABEL)
  Pset_ReinforcementBarPitchOfColumn | properties | on 4 objects (4 IFCCOLUMN) | on 1 type object
    Reference = "1.5" x 1.5"" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 61 objects (61 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "MW 11.5" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 29 objects (29 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "MW 17.5" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 18 objects (14 IFCWALLSTANDARDCASE, 4 IFCWALL) | on 1 type object
    Reference = "STB 20.0" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 8 objects (7 IFCWALLSTANDARDCASE, 1 IFCWALL) | on 1 type object
    Reference = "STB 30.0" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 7 objects (7 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "Lamelle 11.5" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 7 objects (7 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "WC Trennwand 5.0" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 2 objects (2 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "STB 30.0 Rot" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 1 object (1 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "STB 25.0 WD 12.0" (IFCLABEL)
  Pset_WallCommon | properties | on 61 objects (61 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "MW 11.5" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 29 objects (29 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "MW 17.5" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 18 objects (14 IFCWALLSTANDARDCASE, 4 IFCWALL)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "STB 20.0" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 8 objects (7 IFCWALLSTANDARDCASE, 1 IFCWALL)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "STB 30.0" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 7 objects (7 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Lamelle 11.5" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 7 objects (7 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "WC Trennwand 5.0" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 2 objects (2 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "STB 30.0 Rot" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "STB 25.0 WD 12.0" (IFCIDENTIFIER)
  Pset_WallCommon: 8 more contents on 0 objects not shown
  Pset_ReinforcementBarPitchOfSlab | properties | on 33 objects (33 IFCSLAB) | on 33 type objects
    Reference = "FB 15.0 - Teppich" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 18 objects (18 IFCSLAB) | on 18 type objects
    Reference = "Sonnenschutz" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 13 objects (13 IFCSLAB) | on 13 type objects
    Reference = "FB 10.0 - Fliesen 15 x 15" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 7 objects (7 IFCSLAB) | on 7 type objects
    Reference = "FB 15.0 - Holzdielen" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 4 objects (4 IFCSLAB) | on 4 type objects
    Reference = "STB 30.0" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 4 objects (4 IFCSLAB) | on 4 type objects
    Reference = "FB 15.0 - Fliesen 50 x 50" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 4 objects (4 IFCSLAB)
    Reference = "Massiv - Stufen Naturstein" (IFCLABEL)
  Pset_SlabCommon | properties | on 33 objects (33 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "FB 15.0 - Teppich" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 18 objects (18 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Sonnenschutz" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 13 objects (13 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "FB 10.0 - Fliesen 15 x 15" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 7 objects (7 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "FB 15.0 - Holzdielen" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 4 objects (4 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "STB 30.0" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 4 objects (4 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "FB 15.0 - Fliesen 50 x 50" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 4 objects (4 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Massiv - Stufen Naturstein" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 33 type objects
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "FB 15.0 - Teppich" (IFCIDENTIFIER)
  Pset_SlabCommon: 5 more contents on 0 objects not shown
  Pset_OpeningElementCommon | properties | on 45 objects (45 IFCOPENINGELEMENT)
    Reference = "FB 15.0 - Teppich" (IFCIDENTIFIER)
  Pset_OpeningElementCommon | properties | on 44 objects (44 IFCOPENINGELEMENT)
    Reference = "FB 15.0 - Fliesen 50 x 50" (IFCIDENTIFIER)
  Pset_OpeningElementCommon | properties | on 20 objects (20 IFCOPENINGELEMENT)
    Reference = "FB 15.0 - Holzdielen" (IFCIDENTIFIER)
  Pset_OpeningElementCommon | properties | on 11 objects (11 IFCOPENINGELEMENT)
    Reference = "STB 30.0" (IFCIDENTIFIER)
  Pset_OpeningElementCommon | properties | on 9 objects (9 IFCOPENINGELEMENT)
    Reference = "STB 20.0" (IFCIDENTIFIER)
  Pset_OpeningElementCommon | properties | on 6 objects (3 IFCCURTAINWALL, 3 IFCOPENINGELEMENT)
    Reference = "Standard" (IFCIDENTIFIER)
  Pset_OpeningElementCommon | properties | on 6 objects (3 IFCBUILDINGELEMENTPROXY, 3 IFCOPENINGELEMENT)
    Reference = "Aufzug 2-flg" (IFCIDENTIFIER)
  Pset_OpeningElementCommon | properties | on 4 objects (4 IFCOPENINGELEMENT)
    Reference = "MW 11.5" (IFCIDENTIFIER)
  Pset_OpeningElementCommon: 2 more contents on 3 objects not shown
  Pset_DoorCommon | properties | on 95 objects (95 IFCDOOR) | on 11 type objects
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "88.5 x 2.26" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 12 objects (12 IFCDOOR) | on 7 type objects
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "76 x 2.26" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 11 objects (11 IFCDOOR)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Türelement 1-flg - Drehflügel - Glas" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 6 objects (6 IFCDOOR)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Türelement 2-flg - Drehflügel - Glas" (IFCIDENTIFIER)
  Pset_PlateCommon | properties | on 438 objects (438 IFCPLATE)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Verglasung" (IFCIDENTIFIER)
  Pset_PlateCommon | properties | on 191 objects (191 IFCPLATE)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Metallpanel" (IFCIDENTIFIER)
  Pset_MemberCommon | properties | on 331 objects (331 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "6 x 15 mit Deckprofil" (IFCIDENTIFIER)
    Span = 1940. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_MemberCommon | properties | on 123 objects (123 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "6 x 15 mit Deckprofil" (IFCIDENTIFIER)
    Span = 2910. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_MemberCommon | properties | on 108 objects (108 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "6 x 15 mit Deckprofil" (IFCIDENTIFIER)
    Span = 3000.06434845531 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_MemberCommon | properties | on 50 objects (50 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "6 x 15 mit Deckprofil" (IFCIDENTIFIER)
    Span = 3110. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_MemberCommon | properties | on 44 objects (44 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "6 x 10 mit Deckprofil" (IFCIDENTIFIER)
    Span = 500. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_MemberCommon | properties | on 36 objects (36 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "6 x 10 mit Deckprofil" (IFCIDENTIFIER)
    Span = 499.999999999999 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_MemberCommon | properties | on 30 objects (30 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "6 x 10 mit Deckprofil" (IFCIDENTIFIER)
    Span = 3500.5710622249 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_MemberCommon | properties | on 29 objects (29 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "6 x 15 mit Deckprofil" (IFCIDENTIFIER)
    Span = 3010. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_MemberCommon: 119 more contents on 699 objects not shown
  Pset_CurtainWallCommon | properties | on 30 objects (30 IFCCURTAINWALL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Standard" (IFCIDENTIFIER)
  Pset_CurtainWallCommon | properties | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Standard" (IFCIDENTIFIER)
  Pset_StairFlightCommon | properties | on 4 objects (4 IFCSTAIRFLIGHT)
    NosingLength = 282.063974940805 (IFCLENGTHMEASURE) [MILLI METRE]
    NumberOfRiser = 21. (IFCCOUNTMEASURE)
    NumberOfTreads = 21. (IFCCOUNTMEASURE)
    Reference = "Massiv - Stufen Naturstein" (IFCIDENTIFIER)
    RiserHeight = 176.468012529597 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    TreadLength = 282.063974940805 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    TreadLengthAtInnerSide = 30. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    TreadLengthAtOffset = 282.063974940805 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    WalkingLineOffset = 800. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_StairFlightCommon | properties | on 4 objects (4 IFCSTAIRFLIGHT)
    NosingLength = 285. (IFCLENGTHMEASURE) [MILLI METRE]
    NumberOfRiser = 20. (IFCCOUNTMEASURE)
    NumberOfTreads = 20. (IFCCOUNTMEASURE)
    Reference = "Massiv - Stufen Naturstein" (IFCIDENTIFIER)
    RiserHeight = 175. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    TreadLength = 285. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    TreadLengthAtInnerSide = 30. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    TreadLengthAtOffset = 285. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    WalkingLineOffset = 800. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_StairCommon | properties | on 4 objects (4 IFCSTAIR)
    IsExternal = FALSE (IFCBOOLEAN)
    NumberOfRiser = 21. (IFCCOUNTMEASURE)
    NumberOfTreads = 21. (IFCCOUNTMEASURE)
    Reference = "Massiv - Stufen Naturstein" (IFCIDENTIFIER)
    RiserHeight = 176.468012529597 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    TreadLength = 282.063974940805 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_StairCommon | properties | on 2 objects (2 IFCSTAIR)
    IsExternal = FALSE (IFCBOOLEAN)
    NumberOfRiser = 20. (IFCCOUNTMEASURE)
    NumberOfTreads = 20. (IFCCOUNTMEASURE)
    Reference = "Massiv - Stufen Naturstein" (IFCIDENTIFIER)
    RiserHeight = 175. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    TreadLength = 285. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_StairCommon | properties | on 1 object (1 IFCSTAIR)
    IsExternal = FALSE (IFCBOOLEAN)
    NumberOfRiser = 21. (IFCCOUNTMEASURE)
    NumberOfTreads = 21. (IFCCOUNTMEASURE)
    Reference = "Massiv - Stufen Naturstein" (IFCIDENTIFIER)
    RiserHeight = 169.32515538674 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    TreadLength = 296.349689226519 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_StairCommon | properties | on 1 object (1 IFCSTAIR)
    IsExternal = FALSE (IFCBOOLEAN)
    NumberOfRiser = 18. (IFCCOUNTMEASURE)
    NumberOfTreads = 18. (IFCCOUNTMEASURE)
    Reference = "Massiv - Stufen Naturstein" (IFCIDENTIFIER)
    RiserHeight = 194.444444444444 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    TreadLength = 246.111111111111 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_CoveringCommon | properties | on 43 objects (43 IFCCOVERING)
    Finish = "Decke - Deckenraster;" (IFCTEXT)
    Reference = "Abgehängte Decke 5.0cm - 600 x 600" (IFCIDENTIFIER)
    TotalThickness = 50. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_CoveringCommon | properties | on 43 type objects
    Reference = "Abgehängte Decke 5.0cm - 600 x 600" (IFCIDENTIFIER)
    TotalThickness = 50. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_RailingCommon | properties | on 14 objects (14 IFCRAILING)
    Height = 1219.2 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Stahl (1) - Horizontal" (IFCIDENTIFIER)
  Pset_BuildingStoreyCommon | properties | on 4 objects (4 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 4 (IFCINTEGER)
  Drehflügel 1-flg - Stahlzarge:88.5 x 2.26:573577 | predefined | on 2 type objects
  Drehflügel 1-flg - Stahlzarge:88.5 x 2.26:573583 | predefined | on 2 type objects
  Drehflügel 1-flg - Stahlzarge:88.5 x 2.26:573668 | predefined | on 2 type objects
  Drehflügel 1-flg - Stahlzarge:88.5 x 2.26:573673 | predefined | on 2 type objects
  Drehflügel 1-flg - Stahlzarge:76 x 2.26:573783 | predefined | on 2 type objects
  Drehflügel 1-flg - Stahlzarge:88.5 x 2.26:575087 | predefined | on 2 type objects
  Drehflügel 1-flg - Stahlzarge:88.5 x 2.26:575089 | predefined | on 2 type objects
  Drehflügel 1-flg - Stahlzarge:88.5 x 2.26:573747 | predefined | on 2 type objects
  Drehflügel 1-flg - Stahlzarge:88.5 x 2.26:573748 | predefined | on 2 type objects
  Drehflügel 1-flg - Stahlzarge:76 x 2.26:578641 | predefined | on 2 type objects
  Drehflügel 1-flg - Stahlzarge:76 x 2.26:578643 | predefined | on 2 type objects
  Drehflügel 1-flg - Stahlzarge:76 x 2.26:573721 | predefined | on 2 type objects
  Drehflügel 1-flg - Stahlzarge:76 x 2.26:573722 | predefined | on 2 type objects
  Drehflügel 1-flg - Stahlzarge:76 x 2.26:573723 | predefined | on 2 type objects
  Drehflügel 1-flg - Stahlzarge:76 x 2.26:573724 | predefined | on 2 type objects
  Drehflügel 1-flg - Stahlzarge:88.5 x 2.26:579164 | predefined | on 2 type objects
  Drehflügel 1-flg - Stahlzarge:88.5 x 2.26:579165 | predefined | on 2 type objects
  Drehflügel 1-flg - Stahlzarge:88.5 x 2.26:580927 | predefined | on 2 type objects